{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3095,"n_cols":12,"rows_kept":3095,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1604","UTC to Local: ",{"$f":"12","v":12},11,10,null,"Wake Island Mapping - 3/23/2016 to 4/13/2016"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
["UTC Time","Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2016-03-23T00:18:30",{"$f":"((A5)-DATE(1970,1,1))+25569+($C$1/24)","v":"2016-03-23T12:18:30"},"WP","Sonar","Multibeam","New Line","Pinging and Logging, Line 0000, Depart Kwaj"]
["2016-03-23T01:38:31.970","2016-03-23T13:38:31.970","wp","sonar","Multibeam",null,"Marine Mammel protection switched from ON to OFF"]
["2016-03-23T01:58:43.730","2016-03-23T13:58:43.730","DS","XBT",null,null,"XBT cast 01 completed"]
["2016-03-23T02:00:25","2016-03-23T14:00:25","DS","XBT",null,null,"XBT cast 01 applied to line 004"]
["2016-03-23T03:00:55.560","2016-03-23T15:00:55.560","BG","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-23T03:10:45.490","2016-03-23T15:10:45.490","BG","Sonar","Knudsen","Tx Power","1"]
["2016-03-23T03:19:41.030","2016-03-23T15:19:41.030","BG","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-03-23T03:33:17.640","2016-03-23T15:33:17.640","DF","Sonar","Multibeam",null,"Spike filter strength at MED, slope filter is on and sector tracking is on"]
["2016-03-23T03:43:27.060","2016-03-23T15:43:27.060","BG","sonar","Knudsen","Phase Range","2000-2500"]
["2016-03-23T03:56:41.500","2016-03-23T15:56:41.500","BG","Sonar","Multibeam","New Line","started new line for turn, 0006"]
["2016-03-23T03:57:26.470","2016-03-23T15:57:26.470","BG","Sonar","Knudsen","Phase Range","1750-2250"]
["2016-03-23T04:09:28.870","2016-03-23T16:09:28.870","DF","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-03-23T04:18:56.220","2016-03-23T16:18:56.220","DF","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-03-23T04:20:20.370","2016-03-23T16:20:20.370","DF","Sonar","Multibeam","New Line","Ended turn line 0006, started line 0007"]
["2016-03-23T04:58:58.100","2016-03-23T16:58:58.100","BG","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-23T05:17:04.480","2016-03-23T17:17:04.480","DF","Issue/Problem",null,null,"POS-MV UTC time keeps freezing sparatically; Ext. Date, Ext. Time, PU - ZDA are all red in SIS with Ext. Date flashing red, Status lamp 1 is red"]
["2016-03-23T05:26:55.020","2016-03-23T17:26:55.020","DF","Sonar","Multibeam",null,"Penetration filter on weak"]
["2016-03-23T05:27:41.280","2016-03-23T17:27:41.280","DS","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-03-23T05:29:40.630","2016-03-23T17:29:40.630","DF","Sonar","Multibeam","Max Angle","55/50"]
["2016-03-23T05:37:38.600",{"$f":"IF(ISBLANK(A24), \" \", ((A24)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-23T17:37:38.600"},"DF","Sonar","Multibeam",null,"Lost signal of POS-MV to the Multibeam, stopped pinging and logging"]
["2016-03-23T05:40:45.480","2016-03-23T17:40:45.480","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-23T05:41:41","2016-03-23T17:41:41","DF","Sonar","Multibeam","Start Pinging"]
["2016-03-23T05:43:12.640","2016-03-23T17:43:12.640","DF","Sonar","Multibeam",null,"Started logging"]
["2016-03-23T06:08:01.250","2016-03-23T18:08:01.250","BG","sonar","Knudsen","Phase Range","2250-2750"]
["2016-03-23T06:29:06.950","2016-03-23T18:29:06.950","DF","Sonar","Multibeam",null,"UTC time freeze on POS-MV again"]
["2016-03-23T06:33:05.060","2016-03-23T18:33:05.060","BG","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-03-23T06:52:19.210","2016-03-23T18:52:19.210","DF","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-03-23T06:54:17.650","2016-03-23T18:54:17.650","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-23T06:55:19.690","2016-03-23T18:55:19.690","DF","Sonar",null,null,"Knudsen and EK60 started recording, were not recording when pinging started"]
["2016-03-23T06:56:43.940","2016-03-23T18:56:43.940","DF","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-03-23T07:03:01.500","2016-03-23T19:03:01.500","DF","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-03-23T07:09:07.110","2016-03-23T19:09:07.110","DF","Sonar","Multibeam","New Line","started new line to end turn, 0011 started new survey line 0012"]
["2016-03-23T07:20:45.060","2016-03-23T19:20:45.060","DF","Sonar","Knudsen","Phase Range","3250-3750"]
["2016-03-23T08:05:44.200","2016-03-23T20:05:44.200","DS","XBT",null,null,"XBT #002 applied to line 0012. "]
["2016-03-23T08:13:34.150","2016-03-23T20:13:34.150","DF","Sonar","Multibeam",null,"Penetration filter on off"]
["2016-03-23T08:15:56.480","2016-03-23T20:15:56.480","DF","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-03-23T08:18:33.690","2016-03-23T20:18:33.690","DF","Sonar","Multibeam","Ping Mode","DEEP"]
["2016-03-23T08:19:32.300","2016-03-23T20:19:32.300","DF","Sonar","Multibeam","Spike Filter Strength","Strong"]
["2016-03-23T08:21:46.340","2016-03-23T20:21:46.340","DF","Sonar","Multibeam","Along Direction Pitch","-2"]
["2016-03-23T08:22:49.640","2016-03-23T20:22:49.640","DF","Sonar","Knudsen","Phase Range","3250-3750"]
["2016-03-23T08:26:17.240","2016-03-23T20:26:17.240","DF","Sonar","Knudsen","Phase Range","3000-3500, TX Power to 2"]
["2016-03-23T08:29:04.810","2016-03-23T20:29:04.810","DF","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-03-23T08:35:48.470","2016-03-23T20:35:48.470","DF","Sonar","Multibeam","Ping Mode","VERY DEEP, trouble tracking bottom"]
["2016-03-23T08:37:09.370","2016-03-23T20:37:09.370","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-23T08:42:06.490","2016-03-23T20:42:06.490","DF","Sonar","Multibeam","Ping Mode","DEEP"]
["2016-03-23T08:43:48.060","2016-03-23T20:43:48.060","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-23T09:07:51.190","2016-03-23T21:07:51.190","DF","Ship",null,null,"Had ship move 500 m to STBD for better overlap; swath with is reduced due to bad bottom tracking"]
["2016-03-23T09:13:43.260","2016-03-23T21:13:43.260","DF","Sonar","Multibeam",null,"Geographical window randomly stopped showing data but the points were still being collected, fixed by selecting different window and then going back to geographical"]
["2016-03-23T09:33:16.220","2016-03-23T21:33:16.220","DF","Sonar","Multibeam","New Line","Started new line for turn, 0015"]
["2016-03-23T09:37:39.350","2016-03-23T21:37:39.350","DS","Sonar","Knudsen","Gain Mode","turned of time varying gain (TVG), manual gain to 38 dB"]
["2016-03-23T09:46:28.570","2016-03-23T21:46:28.570","DF",null,null,null,"POS-MV UTC time continues to freeze"]
["2016-03-23T09:48:05.660",{"$f":"IF(ISBLANK(A56), \" \", ((A56)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-23T21:48:05.660"},"DF","sonar","Multibeam","Max Angle","45/45"]
["2016-03-23T09:59:40.040","2016-03-23T21:59:40.040","DF","Sonar","Multibeam","New Line","cont. line for end of turn 0015, started track line 0016"]
["2016-03-23T10:01:20.010","2016-03-23T22:01:20.010","DF","Ship",null,null,"Asked bridge to move 500 m to PORT to increase overlap"]
["2016-03-23T10:02:26.090","2016-03-23T22:02:26.090","DF","Sonar","Knudsen","Phase Range","3250-3750"]
["2016-03-23T10:03:26.740","2016-03-23T22:03:26.740","DF","Sonar","Multibeam","Max Angle","45/30"]
["2016-03-23T10:04:52.300","2016-03-23T22:04:52.300","DF","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-03-23T10:06:34.890","2016-03-23T22:06:34.890","DF","Sonar","Knudsen","Range","1000 m, started new line"]
["2016-03-23T10:09:42.990","2016-03-23T22:09:42.990","DF","sonar","Knudsen","Tx Power","3, could not maintain bottom very well"]
["2016-03-23T10:12:46.760","2016-03-23T22:12:46.760","DF","Sonar","Knudsen","Tx Power","2"]
["2016-03-23T11:03:04.720","2016-03-23T23:03:04.720","AB","Sonar","Knudsen","Range","3500-4500m"]
["2016-03-23T11:04:29.390","2016-03-23T23:04:29.390","AB","Sonar","Multibeam","Max Angle","50/50"]
["2016-03-23T11:12:57.650","2016-03-23T23:12:57.650","AB","Sonar","Multibeam","Max Angle","50/40"]
["2016-03-23T11:16:24.010","2016-03-23T23:16:24.010","AB","Sonar","Multibeam","Max Angle","50/35"]
["2016-03-23T11:48:02.910","2016-03-23T23:48:02.910","AB","Ship",null,null,"Shifting 500m to Starboard to come back on Hypck trackline"]
["2016-03-23T12:00:08.100","2016-03-24T00:00:08.100","AB","Sonar","Multibeam","Max Angle","52/45"]
["2016-03-23T12:05:10.310","2016-03-24T00:05:10.310","AB","Sonar","Multibeam","New Line","0018"]
["2016-03-23T12:05:30.080","2016-03-24T00:05:30.080","AB","Sonar","Knudsen","Gain Mode","37"]
["2016-03-23T12:19:28.880","2016-03-24T00:19:28.880","AB","Sonar","Knudsen","Gain Mode","40"]
["2016-03-23T13:01:29.040","2016-03-24T01:01:29.040","AB","Sonar","Multibeam","New Line","0019"]
["2016-03-23T13:01:58.440","2016-03-24T01:01:58.440","AB","Sonar","Knudsen","Range","3000-4000m"]
["2016-03-23T13:45:17.610","2016-03-24T01:45:17.610","SM","Sonar","Multibeam","New Line","0020"]
["2016-03-23T14:11:42.170","2016-03-24T02:11:42.170","AB","XBT",null,null,"0003"]
["2016-03-23T14:12:20.940","2016-03-24T02:12:20.940","AB","Sonar","Knudsen"]
["2016-03-23T14:14:50.310","2016-03-24T02:14:50.310","AB","Sonar","Multibeam","Max Angle","60/60"]
["2016-03-23T14:17:24.990","2016-03-24T02:17:24.990","AB","Sonar","Multibeam","New Line","XBT #3 Added to Line 0021"]
["2016-03-23T14:28:17.960","2016-03-24T02:28:17.960","AB","Sonar","Multibeam","Ping Mode","Deep, New line 0022, Slope off"]
["2016-03-23T15:08:34.560","2016-03-24T03:08:34.560","AB","Sonar","Multibeam","New Line","0023"]
["2016-03-23T15:08:56.980","2016-03-24T03:08:56.980","AB","Issue/Problem",null,null,"PPS Outage"]
["2016-03-23T15:20:21.990","2016-03-24T03:20:21.990","AB","Sonar","Multibeam","New Line","0024 - turn complete"]
["2016-03-23T15:21:08.330","2016-03-24T03:21:08.330","AB","Issue/Problem",null,null,"Lost heading to 0.23 deg accuracy"]
["2016-03-23T15:25:42.810","2016-03-24T03:25:42.810","AB","Issue/Problem",null,null,"PSS Working on POS - still adjusting in EM302"]
["2016-03-23T15:40:48.670","2016-03-24T03:40:48.670","AB","Issue/Problem",null,null,"PSS Out"]
["2016-03-23T15:54:59.090",{"$f":"IF(ISBLANK(A88), \" \", ((A88)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-24T03:54:59.090"},"AB","Sonar","Knudsen","Range","2000-3000m"]
["2016-03-23T16:00:35.640","2016-03-24T04:00:35.640","CA","Sonar","Knudsen","Tx Power","2, started new line"]
["2016-03-23T16:17:53.030",null,"AB","Sonar","Knudsen","Range","3500-4500m"]
["2016-03-23T16:39:05.410",{"$f":"IF(ISBLANK(A91), \" \", ((A91)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-24T04:39:05.410"},"AB","Issue/Problem",null,null,"PPS In"]
["2016-03-23T16:42:23.020","2016-03-24T04:42:23.020","AB","Sonar","Multibeam","New Line","0025 - turn"]
["2016-03-23T16:44:53.020","2016-03-24T04:44:53.020","AB","Sonar","Multibeam","New Line","0026, 0027"]
["2016-03-23T17:04:56.270","2016-03-24T05:04:56.270","AB","Sonar","Multibeam","Max Angle","45/50"]
["2016-03-23T17:08:31.300","2016-03-24T05:08:31.300","AB","Issue/Problem",null,null,"PPS Outage"]
["2016-03-23T17:08:59.080","2016-03-24T05:08:59.080","AB",null,null,null,"PPS Ok"]
["2016-03-23T17:11:24.810","2016-03-24T05:11:24.810","AB","Sonar","Knudsen","Range","3000-4000m"]
["2016-03-23T17:26:06.620","2016-03-24T05:26:06.620","AB","Issue/Problem",null,null,"PPS Outage"]
["2016-03-23T17:41:21.410","2016-03-24T05:41:21.410","AB",null,null,null,"PPS Ok"]
["2016-03-23T17:41:38.090","2016-03-24T05:41:38.090","AB","Sonar","Multibeam","New Line","0028"]
["2016-03-23T17:56:20.260","2016-03-24T05:56:20.260","AB","Sonar","Multibeam","New Line","0029 - turn"]
["2016-03-23T17:57:32.630","2016-03-24T05:57:32.630","AB","Sonar","Multibeam","New Line","0030"]
["2016-03-23T18:15:40.860","2016-03-24T06:15:40.860","AB","Issue/Problem",null,null,"PPS Outage"]
["2016-03-23T18:28:33.620","2016-03-24T06:28:33.620","AB","Sonar","Knudsen","Range","3000-4000m"]
["2016-03-23T18:29:31.190","2016-03-24T06:29:31.190","AB",null,null,null,"PPS Outage"]
["2016-03-23T18:43:53.770","2016-03-24T06:43:53.770","DS","Sonar","Knudsen","Phase Range","2500-3500, watch change"]
["2016-03-23T18:51:57.850","2016-03-24T06:51:57.850","DS","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-23T18:52:41.170","2016-03-24T06:52:41.170","DS","Sonar","Multibeam",null,"PPS errors stopped"]
["2016-03-23T18:56:28.340","2016-03-24T06:56:28.340","DS","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-23T19:06:19.160","2016-03-24T07:06:19.160","CR","Sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-23T19:09:39.870","2016-03-24T07:09:39.870","DS","sonar","Multibeam",null,"PPS Problems intermittent"]
["2016-03-23T19:36:18.830","2016-03-24T07:36:18.830","CR","Sonar","Knudsen","Phase Range","500-1500"]
["2016-03-23T20:13:16.610","2016-03-24T08:13:16.610","WP","Sonar",null,null,"Secured Knudsen and EK60 secure for transit into Kwaj."]
["2016-03-23T21:00:21.640","2016-03-24T09:00:21.640","DS","Sonar","Multibeam","Secure","secured MB near Echo Pier in Kwajalein at 25m."]
["2016-03-24T01:05:14.550","2016-03-24T13:05:14.550","WP","Sonar","Multibeam","Ping Mode","Line 0034, Max Angle 75/75, Very Shallow Mode"]
["2016-03-24T01:29:04.500","2016-03-24T13:29:04.500","WP","Sonar","Multibeam","Ping Mode","Stopped logging, Pilot derparting, leaving Kwajalein"]
["2016-03-24T01:36:36.260","2016-03-24T13:36:36.260","WP","Sonar","Multibeam","Ping Mode","Started Logging, "]
["2016-03-24T02:39:03.640","2016-03-24T14:39:03.640","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-24T02:39:17.720","2016-03-24T14:39:17.720","DF","Sonar",null,null,"Started logging EK60 and Knudsen, Knudsen TX Pulse to 2 and power to 1"]
["2016-03-24T02:45:01.460","2016-03-24T14:45:01.460","DF","Sonar","Knudsen","Tx Pulse","1 ms"]
["2016-03-24T02:50:01.150","2016-03-24T14:50:01.150","DF","Sonar","Multibeam",null,"Line 0036 is a turn line"]
["2016-03-24T03:01:26.010","2016-03-24T15:01:26.010","DF","Sonar","Knudsen","Tx Pulse","2 ms"]
["2016-03-24T03:11:01.050","2016-03-24T15:11:01.050","DF","Sonar","Ek","Change Range","Max recording range to 5000 m"]
["2016-03-24T03:24:24.560","2016-03-24T15:24:24.560","DF","Sonar","Multibeam",null,"PPS Errors continue"]
["2016-03-24T03:25:38.380","2016-03-24T15:25:38.380","DF","Sonar","Knudsen","Range","500 m, started new line, Phase Range at 1000-1500"]
["2016-03-24T03:34:01.830","2016-03-24T15:34:01.830","DF","Sonar","Knudsen",null,"Phase Range to 1250-1750, TX Power to 2"]
["2016-03-24T03:38:41.350","2016-03-24T15:38:41.350","DF",null,null,null,"Heading lamp on POS-MV is out, Lost primary receiver entirely, passing by end of Kwaj"]
["2016-03-24T03:42:32.020","2016-03-24T15:42:32.020","DF","Sonar","Knudsen","Phase Range","1000-1500"]
["2016-03-24T03:48:47.800","2016-03-24T15:48:47.800","DF","Sonar","Knudsen","Phase Range","750-1250"]
["2016-03-24T03:51:38.360","2016-03-24T15:51:38.360","DF","xbt",null,null,"cast called by itself, will pull in fishing lines and try again"]
["2016-03-24T03:52:37.610","2016-03-24T15:52:37.610","DF","Sonar","Knudsen",null,"TX power to 1 and Tx pulse to 1"]
["2016-03-24T04:00:31.870","2016-03-24T16:00:31.870","DF","xbt",null,null,"Cast 004 collected"]
["2016-03-24T04:04:31.630","2016-03-24T16:04:31.630","DF","Sonar","Knudsen","Phase Range","1000-1500"]
["2016-03-24T04:06:34.760","2016-03-24T16:06:34.760","BG","xbt",null,null,"cast 004 applied to line 0038, started line 0039"]
["2016-03-24T04:12:43.200","2016-03-24T16:12:43.200",null,"Sonar","Knudsen","Phase Range","1500-2000m"]
["2016-03-24T04:13:00.330","2016-03-24T16:13:00.330",null,"Sonar","Multibeam","New Line","0040, turn"]
["2016-03-24T04:23:18.330","2016-03-24T16:23:18.330","DF","Sonar","Knudsen","Phase Range","1750-2250"]
["2016-03-24T04:26:41.250","2016-03-24T16:26:41.250","DF","Sonar","Multibeam","Max Angle","65/65"]
["2016-03-24T04:29:56.990","2016-03-24T16:29:56.990","DF","Sonar","Multibeam","Max Angle","70/55"]
["2016-03-24T04:30:16.670","2016-03-24T16:30:16.670","DF","Sonar","Multibeam","Ping Mode","DEEP"]
["2016-03-24T04:32:40.790","2016-03-24T16:32:40.790","DF","Sonar","Knudsen","Phase Range","2000-2500, TX Pulse to 2 ms and TX Power to 2"]
["2016-03-24T04:34:05.230","2016-03-24T16:34:05.230","DF","Sonar","EK","Change Range","Max recording range to 5500 m"]
["2016-03-24T04:35:00.560","2016-03-24T16:35:00.560","DF","Sonar","Multibeam","Max Angle","70/50"]
["2016-03-24T04:43:37.610","2016-03-24T16:43:37.610","BG","sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-24T04:47:00.730","2016-03-24T16:47:00.730","DS","Sonar","Multibeam","New Line","turn line 0041"]
["2016-03-24T04:47:34.010","2016-03-24T16:47:34.010","DS","Sonar","Multibeam","Along Direction Pitch","reduced from -2 to -1"]
["2016-03-24T04:49:55.600","2016-03-24T16:49:55.600","DS","Sonar","EK","Change Range","on 18 kHz from 4000m t0 3500m"]
["2016-03-24T04:52:11.480","2016-03-24T16:52:11.480","DS","Sonar","Multibeam","Ping Mode","from Deep to Auto"]
["2016-03-24T04:52:24.940","2016-03-24T16:52:24.940","DS","Sonar","Multibeam","New Line","transit line 0042"]
["2016-03-24T04:56:33.560","2016-03-24T16:56:33.560","BG","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-03-24T05:09:24.560","2016-03-24T17:09:24.560","DF","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-03-24T05:16:38.380","2016-03-24T17:16:38.380","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2016-03-24T05:20:14.340","2016-03-24T17:20:14.340","DF","Sonar","Multibeam","Max Angle","52/50"]
["2016-03-24T05:35:19.980","2016-03-24T17:35:19.980","DF","Sonar","Multibeam","Spike Filter Strength","Strong"]
["2016-03-24T05:36:42.280",{"$f":"IF(ISBLANK(A155), \" \", ((A155)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-24T17:36:42.280"},"DF","Sonar","Multibeam","Max Angle","55/50"]
["2016-03-24T05:42:06.050","2016-03-24T17:42:06.050","DF","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-03-24T05:42:50.850","2016-03-24T17:42:50.850","DF","Sonar","Multibeam","Max Angle","55/45"]
["2016-03-24T05:50:38.620","2016-03-24T17:50:38.620","DF","Sonar","Multibeam","Slope Filter (On/Off)","on"]
["2016-03-24T05:53:21.270","2016-03-24T17:53:21.270","DF","Sonar","Multibeam","Max Angle","65/45"]
["2016-03-24T05:55:56.230","2016-03-24T17:55:56.230","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-24T05:58:20.950","2016-03-24T17:58:20.950","DF","sonar","Multibeam","Max Angle","65/50"]
["2016-03-24T06:03:06.910","2016-03-24T18:03:06.910","DF","Sonar","Multibeam","Slope Filter (On/Off)","off"]
["2016-03-24T06:10:42.110","2016-03-24T18:10:42.110","DF","Sonar","Multibeam","Ping Mode","VERY DEEP, trouble tracking bottom"]
["2016-03-24T06:12:59.940","2016-03-24T18:12:59.940","DF","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-03-24T06:14:19.490","2016-03-24T18:14:19.490","DF","Sonar","Knudsen","Range","1000, Phase range 2500-3500"]
["2016-03-24T06:16:55.490","2016-03-24T18:16:55.490","DF","Sonar","Multibeam","Aeration Filter (On/Off)","On"]
["2016-03-24T06:19:10.980","2016-03-24T18:19:10.980","DF","Sonar","Multibeam","Along Direction Pitch",-2]
["2016-03-24T06:42:43.930","2016-03-24T18:42:43.930","DF","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-24T06:46:08.920","2016-03-24T18:46:08.920","DF","Sonar","Multibeam","Max Angle","50/50"]
["2016-03-24T06:47:42.820","2016-03-24T18:47:42.820","DF","Sonar","Multibeam","Max Angle","50/45"]
["2016-03-24T07:24:41.970","2016-03-24T19:24:41.970","DF","Sonar","Multibeam","Max Angle","45/40"]
["2016-03-24T07:26:40.100","2016-03-24T19:26:40.100","DF","Sonar","Multibeam","Ping Mode","DEEP"]
["2016-03-24T07:30:32.690","2016-03-24T19:30:32.690","DF","Sonar","Multibeam",null,"Trouble tracking bottom with even slight changes in depth, causing drop out in bottom tracking and penetration artifacts at nadir and sector boundaries"]
["2016-03-24T07:32:42.030","2016-03-24T19:32:42.030","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-24T07:35:01.200","2016-03-24T19:35:01.200","DF","Sonar","Multibeam","Max Angle","50/40"]
["2016-03-24T07:36:42.230","2016-03-24T19:36:42.230","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-24T07:37:15.640","2016-03-24T19:37:15.640","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2016-03-24T07:38:34.250","2016-03-24T19:38:34.250","DF","Sonar","Multibeam","Max Angle","45/40"]
["2016-03-24T07:47:31.100","2016-03-24T19:47:31.100","DF","Sonar","Multibeam","Max Angle","50/45"]
["2016-03-24T07:47:58.310","2016-03-24T19:47:58.310","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-24T07:51:59.420","2016-03-24T19:51:59.420","DF","Sonar","Multibeam","Max Angle","60/50"]
["2016-03-24T07:52:44.290","2016-03-24T19:52:44.290","DF","Sonar","Multibeam","Max Angle","60/60"]
["2016-03-24T07:53:28.750","2016-03-24T19:53:28.750","DF","Sonar","Multibeam","Max Angle","65/50"]
["2016-03-24T08:04:07.860","2016-03-24T20:04:07.860","DF","Sonar","Multibeam","Max Angle","65/45"]
["2016-03-24T08:12:15.160","2016-03-24T20:12:15.160","DF","Sonar","Multibeam","Max Angle","55/45"]
["2016-03-24T08:13:34.270","2016-03-24T20:13:34.270","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-03-24T08:14:01.320","2016-03-24T20:14:01.320","DF","Sonar","Multibeam","Max Angle","50/45"]
["2016-03-24T08:18:02.240","2016-03-24T20:18:02.240","SM","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-24T08:21:00.100","2016-03-24T20:21:00.100","SM","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-24T08:24:24.980","2016-03-24T20:24:24.980","DF","Sonar","Multibeam","Max Angle","50/50"]
["2016-03-24T08:29:52.160","2016-03-24T20:29:52.160","DF","Sonar","Multibeam",null,"Random penetration and bottom loss still occuring in outter beams"]
["2016-03-24T08:30:52.260","2016-03-24T20:30:52.260","DF","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-24T08:31:01.080","2016-03-24T20:31:01.080","SM","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-24T08:32:44.720","2016-03-24T20:32:44.720","DF","sonar","Multibeam","Spike Filter Strength","Medium"]
["2016-03-24T08:38:39.430","2016-03-24T20:38:39.430","DF","Sonar","Multibeam",null,"Depth dropped past max depth for brief period while away from screen"]
["2016-03-24T08:45:18.750","2016-03-24T20:45:18.750","BG","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-24T09:00:15.450","2016-03-24T21:00:15.450","BG","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-24T09:05:10.970","2016-03-24T21:05:10.970","DF","Sonar","Multibeam","Max Angle","40/45"]
["2016-03-24T09:13:58.040","2016-03-24T21:13:58.040","DF","Sonar","Multibeam","New Line","cont line for turn"]
["2016-03-24T09:19:51","2016-03-24T21:19:51","DF","Sonar","Multibeam","New Line","started new line for track line, 0048"]
["2016-03-24T10:13:37.030","2016-03-24T22:13:37.030","SM","xbt",null,null,"cast 005 collected"]
["2016-03-24T10:20:26.330","2016-03-24T22:20:26.330","SM","xbt",null,null,"applied xbt to line 0049, started new line 0050"]
["2016-03-24T10:23:01.770","2016-03-24T22:23:01.770","DF","Sonar","Multibeam","Ping Mode","VERY DEEP, trouble tracking bottom"]
["2016-03-24T10:41:01.410","2016-03-24T22:41:01.410","AB","Sonar","Multibeam",null,"Max Angle 40/30, Slope and aeration filters On."]
["2016-03-24T10:58:50.050","2016-03-24T22:58:50.050","AB","Sonar","Multibeam","New Line","0051"]
["2016-03-24T11:40:47.060","2016-03-24T23:40:47.060","AB","Sonar","Multibeam","Max Angle","35/33"]
["2016-03-24T12:00:15","2016-03-25T00:00:15","AB","Sonar","Multibeam","New Line","0052"]
["2016-03-24T13:00:57.110","2016-03-25T01:00:57.110","AB","Sonar","Multibeam","New Line","0053"]
["2016-03-24T14:02:46","2016-03-25T02:02:46","CA","XBT",null,null,"cast 006 collected"]
["2016-03-24T14:37:25.670","2016-03-25T02:37:25.670","CA","XBT",null,null,"applied xtb to line 0054, started new line 0055"]
["2016-03-24T16:40:26","2016-03-25T04:40:26","AB","sonar","Multibeam","New Line","0057"]
["2016-03-24T17:40:12","2016-03-25T05:40:12","AB","Sonar","Multibeam","New Line","0058"]
["2016-03-24T18:36:40.300","2016-03-25T06:36:40.300","WP","Other",null,null,"Change of Watch"]
["2016-03-24T20:46:09.450","2016-03-25T08:46:09.450","DS","Sonar","Knudsen","Range","changed from 1000 to 500"]
["2016-03-24T21:35:00.400","2016-03-25T09:35:00.400","WP","Sonar","Multibeam",null,"Advanced line, Begin Turn 0062"]
["2016-03-24T21:38:24.850","2016-03-25T09:38:24.850","WP","Sonar","Multibeam",null,"Advanced line, end turn, line 0063"]
["2016-03-24T21:48:16.590","2016-03-25T09:48:16.590","DS","Sonar","Knudsen","Tx Power","increased power to 3, tx pulse to 8, range 500 m"]
["2016-03-24T22:14:29.400","2016-03-25T10:14:29.400","DS","XBT",null,null,"XBT# 7 conducted."]
["2016-03-24T22:23:13.170",{"$f":"IF(ISBLANK(A219), \" \", ((A219)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-25T10:23:13.170"},"DS","XBT",null,null,"XBT#7 applied to line 0063."]
["2016-03-24T22:26:17.470","2016-03-25T10:26:17.470","DS","Sonar","Multibeam","Max Angle","42/40, tilt -1"]
["2016-03-24T22:33:42.080","2016-03-25T10:33:42.080","DS","Sonar","Multibeam","Max Angle","40/37"]
["2016-03-24T22:38:29.870","2016-03-25T10:38:29.870","DS","Sonar","Knudsen","Phase Mode"]
["2016-03-24T22:43:54.410","2016-03-25T10:43:54.410","DS","Sonar","Multibeam","Max Angle","37/35"]
["2016-03-25T00:32:36.880","2016-03-25T12:32:36.880","CR","Sonar","Knudsen","Phase Mode"]
["2016-03-25T01:23:52.710","2016-03-25T13:23:52.710","WP","Sonar","Knudsen","Phase Mode","1750-2250"]
["2016-03-25T01:28:48.400","2016-03-25T13:28:48.400","WP","Sonar","Knudsen",null,"Power down to 2"]
["2016-03-25T01:32:54.670","2016-03-25T13:32:54.670","WP","Sonar","Knudsen","Phase Mode","1500-2000"]
["2016-03-25T01:42:30.560","2016-03-25T13:42:30.560","WP","Sonar","Knudsen","Phase Mode","1750-2250"]
["2016-03-25T01:50:17.860","2016-03-25T13:50:17.860","WP","Sonar","Knudsen","Phase Mode","2000-2500"]
["2016-03-25T02:34:03.200","2016-03-25T14:34:03.200","DF","Sonar","Multibeam","Max Angle","55/55"]
["2016-03-25T02:34:13.560","2016-03-25T14:34:13.560","DF","Sonar","Multibeam","Ping Mode","DEEP"]
["2016-03-25T02:34:27.290","2016-03-25T14:34:27.290","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-25T02:34:52.400","2016-03-25T14:34:52.400","DF","Sonar","Multibeam","Max Angle","60/55"]
["2016-03-25T02:57:15.440","2016-03-25T14:57:15.440","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-03-25T03:20:26.190","2016-03-25T15:20:26.190","DF","Sonar","Multibeam","Ping Mode","VERY DEEP"]
["2016-03-25T03:21:02.260","2016-03-25T15:21:02.260","DF","Sonar","Multibeam","Max Angle","52/52"]
["2016-03-25T03:23:11.370","2016-03-25T15:23:11.370","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-03-25T03:23:53.170","2016-03-25T15:23:53.170","DF","Sonar","Knudsen","Range","1000, started new line"]
["2016-03-25T03:24:50.430","2016-03-25T15:24:50.430","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2016-03-25T03:30:18.800","2016-03-25T15:30:18.800","DF","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-25T03:33:34.100","2016-03-25T15:33:34.100","DF","Sonar","Multibeam","Aeration Filter (On/Off)","On"]
["2016-03-25T03:34:31.060","2016-03-25T15:34:31.060","DF","Sonar","Multibeam","Max Angle","42/42"]
["2016-03-25T03:49:36.210","2016-03-25T15:49:36.210","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-25T04:17:07.630","2016-03-25T16:17:07.630","DF","sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-03-25T04:36:48.420","2016-03-25T16:36:48.420","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-25T04:43:12.160","2016-03-25T16:43:12.160","DF","Sonar","Knudsen","Gain Value",36]
["2016-03-25T05:41:20","2016-03-25T17:41:20","DS","XBT",null,null,"XBT #8 conducted. "]
["2016-03-25T05:54:13.170","2016-03-25T17:54:13.170","BG","XBT",null,null,"XBT #8 applied to line 0071"]
["2016-03-25T06:19:03.170","2016-03-25T18:19:03.170","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-25T06:32:00.600","2016-03-25T18:32:00.600","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-25T06:37:11.250","2016-03-25T18:37:11.250","SM","sonar","ek",null,"max depth range 6000"]
["2016-03-25T06:38:29.920","2016-03-25T18:38:29.920","bg","SONAR","Knudsen","Phase Range","4000-5000"]
["2016-03-25T07:15:30.740","2016-03-25T19:15:30.740","bg","Sonar","Knudsen","Phase Range","4500-5500 and Max depth=6000"]
["2016-03-25T08:23:00.410","2016-03-25T20:23:00.410","DF","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-25T09:05:24.630","2016-03-25T21:05:24.630","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-25T09:25:50.680","2016-03-25T21:25:50.680","BG","sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-25T11:00:46","2016-03-25T23:00:46","AB",null,null,null,"Watch change"]
["2016-03-25T11:02:29.080","2016-03-25T23:02:29.080","AB","Sonar","Multibeam",null,"Interference - Curved distortions. Line 0076 12:02:30"]
["2016-03-25T11:17:57.190","2016-03-25T23:17:57.190","AB","Sonar","Multibeam",null,"Sonar stopped pinging- error"]
["2016-03-25T11:37:40.220","2016-03-25T23:37:40.220","AB","sonar","Multibeam",null,"SIS restarted, BIST Run: TX36 and TRU Power Test, RX Noise Level.  RED."]
["2016-03-25T11:49:42.560","2016-03-25T23:49:42.560","DS","Sonar","Multibeam",null,"restarted TRU, waiting 5 minutes to try starting SIS, BIST showed one TX36 board failed voltage tests. Board 12 is the failing board."]
["2016-03-25T12:12:48.780","2016-03-26T00:12:48.780","DS","Sonar","Multibeam",null,"will ping, but cannot find bottom. Ran second full BIST, TX36 Rxchannels RX noise levels RX noise spectrum failed"]
["2016-03-25T12:26:24.740","2016-03-26T00:26:24.740","AB","Sonar",null,null,"Internal pinging on Knudsen and EK60"]
["2016-03-25T12:47:32.010","2016-03-26T00:47:32.010","DS","Sonar","Multibeam",null,"called out CET to re-seat failed board."]
["2016-03-25T12:57:20.800","2016-03-26T00:57:20.800","DS","Sonar","Multibeam",null,"all BIST passed after reseating TX32 board 12 in slot 11"]
["2016-03-25T13:03:57.760","2016-03-26T01:03:57.760","DS","Sonar","Multibeam","New Line","started logging line 0078, XBT 0010 applied to line 0078"]
["2016-03-25T14:04:23.550","2016-03-26T02:04:23.550","AB","Sonar","Multibeam","New Line","0079"]
["2016-03-25T14:46:29.940","2016-03-26T02:46:29.940","AB","Sonar","Multibeam","New Line","0080 - turn"]
["2016-03-25T14:52:00.780","2016-03-26T02:52:00.780","AB","Sonar","Multibeam","New Line","0081"]
["2016-03-25T14:52:55.930","2016-03-26T02:52:55.930","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-25T14:57:57.810","2016-03-26T02:57:57.810","AB","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-25T15:02:06.780","2016-03-26T03:02:06.780","AB","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-25T15:46:59.480","2016-03-26T03:46:59.480","AB","Sonar","Knudsen","Phase Range","3500-4500m; Gain 37dB"]
["2016-03-25T16:13:25.600","2016-03-26T04:13:25.600","AB","Sonar","Knudsen","Phase Range","3000-4000m, Gain 40dB"]
["2016-03-25T16:22:10.650","2016-03-26T04:22:10.650","AB","Sonar","Knudsen","Tx Pulse","4.0 ms"]
["2016-03-25T16:53:56.080","2016-03-26T04:53:56.080","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-25T17:44:01.800","2016-03-26T05:44:01.800","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-03-25T17:53:15.650","2016-03-26T05:53:15.650","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2016-03-25T17:58:56.510","2016-03-26T05:58:56.510","AB","Sonar","Knudsen","Phase Range","1000-2000m, Tx Pulse 2.0 ms, Tx Power 1, Gain 34 dB"]
["2016-03-25T18:02:37.130","2016-03-26T06:02:37.130","AB","Sonar","Multibeam","Max Angle","70/70"]
["2016-03-25T18:20:10.180","2016-03-26T06:20:10.180","AB","Sonar","Knudsen","Range","500, New line, Phase Range 1000-1500"]
["2016-03-25T18:26:18.420","2016-03-26T06:26:18.420","AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2016-03-25T18:31:38.660",{"$f":"IF(ISBLANK(A283), \" \", ((A283)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-26T06:31:38.660"},"WP","Other",null,null,"Change of Watch"]
["2016-03-25T18:49:26.580","2016-03-26T06:49:26.580","MP","Sonar","Multibeam",null,"Program automatically narrowed coveraged, manually corrected it, line 84"]
["2016-03-25T18:54:42.370","2016-03-26T06:54:42.370","MP","Sonar","Multibeam","New Line","0085"]
["2016-03-25T19:26:10.650","2016-03-26T07:26:10.650","MP","XBT",null,null,"XBT #11 conducted"]
["2016-03-25T19:27:44.960","2016-03-26T07:27:44.960","MP","XBT",null,null,"XBT #11 applied to line 0085"]
["2016-03-25T23:01:03.720","2016-03-26T11:01:03.720","MP","Sonar","Multibeam",null,"Depth too shallow"]
["2016-03-25T23:01:47.410","2016-03-26T11:01:47.410","MP","Sonar","EK","Change Range",4000]
["2016-03-25T23:02:36.140","2016-03-26T11:02:36.140","MP","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-03-25T23:10:44.090","2016-03-26T11:10:44.090","MP","Sonar","Knudsen","Phase Range","3500-4000"]
["2016-03-25T23:13:03.870","2016-03-26T11:13:03.870","MP","Sonar","EK","Change Range",5000]
["2016-03-25T23:18:20.310","2016-03-26T11:18:20.310","MP","Sonar","Knudsen","Phase Range","3750-4250"]
["2016-03-25T23:21:12.550","2016-03-26T11:21:12.550","MP","Sonar","Knudsen","Tx Power","Increased power to 3"]
["2016-03-25T23:28:18.750","2016-03-26T11:28:18.750","MP","Sonar","Knudsen","Phase Range","4000-4500"]
["2016-03-25T23:46:40.090","2016-03-26T11:46:40.090","MP","Sonar","Knudsen","Phase Range","4250-4750"]
["2016-03-25T23:51:04.430","2016-03-26T11:51:04.430","DS","Sonar","Multibeam","Ping Mode","auto"]
["2016-03-25T23:54:38.190","2016-03-26T11:54:38.190","wp","xbt",null,null,"xbt 012 applied line 090"]
["2016-03-26T00:03:14.920","2016-03-26T12:03:14.920","MP","sonar","Knudsen","Phase Range","4750-5250"]
["2016-03-26T00:08:44.040","2016-03-26T12:08:44.040","wp","sonar","all",null,"Multibeam and Knudsun, stopped logging Man Overboard Drill"]
["2016-03-26T00:25:54.900","2016-03-26T12:25:54.900","wp","sonar","all",null,"Multibeam and knudson started logging, end man overboard drill. Line 91"]
["2016-03-26T00:30:22.580","2016-03-26T12:30:22.580","wp","sonar","all",null,"Multibeam and Knusson stopped logging, 2nd Man Overboard Drill."]
["2016-03-26T01:25:13.760","2016-03-26T13:25:13.760","wp","sonar","all",null,"Multibeam and Knudson started logging, line 093"]
["2016-03-26T01:31:48.650","2016-03-26T13:31:48.650","MP","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-26T01:44:52.710","2016-03-26T13:44:52.710","MP","Sonar","Knudsen","Phase Range","5000-6000"]
["2016-03-26T01:48:49.590","2016-03-26T13:48:49.590","wp","sonar","Multibeam",null,"line increased to 094 begin turn"]
["2016-03-26T01:52:50.220","2016-03-26T13:52:50.220","wp","sonar","Multibeam",null,"line increased to 095 end turn"]
["2016-03-26T02:21:42.800","2016-03-26T14:21:42.800","DF","Sonar","EK",null,"Max recording range to 7000"]
["2016-03-26T02:30:49.550","2016-03-26T14:30:49.550","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-26T02:31:28.690","2016-03-26T14:31:28.690","DF","sonar","Multibeam","Max Angle","30/30"]
["2016-03-26T02:31:49.780","2016-03-26T14:31:49.780","DF","Sonar","Multibeam",null,"Aeration and slope filter on, to try and fix sector boundary artifact"]
["2016-03-26T02:36:29.440","2016-03-26T14:36:29.440","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-03-26T02:39:59.280","2016-03-26T14:39:59.280","DF","Sonar","Multibeam",null,"Auto tilt enabled at 2 deg to try and minimize nadir and sector artifacts"]
["2016-03-26T02:48:14.310","2016-03-26T14:48:14.310","DF","Sonar","Multibeam","Spike Filter Strength","STRONG, auto tilt seems to help reduce quantity nadir and sector artifacts but they still happen occasionally"]
["2016-03-26T02:55:17.810","2016-03-26T14:55:17.810","DF","Sonar","Multibeam","Max Angle","28/28"]
["2016-03-26T02:55:37.180","2016-03-26T14:55:37.180","DF","Sonar","Multibeam","Aeration Filter (On/Off)","on, trying to reduce sector and nadir artifacts"]
["2016-03-26T02:58:36.630","2016-03-26T14:58:36.630","DF","Sonar","Multibeam",null,"trying auto tilt on 4 degrees"]
["2016-03-26T03:03:39.030","2016-03-26T15:03:39.030","DF","Sonar","Multibeam",null,"Turned auto tilt off and Along direction angle to 4 degrees. Nadir and sector artifacts were fixed when auto tilt angled the swath fwd."]
["2016-03-26T03:24:48.460","2016-03-26T15:24:48.460","DF","Sonar","Knudsen","Gain Value","38 dB"]
["2016-03-26T04:30:16.560","2016-03-26T16:30:16.560","DS","Sonar","Multibeam",null,"min depth set to 3500"]
["2016-03-26T04:48:44.670","2016-03-26T16:48:44.670","DF","Sonar","Multibeam","Max Angle","30/30"]
["2016-03-26T04:57:48.050","2016-03-26T16:57:48.050","DF","Sonar","Multibeam","Max Angle","35/30"]
["2016-03-26T04:59:30.740","2016-03-26T16:59:30.740","BG","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-26T05:00:23.100","2016-03-26T17:00:23.100","DF","Sonar","Multibeam","Max Angle","30/30"]
["2016-03-26T05:10:58.670","2016-03-26T17:10:58.670","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-26T05:15:41.860","2016-03-26T17:15:41.860","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-26T05:21:57.770","2016-03-26T17:21:57.770","DF","Sonar","Multibeam","Max Angle","35/35"]
["2016-03-26T05:22:14.590","2016-03-26T17:22:14.590","DF","Sonar","Multibeam","Ping Mode","VERY DEEP"]
["2016-03-26T05:22:38.720","2016-03-26T17:22:38.720","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-26T05:26:30.160","2016-03-26T17:26:30.160","DF","Sonar","Multibeam","Aeration Filter (On/Off)","OFF"]
["2016-03-26T05:27:21.780","2016-03-26T17:27:21.780","DS","Sonar","Knudsen","Tx Pulse","increased to 16 ms"]
["2016-03-26T05:30:22.730","2016-03-26T17:30:22.730","DF","Sonar","Knudsen","Phase Range","3000-4000, Minimum depth to 500"]
["2016-03-26T05:43:08.310","2016-03-26T17:43:08.310","DF","Sonar","Multibeam","Max Angle","45/40"]
["2016-03-26T05:43:28.240","2016-03-26T17:43:28.240","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2016-03-26T05:46:52.320","2016-03-26T17:46:52.320","DF","Sonar","Multibeam","Max Angle","50/45"]
["2016-03-26T05:52:53.420","2016-03-26T17:52:53.420","DF","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-26T06:10:28.850","2016-03-26T18:10:28.850","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-26T06:27:42.120","2016-03-26T18:27:42.120","BG","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-26T06:33:17.850","2016-03-26T18:33:17.850","DF","Sonar","Multibeam","Max Angle","35/35"]
["2016-03-26T06:33:49.950","2016-03-26T18:33:49.950","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-26T06:39:42.760","2016-03-26T18:39:42.760","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2016-03-26T06:43:02.650","2016-03-26T18:43:02.650","DF","Sonar","Knudsen","Gain Value","44 dB"]
["2016-03-26T07:05:30.940","2016-03-26T19:05:30.940","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-26T07:10:57.980","2016-03-26T19:10:57.980","DF","Sonar","Multibeam","New Line","New line for turn, 0101"]
["2016-03-26T07:15:00.840","2016-03-26T19:15:00.840","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-26T07:15:53.730","2016-03-26T19:15:53.730","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-26T07:16:31.830",{"$f":"IF(ISBLANK(A347), \" \", ((A347)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-26T19:16:31.830"},"DF","Sonar","Multibeam","Max Angle","45/35"]
["2016-03-26T07:18:17.650","2016-03-26T19:18:17.650","DF","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-26T07:21:12.360","2016-03-26T19:21:12.360","DF","sonar","Knudsen","Tx Pulse","8 ms"]
["2016-03-26T07:24:24.940","2016-03-26T19:24:24.940","DF","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-26T07:30:09.320","2016-03-26T19:30:09.320","DF","sonar","Multibeam","Max Angle","55/45"]
["2016-03-26T07:31:30.140","2016-03-26T19:31:30.140","DF","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-26T07:34:10.240","2016-03-26T19:34:10.240","DF","sonar","Multibeam","Max Angle","45/45"]
["2016-03-26T07:36:54.710","2016-03-26T19:36:54.710","DF","Sonar","Knudsen",null,"TX Pulse to 4 m, TX Power to 2"]
["2016-03-26T07:39:59.790","2016-03-26T19:39:59.790","DF","Sonar","Multibeam","Max Angle","50/45"]
["2016-03-26T07:45:35.280","2016-03-26T19:45:35.280","DF","sonar","Multibeam","Max Angle","45/45"]
["2016-03-26T07:53:33.280","2016-03-26T19:53:33.280","DF","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-26T08:01:43.330","2016-03-26T20:01:43.330","DF","Sonar","Knudsen","Phase Range","3500-4500, Pulse to 8 ms, power to 3"]
["2016-03-26T08:47:37.230","2016-03-26T20:47:37.230","DF","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-26T08:51:35.620","2016-03-26T20:51:35.620","SM","xbt",null,null,"cast 013 collected"]
["2016-03-26T08:58:35.030","2016-03-26T20:58:35.030","BG","XBT",null,null,"applied to 0102, started line  0103"]
["2016-03-26T08:59:17.350","2016-03-26T20:59:17.350","DF","sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-26T09:08:01.070","2016-03-26T21:08:01.070","DF","Sonar","Knudsen","TX Pulse","16 ms"]
["2016-03-26T09:09:25.190","2016-03-26T21:09:25.190","BG","sonar","Knudsen","Phase Range","5000-6000"]
["2016-03-26T09:23:11.660","2016-03-26T21:23:11.660","DF","Sonar","Multibeam","Max Angle","30/30"]
["2016-03-26T09:25:16.260","2016-03-26T21:25:16.260","DF","Sonar","Knudsen","Gain Value","40 dB"]
["2016-03-26T09:26:12.200","2016-03-26T21:26:12.200","DF","Sonar","Multibeam","Max Angle","25/30"]
["2016-03-26T09:35:42.280","2016-03-26T21:35:42.280","BG","Sonar","Knudsen","Phase Range","5500-6500"]
["2016-03-26T10:33:31.390","2016-03-26T22:33:31.390","AB",null,null,null,"Watch change"]
["2016-03-26T10:34:00.210","2016-03-26T22:34:00.210","AB","Sonar","Multibeam","Max Angle","35/30"]
["2016-03-26T10:55:09.240","2016-03-26T22:55:09.240","AB","Sonar","Knudsen","Phase Range","5000-6000m, RNGE 1000M, Tx Pulse 16, Power 3, Gain 47, Losing bottom on steep slope."]
["2016-03-26T11:00:09","2016-03-26T23:00:09","AB","Sonar","Multibeam","New Line","0105"]
["2016-03-26T11:08:20.040","2016-03-26T23:08:20.040","AB","Sonar","Multibeam","Max Angle","35/35"]
["2016-03-26T11:25:51.430","2016-03-26T23:25:51.430","AB","Sonar","Knudsen","Phase Range","2500-3500m, MBES switch to Very Deep on Auto nearing top of feature"]
["2016-03-26T11:47:25.110","2016-03-26T23:47:25.110","AB","Sonar","Multibeam","Max Angle","55/55"]
["2016-03-26T11:47:49.210","2016-03-26T23:47:49.210","AB","Sonar","Knudsen","Phase Range","3000-4000m, Power 3, Pulse 4"]
["2016-03-26T12:33:39.680","2016-03-27T00:33:39.680","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-26T13:00:52","2016-03-27T01:00:52","AB","Sonar","Multibeam","New Line","0107"]
["2016-03-26T13:09:18.260","2016-03-27T01:09:18.260","AB","Sonar","Knudsen","Gain Value","40dB, Power 2, Phase Range 4000-5000m"]
["2016-03-26T13:50:18.370","2016-03-27T01:50:18.370","AB","Sonar","Knudsen",null,"Lost bottom due to traversing slope. Getting 2-3 returns."]
["2016-03-26T13:51:26.620","2016-03-27T01:51:26.620","AB","Sonar","Multibeam","New Line","0108"]
["2016-03-26T14:08:59.140","2016-03-27T02:08:59.140","AB","xbt",null,null,"#14 drop canceled itself."]
["2016-03-26T14:09:25.650","2016-03-27T02:09:25.650","AB","xbt",null,null,"#15"]
["2016-03-26T14:28:52.610","2016-03-27T02:28:52.610","CA","xbt",null,null,"#15 applied, started line 109"]
["2016-03-26T15:30:31","2016-03-27T03:30:31","AB","Sonar","Multibeam","New Line","0110"]
["2016-03-26T16:30:57","2016-03-27T04:30:57","AB","Sonar","Multibeam","New Line","0111"]
["2016-03-26T17:30:18","2016-03-27T05:30:18","AB","Sonar","Multibeam","New Line","0112"]
["2016-03-26T18:29:57.560","2016-03-27T06:29:57.560","AB","sonar","Multibeam","New Line","0113"]
["2016-03-26T18:41:59.690","2016-03-27T06:41:59.690","wp","Other",null,null,"Watch change"]
["2016-03-26T18:42:33.600","2016-03-27T06:42:33.600","wp","Sonar","Knudsen","Phase Range","5000-6000, pulse 8.0, tx power 3."]
["2016-03-26T18:43:38.850","2016-03-27T06:43:38.850","wp","sonar","Multibeam",null,"min 3000, max 6000"]
["2016-03-26T19:52:53.070","2016-03-27T07:52:53.070","MP","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-26T19:57:17.060","2016-03-27T07:57:17.060","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-26T20:12:07.110","2016-03-27T08:12:07.110","WP","SONAR","Multibeam","New Line","Begin Turn 0115"]
["2016-03-26T20:12:54.430","2016-03-27T08:12:54.430","wp","xbt",null,null,"problems with settings on CTD/XBT computer."]
["2016-03-26T20:16:22.400","2016-03-27T08:16:22.400","wp","sonar","multibeam","New Line","begin survey line 0116"]
["2016-03-26T20:18:42.840","2016-03-27T08:18:42.840","MP","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-26T20:29:40.430","2016-03-27T08:29:40.430","MP","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-26T20:31:28.020","2016-03-27T08:31:28.020","MP","XBT",null,null,"first 2 attempts failed, #16 was successful"]
["2016-03-26T20:34:34.660","2016-03-27T08:34:34.660","MP","XBT",null,null,"#16 applied to line 0117"]
["2016-03-26T20:35:44.920","2016-03-27T08:35:44.920","MP","sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-26T20:39:04.870","2016-03-27T08:39:04.870","MP","sonar","Knudsen","Tx Power","1`"]
["2016-03-26T20:39:20.560","2016-03-27T08:39:20.560","MP","sonar","Knudsen","Tx Pulse",4]
["2016-03-26T20:44:50.550","2016-03-27T08:44:50.550","MP","Sonar","Knudsen","Tx Pulse","2, gain value 36dB"]
["2016-03-26T21:24:41.040","2016-03-27T09:24:41.040","MP","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-26T21:35:00.390","2016-03-27T09:35:00.390","MP","sonar","Knudsen","Tx Power",3]
["2016-03-26T21:46:03.640","2016-03-27T09:46:03.640","wp","sonar","multibeam","New Line","line increment for begin turn, line New 119"]
["2016-03-26T21:49:32.850","2016-03-27T09:49:32.850","wp","sonar","multibeam","New Line","line increment for end turn, New line 120"]
["2016-03-26T21:56:09.980","2016-03-27T09:56:09.980","wp","sonar","Knudsen","Phase Mode","1000-2000, power to 1, min 500, max 3500, range 1000"]
["2016-03-26T22:05:44.930","2016-03-27T10:05:44.930","wp","sonar","Multibeam","New Line","Line Incrument for begin turn, new line 121."]
["2016-03-26T22:10:50.930",{"$f":"IF(ISBLANK(A411), \" \", ((A411)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-27T10:10:50.930"},"DS","Sonar","Multibeam","New Line","start survey line 0122, turned on autotilt, stbd max angle to 55"]
["2016-03-26T22:22:52.080","2016-03-27T10:22:52.080","DS","Sonar","Multibeam",null,"Had bridge shift survey line 500m to port (southeast) to ensure coverage"]
["2016-03-26T22:27:51.370","2016-03-27T10:27:51.370","DS","Sonar","EK","Change Range","increased range to 1700 on 70 kHz"]
["2016-03-26T22:50:00.640","2016-03-27T10:50:00.640","DS","Sonar","Knudsen","Tx Pulse","reduced to 2 ms"]
["2016-03-26T23:01:54.650","2016-03-27T11:01:54.650","CR","Sonar","Knudsen","Tx Power","increased to 2 ms"]
["2016-03-26T23:07:39.200","2016-03-27T11:07:39.200","wp","sonar","Knudsen","Phase Mode","1500-2500, pulse to 4"]
["2016-03-26T23:33:54.030","2016-03-27T11:33:54.030","wp","sonar","multibeam","New Line","begin turn, line incremented to line 0124"]
["2016-03-26T23:36:30.260","2016-03-27T11:36:30.260","wp","sonar","multibeam","New Line","end turn, line incremented to line 0125"]
["2016-03-26T23:44:21.540","2016-03-27T11:44:21.540","cr","sonar","knudsen","Phase Range","2500-3500"]
["2016-03-26T23:49:05.180","2016-03-27T11:49:05.180","CR","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-26T23:55:51.810","2016-03-27T11:55:51.810","wp","sonar","Multibeam","New Line","begin turn line incremented to line 0126"]
["2016-03-27T01:00:06.890","2016-03-27T13:00:06.890","wp","sonar","Multibeam","New Line","end turn, line incremented to line 0127"]
["2016-03-27T01:26:31.890","2016-03-27T13:26:31.890","DS","Sonar","Multibeam",null,"Had bridge shift survey line 500m to starboard (southeast) to ensure coverage"]
["2016-03-27T01:38:25.520","2016-03-27T13:38:25.520","wp","sonar","Knudsen","Phase Mode","1500-2500, power 2, pulse, 4.0"]
["2016-03-27T01:43:26.110","2016-03-27T13:43:26.110","DS","Sonar","Multibeam",null,"Had bridge shift survey line 300m to starboard (southeast) to ensure coverage"]
["2016-03-27T01:44:01.970","2016-03-27T13:44:01.970","wp","Sonar","Knudsen","Phase Mode","1000-2000, power 1, pulse 2."]
["2016-03-27T01:45:10.100","2016-03-27T13:45:10.100","wp","Other",null,null,"Caris crashed during processing, and will not re-start. MPROC 1 computer. "]
["2016-03-27T02:02:02.580","2016-03-27T14:02:02.580","wp","sonar","knudsen","phase mode","1500-2500, pulse 8.0, power 2"]
["2016-03-27T02:11:56.870","2016-03-27T14:11:56.870","wp","sonar","knudsen","phase mode","2000-3000, pulse 16, power 3."]
["2016-03-27T02:32:16.050","2016-03-27T14:32:16.050","wp","sonar","multibeam","new line","end survey line plan, seamount, increment line to 0129"]
["2016-03-27T02:47:25.790","2016-03-27T14:47:25.790","wp","sonar","Knudsen","Phase Mode","2500-3500"]
["2016-03-27T02:50:09.520","2016-03-27T14:50:09.520","wp","sonar","multibeam","New Line","begin turn, line incremented to line 0130"]
["2016-03-27T02:52:02.590","2016-03-27T14:52:02.590","wp","sonar","Multibeam","New Line","end turn, line incremented to line 0131"]
["2016-03-27T02:59:01.640","2016-03-27T14:59:01.640","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-27T03:19:42.620","2016-03-27T15:19:42.620","CR","XBT",null,null,"XBT 17 Applied to line 131"]
["2016-03-27T03:21:47.150","2016-03-27T15:21:47.150","BG","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-27T03:22:39.170","2016-03-27T15:22:39.170","BG","sonar","Knudsen","Tx Pulse","16 ms"]
["2016-03-27T03:30:25.690","2016-03-27T15:30:25.690","BG","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-27T04:01:26.080","2016-03-27T16:01:26.080","BG","Sonar","EK","Change Range","5500 on 18kHz"]
["2016-03-27T04:15:28.970","2016-03-27T16:15:28.970","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-27T04:15:56.270","2016-03-27T16:15:56.270","DF","sonar","Multibeam",null,"auto tilt disabled and 4 degree along direciton angle set"]
["2016-03-27T04:38:47.250","2016-03-27T16:38:47.250","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-27T04:44:22.170","2016-03-27T16:44:22.170","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-27T04:49:34.540","2016-03-27T16:49:34.540","DF","Sonar","Multibeam","Max Angle","55/55"]
["2016-03-27T04:55:34.480",{"$f":"IF(ISBLANK(A445), \" \", ((A446)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-27T17:02:35.660"},"BG","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-27T05:02:35.660",{"$f":"IF(ISBLANK(A446), \" \", ((A446)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-27T17:02:35.660"},"BG","sonar","Knudsen",null,"tx pulse to 8 m, pulse to 2"]
["2016-03-27T05:03:17.400","2016-03-27T17:03:17.400","BG","sonar","knudsen","Phase Range","2000-3000"]
["2016-03-27T05:14:59.660","2016-03-27T17:14:59.660","DF","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-27T05:19:13.440","2016-03-27T17:19:13.440","DF","sonar","multibeam","Max Angle","55/45"]
["2016-03-27T05:21:52.780","2016-03-27T17:21:52.780","DF","sonar","multibeam",null,"auto tilt enabled at 4 degrees to reduce holes in bottom tracking while going over seamount"]
["2016-03-27T05:35:49.120","2016-03-27T17:35:49.120","DF","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-27T05:39:36.920","2016-03-27T17:39:36.920","DS","Sonar","Knudsen","Tx Power","increased to 3"]
["2016-03-27T05:40:32.440","2016-03-27T17:40:32.440","BG","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-27T05:57:01.030","2016-03-27T17:57:01.030","BG","sonar","Knudsen",null,"max depth 6000, phase range 4500-5500"]
["2016-03-27T06:21:52.150","2016-03-27T18:21:52.150","DF","Sonar","multibeam","New Line","new line for turn, 0135"]
["2016-03-27T06:30:28.480","2016-03-27T18:30:28.480","DF","sonar","multibeam","New Line","new line for back on survey line, 0136"]
["2016-03-27T06:43:50.450","2016-03-27T18:43:50.450","DS","Sonar","Multibeam","Max Angle","31/30"]
["2016-03-27T07:08:59.340","2016-03-27T19:08:59.340","DS",null,null,null,"Asked bridge to speed up a little bit. They are only on 2 generators, but can go a little faster. "]
["2016-03-27T07:22:22.480","2016-03-27T19:22:22.480","BG","sonar","Knudsen","Phase Range","5000-6000"]
["2016-03-27T07:48:23.770","2016-03-27T19:48:23.770","DF","sonar","Multibeam",null,"auto tilt turned off and -4 degree turned on"]
["2016-03-27T07:55:39.810","2016-03-27T19:55:39.810","DF","Sonar","Multibeam","Along Direction Pitch","moving from -5 fwd to plus 2"]
["2016-03-27T08:32:51.200","2016-03-27T20:32:51.200","DF","Sonar","Multibeam","Along Direction Pitch","slowly moving fwd to +3"]
["2016-03-27T09:12:01.590","2016-03-27T21:12:01.590","DF","xbt",null,null,"Cast 018 collected"]
["2016-03-27T09:13:06.240","2016-03-27T21:13:06.240","DF","xbt",null,null,"cast 018 applied to line 0138, started new line 0139"]
["2016-03-27T09:13:39.580","2016-03-27T21:13:39.580","DF","Sonar","multibeam","Aeration Filter (On/Off)","on"]
["2016-03-27T09:43:33.830","2016-03-27T21:43:33.830","DF","sonar","multibeam","New Line","cont line for turn, 0140 back on survey trackline"]
["2016-03-27T09:49:22.390","2016-03-27T21:49:22.390","DF","sonar","multibeam","Max Angle","35/35"]
["2016-03-27T09:55:14.980","2016-03-27T21:55:14.980","DF","sonar","multibeam","Along Direction Pitch",2]
["2016-03-27T09:58:37.490","2016-03-27T21:58:37.490","DF","sonar","knudsen","Phase Range","4000-5000"]
["2016-03-27T10:05:09.520","2016-03-27T22:05:09.520","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-27T11:00:55.210","2016-03-27T23:00:55.210","DF","sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-27T11:03:55.030","2016-03-27T23:03:55.030","DF","sonar","Multibeam","Max Angle","40/35"]
["2016-03-27T11:19:05.130","2016-03-27T23:19:05.130","SM","Sonar","Knudsen","Phase Range","5000-6000"]
["2016-03-27T11:30:38","2016-03-27T23:30:38","AB",null,null,null,"Watch change"]
["2016-03-27T12:06:36.100","2016-03-28T00:06:36.100","AB","Sonar","Multibeam","new line","0143"]
["2016-03-27T12:17:37.910","2016-03-28T00:17:37.910","AB","Sonar","multibeam","new line","0144"]
["2016-03-27T12:28:43.260","2016-03-28T00:28:43.260","AB","sonar","multibeam","new line","0145"]
["2016-03-27T13:31:06.850","2016-03-28T01:31:06.850","AB","sonar","multibeam","new line","0146"]
["2016-03-27T13:31:20.440","2016-03-28T01:31:20.440","AB","sonar","multibeam","Max Angle","52/52, Very Deep Mode"]
["2016-03-27T13:54:52.770","2016-03-28T01:54:52.770","Ab","sonar","Knudsen",null,"Lost bottom on shelf."]
["2016-03-27T14:01:35.520","2016-03-28T02:01:35.520","AB","sonar","Knudsen",null,"New line started for lost bottom, new line started again with bottom found. Power 3, Pulse 8, Range 1000, Phase 3000-4000m"]
["2016-03-27T14:30:03","2016-03-28T02:30:03","AB","sonar","multibeam","New Line","0147"]
["2016-03-27T14:39:57.370","2016-03-28T02:39:57.370","AB","sonar","Knudsen","Phase Range","4500-5500m"]
["2016-03-27T14:40:34.100","2016-03-28T02:40:34.100","AB","Sonar","Multibeam","New Line","0148 turn"]
["2016-03-27T15:01:47.540","2016-03-28T03:01:47.540","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-27T15:16:40.540","2016-03-28T03:16:40.540","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-03-27T15:17:01.040","2016-03-28T03:17:01.040","AB","xbt",null,null," #19 complete"]
["2016-03-27T15:17:45.550","2016-03-28T03:17:45.550","AB","xbt",null,null,"#19 applied to new line 0150"]
["2016-03-27T15:47:42.370","2016-03-28T03:47:42.370","AB","Sonar","Multibeam",null,"Deep Mode for sea mount, Max angle 60/60"]
["2016-03-27T15:48:05.910","2016-03-28T03:48:05.910","AB","sonar","Knudsen","Phase Range","1500-2500m, Power 1, Pulse 2"]
["2016-03-27T16:03:05.440","2016-03-28T04:03:05.440","CA","sonar","Knudsen","Phase Range","2000-3000m"]
["2016-03-27T16:06:48.450","2016-03-28T04:06:48.450","CA","Sonar","Knudsen","Phase Range","2500-3500m, Power 2, Pulse 4"]
["2016-03-27T16:15:31.640","2016-03-28T04:15:31.640","CA","sonar","Knudsen","Phase Range","3000-4000m, Power 3, Pulse 8, Gain 39"]
["2016-03-27T16:27:31.700","2016-03-28T04:27:31.700","CA","Sonar","Knudsen","Phase Range","4000-4500m, Pulse 16, Gain 40"]
["2016-03-27T16:31:00","2016-03-28T04:31:00","CA","sonar","Knudsen","Phase Range","4250-4750m"]
["2016-03-27T16:32:47.920","2016-03-28T04:32:47.920","CA","sonar","Knudsen","Phase Range","4500-5000m"]
["2016-03-27T16:37:59.020","2016-03-28T04:37:59.020","AB","sonar","knudsen","Phase Range","4750-5250m"]
["2016-03-27T16:49:29.100","2016-03-28T04:49:29.100","CA","sonar","Knudsen","Phase Range","4500-5000m"]
["2016-03-27T16:51:19.620","2016-03-28T04:51:19.620","CA","sonar","Knudsen","Phase Range","4250-4750m"]
["2016-03-27T16:58:55.960","2016-03-28T04:58:55.960","CA","sonar","Knudsen","Phase Range","4500-5000m"]
["2016-03-27T17:02:43.820","2016-03-28T05:02:43.820","CA","sonar","Knudsen","Phase Range","4750-5250m"]
["2016-03-27T17:05:30.340","2016-03-28T05:05:30.340","CA","Sonar","Knudsen","Phase Range","5000-5500m"]
["2016-03-27T17:06:19.570","2016-03-28T05:06:19.570","CA","sonar","multibeam","New Line","0152 - turn"]
["2016-03-27T17:07:39.420","2016-03-28T05:07:39.420","CA","sonar","Knudsen","phase range","5250-5750m"]
["2016-03-27T17:36:46.080","2016-03-28T05:36:46.080","AB","Sonar","multibeam","New Line","0153"]
["2016-03-27T17:37:53.170","2016-03-28T05:37:53.170","AB","sonar","Knudsen","Phase Range","5000-5500m"]
["2016-03-27T17:46:28.880","2016-03-28T05:46:28.880","AB","Sonar","Knudsen","Phase Range","4750-5250m"]
["2016-03-27T17:51:44.040","2016-03-28T05:51:44.040","AB","sonar","Knudsen","Phase Range","5000-5500m"]
["2016-03-27T17:56:11.990","2016-03-28T05:56:11.990","AB","sonar","Knudsen","Phase Range","4750-5250m"]
["2016-03-27T17:59:22.820",{"$f":"IF(ISBLANK(A510), \" \", ((A510)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-28T05:59:22.820"},"AB","sonar","knudsen","Phase Range","4500-5000m, Pulse 8.0ms"]
["2016-03-27T18:03:11.430","2016-03-28T06:03:11.430","AB","Sonar","knudsen","Phase Range","4250-4750m"]
["2016-03-27T18:12:57.460","2016-03-28T06:12:57.460","AB","Sonar","knudsen","Phase Range","4000-4500m"]
["2016-03-27T18:19:36.510","2016-03-28T06:19:36.510","AB","Sonar","knudsen","Phase Range","3750-4250m"]
["2016-03-27T18:25:04.460","2016-03-28T06:25:04.460","AB","Sonar","knudsen","Phase Range","3500-4000m"]
["2016-03-27T18:35:13.410","2016-03-28T06:35:13.410","AB","Sonar","knudsen","Phase Range","3250-3750m"]
["2016-03-27T18:36:50.120","2016-03-28T06:36:50.120","AB","sonar","knudsen","Phase Range","3000-3500m"]
["2016-03-27T18:37:56.860","2016-03-28T06:37:56.860","AB","sonar","knudsen","Phase Range","2750-3250m"]
["2016-03-27T18:39:50.810","2016-03-28T06:39:50.810","AB","sonar","knudsen",null,"Power 2, Pulse 4"]
["2016-03-27T18:42:55.610","2016-03-28T06:42:55.610","AB","sonar","knudsen","Phase Range","2500-3000m, reduced depth limits"]
["2016-03-27T18:44:44.410","2016-03-28T06:44:44.410","AB","Sonar","Multibeam","Max Angle","70/70, auto ping mode"]
["2016-03-27T18:57:12.700","2016-03-28T06:57:12.700","AB","sonar","Multibeam","new line",155]
["2016-03-27T19:15:38.720","2016-03-28T07:15:38.720","AB","sonar","Multibeam","new line","0156-turn"]
["2016-03-27T19:16:17.100","2016-03-28T07:16:17.100","AB","Sonar","Knudsen","Phase Range","4000-4500m; New line"]
["2016-03-27T19:22:37.950","2016-03-28T07:22:37.950","AB","Sonar","Multibeam","new line","0156"]
["2016-03-27T19:24:24.600","2016-03-28T07:24:24.600","AB","Sonar","Knudsen","Phase Range","4500-5000m"]
["2016-03-27T19:30:04.360","2016-03-28T07:30:04.360","AB","Sonar","Knudsen","Phase Range","4750-5250m"]
["2016-03-27T19:32:23.640","2016-03-28T07:32:23.640","AB","sonar","Knudsen","Phase Range","5000-5500m"]
["2016-03-27T19:42:18.070","2016-03-28T07:42:18.070","wp",null,null,null,"Watch Change"]
["2016-03-27T20:44:00.170","2016-03-28T08:44:00.170","wp","sonar","knudsen","phase range","5250-5750"]
["2016-03-27T21:11:50.240","2016-03-28T09:11:50.240","DS","XBT",null,null,"first XBT failed just after starting data collection. Switched launchers. Second cast successful (named cast 20)"]
["2016-03-27T21:18:03.900","2016-03-28T09:18:03.900","MP","sonar","multibeam",null,"cast xbt 020 applied to line 0158"]
["2016-03-27T21:58:28.010","2016-03-28T09:58:28.010","CR",null,null,null,"Caris giving issues. Deleted old sessions & created new work session EX1604_CleaningSession under same location "]
["2016-03-27T22:10:34.400","2016-03-28T10:10:34.400","DS","Sonar","Knudsen","Phase Mode","range from 500 to 1000. phase shift"]
["2016-03-27T22:49:14.930","2016-03-28T10:49:14.930","DS","sonar","knudsen","phase mode","range from 35oo-4500"]
["2016-03-27T23:12:00.390","2016-03-28T11:12:00.390","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-27T23:22:06.030","2016-03-28T11:22:06.030","CR","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-27T23:32:12.710","2016-03-28T11:32:12.710","wp","sonar","knudsen","phase range","2000-3000, pulse 2, power 2"]
["2016-03-28T00:18:51.290","2016-03-28T12:18:51.290","wp","Other",null,null,"Day Change from Julian Day 087 to Julian Day 088."]
["2016-03-28T00:42:04.810","2016-03-28T12:42:04.810","wp","sonar","knudsen","phase range","range 4000-5000, power 3 pulse 32, gain 32"]
["2016-03-28T01:04:33.270","2016-03-28T13:04:33.270","wp","sonar","multibeam","new line","begin turn, new line 0162"]
["2016-03-28T01:07:09.390","2016-03-28T13:07:09.390","wp","sonar","multibeam","new line","end turn, new line 0163"]
["2016-03-28T01:15:25.350","2016-03-28T13:15:25.350","wp","sonar","multibeam","New Line","begin turn, new line 0164"]
["2016-03-28T01:17:01.330","2016-03-28T13:17:01.330","wp","sonar","multibeam","New Line","end turn, new line 0165"]
["2016-03-28T01:33:22.120","2016-03-28T13:33:22.120","CR","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-28T01:45:32.380","2016-03-28T13:45:32.380","CR","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-28T01:52:46.050","2016-03-28T13:52:46.050","CR","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T02:01:54.300","2016-03-28T14:01:54.300","wp","sonar","knudsen","phase range","2500-3500"]
["2016-03-28T02:10:04.020","2016-03-28T14:10:04.020","wp","sonar","knudsen","Phase Range","2000-3000"]
["2016-03-28T02:14:08.960","2016-03-28T14:14:08.960","Ds","sonar","Knudsen","Gain Value","38dB"]
["2016-03-28T02:15:00.190","2016-03-28T14:15:00.190","CR","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-28T02:15:00.190","2016-03-28T14:15:00.190","CR","sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-28T02:19:29.420","2016-03-28T14:19:29.420","CR","Sonar","Knudsen","Tx Power","down to 1"]
["2016-03-28T02:20:04.070","2016-03-28T14:20:04.070","CR","sonar","Knudsen","Gain Value","32dB"]
["2016-03-28T02:34:35.530","2016-03-28T14:34:35.530","CR","sonar","Knudsen","Gain Value","38dB"]
["2016-03-28T02:34:51.160","2016-03-28T14:34:51.160","CR","sonar","Knudsen","Tx Power","up to 3"]
["2016-03-28T02:35:37.050","2016-03-28T14:35:37.050","CR","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-28T02:36:28.720","2016-03-28T14:36:28.720","CR","Sonar","Knudsen","Tx Power","down to 2"]
["2016-03-28T02:37:22.120","2016-03-28T14:37:22.120","CR","Sonar","Knudsen","Gain Value","36dB"]
["2016-03-28T02:40:22.600","2016-03-28T14:40:22.600","CR","Sonar","Knudsen","Gain Value","38dB"]
["2016-03-28T02:41:38.600","2016-03-28T14:41:38.600","CR","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-28T02:42:39.910","2016-03-28T14:42:39.910","CR","Sonar","Knudsen","Gain Value","32dB"]
["2016-03-28T03:09:27.180","2016-03-28T15:09:27.180","ds","sonar","knudsen","Tx Power","Power to 3, pulse at 16, gain at 37db, phase at 2500-3500"]
["2016-03-28T03:17:32.920","2016-03-28T15:17:32.920","wp","sonar","Multibeam","new line","begin turn, new line 0168"]
["2016-03-28T03:18:28.380","2016-03-28T15:18:28.380","mp","XBT",null,null,"XBT 21 applied to line 0168."]
["2016-03-28T03:19:41.550","2016-03-28T15:19:41.550","wp","sonar","knudsen","Phase Mode","3500-4500"]
["2016-03-28T03:25:48.580","2016-03-28T15:25:48.580","wp","sonar","Multibeam","new line","end turn, new line 0169"]
["2016-03-28T03:33:05.500","2016-03-28T15:33:05.500","BG","sonar","knudsen","phase range","3000-4000"]
["2016-03-28T03:40:29.180","2016-03-28T15:40:29.180","wp","sonar","knudsen","phase range","phase 2500 - 3500"]
["2016-03-28T03:52:14.540","2016-03-28T15:52:14.540","BG","sonar","knudsen","Phase Range"," 2000- 3000"]
["2016-03-28T03:57:39.880","2016-03-28T15:57:39.880","BG","sonar","Knudsen","Phase Range"," 1500-2500"]
["2016-03-28T03:58:54.090","2016-03-28T15:58:54.090","BG","sonar","Knudsen","phase range","1000-2000"]
["2016-03-28T04:37:15.770","2016-03-28T16:37:15.770","BG","sonar","Knudsen",null,"phase 2000-3000, tx power 3"]
["2016-03-28T04:42:11.800","2016-03-28T16:42:11.800","BG","sonar","Knudsen","phase range","2500-3500"]
["2016-03-28T04:51:04.290",{"$f":"IF(ISBLANK(A574), \" \", ((A574)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-28T16:51:04.290"},"BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T05:00:05.300","2016-03-28T17:00:05.300","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-28T05:07:44.310","2016-03-28T17:07:44.310","wp","sonar","multibeam","new line","begin turn, new line 0171"]
["2016-03-28T05:09:01.510","2016-03-28T17:09:01.510","wp","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-28T05:13:06","2016-03-28T17:13:06","wp","sonar","multibeam","new line","end turn, new line 0172"]
["2016-03-28T05:16:20.780","2016-03-28T17:16:20.780","wp","sonar","knudsen","phase range","3500-4500"]
["2016-03-28T05:20:31.200","2016-03-28T17:20:31.200","BG","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-28T05:26:11.410","2016-03-28T17:26:11.410","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T05:31:05.860","2016-03-28T17:31:05.860","DF","Sonar","multibeam","new line","end turn line 0172, started new survey trackline 0173"]
["2016-03-28T05:34:00.980","2016-03-28T17:34:00.980","DF","Sonar","multibeam","Aeration Filter (On/Off)","off, sea bottom is highly variable"]
["2016-03-28T05:34:29.940","2016-03-28T17:34:29.940","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-03-28T05:42:10.720","2016-03-28T17:42:10.720","DS","Sonar","Knudsen","Phase Range","2000-3000, power reduced to 2"]
["2016-03-28T05:50:47.510","2016-03-28T17:50:47.510","BG","sonar","Knudsen","phase range","1500-2500"]
["2016-03-28T05:54:51.170","2016-03-28T17:54:51.170","BG","sonar","knudsen","phase range","1000-2000"]
["2016-03-28T05:56:48.250","2016-03-28T17:56:48.250","BG","sonar","knudsen","Tx Power","reduced to 1"]
["2016-03-28T06:05:04.110","2016-03-28T18:05:04.110","BG","sonar","knudsen","Gain Value","reduced to 34 db"]
["2016-03-28T06:07:32.810","2016-03-28T18:07:32.810","BG","sonar","Knudsen","Tx Pulse","reduced tp 4ms"]
["2016-03-28T06:10:34.270","2016-03-28T18:10:34.270","DF","sonar","multibeam","Max Angle","70/70"]
["2016-03-28T06:12:37.180","2016-03-28T18:12:37.180","DF","sonar","multibeam","Max Angle","65/70"]
["2016-03-28T06:15:56.970","2016-03-28T18:15:56.970","DF","sonar","multibeam","Aeration Filter (On/Off)","on"]
["2016-03-28T06:36:21.780","2016-03-28T18:36:21.780","BG","sonar","Knudsen",null,"range 1500-2500, tx power increased to 2, gain changed to 36"]
["2016-03-28T06:38:29.230","2016-03-28T18:38:29.230","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off, sea bottom is highly variable"]
["2016-03-28T06:49:09.580","2016-03-28T18:49:09.580","BG","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-28T06:59:53.560","2016-03-28T18:59:53.560","DF","sonar","Multibeam","new line","begin turn line 0175"]
["2016-03-28T07:05:00.270","2016-03-28T19:05:00.270","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-03-28T07:08:00.660","2016-03-28T19:08:00.660","DF","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T07:16:51.150","2016-03-28T19:16:51.150","df","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-28T07:23:07.090","2016-03-28T19:23:07.090","df","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T07:27:25.170","2016-03-28T19:27:25.170","df","Sonar","Multibeam","new line","end turn line 0175, started new survey trackline 0176"]
["2016-03-28T07:34:19.950","2016-03-28T19:34:19.950","df","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-28T07:36:07.830","2016-03-28T19:36:07.830","df","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-28T07:41:45.750","2016-03-28T19:41:45.750","df","sonar","Knudsen",null,"tx pulse to 4 ms, tx power to 1, phase to 1500-2500"]
["2016-03-28T07:46:37.040","2016-03-28T19:46:37.040","df","sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-28T07:53:42.270","2016-03-28T19:53:42.270","df","Sonar","Knudsen",null,"tx pulse to 2 ms, gain to 36 dB"]
["2016-03-28T08:35:06.030","2016-03-28T20:35:06.030","BG","sonar","knudsen",null,"phase range to 2000-3000, tx power to 3, tx pulse to 8ms"]
["2016-03-28T08:40:54.130","2016-03-28T20:40:54.130","BG","sonar","Knudsen","Tx Power","decreased to 2"]
["2016-03-28T08:50:36.990","2016-03-28T20:50:36.990","df","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-28T08:54:52.810","2016-03-28T20:54:52.810","BG","Sonar","Multibeam","New Line","Begin turn line 0178"]
["2016-03-28T08:56:03.170","2016-03-28T20:56:03.170","BG","sonar","knudsen","phase range","3000-4000"]
["2016-03-28T09:00:21.610","2016-03-28T21:00:21.610","bg","sonar","knudsen","Tx Pulse","16ms"]
["2016-03-28T09:06:20.400","2016-03-28T21:06:20.400","df","sonar","knudsen","TX Power",3]
["2016-03-28T09:11:14.340","2016-03-28T21:11:14.340","BG","sonar","knudsen","phase range","3500-4500"]
["2016-03-28T09:21:35.380","2016-03-28T21:21:35.380","BG","sonar","Multibeam","New Line","begin new survey line 0179"]
["2016-03-28T09:25:39.320","2016-03-28T21:25:39.320","SM","Sonar","knudsen","phase range","3000-4000"]
["2016-03-28T09:35:50.430","2016-03-28T21:35:50.430","BG","sonar","knudsen","phase range","2500-3500"]
["2016-03-28T09:40:14.700","2016-03-28T21:40:14.700","BG","sonar","knudsen",null,"phase range to 2000-3000, tx power to 2"]
["2016-03-28T09:44:50.930","2016-03-28T21:44:50.930","SM","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-28T09:45:29.350","2016-03-28T21:45:29.350","BG","XBT",null,null,"applied new xbt to 0179"]
["2016-03-28T09:54:50.350","2016-03-28T21:54:50.350","BG","sonar","Knudsen","phase range","2000-3000"]
["2016-03-28T10:15:23.960","2016-03-28T22:15:23.960","BG","sonar","Knudsen","phase range","2500-3500"]
["2016-03-28T10:40:21.620","2016-03-28T22:40:21.620","BG","sonar","Knudsen","Tx Power","increased to 3"]
["2016-03-28T10:48:49.350","2016-03-28T22:48:49.350","BG","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T10:53:03.140","2016-03-28T22:53:03.140","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-28T10:54:56.160","2016-03-28T22:54:56.160","BG","Sonar","Multibeam","New Line","begin turn line 0181"]
["2016-03-28T11:02:55.500","2016-03-28T23:02:55.500","BG","sonar","multibeam","new line","begin new survey line 0182"]
["2016-03-28T11:12:48.480","2016-03-28T23:12:48.480","BG","sonar","knudsen","phase range","4000-5000"]
["2016-03-28T11:16:18.170","2016-03-28T23:16:18.170","bg","sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-28T11:31:59.460","2016-03-28T23:31:59.460","bg","sonar","Knudsen","Phase Range","5000-6000"]
["2016-03-28T11:50:35.510","2016-03-28T23:50:35.510","SM","Sonar","EK","Change Range","max 6000"]
["2016-03-28T12:04:52.290","2016-03-29T00:04:52.290","ab","Sonar","EK","Change Range","max 6500"]
["2016-03-28T14:27:30.970","2016-03-29T02:27:30.970","ca","sonar","knudsen","Phase Range","4500-5500m"]
["2016-03-28T14:31:16.840","2016-03-29T02:31:16.840","ca","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-28T15:02:52.320","2016-03-29T03:02:52.320","AB","XBT",null,null,"#23"]
["2016-03-28T15:07:00.510","2016-03-29T03:07:00.510","AB","sonar","knudsen","phase range","4500-5500m"]
["2016-03-28T15:08:17.950",{"$f":"IF(ISBLANK(A638), \" \", ((A638)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-29T03:08:17.950"},"AB","XBT",null,null,"#23 applied to New Line 0187 - wrong SV; make get bad data in processing"]
["2016-03-28T15:12:13.550","2016-03-29T03:12:13.550","AB","XBT",null,null,"#23 applied to New Line 0188"]
["2016-03-28T15:34:22.110","2016-03-29T03:34:22.110","AB","sonar","multibeam","Ping Mode","Very Deep"]
["2016-03-28T16:03:39.170","2016-03-29T04:03:39.170","AB","sonar","multibeam","new line","0189 - 270 deg turn"]
["2016-03-28T16:22:17.780","2016-03-29T04:22:17.780","AB","sonar","multibeam","new line","0190"]
["2016-03-28T16:22:53.270","2016-03-29T04:22:53.270","AB","sonar","Knudsen","phase range","4000-5000m"]
["2016-03-28T16:29:14.090","2016-03-29T04:29:14.090","Ab","sonar","Knudsen","phase range","3500-4500m"]
["2016-03-28T16:34:20.280","2016-03-29T04:34:20.280","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-03-28T16:37:50.440","2016-03-29T04:37:50.440","AB","sonar","Knudsen","phase range","2500-3500m"]
["2016-03-28T16:41:45.920","2016-03-29T04:41:45.920","AB","Sonar","knudsen","Phase range","2000-3000m"]
["2016-03-28T16:45:15.700","2016-03-29T04:45:15.700","AB","Sonar","knudsen",null,"Pulse 4, Power 2"]
["2016-03-28T16:45:38.050","2016-03-29T04:45:38.050","AB","sonar","Multibeam",null,"Auto Mode (Deep), Max Angle 70/70"]
["2016-03-28T16:53:43.870","2016-03-29T04:53:43.870","AB","sonar","Knudsen","Phase range","2500-3500m"]
["2016-03-28T17:03:06.450","2016-03-29T05:03:06.450","ca","sonar","Knudsen","Phase Range","3000-4000m, Pulse 8, Power 3"]
["2016-03-28T17:10:39.020","2016-03-29T05:10:39.020","ca","Sonar","Knudsen",null,"Pulse 4, Power 2"]
["2016-03-28T18:01:52.550","2016-03-29T06:01:52.550","ca","sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-28T18:17:08.020","2016-03-29T06:17:08.020","ca","sonar","Knudsen","phase range","3500-4500m"]
["2016-03-28T18:58:49.850","2016-03-29T06:58:49.850","AB","sonar","Knudsen","Phase Range","3000-4000m; Gain 39dB"]
["2016-03-28T19:10:20.960","2016-03-29T07:10:20.960","AB","sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-28T19:14:54.280","2016-03-29T07:14:54.280","AB","sonar","Knudsen","Phase Range","2000-3000m; Power 2, Pulse 4"]
["2016-03-28T19:20:37.910","2016-03-29T07:20:37.910","AB","sonar","knudsen","Phase Range","1500-2500m "]
["2016-03-28T19:26:56.600","2016-03-29T07:26:56.600","AB","sonar","Knudsen","Phase range","2000-3000m, Power 3, Pulse 8"]
["2016-03-28T19:46:15.660","2016-03-29T07:46:15.660","DS","Sonar","Multibeam",null,"Mode is stuck in auto and is not adjusting mode right. FM disable was checked - I turned it off. "]
["2016-03-28T20:04:08.050","2016-03-29T08:04:08.050","ds","Sonar","Multibeam",null,"Stopped logging, problems with SIS app - tear off, will not come out of Auto mode. Line 0195."]
["2016-03-28T20:05:44.300","2016-03-29T08:05:44.300","DS","Sonar","Multibeam","New Line","End turn, new line 0196."]
["2016-03-28T20:08:32.090","2016-03-29T08:08:32.090","DS","Sonar","Multibeam",null,"Switched \"Runtime Parameters\" to \"Mini Runtime Parameters\", and switched out of Auto, Problem resolved when the tear off was switched back to \"Runtime Parameters.\""]
["2016-03-28T20:22:03.410","2016-03-29T08:22:03.410","DS","Sonar","Multibeam","New Line","Begin Turn line 0197"]
["2016-03-28T20:26:07.420","2016-03-29T08:26:07.420","DS","Sonar","Multibeam","New Line","start survey line 0198."]
["2016-03-28T20:36:23.220","2016-03-29T08:36:23.220","wp","sonar","knudsen","Phase Mode","4000-5000, pulse 8, power 3"]
["2016-03-28T20:49:26.830","2016-03-29T08:49:26.830","wp","sonar","knudsen","Phase Mode","3500-4500"]
["2016-03-28T20:51:05.760","2016-03-29T08:51:05.760","wp","sonar","Multibeam","New Line","Line Missing NO LINE 0194, line skipped in Line Cnt."]
["2016-03-28T21:08:30.650","2016-03-29T09:08:30.650","MP","XBT",null,null,"#24, Lat 17 32.58, Lon 166 39.68 "]
["2016-03-28T21:08:52.650","2016-03-29T09:08:52.650","MP","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T21:15:59.900","2016-03-29T09:15:59.900","CR","XBT",null,null,"Applied XBT to line 198"]
["2016-03-28T21:23:42.110","2016-03-29T09:23:42.110","wp","sonar","knudsen","phase range","3500-4500"]
["2016-03-28T21:53:20.030","2016-03-29T09:53:20.030","CR","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-28T21:58:00.600","2016-03-29T09:58:00.600","CR","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-28T22:19:15.900","2016-03-29T10:19:15.900","wp","sonar","Multibeam","New Line","End Survey Line, Begin Turn, New Line 0200"]
["2016-03-28T22:30:48.560","2016-03-29T10:30:48.560","wp","sonar","knudsen","Phase Range","Pulse 4, Power3, phase range 4000-5000."]
["2016-03-28T22:41:10.210","2016-03-29T10:41:10.210","CR","Sonar","knudsen","Phase Range","4500-5500"]
["2016-03-28T22:45:59.180","2016-03-29T10:45:59.180","DS","Sonar","Multibeam","Ping Mode","changed from auto (xtra deep) to very deep, max angles 35/35"]
["2016-03-28T23:00:44.710","2016-03-29T11:00:44.710","DS","Sonar","Multibeam","Max Angle","30/3027"]
["2016-03-29T00:23:27.080","2016-03-29T12:23:27.080","CR","sonar","Knudsen","Phase Range","4000-5000, Pulse 4, Power 3."]
["2016-03-29T00:31:56.990","2016-03-29T12:31:56.990","CR","Sonar","Knudsen","Phase Mode","3500-4500"]
["2016-03-29T00:36:31.800","2016-03-29T12:36:31.800","CR","Sonar","knudsen","Tx Pulse",8]
["2016-03-29T00:36:50.880","2016-03-29T12:36:50.880","CR","Sonar","knudsen","Phase Range","3000-4000"]
["2016-03-29T00:45:27.180","2016-03-29T12:45:27.180","Wp","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-29T01:04:30.850","2016-03-29T13:04:30.850","CR","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-29T01:16:51.420","2016-03-29T13:16:51.420","CR","Sonar","knudsen","Phase Range","4000-5000"]
["2016-03-29T01:21:39.810","2016-03-29T13:21:39.810","CR","sonar","knudsen","Phase Range","4500-5500"]
["2016-03-29T01:38:22.400","2016-03-29T13:38:22.400","wp","sonar","Multibeam","new line","Begin Turn, new line 0204"]
["2016-03-29T01:41:10.710","2016-03-29T13:41:10.710","wp","sonar","multibeam","new line","Begin Survey line 0205."]
["2016-03-29T01:44:54.400","2016-03-29T13:44:54.400","CR","Sonar","Knudsen","Phase Range","5000-6000, pulse 16, power 2, Gain 35"]
["2016-03-29T01:50:15.200","2016-03-29T13:50:15.200","CR","sonar","Knudsen","Tx PUlse","3 / gain to 39"]
["2016-03-29T03:08:32.060","2016-03-29T15:08:32.060","wp","xbt",null,null,"xbt applied to line 206"]
["2016-03-29T03:27:05.980","2016-03-29T15:27:05.980","BG","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-29T03:28:21.750","2016-03-29T15:28:21.750","BG","Sonar","Knudsen","Tx Pulse","32 ms"]
["2016-03-29T03:29:59.030","2016-03-29T15:29:59.030","DS","Sonar","Knudsen","Gain Value","47 dB"]
["2016-03-29T03:35:11.860","2016-03-29T15:35:11.860","DS","Sonar","Multibeam","Max Angle","reduced to 27/27 to get better quality swath"]
["2016-03-29T03:39:12.130","2016-03-29T15:39:12.130","DS","Sonar","Multibeam","Aeration Filter (On/Off)","turned on aeration filter and set range gate to small to clean up swath"]
["2016-03-29T03:53:40.330","2016-03-29T15:53:40.330","DS","Sonar","Multibeam","Start Line","turn line 0208"]
["2016-03-29T03:55:39.550","2016-03-29T15:55:39.550","DS","Sonar","Multibeam","Start Line","survey line 0209"]
["2016-03-29T04:03:48.960","2016-03-29T16:03:48.960","DS","sonar","Multibeam",null,"Range Gate to Normal"]
["2016-03-29T04:04:50.200","2016-03-29T16:04:50.200","DS","sonar","Multibeam","Along Direction Pitch","from 2 to -2"]
["2016-03-29T04:08:56.860",{"$f":"IF(ISBLANK(A702), \" \", ((A702)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-29T16:08:56.860"},"DS","Sonar","Multibeam","Max Angle","29/29"]
["2016-03-29T04:09:24.650","2016-03-29T16:09:24.650","BG","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-29T04:10:12.670","2016-03-29T16:10:12.670","DF","sonar","Multibeam","Along Direction Pitch",-1]
["2016-03-29T04:11:54.960","2016-03-29T16:11:54.960","BG","sonar","Knudsen","Gain Value","42 dB"]
["2016-03-29T04:12:38.490","2016-03-29T16:12:38.490","DF","sonar","Multibeam","Along Direction Pitch",-2]
["2016-03-29T04:12:48.140","2016-03-29T16:12:48.140","DF","sonar","Multibeam","Spike Filter Strength","STRONG"]
["2016-03-29T04:13:30.500","2016-03-29T16:13:30.500","DF","sonar","Multibeam","Along Direction Pitch",-3]
["2016-03-29T04:15:31.690","2016-03-29T16:15:31.690","BG","sonar","Knudsen","Tx Pulse","16 ms"]
["2016-03-29T04:16:09.330","2016-03-29T16:16:09.330","DF","Sonar","Multibeam",null,"along direction angle to -4, max angles 30/30"]
["2016-03-29T04:22:24.680","2016-03-29T16:22:24.680","BG","Sonar","knudsen","Gain Value",40]
["2016-03-29T04:25:36.820","2016-03-29T16:25:36.820","BG","Sonar","knudsen","Gain Value",42]
["2016-03-29T05:03:44.970","2016-03-29T17:03:44.970","BG","Sonar","knudsen","Gain Value"," 46 dB"]
["2016-03-29T05:05:09.530","2016-03-29T17:05:09.530","BG","Sonar","knudsen","Phase Range","3500-4500"]
["2016-03-29T05:27:47.980","2016-03-29T17:27:47.980","BG","sonar","knudsen","Phase Range","4000-5000"]
["2016-03-29T05:33:52.310","2016-03-29T17:33:52.310","BG","Sonar","Multibeam","New Line","begin turn line 0211"]
["2016-03-29T05:39:46.800","2016-03-29T17:39:46.800","BG","sonar","Multibeam","New Line","begin new survey line 0213, line 0212 skipped"]
["2016-03-29T06:00:00.540","2016-03-29T18:00:00.540","BG","sonar","Knudsen","Phase Range","3500--4500"]
["2016-03-29T06:02:55.480","2016-03-29T18:02:55.480","DS","Sonar","Multibeam","Max Angle","opened angles to 39/39"]
["2016-03-29T06:06:04.670","2016-03-29T18:06:04.670","DF","sonar","Multibeam","Max Angle","38/38"]
["2016-03-29T06:06:35.620","2016-03-29T18:06:35.620","DF","sonar","Multibeam","Aeration Filter (On/Off)","off, sea bottom is highly variable"]
["2016-03-29T06:07:20.620","2016-03-29T18:07:20.620","DF","sonar","Multibeam","Max Angle","35/38"]
["2016-03-29T06:08:07.570","2016-03-29T18:08:07.570","DF","sonar","Multibeam","Max Angle","30/38"]
["2016-03-29T06:23:17.290","2016-03-29T18:23:17.290","DF","sonar","Multibeam","Aeration Filter (On/Off)","on"]
["2016-03-29T06:24:22.530","2016-03-29T18:24:22.530","DF","sonar","Multibeam","Along Direction Pitch",-4]
["2016-03-29T06:24:40.960","2016-03-29T18:24:40.960","BG","sonar","knudsen","Phase Range","3000-4000"]
["2016-03-29T06:25:07.690","2016-03-29T18:25:07.690","DF","Sonar","Multibeam","Max Angle","30/30"]
["2016-03-29T06:25:30.440","2016-03-29T18:25:30.440","DF","Sonar","Multibeam","Along Direction Pitch",-5]
["2016-03-29T06:27:24.940","2016-03-29T18:27:24.940","DF","Sonar","Multibeam","Ping Mode","VERY DEEP"]
["2016-03-29T06:29:31.420","2016-03-29T18:29:31.420","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-29T06:35:46.470","2016-03-29T18:35:46.470","BG","Sonar","Multibeam","new line","begin turn line 0124"]
["2016-03-29T06:42:15.110","2016-03-29T18:42:15.110","BG","sonar","Multibeam","new line","begin survey line 0125"]
["2016-03-29T06:43:01.070","2016-03-29T18:43:01.070","DF","Sonar","Multibeam","Max Angle","30/30"]
["2016-03-29T06:43:56.630","2016-03-29T18:43:56.630","DF","Sonar","Multibeam",null,"auto tilt on"]
["2016-03-29T06:50:55.960","2016-03-29T18:50:55.960","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-29T07:02:50.520","2016-03-29T19:02:50.520","DF","Sonar","knudsen","Phase Range","2500-3500"]
["2016-03-29T07:15:17.340","2016-03-29T19:15:17.340","BG","sonar","knudsen","Phase Range","2000-3000"]
["2016-03-29T07:16:39.430","2016-03-29T19:16:39.430","BG","sonar","Knudsen",null,"tx pulse 8ms, tx power 2"]
["2016-03-29T07:18:25.850","2016-03-29T19:18:25.850","DS","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-29T07:22:01.890","2016-03-29T19:22:01.890","BG","Sonar","Knudsen",null,"phase range 1500-2500, gain 36 dB"]
["2016-03-29T07:26:40.550","2016-03-29T19:26:40.550","BG","sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-29T07:28:50.020","2016-03-29T19:28:50.020","DS","Sonar","Multibeam","Ping Mode","switched to auto, max angles 60/60"]
["2016-03-29T07:33:24.510","2016-03-29T19:33:24.510","BG","sonar","Knudsen","Tx Pulse","4 ms"]
["2016-03-29T07:34:14.060","2016-03-29T19:34:14.060","DF","Sonar","Multibeam","Max Angle","50/50"]
["2016-03-29T07:35:46.920","2016-03-29T19:35:46.920","DF","Sonar","Multibeam","Max Angle","48/48"]
["2016-03-29T07:42:38.740","2016-03-29T19:42:38.740","DF","Sonar","Multibeam","Max Angle","52/48"]
["2016-03-29T07:43:42.910","2016-03-29T19:43:42.910","BG","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-29T07:46:36.880","2016-03-29T19:46:36.880","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off, sea bottom is highly variable"]
["2016-03-29T07:47:57.670","2016-03-29T19:47:57.670","DF","Sonar","Multibeam","Max Angle","45/45"]
["2016-03-29T07:49:11.680","2016-03-29T19:49:11.680","DF","sonar","Multibeam","Max Angle","45/40"]
["2016-03-29T07:53:16.630","2016-03-29T19:53:16.630","DF","sonar","Multibeam","Max Angle","40/35"]
["2016-03-29T07:53:55.250","2016-03-29T19:53:55.250","DF","Sonar","Multibeam","Max Angle","45/30"]
["2016-03-29T07:58:12.370","2016-03-29T19:58:12.370","BG","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-29T08:08:09.330","2016-03-29T20:08:09.330","DF","sonar","Multibeam","Max Angle","42/28"]
["2016-03-29T08:11:24.310","2016-03-29T20:11:24.310","SM","sonar","Knudsen","phase range","2500-3500"]
["2016-03-29T08:11:51.240","2016-03-29T20:11:51.240","DF","sonar","Multibeam","Max Angle","40/28"]
["2016-03-29T08:12:44.450","2016-03-29T20:12:44.450","DF","sonar","Multibeam","Along Direction Pitch","auto tilt off and degree to -1"]
["2016-03-29T08:18:36.770","2016-03-29T20:18:36.770","DF","sonar","Multibeam","Max Angle","35/25"]
["2016-03-29T08:20:33.030","2016-03-29T20:20:33.030","DF","sonar","Multibeam","New Line","start turn line 0217"]
["2016-03-29T08:26:54.790","2016-03-29T20:26:54.790","DF","Sonar","Multibeam","Max Angle","35/30"]
["2016-03-29T08:30:17.120","2016-03-29T20:30:17.120","DF","Sonar","Multibeam","Max Angle","35/35"]
["2016-03-29T08:32:01.810","2016-03-29T20:32:01.810","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-29T08:35:15.800","2016-03-29T20:35:15.800","DF","Sonar","Multibeam","New Line","started survey trackline 0218"]
["2016-03-29T08:36:20.760","2016-03-29T20:36:20.760","DF","Sonar","Multibeam","Max Angle","42/42"]
["2016-03-29T08:40:17.120","2016-03-29T20:40:17.120","DF","sonar","Multibeam","Along Direction Pitch",1]
["2016-03-29T08:41:21.470",{"$f":"IF(ISBLANK(A766), \" \", ((A766)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-29T20:41:21.470"},"DF","Sonar","Multibeam","Max Angle","40/42"]
["2016-03-29T08:45:35.530","2016-03-29T20:45:35.530","DF","sonar","Multibeam","Max Angle","40/40"]
["2016-03-29T09:04:08.020","2016-03-29T21:04:08.020","SM","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-29T09:04:25.370","2016-03-29T21:04:25.370","SM","Sonar","knudsen","Phase Range","1500-2500"]
["2016-03-29T09:28:19","2016-03-29T21:28:19","SM","xbt",null,null,"cast 026 collected"]
["2016-03-29T09:42:24.830","2016-03-29T21:42:24.830","SM","xbt",null,null,"Cast 026 applied to line 0219"]
["2016-03-29T09:48:40.270","2016-03-29T21:48:40.270","DF","sonar","Multibeam","Max Angle","38/38"]
["2016-03-29T09:48:55.120","2016-03-29T21:48:55.120","BG","sonar","knudsen","Phase Range","2000-3000"]
["2016-03-29T09:50:59.960","2016-03-29T21:50:59.960","bg","sonar","knudsen",null,"phase range 2500-3500, tx power 3, tx pulse 8ms"]
["2016-03-29T09:51:41.530","2016-03-29T21:51:41.530","DF","sonar","Multibeam","Max Angle","35/35"]
["2016-03-29T09:54:29.730","2016-03-29T21:54:29.730","DF","sonar","Multibeam","Ping Mode","VERY DEEP"]
["2016-03-29T09:56:41.060","2016-03-29T21:56:41.060","DF","Sonar","Knudsen","Gain Value",40]
["2016-03-29T10:01:06.260","2016-03-29T22:01:06.260","BG","Sonar","Multibeam","new line","begin turn line 0220"]
["2016-03-29T10:03:34.560","2016-03-29T22:03:34.560","BG","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-29T10:10:37.560","2016-03-29T22:10:37.560","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-29T10:14:19.600","2016-03-29T22:14:19.600","DF","Sonar","Multibeam","new line","begin survey trackline 0221"]
["2016-03-29T10:21:06.640","2016-03-29T22:21:06.640","DF","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-29T10:30:09.790","2016-03-29T22:30:09.790","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-29T10:35:07.910","2016-03-29T22:35:07.910","DF","Sonar","Multibeam","Ping Mode","deep"]
["2016-03-29T10:36:06.610","2016-03-29T22:36:06.610","Df","sonar","Multibeam","Max Angle","30/30"]
["2016-03-29T10:37:16.680","2016-03-29T22:37:16.680","DF","Sonar","Multibeam","Ping Mode","very deep"]
["2016-03-29T10:40:39.860","2016-03-29T22:40:39.860","DF","sonar","Multibeam","Along Direction Pitch",-1]
["2016-03-29T10:43:37.420","2016-03-29T22:43:37.420","DF","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-29T10:51:59.930","2016-03-29T22:51:59.930","DF","Sonar","Multibeam","Max Angle","35/35"]
["2016-03-29T10:54:59.290","2016-03-29T22:54:59.290","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-29T10:55:34.060","2016-03-29T22:55:34.060","DF","sonar","Knudsen",null,"tx pulse to 8, tx power to 2"]
["2016-03-29T10:58:40.230","2016-03-29T22:58:40.230","DF","Sonar","Multibeam","Max Angle","40/35"]
["2016-03-29T11:18:11.880","2016-03-29T23:18:11.880","BG","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-29T11:20:07.200","2016-03-29T23:20:07.200","DF","Sonar","Multibeam","Max Angle","38/30"]
["2016-03-29T11:25:30.100","2016-03-29T23:25:30.100","DF","Sonar","Knudsen",null,"tx pulse to 4 ms, tx power to 3"]
["2016-03-29T11:42:00.520","2016-03-29T23:42:00.520","AB","Sonar","Multibeam","New Line","0223 - turn"]
["2016-03-29T11:51:25.770","2016-03-29T23:51:25.770","AB","Sonar","Multibeam","New Line","0224'"]
["2016-03-29T12:11:18.830","2016-03-30T00:11:18.830","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-29T12:22:17.150","2016-03-30T00:22:17.150","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-03-29T12:36:35.820","2016-03-30T00:36:35.820","ca","sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-29T12:53:30.220","2016-03-30T00:53:30.220","AB","sonar","Knudsen","Phase Range","3000-4000m"]
["2016-03-29T12:55:01.950","2016-03-30T00:55:01.950","AB","Sonar","Multibeam","Max Angle","45/40"]
["2016-03-29T13:05:44.120","2016-03-30T01:05:44.120","AB","sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-29T13:09:45.200","2016-03-30T01:09:45.200","AB","sonar","Multibeam","New Line","0226 - turn"]
["2016-03-29T13:11:14.380","2016-03-30T01:11:14.380","AB","sonar","Multibeam","Max Angle","40/40"]
["2016-03-29T13:21:58.260","2016-03-30T01:21:58.260","AB","sonar","Multibeam","New Line","0227"]
["2016-03-29T13:26:35.340","2016-03-30T01:26:35.340","AB","sonar","Multibeam",null,"Data deteriorating after turn due to weather"]
["2016-03-29T13:43:42.890","2016-03-30T01:43:42.890","AB","sonar","Knudsen",null,"Power 3, Pulse 4, Phase range 3000-4000m"]
["2016-03-29T14:12:47.340","2016-03-30T02:12:47.340","AB","sonar","Knudsen","Phase Range","3000-4000m"]
["2016-03-29T14:21:18.970","2016-03-30T02:21:18.970","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-29T14:40:58.130","2016-03-30T02:40:58.130","AB","Sonar","Multibeam","New Line","0229 - turn"]
["2016-03-29T14:53:27.040","2016-03-30T02:53:27.040","AB","Sonar","Multibeam","New Line","0230"]
["2016-03-29T15:07:28.740","2016-03-30T03:07:28.740","AB","xbt",null,null,"#30 completed and added to new line 0231"]
["2016-03-29T16:01:53.270","2016-03-30T04:01:53.270","AB","Sonar","Multibeam","new line","0232 - turn"]
["2016-03-29T16:06:28.570","2016-03-30T04:06:28.570","AB","sonar","Multibeam","new line","0233"]
["2016-03-29T16:18:22.770","2016-03-30T04:18:22.770","AB","Sonar","Knudsen","Phase range","3000-4000m"]
["2016-03-29T16:26:13.240","2016-03-30T04:26:13.240","AB","sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-29T16:32:53.450","2016-03-30T04:32:53.450","AB","sonar","Knudsen","Phase Range","2000-3000m"]
["2016-03-29T16:42:54.030","2016-03-30T04:42:54.030","AB","Sonar","knudsen","Phase Range","2500-3500m"]
["2016-03-29T16:48:28.710","2016-03-30T04:48:28.710","AB","sonar","knudsen","Phase Range","3000-4000m"]
["2016-03-29T16:49:28.850","2016-03-30T04:49:28.850","AB","sonar","Multibeam","Max Angle","42/52"]
["2016-03-29T16:53:09.240","2016-03-30T04:53:09.240","AB","sonar","Multibeam","new line","0234 - turn"]
["2016-03-29T17:00:46.220","2016-03-30T05:00:46.220","AB","sonar","Multibeam","new line","0235, Max angles 52/52"]
["2016-03-29T17:04:57.300","2016-03-30T05:04:57.300","AB","sonar","Multibeam","Max Angle","40/50"]
["2016-03-29T17:09:02.920","2016-03-30T05:09:02.920","AB","sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-29T17:15:54.270","2016-03-30T05:15:54.270","AB","sonar","Multibeam","Phase Range","2000-3000m"]
["2016-03-29T17:20:16.750","2016-03-30T05:20:16.750","AB","Sonar","Multibeam","Ping Mode","DEEP; Max Angle 55/70"]
["2016-03-29T17:21:49.910","2016-03-30T05:21:49.910","AB","Sonar","Knudsen","Phase Range","1500-2500m , Power 2, Gain 37"]
["2016-03-29T17:29:33.410","2016-03-30T05:29:33.410","AB","Sonar","Knudsen","Phase Range","1000-2000m, Power 1, Pulse 2"]
["2016-03-29T18:18:02.540",{"$f":"IF(ISBLANK(A830), \" \", ((A830)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-30T06:18:02.540"},"AB","sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-29T18:43:24.240","2016-03-30T06:43:24.240","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-03-29T18:43:50.370","2016-03-30T06:43:50.370","AB","sonar","Multibeam","Ping Mode","Very Deep, Max Angles 52/50"]
["2016-03-29T18:54:08.280","2016-03-30T06:54:08.280","AB","Sonar","Multibeam","New Line","0238 - turn"]
["2016-03-29T19:14:01.350","2016-03-30T07:14:01.350","AB","Sonar","Multibeam","New Line","0239, Max Angles 52/52"]
["2016-03-29T19:16:52.010","2016-03-30T07:16:52.010","AB","sonar","Knudsen","Phase Range","2000-3000m"]
["2016-03-29T19:35:22.960","2016-03-30T07:35:22.960","AB","Sonar","Multibeam","Ping Mode","Deep Mode, Max Angle 50/60"]
["2016-03-29T19:38:06.350","2016-03-30T07:38:06.350","AB","sonar","Multibeam","Max Angle","55/65"]
["2016-03-29T19:40:05.380","2016-03-30T07:40:05.380","wp","Other",null,null,"Watch Change"]
["2016-03-29T20:07:35.090","2016-03-30T08:07:35.090","wp","sonar","Knudsen","Gain Value","31 dB, pulse 4, power 2, phase range, 1500-2500."]
["2016-03-29T20:31:37.630","2016-03-30T08:31:37.630","wp","sonar","Knudsen","Phase Range","2000-3000, pulse 8, power 3, gain 31"]
["2016-03-29T20:34:53.240","2016-03-30T08:34:53.240","wp","sonar","Knudsen","Tx Pulse",16]
["2016-03-29T20:41:00.100","2016-03-30T08:41:00.100","wp","Sonar","Knudsen","Gain Value",36]
["2016-03-29T20:43:00.580","2016-03-30T08:43:00.580","wp","sonar","Knudsen","Phase Range","2500-3500, gain 41dB"]
["2016-03-29T20:52:26.910",{"$f":"((A844)-DATE(1970,1,1))+25569+($C$1/24)","v":"2016-03-30T08:52:26.910"},"wp","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-29T20:54:23.720","2016-03-30T08:54:23.720","wp","sonar","knudsen","Tx Pulse","pulse 8, power 3, gain 34."]
["2016-03-29T20:59:14.840","2016-03-30T08:59:14.840","wp","sonar","multibeam","New Line","begin turn, new line 0241"]
["2016-03-29T21:05:13.840","2016-03-30T09:05:13.840","wp","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-29T21:23:57.220","2016-03-30T09:23:57.220","wp","sonar","Multibeam","New Line","begin survey line, new line 0242"]
["2016-03-29T21:37:19.780","2016-03-30T09:37:19.780","wp","sonar","knudsen","Tx Pulse","pulse 16, gain 34, power 3"]
["2016-03-29T21:39:02.310","2016-03-30T09:39:02.310","MP","xbt",null,null,"XBT applied to line 0242"]
["2016-03-29T21:45:10.650","2016-03-30T09:45:10.650","wp","sonar","knudsen","Phase Range","3000-4000, pulse 16, power 3, gain 34"]
["2016-03-29T21:50:26.920","2016-03-30T09:50:26.920","wp","sonar","knudsen","Tx Pulse","pulse 32"]
["2016-03-29T21:54:23.360","2016-03-30T09:54:23.360","wp","sonar","Knudsen","Gain Value","gain 41 dB"]
["2016-03-29T21:55:13.140","2016-03-30T09:55:13.140","wp","sonar","Knudsen","Phase Range","Range 2500-3500"]
["2016-03-29T21:57:33.070","2016-03-30T09:57:33.070","wp","sonar","knudsen","Tx Pulse","Pulse 32, power 3, gain 37 dB, range 2500-3500."]
["2016-03-29T22:04:45.150","2016-03-30T10:04:45.150","wp","sonar","knudsen","Phase Range","range 2000-3000"]
["2016-03-29T22:18:37.180","2016-03-30T10:18:37.180","wp","sonar","Knudsen","Phase Range","range 1500-2500 "]
["2016-03-29T22:19:33.840","2016-03-30T10:19:33.840","wp","sonar","knudsen","Tx Pulse","pulse 8.0, power 3, gain 32dB, phase 1500-2500"]
["2016-03-29T22:25:14.010","2016-03-30T10:25:14.010","MP","sonar","knudsen","phase range","range 1000-2000, tx pulse 4.0, tx power 2, gain value 32dB'"]
["2016-03-29T22:30:05.110","2016-03-30T10:30:05.110","WP","Sonar","Knudsen","tx pulse","pulse 4.0, power 1, gain value 28, phase 1000-2000."]
["2016-03-29T23:02:55.220","2016-03-30T11:02:55.220","MP","Sonar","Knudsen","Tx Power","power 3, pulse 16, gain 31"]
["2016-03-29T23:08:26.860","2016-03-30T11:08:26.860","wp","sonar","knudsen","Phase range","1500-2500"]
["2016-03-29T23:16:19.380","2016-03-30T11:16:19.380","MP","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-29T23:22:58.980","2016-03-30T11:22:58.980","MP","Sonar","Knudsen","Gain Value","36dB"]
["2016-03-29T23:32:01.060","2016-03-30T11:32:01.060","MP","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-29T23:32:39.030","2016-03-30T11:32:39.030","wp","Sonar","Multibeam","new line","Begin turn, new line 0245"]
["2016-03-29T23:36:54.370","2016-03-30T11:36:54.370","wp","sonar","Knudsen","Tx Pulse","tx pulse 32ms, tx power 3, Gain Value 37 dB, Phase Range 2500-3500"]
["2016-03-29T23:51:43.740","2016-03-30T11:51:43.740","WP","Sonar","Multibeam","new line","begin survey line, new line 0246"]
["2016-03-29T23:53:17.680","2016-03-30T11:53:17.680","WP","Sonar","Knudsen","Phase Range","Range 2000-3000, Pulse 32, Power 3, gain 37"]
["2016-03-29T23:59:29.840","2016-03-30T11:59:29.840","WP","Sonar","Knudsen","Phase Range","Range 1500-2500, Pulse 16, power 2, gain 35 dB"]
["2016-03-30T00:15:22.650","2016-03-30T12:15:22.650","WP","Sonar","Knudsen","Phase Range","Range 1000-2000 , pulse 2.0, power 2, gain 27dB."]
["2016-03-30T00:19:30.840","2016-03-30T12:19:30.840","WP","sonar","Knudsen","Tx Pulse","pulse 8 ms, power 2, gain 27dB, range 1000-2000"]
["2016-03-30T00:34:36.500","2016-03-30T12:34:36.500","WP","Sonar","Knudsen","Tx Pulse","Pulse 2.0, Power 2.0,. Gain 24 dB, Range 1000-2000."]
["2016-03-30T01:07:08.710","2016-03-30T13:07:08.710","WP","Sonar","Knudsen","Phase Range","Range 1500-2500, Pulse 16, power 3, gain 24 dB"]
["2016-03-30T01:11:39.900","2016-03-30T13:11:39.900","DS","Sonar","Knudsen","Phase Range","Range 2000-3000, Pulse 16, Power 3, gain 29 dB."]
["2016-03-30T01:20:59.490",{"$f":"((A876)-DATE(1970,1,1))+25569+($C$1/24)","v":"2016-03-30T13:20:59.490"},"DS","Other",null,null,"asked ship to finish line 0247, then shift line plan 1000m to the NE"]
["2016-03-30T01:22:20.870","2016-03-30T13:22:20.870","MP","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-30T01:28:05.130","2016-03-30T13:28:05.130","MP","Sonar","Knudsen","Phase Range","3000-4000, gain 40dB, Tx Pulse 32"]
["2016-03-30T01:33:49.770","2016-03-30T13:33:49.770","MP","Sonar","Knudsen","Tx Power","16, gain 36dB"]
["2016-03-30T01:44:53.480","2016-03-30T13:44:53.480","MP","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-30T01:49:07.300","2016-03-30T13:49:07.300","MP","Sonar","Knudsen","Tx Pulse","32, gain 41dB"]
["2016-03-30T01:50:24.830","2016-03-30T13:50:24.830","WP","Sonar","Multibeam","New Line","Begin turn, new line 0248"]
["2016-03-30T02:13:36.030","2016-03-30T14:13:36.030","MP","Sonar","Multibeam","New Line","Begin survey line 0249"]
["2016-03-30T02:34:37.770","2016-03-30T14:34:37.770","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-30T02:39:28.450","2016-03-30T14:39:28.450","CR","Sonar","Knudsen","Tx Pulse","16ms"]
["2016-03-30T02:40:14.930","2016-03-30T14:40:14.930","CR","Sonar","Knudsen","Gain Value","36dB"]
["2016-03-30T02:49:18.980","2016-03-30T14:49:18.980","CR","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-30T02:52:33.100","2016-03-30T14:52:33.100","CR","sonar","Knudsen","Phase Range","1500-2500, gain 34dB, TxPower 2, TxPulse 8"]
["2016-03-30T03:08:30.320","2016-03-30T15:08:30.320","MP","sonar","Knudsen","Phase Range","1000-2000, dB32, Tx Pulse 8, Tx Pulse 1"]
["2016-03-30T03:11:00.210","2016-03-30T15:11:00.210","MP","XBT",null,null,"xbt 29"]
["2016-03-30T03:16:29.930","2016-03-30T15:16:29.930","MP","XBT",null,null,"XBT 29 applied to line 0250"]
["2016-03-30T03:45:09.380","2016-03-30T15:45:09.380","BG","Sonar","Knudsen","Tx Power",2]
["2016-03-30T03:52:01.490","2016-03-30T15:52:01.490","BG","sonar","Knudsen","Tx Power",3]
["2016-03-30T03:52:27.260","2016-03-30T15:52:27.260","bg","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-30T04:02:15.940","2016-03-30T16:02:15.940","bg","sonar","knudsen",null,"tx power 2, tx pulse 4 ms"]
["2016-03-30T04:10:40.100","2016-03-30T16:10:40.100","DF","sonar","multibeam","Max Angle","50/60"]
["2016-03-30T04:14:02.790",{"$f":"IF(ISBLANK(A897),\" \",((A897)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-30T16:14:02.790"},"BG","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-30T04:14:27.070","2016-03-30T16:14:27.070","df","sonar","Multibeam","Max Angle","50/55"]
["2016-03-30T04:15:06.090","2016-03-30T16:15:06.090","BG","sonar","knudsen",null,"tx power 3, gain value 36"]
["2016-03-30T04:15:56.190","2016-03-30T16:15:56.190","BG","sonar","knudsen","Phase Range","2500-3500"]
["2016-03-30T04:16:57.010","2016-03-30T16:16:57.010","DF","sonar","Multibeam","Max Angle","50/50"]
["2016-03-30T04:48:42.750","2016-03-30T16:48:42.750","DF","sonar","Multibeam",null,"geographical mapping stopped again while data was still recording, fixed it self!"]
["2016-03-30T04:52:54.540","2016-03-30T16:52:54.540","DF","sonar","Knudsen","tx pulse","8 ms"]
["2016-03-30T04:55:27.590","2016-03-30T16:55:27.590","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-30T05:02:07.330","2016-03-30T17:02:07.330","DF","sonar","knudsen","Tx Pulse","4 ms, gain to 40"]
["2016-03-30T05:03:32.850","2016-03-30T17:03:32.850","DF","sonar","knudsen","Phase Range","3500-4500"]
["2016-03-30T05:14:39.810","2016-03-30T17:14:39.810","DF","sonar","Multibeam","Max Angle","50/45"]
["2016-03-30T05:15:11.520","2016-03-30T17:15:11.520","DF","sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-03-30T05:43:56.620","2016-03-30T17:43:56.620","DF","sonar","Multibeam","Aeration Filter (On/Off)","on"]
["2016-03-30T05:46:11.900","2016-03-30T17:46:11.900","BG","Sonar","Knudsen","Phase range","4000-5000"]
["2016-03-30T06:11:16.820","2016-03-30T18:11:16.820","BG","Sonar","Knudsen","Phase range","4500-5500"]
["2016-03-30T06:13:25.670","2016-03-30T18:13:25.670","DF","sonar","Multibeam","Max Angle","35/35"]
["2016-03-30T06:21:27.240","2016-03-30T18:21:27.240","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-30T06:24:50.880","2016-03-30T18:24:50.880","BG","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-30T06:30:49.130","2016-03-30T18:30:49.130","DF","sonar","Multibeam","new line","begin turn line 0254"]
["2016-03-30T06:53:00.790","2016-03-30T18:53:00.790","BG","Sonar","Multibeam","new line","begin survey line 0255"]
["2016-03-30T07:04:14.620","2016-03-30T19:04:14.620","DF","sonar","Multibeam",null,"aeration filter off, max angles to 38/35"]
["2016-03-30T07:07:07.970","2016-03-30T19:07:07.970","DF","Sonar","Multibeam","Max Angle","40/40"]
["2016-03-30T07:13:30.370","2016-03-30T19:13:30.370","BG","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-30T07:31:12.040","2016-03-30T19:31:12.040","bg","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-30T07:47:28.660","2016-03-30T19:47:28.660","bg","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-30T07:55:52.710","2016-03-30T19:55:52.710","DF","sonar","Multibeam","Max Angle","45-45"]
["2016-03-30T08:00:36.180","2016-03-30T20:00:36.180","bg","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-30T08:02:10.770","2016-03-30T20:02:10.770","DF","Sonar","Multibeam","Max Angle","48/48"]
["2016-03-30T08:03:54.450","2016-03-30T20:03:54.450","bg","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-30T08:05:12.580","2016-03-30T20:05:12.580","DF","Sonar","Multibeam","Max Angle","50/50"]
["2016-03-30T08:14:16.670","2016-03-30T20:14:16.670","bg","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-30T08:55:14.790","2016-03-30T20:55:14.790","DF","Sonar","Knudsen","tx power",2]
["2016-03-30T08:58:57","2016-03-30T20:58:57","DF","Sonar","Multibeam","Max Angle","55/50"]
["2016-03-30T09:03:38.360","2016-03-30T21:03:38.360","DF","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-30T09:07:12.940","2016-03-30T21:07:12.940","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-30T09:21:08.760","2016-03-30T21:21:08.760","SM","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-30T09:31:35.790","2016-03-30T21:31:35.790","DS","Sonar","Multibeam",null,"requested line shift 1000m to port (southwest) to fill hole, port max to 70"]
["2016-03-30T09:35:08.450","2016-03-30T21:35:08.450","BG","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-30T09:40:55.530","2016-03-30T21:40:55.530","BG","Sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-30T09:41:41.350","2016-03-30T21:41:41.350","SM","XBT",null,null,"XBT Cast 030 applied to line 0257"]
["2016-03-30T09:45:46.280","2016-03-30T21:45:46.280","bg","sonar","Knudsen","Gain Value","36 dB"]
["2016-03-30T09:58:04.410","2016-03-30T21:58:04.410","DF","sonar","Knudsen",null,"tx power to 1 tx pulse to 2 ms"]
["2016-03-30T09:58:22.930","2016-03-30T21:58:22.930","DF","Ship",null,null,"requested line shift 200m to port (southwest) to fill hole, port max to 70"]
["2016-03-30T10:04:14.910","2016-03-30T22:04:14.910","DF","Sonar","multibeam","Max Angle","70/60"]
["2016-03-30T10:06:06.090","2016-03-30T22:06:06.090","DF","ship",null,null,"requested line shift 300m to port (SW) to fill hole, port still at max"]
["2016-03-30T10:08:43.860","2016-03-30T22:08:43.860","DF","Sonar","Knudsen","tx pulse",1]
["2016-03-30T10:08:53.620","2016-03-30T22:08:53.620","DF","sonar","ek",null,"max record range to 4000"]
["2016-03-30T10:10:24.420","2016-03-30T22:10:24.420","DF","sonar","multibeam","Max Angle","70/55"]
["2016-03-30T10:13:22.860","2016-03-30T22:13:22.860","df","sonar","multibeam","Max Angle","65/55"]
["2016-03-30T10:15:20.530","2016-03-30T22:15:20.530","df","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-30T10:16:56.120","2016-03-30T22:16:56.120","df","sonar","Multibeam","Max Angle","70/65"]
["2016-03-30T10:18:16.040","2016-03-30T22:18:16.040","df","sonar","knudsen",null,"tx power to 2 and tx pulse to 2"]
["2016-03-30T10:34:51.490","2016-03-30T22:34:51.490","bg","sonar","knudsen",null,"phase range 3000-4000, tx pulse 4 ms"]
["2016-03-30T10:39:08.430","2016-03-30T22:39:08.430","df","sonar","ek","Change Range",6000]
["2016-03-30T10:46:09.050","2016-03-30T22:46:09.050","df","sonar","Multibeam","new line","begin turn line 0259"]
["2016-03-30T10:53:54.940","2016-03-30T22:53:54.940","df","sonar","Knudsen","tx power",3]
["2016-03-30T10:58:15.170","2016-03-30T22:58:15.170","bg","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-30T10:58:53.390","2016-03-30T22:58:53.390","bg","sonar","Knudsen",null,"tx pulse 8 ms, gain 40dB"]
["2016-03-30T11:00:13.520","2016-03-30T23:00:13.520","df","sonar","knudsen","tx pulse",4]
["2016-03-30T11:05:58.550","2016-03-30T23:05:58.550","df","sonar","Multibeam","new line","begin survey trackline 0260"]
["2016-03-30T11:12:01.240","2016-03-30T23:12:01.240","df","sonar","Knudsen","Phase range","3000-4000"]
["2016-03-30T11:22:30.040","2016-03-30T23:22:30.040","df","sonar","Knudsen","Phase range","2500-3500"]
["2016-03-30T11:23:04.410","2016-03-30T23:23:04.410","df","sonar","Knudsen",null,"tx power to 2, tx pulse to 4, phasew range to 2000-3000"]
["2016-03-30T12:03:27.680","2016-03-31T00:03:27.680","AB","Sonar","Knudsen","Phase range","2000-3000m, Gain 38dB"]
["2016-03-30T12:11:41.150",{"$f":"IF(ISBLANK(A961),\" \",((A961)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-31T00:11:41.150"},"AB","Ship",null,null,"Shift lines 1000m to port."]
["2016-03-30T12:19:27.580","2016-03-31T00:19:27.580","AB","sonar","Knudsen","Phase Range","2500-3500m, Pulse 4, Max Angle 55/70"]
["2016-03-30T12:26:24.710","2016-03-31T00:26:24.710","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max Angles 52/52"]
["2016-03-30T12:38:26.510","2016-03-31T00:38:26.510","AB","SOnar","Knudsen","Phase Range","3000-4000m"]
["2016-03-30T12:56:22.940","2016-03-31T00:56:22.940","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-30T13:07:37.300","2016-03-31T01:07:37.300","AB","Ship","Multibeam",null,"Shift line additional 700m to port."]
["2016-03-30T13:08:30","2016-03-31T01:08:30","AB","sonar","Multibeam","new line","0262"]
["2016-03-30T13:29:19.240","2016-03-31T01:29:19.240","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-03-30T13:58:18.400","2016-03-31T01:58:18.400","AB","Sonar","Multibeam","new line","0263"]
["2016-03-30T14:04:23.390","2016-03-31T02:04:23.390","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-03-30T14:54:49.780","2016-03-31T02:54:49.780","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2016-03-30T14:57:04.140","2016-03-31T02:57:04.140","AB","sonar","Multibeam","new line","0264"]
["2016-03-30T15:19:30.690","2016-03-31T03:19:30.690","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-30T15:22:26.550","2016-03-31T03:22:26.550","AB","Sonar","Knudsen","Phase Range","4500-5500m, Power 3, Pulse 8"]
["2016-03-30T15:22:35.450","2016-03-31T03:22:35.450","AB","XBT",null,null,"#31"]
["2016-03-30T15:29:23.220","2016-03-31T03:29:23.220","AB","XBT",null,null,"#31 added to new line 0265"]
["2016-03-30T15:30:31.830","2016-03-31T03:30:31.830","AB","Ship",null,null,"Shift 1000m to Starboard"]
["2016-03-30T16:39:34.060","2016-03-31T04:39:34.060","AB","Sonar","Multibeam","new line","0267 - turn"]
["2016-03-30T16:45:14.390","2016-03-31T04:45:14.390","CA","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-30T16:58:04.300","2016-03-31T04:58:04.300","AB","sonar","Multibeam","new line","0268"]
["2016-03-30T17:58:07.700","2016-03-31T05:58:07.700","AB","Sonar","Multibeam","new line","0269, very deep mode, max angles 50/50"]
["2016-03-30T18:01:47.440","2016-03-31T06:01:47.440","AB","Sonar",null,null,"New lines started for EK60 and Knudsen"]
["2016-03-30T18:35:48.970","2016-03-31T06:35:48.970","AB","Sonar","Multibeam","Max Angle","42/42, spike filter medium, slope filter off"]
["2016-03-30T18:46:42.790","2016-03-31T06:46:42.790","AB","Sonar","Knudsen",null,"Gain 42dB, Pulse 16ms"]
["2016-03-30T18:52:17.030","2016-03-31T06:52:17.030","AB","Sonar","multibeam","Max Angle","45/45"]
["2016-03-30T19:00:05","2016-03-31T07:00:05","AB","Sonar","multibeam","new line","0270"]
["2016-03-30T19:14:46.350","2016-03-31T07:14:46.350","Ab","sonar","multibeam","Max Angle","40/40"]
["2016-03-30T19:44:28.570","2016-03-31T07:44:28.570","wp","Other",null,null,"Watch Change"]
["2016-03-30T19:54:04.100","2016-03-31T07:54:04.100","wp","sonar","multibeam","new line","Begin Turn, new line 0271"]
["2016-03-30T19:57:15.810","2016-03-31T07:57:15.810","wp","sonar","multibeam","new line","Begin Survey line, new line 0272"]
["2016-03-30T20:15:57.170","2016-03-31T08:15:57.170","CA","sonar","knudsen","Phase Range","range 4000-5000 "]
["2016-03-30T20:37:15.590","2016-03-31T08:37:15.590","CA","sonar","knudsen","Phase Range","range 3500-4500"]
["2016-03-30T20:47:05.890","2016-03-31T08:47:05.890","wp","sonar","knudsen","Phase Range","range 3000-4000, tx pulse 8.0, power 3, gain 36 dB."]
["2016-03-30T20:50:34.810","2016-03-31T08:50:34.810","MP","sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-30T20:57:27.450","2016-03-31T08:57:27.450","MP","XBT",null,null,"#32"]
["2016-03-30T21:02:55.270","2016-03-31T09:02:55.270","CR","XBT",null,null,"Applied to line 273"]
["2016-03-30T21:10:39.470","2016-03-31T09:10:39.470","cr","sonar","knudsen","Phase Range","range 2000-3000, pulse 8 ms, power 3, gain 35 dB"]
["2016-03-30T21:29:49.590","2016-03-31T09:29:49.590","CR","sonar","knudsen","Phase Range","Range 2500-3500"]
["2016-03-30T21:40:04.060","2016-03-31T09:40:04.060","WP","Sonar","Knudsen","Phase Range","Range 3000-4000, tx pulse 16 ms, power 3.0, gain 39dB."]
["2016-03-30T22:00:40.600","2016-03-31T10:00:40.600","wp","sonar","Knudsen","Phase Range","range 3500-4500, tx Pulse 8 ms, power 3, gain 38 dB."]
["2016-03-30T22:25:55.660","2016-03-31T10:25:55.660","CR","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-30T22:29:22.490","2016-03-31T10:29:22.490","wp","sonar","multibeam","new line","Begin Turn, new line 0275"]
["2016-03-30T22:47:12.560","2016-03-31T10:47:12.560","wp","sonar","multibeam","new line","Begin Survey line, new line 0276."]
["2016-03-30T22:59:05.390","2016-03-31T10:59:05.390","CR","sonar","Knudsen","Tx Power","down to 2"]
["2016-03-30T23:02:57.050","2016-03-31T11:02:57.050","MP","sonar","knudsen","Phase Range","3500-4500"]
["2016-03-30T23:16:45.960","2016-03-31T11:16:45.960","WP","sonar","Knudsen","Phase range","3000-4000"]
["2016-03-30T23:24:13.700","2016-03-31T11:24:13.700","MP","sonar","Knudsen","Phase Range","2500-3500; EK60 environmental settings set to match TSG"]
["2016-03-30T23:39:02.640","2016-03-31T11:39:02.640","MP","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-30T23:48:01.810","2016-03-31T11:48:01.810","MP","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-30T23:55:58.840","2016-03-31T11:55:58.840","MP","Sonar","Knudsen","Phase Range","1000-2000"]
["2016-03-31T00:03:03.470","2016-03-31T12:03:03.470","MP","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-31T00:15:10.540","2016-03-31T12:15:10.540","CR","sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-31T00:17:48.070","2016-03-31T12:17:48.070","CR","Sonar","Knudsen","Gain Value",34]
["2016-03-31T00:26:17.990","2016-03-31T12:26:17.990","CR","SOnar","Knudsen","Tx Power",3]
["2016-03-31T00:26:51.300","2016-03-31T12:26:51.300","CR","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-03-31T00:39:02.100","2016-03-31T12:39:02.100","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-31T00:51:18.950","2016-03-31T12:51:18.950","CR","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-31T01:04:58.710","2016-03-31T13:04:58.710","CR","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-31T01:18:28.850","2016-03-31T13:18:28.850","WP","Sonar","Multibeam","new line","Begin Turn, new line 0279"]
["2016-03-31T01:37:30.550","2016-03-31T13:37:30.550","WP","Sonar","Multibeam","new line","Begin Survey line, new line 0280"]
["2016-03-31T02:01:28.490","2016-03-31T14:01:28.490","CR","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-31T02:51:28.340","2016-03-31T14:51:28.340","CR","sonar","Knudsen","Gain Value","32; Tx Power 1"]
["2016-03-31T02:59:50.940","2016-03-31T14:59:50.940","DS","Sonar","Knudsen","tx pulse","pulse 2, power 1, gain 31, range 1000-2000"]
["2016-03-31T03:05:20.040","2016-03-31T15:05:20.040","MP","Sonar","Knudsen","Tx Power","power 2, pulse 16, gain 36dB"]
["2016-03-31T03:09:36.120",{"$f":"IF(ISBLANK(A1025),\" \",((A1025)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-03-31T15:09:36.120"},"MP","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-31T03:10:50.570","2016-03-31T15:10:50.570","MP","XBT",null,null,"#33"]
["2016-03-31T03:12:29.940","2016-03-31T15:12:29.940","MP","XBT",null,null,"applied to line 0281"]
["2016-03-31T03:16:35.190","2016-03-31T15:16:35.190","DS","Sonar","Multibeam","Max Angle","60/60"]
["2016-03-31T03:20:18.170","2016-03-31T15:20:18.170","MP","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-03-31T03:29:51.740","2016-03-31T15:29:51.740","MP","sonar","Knudsen","Phase Range","2500-3500, pulse 32, power 3"]
["2016-03-31T03:31:36.830","2016-03-31T15:31:36.830","BG","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-03-31T03:48:08.950","2016-03-31T15:48:08.950","BG","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-31T04:00:19.650","2016-03-31T16:00:19.650","BG","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-31T04:09:33.950","2016-03-31T16:09:33.950","BG","SONAR","multibeam","new line","Begin turn line 0283"]
["2016-03-31T04:22:49.250","2016-03-31T16:22:49.250","bg","Sonar","knudsen","Gain Value","40 dB"]
["2016-03-31T04:41:28.410","2016-03-31T16:41:28.410","bg","Sonar","multibeam","new line","begin survey line 0284"]
["2016-03-31T04:56:42.430","2016-03-31T16:56:42.430","bg","sonar","knudsen","Phase Range","3000-4000"]
["2016-03-31T05:17:57.740","2016-03-31T17:17:57.740","df","sonar","knudsen","Phase Range","2500-3500"]
["2016-03-31T05:18:40.280","2016-03-31T17:18:40.280","df","sonar","knudsen",null,"tx pulse to 8 ms, phase range to 2000-3000"]
["2016-03-31T05:35:53.010","2016-03-31T17:35:53.010","df","sonar","knudsen","Tx Power",2]
["2016-03-31T05:51:53.450","2016-03-31T17:51:53.450","bg","sonar","knudsen","Phase Range","1500-2500"]
["2016-03-31T06:02:17.710","2016-03-31T18:02:17.710","DS","Sonar","Multibeam",null,"display issue. Realtime grid would not updata, no data was lost. Grid view missing a few minutes of pings. "]
["2016-03-31T06:04:02.460","2016-03-31T18:04:02.460","BG","sonar","knudsen","Phase Range","2000-3000"]
["2016-03-31T06:11:34.980","2016-03-31T18:11:34.980","DS","Sonar","Multibeam","Max Angle","62/52"]
["2016-03-31T06:13:39.930","2016-03-31T18:13:39.930","bg","sonar","knudsen",null,"tx power 3, phase range 2500-3500"]
["2016-03-31T06:15:09.600","2016-03-31T18:15:09.600","df","sonar","multibeam","Max Angle","62/50"]
["2016-03-31T06:19:58.050","2016-03-31T18:19:58.050","bg","sonar","knudsen","Phase Range","3000-4000"]
["2016-03-31T06:32:29.110","2016-03-31T18:32:29.110","bg","sonar","knudsen","Phase Range","3500-4500"]
["2016-03-31T06:32:56.820","2016-03-31T18:32:56.820","df","Sonar","multibeam","Max Angle","52/52"]
["2016-03-31T06:39:50.970","2016-03-31T18:39:50.970","df","sonar","multibeam","new line","begin turn line 0286"]
["2016-03-31T06:44:27.380","2016-03-31T18:44:27.380","df","Ship",null," ","requested ship to move trackline 800 m to the NE"]
["2016-03-31T07:07:12.570","2016-03-31T19:07:12.570","df","sonar","multibeam","new line","begin survey trackline 0287"]
["2016-03-31T07:12:39.490","2016-03-31T19:12:39.490","df","sonar","multibeam","Max Angle","50/55"]
["2016-03-31T07:12:56.080","2016-03-31T19:12:56.080","df","sonar","Knudsen","Phase Range","3000-4000"]
["2016-03-31T07:13:32.500","2016-03-31T19:13:32.500","df","sonar","Multibeam","Max Angle","50/52"]
["2016-03-31T07:14:34.740","2016-03-31T19:14:34.740","df","sonar","Knudsen","tx pulse","4 ms"]
["2016-03-31T07:30:15.080","2016-03-31T19:30:15.080","df","sonar","Multibeam","Max Angle","50/55"]
["2016-03-31T07:43:04.680","2016-03-31T19:43:04.680","bg","sonar","Knudsen","Phase Range","3500-4500"]
["2016-03-31T07:49:28.960","2016-03-31T19:49:28.960","bg","sonar","Knudsen","Tx Power",2]
["2016-03-31T07:57:14.100","2016-03-31T19:57:14.100","bg","Sonar","Knudsen","Gain Value","36 dB"]
["2016-03-31T08:14:13.960","2016-03-31T20:14:13.960","df","Sonar","Knudsen","tx power",3]
["2016-03-31T08:35:50.680","2016-03-31T20:35:50.680","df","sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-31T08:52:19.790","2016-03-31T20:52:19.790","df","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-31T08:52:47.640","2016-03-31T20:52:47.640","df","SOnar","Knudsen",null,"gain to 40, tx pulse to 8"]
["2016-03-31T09:08:12.880","2016-03-31T21:08:12.880","df","xbt",null,null,"cast 034 collected"]
["2016-03-31T09:11:32.140","2016-03-31T21:11:32.140","df","xbt",null,null,"cast 034 applied to line 0289"]
["2016-03-31T09:11:47.710","2016-03-31T21:11:47.710","df","sonar","Multibeam","new line","began turn line 0290"]
["2016-03-31T09:16:12.040","2016-03-31T21:16:12.040","df","Sonar","Multibeam","new line","began survey line 0291"]
["2016-03-31T09:38:00.280","2016-03-31T21:38:00.280","df","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-31T10:38:27.850","2016-03-31T22:38:27.850","SM","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-03-31T10:39:25.810","2016-03-31T22:39:25.810","BG","Sonar","Multibeam","new line","begin turn line 0293"]
["2016-03-31T10:46:46.060","2016-03-31T22:46:46.060","bg","sonar","Multibeam","new line","begin survey line 0294"]
["2016-03-31T11:02:05.640","2016-03-31T23:02:05.640","df","Sonar","Multibeam","Max Angle","40/50"]
["2016-03-31T11:19:57.540","2016-03-31T23:19:57.540","bg","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-03-31T11:30:00","2016-03-31T23:30:00","AB",null,null,null,"Watch Change, EK60 environmental settings set to match TSG"]
["2016-03-31T11:49:13.710","2016-03-31T23:49:13.710","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-31T12:07:15.490","2016-04-01T00:07:15.490","AB","Sonar","Multibeam","Max Angle","40/52"]
["2016-03-31T12:17:21.090","2016-04-01T00:17:21.090","BG","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-31T12:21:20.300","2016-04-01T00:21:20.300","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-31T12:32:45.100","2016-04-01T00:32:45.100","AB","sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-31T13:03:15.630","2016-04-01T01:03:15.630","AB","Sonar","multibeam","new line","0297 - turn"]
["2016-03-31T13:07:15.430","2016-04-01T01:07:15.430","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2016-03-31T13:09:06.720","2016-04-01T01:09:06.720","AB","Sonar","multibeam","Ping Mode","Auto: Extra Deep, Max Angles 35/35"]
["2016-03-31T13:09:51.090","2016-04-01T01:09:51.090","AB","Sonar","multibeam","new line","0298"]
["2016-03-31T14:09:42","2016-04-01T02:09:42","AB","Sonar","multibeam","new line","0299"]
["2016-03-31T14:25:23.780","2016-04-01T02:25:23.780","AB","Sonar","EK",null,"Environmental parameters updated"]
["2016-03-31T14:48:20.100","2016-04-01T02:48:20.100","AB","sonar","Multibeam","new line","0300 - turn, max angle 35/30"]
["2016-03-31T14:50:41.150","2016-04-01T02:50:41.150","AB","sonar","Multibeam","new line","0301, max angle 30/30"]
["2016-03-31T14:51:21.270",{"$f":"IF(ISBLANK(A1089),\" \",((A1089)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-01T02:51:21.270"},"AB","sonar","knudsen","Phase Range","5000-6000m"]
["2016-03-31T15:00:32","2016-04-01T03:00:32","AB","xbt",null,null,"#35 - faulty"]
["2016-03-31T15:05:59.400","2016-04-01T03:05:59.400","AB","xbt",null,null,"#36"]
["2016-03-31T15:10:40.500","2016-04-01T03:10:40.500","AB","Sonar","Multibeam","new line","XBT #36 applied to new line 0302"]
["2016-03-31T15:12:16.310","2016-04-01T03:12:16.310","AB","sonar","knudsen","Phase Range","4500-5500m"]
["2016-03-31T15:32:36.780","2016-04-01T03:32:36.780","AB","Sonar","knudsen","Phase Range","5000-6000m"]
["2016-03-31T15:37:13.320","2016-04-01T03:37:13.320","ca","sonar","multibeam","new line","0303 - turn"]
["2016-03-31T15:45:05.340","2016-04-01T03:45:05.340","ca","sonar","multibeam","new line","0304"]
["2016-03-31T17:12:33.860","2016-04-01T05:12:33.860","AB","sonar","knudsen","Phase Range","4500-5500m"]
["2016-03-31T17:28:54.090","2016-04-01T05:28:54.090","AB","sonar","multibeam","Ping Mode","Very Deep, Max Angles 40/40"]
["2016-03-31T17:51:23","2016-04-01T05:51:23","AB","Sonar","multibeam","Max Angle","45/45"]
["2016-03-31T18:00:06.420","2016-04-01T06:00:06.420","AB","sonar","Knudsen","Phase Range","4000-5000m"]
["2016-03-31T18:01:05.670","2016-04-01T06:01:05.670","AB","sonar","multibeam","Max Angle","48/48"]
["2016-03-31T18:15:02.950","2016-04-01T06:15:02.950","AB","sonar","Knudsen",null," new line started"]
["2016-03-31T18:20:21.790","2016-04-01T06:20:21.790","AB","sonar","Knudsen","Phase Range","3500-4500m"]
["2016-03-31T18:29:45.250","2016-04-01T06:29:45.250","AB","sonar","Multibeam",null,"307 - New line Started, Restricted Files for Wake Island Wreck search."]
["2016-03-31T18:32:54.590","2016-04-01T06:32:54.590","AB","sonar","Multibeam","Max Angle","52/52"]
["2016-03-31T18:34:30.960","2016-04-01T06:34:30.960","AB","sonar","Multibeam","new line","0308"]
["2016-03-31T19:29:41.540","2016-04-01T07:29:41.540","AB","sonar","Multibeam","Max Angle","60/75"]
["2016-03-31T19:30:29.730","2016-04-01T07:30:29.730","ca","sonar","Knudsen","Phase Range","1000-2000m, Power 1, Pulse 2"]
["2016-03-31T19:42:29.650","2016-04-01T07:42:29.650","wp","Other",null,null,"watch change"]
["2016-03-31T19:43:07.590","2016-04-01T07:43:07.590","wp","sonar","multibeam","new line","false start, new line 0310"]
["2016-03-31T20:01:47.150","2016-04-01T08:01:47.150","CR","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-31T20:02:52.500","2016-04-01T08:02:52.500","wp","sonar","Multibeam","new line","Begin Survey line, new line 0311"]
["2016-03-31T20:16:24.030","2016-04-01T08:16:24.030","CR","Sonar","Knudsen","Gain Value",34]
["2016-03-31T20:18:37.660","2016-04-01T08:18:37.660","CR","SOnar","Knudsen","Phase Range","500-1500"]
["2016-03-31T20:21:41.700","2016-04-01T08:21:41.700","DS","Sonar","Multibeam",null,"settings 65/65 max angles, 1500/1500 coverage, auto mode"]
["2016-03-31T20:36:42.410","2016-04-01T08:36:42.410","CR","sonar","Knudsen","Phase Range",36]
["2016-03-31T20:50:47.500","2016-04-01T08:50:47.500","CR","sonar","Knudsen","Tx Power",2]
["2016-03-31T20:51:05.160","2016-04-01T08:51:05.160","CR","XBT",null,null,"XBT cast 037 completed"]
["2016-03-31T20:51:43.610","2016-04-01T08:51:43.610","CR","Sonar","Knudsen","Tx Power",1]
["2016-03-31T20:55:04.660","2016-04-01T08:55:04.660","CR","XBT",null,null,"XBT applied to line 0311"]
["2016-03-31T21:01:40.450","2016-04-01T09:01:40.450","DS","Sonar","Multibeam","new line","Start Line 0312"]
["2016-03-31T21:30:49.650","2016-04-01T09:30:49.650","CR","sonar","Knudsen","Gain Value","32dB"]
["2016-03-31T21:43:18.410","2016-04-01T09:43:18.410","wp","sonar","multibeam","new line","begin turn, new line 0313"]
["2016-03-31T21:52:48.040","2016-04-01T09:52:48.040","wp","sonar","multibeam","new line","begin survey line, new line 0314."]
["2016-03-31T22:33:20.670","2016-04-01T10:33:20.670","DS","Ship",null,null,"requested ship move 250 m north at slow to 4 knots."]
["2016-03-31T22:53:04.250","2016-04-01T10:53:04.250","CR","Sonar","Knudsen","Tx Pulse","4ms"]
["2016-03-31T23:03:43.920","2016-04-01T11:03:43.920","DS","Ship",null,null,"requested ship finish this line then shift line plan back to original, 250m south"]
["2016-03-31T23:32:29.910","2016-04-01T11:32:29.910","AB","Sonar","knudsen","Phase Range","1000-2000, power 2.0"]
["2016-03-31T23:34:51.110","2016-04-01T11:34:51.110","WP","Sonar","multibeam","new line","begin turn, new line 0316"]
["2016-03-31T23:43:59.500","2016-04-01T11:43:59.500","MP","sonar","Knudsen","Phase Range","1500-2500"]
["2016-03-31T23:54:29.080","2016-04-01T11:54:29.080","MP","Sonar","multibeam","New Line","begin survey line 0317"]
["2016-04-01T00:06:00.450","2016-04-01T12:06:00.450","CR","Sonar","Knudsen","Tx Power",1]
["2016-04-01T01:22:54.290","2016-04-01T13:22:54.290","MP","Sonar","knudsen","Phase Range","500-1500"]
["2016-04-01T01:33:05.910","2016-04-01T13:33:05.910","MP","Sonar","multibeam","New Line","begin turn, new line 0319"]
["2016-04-01T01:39:46.900","2016-04-01T13:39:46.900","MP","Sonar","Knudsen","Phase Range","1000-2000, pulse 2"]
["2016-04-01T01:44:03.290","2016-04-01T13:44:03.290","CR","Sonar","knudsen","Phase Range","1500-2500"]
["2016-04-01T01:59:05.340","2016-04-01T13:59:05.340","CR","sonar","Multibeam","new line","end turn, new survey line 0320"]
["2016-04-01T02:45:25.990","2016-04-01T14:45:25.990","WP","XBT",null,null,"XBT 038 Applied to line 0320"]
["2016-04-01T03:24:02.920","2016-04-01T15:24:02.920","WP","Sonar","Multibeam","new line","Begin Turn, New Line 0322"]
["2016-04-01T03:26:42.710","2016-04-01T15:26:42.710","BG","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-04-01T03:36:53.730","2016-04-01T15:36:53.730","DF","Sonar","knudsen","Phase Range","1000-2000"]
["2016-04-01T03:50:05.820","2016-04-01T15:50:05.820","BG","Sonar","knudsen","Phase Range","500-1500"]
["2016-04-01T03:56:26.110","2016-04-01T15:56:26.110","DF","sonar","multibeam","new line","begin survey trackline 0323"]
["2016-04-01T04:02:13.600","2016-04-01T16:02:13.600","DF","Sonar","knudsen",null,"tx power to 1 tx pulse to 2 ms, gain to 38"]
["2016-04-01T04:07:50.070","2016-04-01T16:07:50.070","DF","sonar","knudsen","Tx Power",2]
["2016-04-01T04:20:04.360","2016-04-01T16:20:04.360","DF","sonar","knudsen","Phase Range","1000-2000"]
["2016-04-01T04:21:26.700","2016-04-01T16:21:26.700","DS","Sonar","Multibeam","Start Line",324]
["2016-04-01T04:34:03.990","2016-04-01T16:34:03.990","DF","sonar","Knudsen","Phase Range","500-1500"]
["2016-04-01T04:34:58.420","2016-04-01T16:34:58.420","DF","Sonar","Knudsen","tx power",1]
["2016-04-01T04:42:35.750","2016-04-01T16:42:35.750","DF","sonar","multibeam","Max Angle","70/65"]
["2016-04-01T04:43:32.940","2016-04-01T16:43:32.940","DF","sonar","multibeam","Along Direction Pitch",0]
["2016-04-01T04:49:46.680","2016-04-01T16:49:46.680","DF","sonar","Multibeam","Max Angle","75/65"]
["2016-04-01T04:52:19.820",{"$f":"IF(ISBLANK(A1153),\" \",((A1153)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-01T16:52:19.820"},"DF","sonar","Multibeam","new line","begin turn line 0325"]
["2016-04-01T04:56:21.350","2016-04-01T16:56:21.350","DF","sonar","Multibeam","new line","begin survey linme 0326"]
["2016-04-01T05:04:14.210","2016-04-01T17:04:14.210","DF","sonar","Multibeam",null,"max coverage to 5000/5000"]
["2016-04-01T05:04:38.750","2016-04-01T17:04:38.750","DF","sonar","Multibeam","Max Angle","75/75"]
["2016-04-01T05:08:34.550","2016-04-01T17:08:34.550","DF","sonar","Knudsen",null,"phase range to 1000-2000, tx power to 2"]
["2016-04-01T05:15:02.990","2016-04-01T17:15:02.990","DF","sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-01T05:28:11.130","2016-04-01T17:28:11.130","DF","sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-01T05:32:50.450","2016-04-01T17:32:50.450","DF","sonar","Knudsen","Tx Pulse",4]
["2016-04-01T05:39:19.120","2016-04-01T17:39:19.120","BG","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-01T05:41:00.620","2016-04-01T17:41:00.620","DF","sonar","Multibeam","Max Angle","52/52"]
["2016-04-01T06:13:30.230","2016-04-01T18:13:30.230","BG","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-01T06:15:13.750","2016-04-01T18:15:13.750","DF","SOnar","Multibeam","Max Angle","52/46"]
["2016-04-01T06:16:14.670","2016-04-01T18:16:14.670","DF","Sonar","Knudsen",null,"tx power to 3, tx pulse to 8"]
["2016-04-01T06:18:37.240","2016-04-01T18:18:37.240","DF","sonar",null,null,"changed sonars out of restricted modes"]
["2016-04-01T07:32:21.300","2016-04-01T19:32:21.300","BG","XBT",null,null,"applied to 0328"]
["2016-04-01T07:34:13.950","2016-04-01T19:34:13.950","BG","sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-01T07:39:16.940","2016-04-01T19:39:16.940","BG","sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-01T07:41:45","2016-04-01T19:41:45","DF","Sonar","Multibeam","Max Angle","55/55"]
["2016-04-01T07:42:15.990","2016-04-01T19:42:15.990","DF","Sonar","Multibeam","Max Angle","65/65"]
["2016-04-01T07:44:21.690","2016-04-01T19:44:21.690","DF","sonar","multibeam","Max Angle","70/65"]
["2016-04-01T07:52:47.150","2016-04-01T19:52:47.150","DF","sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-01T07:53:33.580","2016-04-01T19:53:33.580","DF","sonar","multibeam","new line","begin turn line 0329"]
["2016-04-01T08:00:43.310","2016-04-01T20:00:43.310","BG","sonar","multibeam","new line","begin survey line 0330"]
["2016-04-01T08:08:10.550","2016-04-01T20:08:10.550","DF","Sonar","multibeam","Max Angle","58/55"]
["2016-04-01T08:11:39.620","2016-04-01T20:11:39.620","DF","Sonar","knudsen",null,"tx pulse to 4 ms, tx power to 2"]
["2016-04-01T08:19:53.570","2016-04-01T20:19:53.570","DF","Sonar","multibeam","Max Angle","65/65"]
["2016-04-01T08:23:49.510","2016-04-01T20:23:49.510","BG","Sonar","Knudsen","Phase Range","1000-2000"]
["2016-04-01T08:26:45.690","2016-04-01T20:26:45.690","DF","sonar","multibeam","Max Angle","60/65"]
["2016-04-01T08:32:02.810","2016-04-01T20:32:02.810","DF","Sonar","multibeam","Max Angle","55/65"]
["2016-04-01T08:32:31.280","2016-04-01T20:32:31.280","DF","Sonar","multibeam","Spike Filter Strength","strong"]
["2016-04-01T08:34:33.170","2016-04-01T20:34:33.170","DF","Sonar","multibeam","Max Angle","55/60"]
["2016-04-01T08:38:12.780","2016-04-01T20:38:12.780","BG","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-01T08:38:34.180","2016-04-01T20:38:34.180","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2016-04-01T08:53:53.900","2016-04-01T20:53:53.900","BG","Sonar","knudsen","Phase Range","1000-2000"]
["2016-04-01T09:02:07.690","2016-04-01T21:02:07.690","DF","sonar","Multibeam","Max Angle","60/65"]
["2016-04-01T09:04:05.210","2016-04-01T21:04:05.210","DF","Sonar","Multibeam","Max Angle","65/65"]
["2016-04-01T09:24:51.620","2016-04-01T21:24:51.620","DF","Sonar","Multibeam","Max Angle","50/65"]
["2016-04-01T09:26:06.140","2016-04-01T21:26:06.140","DF","Sonar","knudsen","tx power",1]
["2016-04-01T09:28:37.490","2016-04-01T21:28:37.490","DF","Sonar","multibeam","Max Angle","55/65"]
["2016-04-01T09:29:06.280","2016-04-01T21:29:06.280","DF","Sonar","multibeam","Max Angle","70/70, soft sediment causing holes in swath"]
["2016-04-01T09:35:55.760","2016-04-01T21:35:55.760","DF","sonar","multibeam","Max Angle","65/70"]
["2016-04-01T09:36:14.330","2016-04-01T21:36:14.330","DF","Sonar","Multibeam","Max Angle","55/70"]
["2016-04-01T09:40:44.790","2016-04-01T21:40:44.790","DF","sonar","Multibeam","Spike Filter Strength","Medium"]
["2016-04-01T09:50:49.620","2016-04-01T21:50:49.620","DF","sonar","Multibeam","Max Angle","55/75"]
["2016-04-01T10:01:01.960","2016-04-01T22:01:01.960","bg","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-01T10:05:51.910","2016-04-01T22:05:51.910","bg","sonar","Knudsen","Tx Power",2]
["2016-04-01T10:07:35.290","2016-04-01T22:07:35.290","bg","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-01T10:12:11.200","2016-04-01T22:12:11.200","BG","sonar","multibeam","new line","begin new turn line 0333"]
["2016-04-01T10:32:20.340","2016-04-01T22:32:20.340","bg","sonar","multibeam","new line","begin new survey line 0334"]
["2016-04-01T10:37:16.820","2016-04-01T22:37:16.820","bg","sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-01T10:42:04.170","2016-04-01T22:42:04.170","bg","sonar","Knudsen","Phase Range","1000-2000"]
["2016-04-01T10:53:59.190","2016-04-01T22:53:59.190","bg","sonar","Knudsen","Tx Power",1]
["2016-04-01T10:54:17.320","2016-04-01T22:54:17.320","DF","sonar","Multibeam","Max Angle","60/75"]
["2016-04-01T10:55:10.580","2016-04-01T22:55:10.580","DF","sonar","Multibeam","Max Angle","63/70"]
["2016-04-01T11:21:26.400","2016-04-01T23:21:26.400","BG","sonar","Knudsen","Phase Range","500-1500"]
["2016-04-01T11:31:16.040","2016-04-01T23:31:16.040","DF","ship",null,null,"requested ship move 1000 m to STBD to get overlap; watch change"]
["2016-04-01T11:38:42.020","2016-04-01T23:38:42.020","AB","sonar","Knudsen","Tx Pulse",2]
["2016-04-01T11:43:23.830","2016-04-01T23:43:23.830","AB","sonar","Knudsen","Phase Range","1000-2000m"]
["2016-04-01T11:50:31.970","2016-04-01T23:50:31.970","AB","Sonar","Knudsen","Tx Power","2, Gain 36dB"]
["2016-04-01T12:10:22.660","2016-04-02T00:10:22.660","AB","sonar","Knudsen","Gain Value","31dB"]
["2016-04-01T12:22:06.010","2016-04-02T00:22:06.010","AB","Ship",null,null,"Line extended three minutes to turn due to traffic"]
["2016-04-01T12:23:20.860","2016-04-02T00:23:20.860","AB","SOnar","Multibeam","new line","0336 - turn"]
["2016-04-01T12:26:27.300","2016-04-02T00:26:27.300","AB","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-01T12:27:13.530","2016-04-02T00:27:13.530","AB","sonar","Knudsen","Range","Range 500m"]
["2016-04-01T12:30:51.460",{"$f":"IF(ISBLANK(A1217),\" \",((A1217)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-02T00:30:51.460"},"AB","sonar","Knudsen",null,"Tx Power 3, Pulse 4, Gain 37dB (steep slope downward), Phase Range 2000-2500m"]
["2016-04-01T12:34:10.690","2016-04-02T00:34:10.690","AB","sonar","Knudsen","Phase Range","Phase Range 2250-2750"]
["2016-04-01T12:43:17.230","2016-04-02T00:43:17.230","AB","sonar","Multibeam","new line","0337"]
["2016-04-01T12:43:32.490","2016-04-02T00:43:32.490","AB","Sonar","Knudsen","Phase Range","2250-2750m"]
["2016-04-01T12:47:44.160","2016-04-02T00:47:44.160","AB","Sonar","Knudsen","Phase Range","1750-2250m, Tx power 2"]
["2016-04-01T12:51:37.690","2016-04-02T00:51:37.690","AB","sonar","Knudsen","Tx Power","1, Pulse 2"]
["2016-04-01T12:54:22.860","2016-04-02T00:54:22.860","AB","sonar","Knudsen","Tx Power","2, Pulse 2"]
["2016-04-01T12:59:17.810","2016-04-02T00:59:17.810","AB","sonar","knudsen",null,"Phase Range 1250-1750m"]
["2016-04-01T13:01:33.430","2016-04-02T01:01:33.430","AB","Xbt",null,null,"#40"]
["2016-04-01T13:06:55.960","2016-04-02T01:06:55.960","AB","Xbt",null,null,"Applied to new line 0338"]
["2016-04-01T13:14:22.590","2016-04-02T01:14:22.590","AB","Sonar","knudsen","Phase Range","1500-2000m"]
["2016-04-01T13:27:53.800","2016-04-02T01:27:53.800","AB","Sonar","Knudsen","Phase Range","1250-1750m, Gain 32dB"]
["2016-04-01T13:34:01.630","2016-04-02T01:34:01.630","Ab","Ship",null,null,"Shifting to starboard 500m"]
["2016-04-01T13:40:05.410","2016-04-02T01:40:05.410","AB","sonar","Knudsen","Phase Range","1250-1750"]
["2016-04-01T13:44:47.530","2016-04-02T01:44:47.530","AB","Sonar","multibeam","Max Angle","75/50"]
["2016-04-01T13:50:45.990","2016-04-02T01:50:45.990","AB","Ship",null,null,"Shifting to starboard 500m, on original line track"]
["2016-04-01T13:57:14.610","2016-04-02T01:57:14.610","SM","Sonar","Knudsen","Phase Range","1500-2000"]
["2016-04-01T13:57:53.660","2016-04-02T01:57:53.660","SM","Sonar","Knudsen","Gain Value","38dB"]
["2016-04-01T13:58:29.230","2016-04-02T01:58:29.230","SM","Sonar","knudsen","Phase Range","1750-2250"]
["2016-04-01T14:05:47.770","2016-04-02T02:05:47.770","SM","Sonar","knudsen","Phase Range","1500-2000"]
["2016-04-01T14:08:54.740","2016-04-02T02:08:54.740","SM","sonar","knudsen","Phase Range","1250-1750"]
["2016-04-01T14:14:28.070","2016-04-02T02:14:28.070","SM","Sonar","knudsen","Phase Range","1500-2000"]
["2016-04-01T14:19:08.760","2016-04-02T02:19:08.760","SM","Sonar","knudsen","Phase Range","1750-2250"]
["2016-04-01T14:19:53.330","2016-04-02T02:19:53.330","SM","Sonar","knudsen","Phase Range","2000-2500"]
["2016-04-01T14:21:18.950","2016-04-02T02:21:18.950","SM","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-04-01T14:24:04.730","2016-04-02T02:24:04.730","AB","Sonar","Knudsen","Phase Range","2500-3000m"]
["2016-04-01T14:29:36.590","2016-04-02T02:29:36.590","AB","sonar","Knudsen",null,"pulse 8, power 3, gain 38; downslope"]
["2016-04-01T14:30:25.880","2016-04-02T02:30:25.880","AB","Sonar","Multibeam","new line","0340 - turn"]
["2016-04-01T14:32:19","2016-04-02T02:32:19","AB","sonar","Knudsen","Phase Range","3000-3500m"]
["2016-04-01T14:32:57.590","2016-04-02T02:32:57.590","AB","sonar","Multibeam","new line","0341"]
["2016-04-01T14:36:52.930","2016-04-02T02:36:52.930","AB","sonar","Knudsen","Phase Range","2750-3250m"]
["2016-04-01T14:43:23.180","2016-04-02T02:43:23.180","AB","sonar","Knudsen","Phase Range","2250-2750m"]
["2016-04-01T14:51:25.690","2016-04-02T02:51:25.690","AB","sonar","Knudsen","Phase Range","1750-2250m "]
["2016-04-01T14:56:39.640","2016-04-02T02:56:39.640","SM","sonar","Knudsen","Phase Range","1750-2250"]
["2016-04-01T15:03:50.640","2016-04-02T03:03:50.640","AB","sonar","Knudsen","Phase Range","2000-2500"]
["2016-04-01T15:05:11.640","2016-04-02T03:05:11.640","AB","sonar","Knudsen","Phase Range","2250-2750"]
["2016-04-01T15:09:03.660","2016-04-02T03:09:03.660","SM","sonar","Knudsen","Phase Range","2750-3250"]
["2016-04-01T15:13:09.610","2016-04-02T03:13:09.610","SM","sonar","Knudsen","Phase Range","3000-3500"]
["2016-04-01T15:16:05.800","2016-04-02T03:16:05.800","AB","sonar","Multibeam","Max Angle","52/52, Ping Mode Very Deep"]
["2016-04-01T15:16:44.010","2016-04-02T03:16:44.010","AB","sonar","Knudsen","Phase Range","3250-3750m, gain 38"]
["2016-04-01T15:20:55.850","2016-04-02T03:20:55.850","AB","sonar","Multibeam","new line","0342 - turn"]
["2016-04-01T15:22:41.580","2016-04-02T03:22:41.580","AB","sonar","Multibeam","new line","0343"]
["2016-04-01T15:28:47.230","2016-04-02T03:28:47.230","AB","sonar","Knudsen","Phase Range","3000-3500m"]
["2016-04-01T15:30:04.440","2016-04-02T03:30:04.440","AB","sonar","Knudsen","Phase Range","2750-3250m"]
["2016-04-01T15:36:51.870","2016-04-02T03:36:51.870","AB","Ship",null,null,"Slowing speed to 7.5 kts to meet morning arrival on time."]
["2016-04-01T15:37:49.500","2016-04-02T03:37:49.500","AB","sonar","Knudsen","Phase Range","2250-2750m, Power 2, Pulse 4"]
["2016-04-01T15:39:53.660","2016-04-02T03:39:53.660","AB","sonar","Multibeam","Ping Mode","Deep; Max Angle 60/48"]
["2016-04-01T15:49:34.650","2016-04-02T03:49:34.650","AB","Sonar","Multibeam","Max Angle","70/48"]
["2016-04-01T17:08:51.370","2016-04-02T05:08:51.370","AB","Sonar","Multibeam","new line","0345 - turn"]
["2016-04-01T17:19:20.120","2016-04-02T05:19:20.120","AB","sonar","Multibeam","new line","0346"]
["2016-04-01T17:20:47.410","2016-04-02T05:20:47.410","AB","Sonar","Knudsen",null,"New line, Range 1000m, Phase Range 2500-3500m, Power 3, Pulse 4ms"]
["2016-04-01T17:21:55.530","2016-04-02T05:21:55.530","AB","sonar","Multibeam","Max Angle","55/55"]
["2016-04-01T17:39:50.400","2016-04-02T05:39:50.400","AB","sonar","Multibeam","Max Angle","52/52, Ping Mode Very Deep"]
["2016-04-01T18:52:59.400","2016-04-02T06:52:59.400","AB","Sonar","multibeam","new line","0348 - turn"]
["2016-04-01T18:56:23.660","2016-04-02T06:56:23.660","AB","Sonar","multibeam","new line","0349"]
["2016-04-01T19:08:57.870","2016-04-02T07:08:57.870","AB","sonar","multibeam","Max Angle","52/75"]
["2016-04-01T19:45:03.040","2016-04-02T07:45:03.040","WP","other",null,null,"Watch Change"]
["2016-04-01T20:05:52.860","2016-04-02T08:05:52.860","WP","sonar","knudsen","Phase Range","1000-2000"]
["2016-04-01T20:07:28.110","2016-04-02T08:07:28.110","WP","sonar","knudsen","Phase Range","500-1500, tx pulse 4.0, Power 1, Gain 32"]
["2016-04-01T20:16:54.800","2016-04-02T08:16:54.800","wp","sonar","all","Secure","On station, all sonar secure."]
["2016-04-01T20:19:35.900","2016-04-02T08:19:35.900","wp","Other",null,null,"ADCP pinging and logging."]
["2016-04-01T20:41:15.490","2016-04-02T08:41:15.490","wp","other",null,null,"ADCP stopped logging, stopped pining."]
["2016-04-01T22:18:31.510","2016-04-02T10:18:31.510","wp","sonar","multibeam",null,"Application closed and re-started."]
["2016-04-01T22:57:45.850","2016-04-02T10:57:45.850","MP","XBT",null,null,"#41 (cancelled at 580 m)"]
["2016-04-01T23:02:30.570",{"$f":"IF(ISBLANK(A1281),\" \",((A1281)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-02T11:02:30.570"},"MP","Sonar","Knudsen","Start Pinging","Power 2, Gain 36dB, phase range 1000-2000"]
["2016-04-01T23:03:24.940","2016-04-02T11:03:24.940","MP","Sonar","Multibeam","Start Pinging"]
["2016-04-01T23:04:09.810","2016-04-02T11:04:09.810","MP","Sonar","EK","Start Pinging"]
["2016-04-01T23:08:54.960","2016-04-02T11:08:54.960","MP","Sonar","Multibeam","New Line",352]
["2016-04-01T23:09:16.070","2016-04-02T11:09:16.070","MP","XBT",null,null,"#41 applied to line 0352"]
["2016-04-01T23:15:23.660","2016-04-02T11:15:23.660","MP","Sonar","knudsen","Phase Range","1500-2500"]
["2016-04-01T23:23:49","2016-04-02T11:23:49","DS","Sonar",null,null,"turned off OS38 deck unit"]
["2016-04-01T23:26:01.360","2016-04-02T11:26:01.360","wp","sonar","knudsen","Phase Range","2000-3000, pulse 2.0, power 2, gain 32 dB"]
["2016-04-01T23:27:15.170","2016-04-02T11:27:15.170","DS","Sonar",null,null,"began logging with 300 kHz ADCP, monitoring for intereference"]
["2016-04-01T23:45:25.340","2016-04-02T11:45:25.340","MP","Sonar","knudsen","Tx Power","power 3, pulse 16, gain 38dB"]
["2016-04-01T23:50:25.430","2016-04-02T11:50:25.430","MP","Sonar","Knudsen","Phase Range","2500-3500, pulse 32"]
["2016-04-01T23:58:11.820","2016-04-02T11:58:11.820","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-02T00:09:32.080","2016-04-02T12:09:32.080","DS","sonar","Knudsen","Phase Range","3500-4500, tx pulse 32, power 3, gain 38 dB."]
["2016-04-02T00:21:44.530","2016-04-02T12:21:44.530","WP","Sonar","Knudsen","Phase Range","4000-5000, tx Pulse 32, power 3, gain 38 dB."]
["2016-04-02T00:44:26.360","2016-04-02T12:44:26.360","DS","Sonar",null,null,"turned off 300 kHz ADCP due to interference with em302 starboard beam sector. Secured deck unit. "]
["2016-04-02T00:48:18.750","2016-04-02T12:48:18.750","MP","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-04-02T01:11:27.060","2016-04-02T13:11:27.060","CR","sonar","Knudsen","Phase Range","5000-6000, Tx Power to 2"]
["2016-04-02T01:27:14.210","2016-04-02T13:27:14.210","MP","sonar","Knudsen","Gain Value","34dB"]
["2016-04-02T01:33:09.420","2016-04-02T13:33:09.420","MP","sonar","Multibeam",null,"tilt 2"]
["2016-04-02T01:35:40.770","2016-04-02T13:35:40.770","MP","sonar","Knudsen","Gain Value","32dB"]
["2016-04-02T02:07:57.900","2016-04-02T14:07:57.900","CR","sonar","Knudsen","Gain Value","38dB"]
["2016-04-02T02:16:27.140","2016-04-02T14:16:27.140","CR","sonar","Knudsen","Gain Value","34dB"]
["2016-04-02T02:32:07.400","2016-04-02T14:32:07.400","CR","sonar","Knudsen","Gain Value","38dB"]
["2016-04-02T03:11:21.910","2016-04-02T15:11:21.910","WP","sonar","Multibeam","new line","New Survey line, new line 0357"]
["2016-04-02T03:17:16.660","2016-04-02T15:17:16.660","WP","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-04-02T03:19:34.470","2016-04-02T15:19:34.470","CR","sonar","Knudsen","Tx Power",3]
["2016-04-02T03:23:08.610","2016-04-02T15:23:08.610","BG","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-04-02T03:26:39.550","2016-04-02T15:26:39.550","DF","sonar","Multibeam","Along Direction Pitch",2]
["2016-04-02T03:27:14.110","2016-04-02T15:27:14.110","BG","sonar","Knudsen","Tx Pulse","16 ms"]
["2016-04-02T03:30:22.840","2016-04-02T15:30:22.840","bg","sonar","Knudsen","Phase Range","4000-5000"]
["2016-04-02T03:31:40.210","2016-04-02T15:31:40.210","DF","sonar","Multibeam",null,"max coverage to 5000/5000"]
["2016-04-02T03:32:37.790","2016-04-02T15:32:37.790","BG","sonar","Knudsen","Tx Pulse","8 ms"]
["2016-04-02T03:39:29.370","2016-04-02T15:39:29.370","DF","sonar","Knudsen","TX Pulse","4 ms"]
["2016-04-02T04:15:25.170","2016-04-02T16:15:25.170","bg","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-02T04:23:40.230","2016-04-02T16:23:40.230","bg","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-02T04:30:25.190","2016-04-02T16:30:25.190","bg","sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-02T04:53:44.820","2016-04-02T16:53:44.820","df","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-04-02T05:06:14.530","2016-04-02T17:06:14.530","df","xbt",null,null,"xbt 042 collected"]
["2016-04-02T05:08:32.500","2016-04-02T17:08:32.500","df","xbt",null,null,"cast 042 applied to line 0358"]
["2016-04-02T05:29:13.720","2016-04-02T17:29:13.720","BG","Sonar","knudsen","Phase Range","5000-6000"]
["2016-04-02T05:34:31.330","2016-04-02T17:34:31.330","DF","Sonar","multibeam","new line","begin turn line 0360"]
["2016-04-02T06:00:35.820","2016-04-02T18:00:35.820","BG","sonar","multibeam","New Line","begin survey line 0361"]
["2016-04-02T06:12:03.040","2016-04-02T18:12:03.040","BG","sonar","knudsen","Phase Range","4500-5500"]
["2016-04-02T06:31:32.070","2016-04-02T18:31:32.070","BG","sonar","knudsen","Phase Range","4000-5000"]
["2016-04-02T06:46:59.100","2016-04-02T18:46:59.100","BG","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-02T06:53:09.620","2016-04-02T18:53:09.620","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-02T07:02:57.630","2016-04-02T19:02:57.630","BG","sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-02T07:08:28.330","2016-04-02T19:08:28.330","DS","Sonar",null,null,"Requested bridge shift line plan 1000m starboard (west)."]
["2016-04-02T07:14:00.850","2016-04-02T19:14:00.850","BG","sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-02T07:22:58.880","2016-04-02T19:22:58.880","BG","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-02T07:24:27","2016-04-02T19:24:27","DF","Sonar","Multibeam","Max Angle","60/75"]
["2016-04-02T07:46:04.230","2016-04-02T19:46:04.230","DF","Sonar","knudsen","Phase Range","3000-4000"]
["2016-04-02T08:01:57.770","2016-04-02T20:01:57.770","BG","Sonar","knudsen","Phase Range","3500-4500"]
["2016-04-02T08:07:13.930","2016-04-02T20:07:13.930","DF","Sonar","knudsen","Phase Range","4000-5000"]
["2016-04-02T08:23:08.620","2016-04-02T20:23:08.620","BG","Sonar","knudsen","Phase Range","4500-5500"]
["2016-04-02T08:43:19.820","2016-04-02T20:43:19.820","BG","Sonar","knudsen","Phase Range","5000-6000"]
["2016-04-02T08:56:43.450","2016-04-02T20:56:43.450","DF","Sonar","Multibeam","new line","begin turn line 0364"]
["2016-04-02T09:18:28.030","2016-04-02T21:18:28.030","DF","sonar","Multibeam","new line","begin survey trackline 0365"]
["2016-04-02T09:38:07.680","2016-04-02T21:38:07.680","BG","Sonar","knudsen","Phase Range","4500-5500"]
["2016-04-02T09:56:54.920","2016-04-02T21:56:54.920","BG","Sonar","knudsen","Phase Range","4000-5000"]
["2016-04-02T10:21:04.960","2016-04-02T22:21:04.960","BG","Sonar","Knudsen","Phase Range","2500-35000"]
["2016-04-02T10:24:08.870","2016-04-02T22:24:08.870","BG","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-02T10:32:29.260","2016-04-02T22:32:29.260","BG","sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-02T10:33:44","2016-04-02T22:33:44","DF","Sonar","Multibeam","Max Angle","75/75"]
["2016-04-02T10:37:40.020",{"$f":"IF(ISBLANK(A1345),\" \",((A1345)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-02T22:37:40.020"},"BG","Sonar","Knudsen",null,"phase range 1000-2000, tx power 2"]
["2016-04-02T10:50:02.290","2016-04-02T22:50:02.290","bg","Sonar","Knudsen","Tx Power",1]
["2016-04-02T10:58:11.650","2016-04-02T22:58:11.650","bg","sonar","Knudsen","Tx Power",2]
["2016-04-02T10:59:06.570","2016-04-02T22:59:06.570","bg","sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-02T11:12:25.060","2016-04-02T23:12:25.060","bg","xbt",null,null,"Cast 043 applied to line 0366"]
["2016-04-02T11:18:21.910","2016-04-02T23:18:21.910","DF","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-02T11:28:40.270","2016-04-02T23:28:40.270","AB",null,null,null,"watch Change"]
["2016-04-02T11:28:51.680","2016-04-02T23:28:51.680","AB","sonar","Knudsen","Phase Range","3500-4500m"]
["2016-04-02T11:35:50.560","2016-04-02T23:35:50.560","AB","sonar","Knudsen","Phase Range","4000-5000m"]
["2016-04-02T11:53:27.260","2016-04-02T23:53:27.260","AB","sonar","Knudsen","Phase Range","4500-5500m"]
["2016-04-02T11:56:40.150","2016-04-02T23:56:40.150","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max Angles 52/52"]
["2016-04-02T12:04:28.670","2016-04-03T00:04:28.670","AB","sonar","Multibeam","new line","0368 - turn"]
["2016-04-02T12:13:08.340","2016-04-03T00:13:08.340","AB","sonar","Multibeam",null,"Spike Filter Strength - Strong"]
["2016-04-02T12:27:16.160","2016-04-03T00:27:16.160","AB","sonar","Multibeam","new line","0369"]
["2016-04-02T12:55:31.470","2016-04-03T00:55:31.470","CA","sonar","Knudsen","Phase Range","3500-4500m"]
["2016-04-02T13:05:20.150","2016-04-03T01:05:20.150","AB","sonar","Knudsen","Phase Range","3000-4000m, Power 2, Pulse 4"]
["2016-04-02T13:12:43.630","2016-04-03T01:12:43.630","AB","sonar","Knudsen","Phase Range","2500-3500m"]
["2016-04-02T13:25:53.530","2016-04-03T01:25:53.530","AB","sonar","Knudsen","Phase Range","1500-2500m "]
["2016-04-02T13:26:32.460","2016-04-03T01:26:32.460","AB","sonar","multibeam","new line","0370"]
["2016-04-02T13:28:37.200","2016-04-03T01:28:37.200","AB","Sonar","Knudsen",null,"Power 2, Gain 37dB"]
["2016-04-02T13:32:45.970","2016-04-03T01:32:45.970","AB","Sonar","Knudsen","Phase Range","Pulse 2, Phase 1000-2000m"]
["2016-04-02T13:34:00.260","2016-04-03T01:34:00.260","AB","sonar","multibeam","Spike Filter Strength","Spike Filter Strength - Medium"]
["2016-04-02T14:03:32.710","2016-04-03T02:03:32.710","AB","Sonar","Knudsen","Phase Range","1500-2500m, Power 2, Pulse 4."]
["2016-04-02T14:10:33.530","2016-04-03T02:10:33.530","AB","Sonar","knudsen","Phase Range","2000-3000m, Power 3, Pulse 8, Gain 38dB, steep drop "]
["2016-04-02T14:19:05","2016-04-03T02:19:05","AB","Sonar","knudsen","Phase Range","2500-3500m, new line"]
["2016-04-02T14:20:31.790","2016-04-03T02:20:31.790","AB","Sonar","knudsen","Phase Range","3000-4000m"]
["2016-04-02T14:20:59.420","2016-04-03T02:20:59.420","AB","Sonar","multibeam","Ping Mode","Very Deep, Max Angle 52/52"]
["2016-04-02T14:35:04.620","2016-04-03T02:35:04.620","AB","Ship",null,null,"Shift 1000m to Starboard"]
["2016-04-02T14:37:21.450","2016-04-03T02:37:21.450","AB","sonar","knudsen","Phase Range","4000-5000m"]
["2016-04-02T14:40:31.820","2016-04-03T02:40:31.820","AB","sonar","knudsen","Phase Range","4500-5500m"]
["2016-04-02T14:50:28.480","2016-04-03T02:50:28.480","AB","sonar","Multibeam","Ping Mode","Extra Deep, Max angle 35/35"]
["2016-04-02T14:52:41.810","2016-04-03T02:52:41.810","AB","sonar","Knudsen","Phase Range","5000-6000m"]
["2016-04-02T15:13:21.100","2016-04-03T03:13:21.100","AB","sonar","Multibeam","new line","0372- turn"]
["2016-04-02T15:17:56.240","2016-04-03T03:17:56.240","AB","Ship",null,null,"Steering issues."]
["2016-04-02T15:33:58.090","2016-04-03T03:33:58.090","AB","sonar","Multibeam","new line","0378"]
["2016-04-02T15:55:30.060","2016-04-03T03:55:30.060","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max angle 40/40"]
["2016-04-02T16:00:13.740","2016-04-03T04:00:13.740","AB","Sonar","knudsen","Phase Range","4500-5500m"]
["2016-04-02T16:08:50.420","2016-04-03T04:08:50.420","AB","Sonar","Multibeam","Max Angle","52/52"]
["2016-04-02T16:09:10.420","2016-04-03T04:09:10.420","AB","Sonar","knudsen","Phase Range","4000-5000m"]
["2016-04-02T16:32:00.410","2016-04-03T04:32:00.410","AB","Sonar","Multibeam","Ping Mode","Deep, Max Angle 55/70"]
["2016-04-02T16:32:19.700","2016-04-03T04:32:19.700","AB","Sonar","knudsen","Phase Range","2500-3500m, Pulse 4 "]
["2016-04-02T16:35:56","2016-04-03T04:35:56","Ab","Sonar","Multibeam","new line","0374"]
["2016-04-02T16:59:49.430","2016-04-03T04:59:49.430","AB","xbt",null,null,"#44"]
["2016-04-02T17:04:44.520","2016-04-03T05:04:44.520","AB","xbt",null,null,"#44 Applied to new line 0375"]
["2016-04-02T17:35:07.720","2016-04-03T05:35:07.720","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max Angles 52/52"]
["2016-04-02T17:45:17","2016-04-03T05:45:17","AB","Sonar","knudsen","Phase Range","4000-5000m"]
["2016-04-02T18:04:57","2016-04-03T06:04:57","AB","Sonar","Multibeam","new line","0376"]
["2016-04-02T18:10:10.860","2016-04-03T06:10:10.860","AB","Sonar","Multibeam","Ping Mode","Auto: Extra Deep, Max Angles 35/35"]
["2016-04-02T18:19:34.830","2016-04-03T06:19:34.830","AB","sonar","Multibeam","new line","0377 - turn"]
["2016-04-02T18:28:32.460","2016-04-03T06:28:32.460","AB","Sonar","Multibeam","new line","0378 - transit line to next seamount"]
["2016-04-02T18:28:58","2016-04-03T06:28:58","AB","Sonar",null,null,"New lines started for EK60 and Knudsen"]
["2016-04-02T19:34:01.760","2016-04-03T07:34:01.760","wp","sonar","knudsen","Phase Range","5000-6000"]
["2016-04-02T19:34:46","2016-04-03T07:34:46","wp","Other",null,null,"Watch Change"]
["2016-04-02T19:57:49.570","2016-04-03T07:57:49.570","CR","sonar","Knudsen","Gain Value","36dB"]
["2016-04-02T21:58:31.370","2016-04-03T09:58:31.370","wp","sonar","all","Secure","Ship in DP, all sonar pinging but not logging."]
["2016-04-02T22:10:32.400","2016-04-03T10:10:32.400","DS","Sonar","All","Start up","ship out of DP. All sonars pinging and logging again. "]
["2016-04-02T22:43:33.120","2016-04-03T10:43:33.120","MP","XBT",null,null,"#45"]
["2016-04-02T22:43:54.020","2016-04-03T10:43:54.020","MP","XBT",null,null,"#45 applied to line 0382"]
["2016-04-02T23:17:05.490","2016-04-03T11:17:05.490","wp","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-02T23:33:37.390","2016-04-03T11:33:37.390","MP","sonar","Knudsen","Tx Pulse",32]
["2016-04-02T23:35:35.380","2016-04-03T11:35:35.380","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-02T23:54:33.800","2016-04-03T11:54:33.800","MP","sonar","Knudsen","Tx Power","Power 2, Pulse 8"]
["2016-04-03T00:13:54.560","2016-04-03T12:13:54.560","MP","sonar","Knudsen","Gain Value","38dB"]
["2016-04-03T01:27:24.450","2016-04-03T13:27:24.450","CR","sonar","Knudsen","Tx Power",2]
["2016-04-03T01:34:03.420",{"$f":"IF(ISBLANK(A1409),\" \",((A1409)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-03T13:34:03.420"},"CR","sonar","Knudsen","Tx Pulse","8ms"]
["2016-04-03T01:39:14.170","2016-04-03T13:39:14.170","MP","sonar","multibeam","New Line","begin turn, new line 0386"]
["2016-04-03T01:45:14.220","2016-04-03T13:45:14.220","MP","Sonar","multibeam","New Line","begin survey line 0387"]
["2016-04-03T02:02:50.260","2016-04-03T14:02:50.260","MP","sonar","Knudsen","Gain Value","38dB, pulse 16, phase range 2500-3500"]
["2016-04-03T02:04:38.660","2016-04-03T14:04:38.660","CR","sonar","Knudsen","Gain Value","36Db"]
["2016-04-03T03:24:03.800","2016-04-03T15:24:03.800","cr","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-03T03:44:53.510","2016-04-03T15:44:53.510","BG","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-03T04:10:23.580","2016-04-03T16:10:23.580","BG","sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-03T04:15:38.640","2016-04-03T16:15:38.640","bg","Sonar","Knudsen","Tx Pulse","8ms"]
["2016-04-03T04:17:41.240","2016-04-03T16:17:41.240","bg","Sonar","knudsen","Phase Range","2000-3000"]
["2016-04-03T04:18:22.900","2016-04-03T16:18:22.900","DF","Sonar","multibeam","Max Angle","70/70"]
["2016-04-03T04:18:39.070","2016-04-03T16:18:39.070","DF","Sonar","multibeam","Spike Filter Strength","strong"]
["2016-04-03T04:24:17.050","2016-04-03T16:24:17.050","bg","Sonar","knudsen","tx power",2]
["2016-04-03T04:57:25.470","2016-04-03T16:57:25.470","DF","xbt",null,null,"cast 046 collected"]
["2016-04-03T04:58:05.090","2016-04-03T16:58:05.090","DF","xbt",null,null,"cast 046 applied to line 0390"]
["2016-04-03T05:07:32.850","2016-04-03T17:07:32.850","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-03T05:26:16.420","2016-04-03T17:26:16.420","bg","sonar","Multibeam","new line","begin turn line 0391"]
["2016-04-03T05:29:55.230","2016-04-03T17:29:55.230","bg","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-03T05:34:46.590","2016-04-03T17:34:46.590","bg","sonar","knudsen",null,"phase range 3500-4500, tx power 3"]
["2016-04-03T05:48:15.560","2016-04-03T17:48:15.560","bg","sonar","Multibeam","new line","begin survey line 0392"]
["2016-04-03T05:53:04.930","2016-04-03T17:53:04.930","bg","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-03T06:03:28.520","2016-04-03T18:03:28.520","bg","Sonar","knudsen","Phase Range","2500-3500"]
["2016-04-03T06:08:22.960","2016-04-03T18:08:22.960","bg","Sonar","knudsen","Phase Range","2000-3000"]
["2016-04-03T06:13:04.920","2016-04-03T18:13:04.920","bg","Sonar","knudsen","Phase Range","1500-2500"]
["2016-04-03T06:16:55.710","2016-04-03T18:16:55.710","bg","Sonar","knudsen","tx power",2]
["2016-04-03T06:19:43.440","2016-04-03T18:19:43.440","df","Sonar","knudsen",null,"tx power to 1, tx pulse to 4 ms"]
["2016-04-03T06:22:43.620","2016-04-03T18:22:43.620","df","Sonar","Multibeam","Max Angle","70/58"]
["2016-04-03T06:45:10.590","2016-04-03T18:45:10.590","df","Sonar","Multibeam","Max Angle","70/70"]
["2016-04-03T06:45:57.660","2016-04-03T18:45:57.660","df","Sonar","knudsen",null,"tx power to 2, phase range to 2000-3000"]
["2016-04-03T06:50:11.020","2016-04-03T18:50:11.020","df","Sonar","knudsen","Phase Range","2500-3500"]
["2016-04-03T06:56:41.210","2016-04-03T18:56:41.210","df","Sonar","knudsen",null,"tx power to 3, phase range to 3000-4000"]
["2016-04-03T07:12:49.890","2016-04-03T19:12:49.890","DS","Other",null,null,"requested 500 m line shift to starboard (southwest)"]
["2016-04-03T07:13:37.240","2016-04-03T19:13:37.240","DF","Sonar","knudsen","Phase Range","3500-4500"]
["2016-04-03T08:09:00.680","2016-04-03T20:09:00.680","DF","Sonar","knudsen","tx pulse",4]
["2016-04-03T08:40:40.310","2016-04-03T20:40:40.310","DF","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-03T08:49:03.360","2016-04-03T20:49:03.360","DF","Sonar","knudsen","tx power",2]
["2016-04-03T09:24:24.060","2016-04-03T21:24:24.060","DF","Sonar","multibeam","New Line","begin turn line 0396"]
["2016-04-03T09:48:10.940","2016-04-03T21:48:10.940","BG","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-03T09:52:15.370","2016-04-03T21:52:15.370","df","sonar","multibeam","New Line","begin survey line 0397"]
["2016-04-03T11:03:09.030","2016-04-03T23:03:09.030","SM","sonar","Knudsen","Phase Range","4000-5000"]
["2016-04-03T11:08:40.980","2016-04-03T23:08:40.980","SM","sonar","knudsen","Tx Power",3]
["2016-04-03T11:19:40.130","2016-04-03T23:19:40.130","SM","XBT",null,null,"Cast 047 applied to line 0398"]
["2016-04-03T11:30:26","2016-04-03T23:30:26","AB",null,null,null,"Watch Change"]
["2016-04-03T12:27:24.560","2016-04-04T00:27:24.560","AB","sonar","knudsen","Phase Range","3500-4500m"]
["2016-04-03T12:36:08.670","2016-04-04T00:36:08.670","AB","Ship",null,null,"Shift to Starboard 500m"]
["2016-04-03T12:38:31.440","2016-04-04T00:38:31.440","AB","sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-03T12:43:00.700","2016-04-04T00:43:00.700","AB","sonar","knudsen","Phase Range","2000-3000m"]
["2016-04-03T12:43:07.800","2016-04-04T00:43:07.800","AB","sonar","multibeam","Ping Mode","Deep, Max Angle 50/74"]
["2016-04-03T12:52:54.260","2016-04-04T00:52:54.260","AB","sonar","knudsen","Phase Range","3000-4000m, Pulse 8 "]
["2016-04-03T12:53:26.240","2016-04-04T00:53:26.240","AB","sonar","multibeam","New Line","0400"]
["2016-04-03T12:57:34.760","2016-04-04T00:57:34.760","AB","sonar","multibeam","Ping Mode","Very Deep, Max angles 40/52"]
["2016-04-03T13:22:35.620","2016-04-04T01:22:35.620","AB","sonar","knudsen","Phase Range","3500-4500m"]
["2016-04-03T13:37:19.190","2016-04-04T01:37:19.190","AB","sonar","multibeam","New Line","0401-turn"]
["2016-04-03T13:42:34.620","2016-04-04T01:42:34.620","AB","sonar","multibeam","New Line","0402, Max angles 52/52"]
["2016-04-03T14:35:44","2016-04-04T02:35:44","AB","sonar","multibeam","New Line","0403"]
["2016-04-03T14:40:58","2016-04-04T02:40:58","AB","sonar","multibeam","New Line","0404"]
["2016-04-03T14:52:33.910","2016-04-04T02:52:33.910","AB","sonar","knudsen","Phase Range","3500-4500m"]
["2016-04-03T15:09:40.470","2016-04-04T03:09:40.470","AB","sonar","knudsen","Phase Range","3000-4000m, Pulse 8"]
["2016-04-03T15:15:07.300","2016-04-04T03:15:07.300","AB","XBT",null,null,"#48"]
["2016-04-03T15:20:20.910","2016-04-04T03:20:20.910","AB","XBT",null,null,"#48 applied to new line 0405"]
["2016-04-03T15:23:13.320","2016-04-04T03:23:13.320","AB","sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-03T15:30:38.610","2016-04-04T03:30:38.610","AB","sonar","multibeam","Max Angle","Ping mode Deep, Max Angles 50/65"]
["2016-04-03T15:31:06.660","2016-04-04T03:31:06.660","AB","sonar","knudsen","Phase Range","2000-3000, Pulse 4, Power 2"]
["2016-04-03T15:37:48.230","2016-04-04T03:37:48.230","AB","sonar","knudsen","Phase Range","1500-2500m, Gain 37dB"]
["2016-04-03T15:40:08.590",{"$f":"IF(ISBLANK(A1473),\" \",((A1473)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-04T03:40:08.590"},"AB","Ship",null,null,"WX deterio, ship rolling more."]
["2016-04-03T15:42:28.570","2016-04-04T03:42:28.570","AB","sonar","knudsen","Tx Pulse","2, Gain 35dB"]
["2016-04-03T15:48:45.960","2016-04-04T03:48:45.960","AB","sonar","knudsen","Phase Range","2000-3000m"]
["2016-04-03T15:52:23.050","2016-04-04T03:52:23.050","AB","sonar","multibeam","Max Angle","75/55"]
["2016-04-03T16:18:34.710","2016-04-04T04:18:34.710","AB","sonar","Knudsen","Phase Range","2500-3500m, Power 2, Pulse 4, Gain 38dB"]
["2016-04-03T16:20:21","2016-04-04T04:20:21","AB","sonar","multibeam","New Line","0406"]
["2016-04-03T16:28:02.500","2016-04-04T04:28:02.500","AB","sonar","multibeam","Ping Mode","Auto: Very Deep, Max angles 52/52"]
["2016-04-03T16:35:33.710","2016-04-04T04:35:33.710","AB","Ship",null,null,"Shift 500m to Port"]
["2016-04-03T16:38:08.810","2016-04-04T04:38:08.810","AB","sonar","multibeam","Ping Mode","Deep Mode, Max Angle 60/50"]
["2016-04-03T16:52:16.460","2016-04-04T04:52:16.460","AB","sonar","knudsen","Phase Range","1500-2500m"]
["2016-04-03T16:53:50.510","2016-04-04T04:53:50.510","AB","sonar","multibeam","Max Angle","70/60"]
["2016-04-03T17:23:53.320","2016-04-04T05:23:53.320","AB","sonar","multibeam","New Line","Lost coverage in SIS, Data ok; Line 0408"]
["2016-04-03T17:25:27.990","2016-04-04T05:25:27.990","AB","sonar","multibeam","Aeration Filter (On/Off)","On , Max angles 65/55"]
["2016-04-03T17:32:57.200","2016-04-04T05:32:57.200","AB","sonar","multibeam","Along Direction Pitch","Gradually moved from 2.0 to -1.0 "]
["2016-04-03T17:35:32.290","2016-04-04T05:35:32.290","AB","sonar","multibeam","Max Angle","55/50"]
["2016-04-03T17:35:46.700","2016-04-04T05:35:46.700","AB","sonar","knudsen","Gain Value","37, Phase Range 2000-3000m, Pulse 2, Power 2"]
["2016-04-03T18:39:36.350","2016-04-04T06:39:36.350","AB","Ship",null,null,"Shift 1000m to Starboard"]
["2016-04-03T18:46:43.580","2016-04-04T06:46:43.580","AB","sonar","knudsen","Phase Range","2000-3000m, Pulse 4, Gain 37dB"]
["2016-04-03T18:52:24.900","2016-04-04T06:52:24.900","AB","sonar","multibeam","New Line","0411 - turn"]
["2016-04-03T18:53:14.930","2016-04-04T06:53:14.930","AB","sonar","knudsen","Phase Range","2500-3500m, Power 3, Pulse 4"]
["2016-04-03T18:56:17.550","2016-04-04T06:56:17.550","AB","sonar","multibeam","New Line","0412"]
["2016-04-03T19:01:42.790","2016-04-04T07:01:42.790","AB","sonar","multibeam","Ping Mode","Very Deep, 52/50"]
["2016-04-03T19:06:53.360","2016-04-04T07:06:53.360","AB","sonar","multibeam","New Line","0413 - turn"]
["2016-04-03T19:12:07.920","2016-04-04T07:12:07.920","AB","sonar","multibeam","New Line","0414"]
["2016-04-03T19:15:00.710","2016-04-04T07:15:00.710","AB","sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-03T19:17:08.910","2016-04-04T07:17:08.910","AB","Ship",null,null,"Shift 900m to Port"]
["2016-04-03T19:19:45.430","2016-04-04T07:19:45.430","AB","sonar","knudsen","Phase Range","2000-3000m, Power 2, Pulse 4, Gain 40dB"]
["2016-04-03T19:23:42.320","2016-04-04T07:23:42.320","AB","sonar","multibeam","Along Direction Pitch",-2]
["2016-04-03T19:24:26.340","2016-04-04T07:24:26.340","AB","sonar","multibeam","Ping Mode","Deep, Max Angles 60/50"]
["2016-04-03T19:25:50.220","2016-04-04T07:25:50.220","AB","sonar","knudsen","Tx Pulse","2, Gain 36dB"]
["2016-04-03T19:44:47.290","2016-04-04T07:44:47.290","WP","Other",null,null,"Watch Change"]
["2016-04-03T20:25:35.990","2016-04-04T08:25:35.990","DS","Other",null,null,"Requested bridge slow down to 7.5-8 knots due to rough seas and poor data. "]
["2016-04-03T21:06:24.070","2016-04-04T09:06:24.070","MP","XBT",null,null,"#49"]
["2016-04-03T21:08:55.390","2016-04-04T09:08:55.390","wp","XBT",null,null,"XBT 049 applied to line 0415"]
["2016-04-03T21:28:42.780","2016-04-04T09:28:42.780","cr","sonar","knudsen","Phase Range","2000-3000, tx pulse 8.0, power 3, gain 34"]
["2016-04-03T22:07:41.100","2016-04-04T10:07:41.100","MP","sonar","knudsen","Phase Range","1500-2500, gain 36dB, power 2, pulse 16"]
["2016-04-03T22:10:40.230","2016-04-04T10:10:40.230","MP","sonar","knudsen","Gain Value","34dB, power 1"]
["2016-04-03T22:21:39.360","2016-04-04T10:21:39.360","MP","sonar","Knudsen","Gain Value","32dB"]
["2016-04-03T22:32:45.730","2016-04-04T10:32:45.730","MP","sonar","knudsen","Tx Power","3, gain value 34dB, pulse 32"]
["2016-04-03T22:38:28.530","2016-04-04T10:38:28.530","MP","Sonar","knudsen","Phase Range","2000-3000"]
["2016-04-03T22:52:27.320","2016-04-04T10:52:27.320","WP","Sonar","knudsen","Phase Range","2500-3500, Pulse 16.0, Power 3, gain 39."]
["2016-04-03T22:58:29.760","2016-04-04T10:58:29.760","MP","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-03T23:02:07.690","2016-04-04T11:02:07.690","MP","sonar","knudsen","Gain Value","45dB"]
["2016-04-03T23:10:51.200","2016-04-04T11:10:51.200","MP","sonar","knudsen","Phase Range","3500-4500, gain 41dB"]
["2016-04-03T23:25:03.410","2016-04-04T11:25:03.410","MP","sonar","knudsen","Gain Value","38dB"]
["2016-04-03T23:35:53.620","2016-04-04T11:35:53.620","MP","Sonar","knudsen","Phase Range","4000-5000, gain 36dB"]
["2016-04-03T23:42:25.640","2016-04-04T11:42:25.640","WP","Sonar","multibeam","new line","Begin Turn, new line 0419"]
["2016-04-03T23:43:40.810","2016-04-04T11:43:40.810","MP","sonar","knudsen","Gain Value","38dB"]
["2016-04-03T23:58:39.980","2016-04-04T11:58:39.980","WP","sonar","multibeam","New Line","Begin Survey line, new line 0420"]
["2016-04-04T00:23:33.950","2016-04-04T12:23:33.950","wp","sonar","knudsen","Phase Range","3000-4000, pulse 8.0, power 3, gain 34"]
["2016-04-04T00:53:54.790","2016-04-04T12:53:54.790","wp","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-04T01:09:35.400","2016-04-04T13:09:35.400","CR","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-04T01:14:12.010","2016-04-04T13:14:12.010","CR","sonar","knudsen","Tx Power","2, gain value 34dB"]
["2016-04-04T01:19:01.540","2016-04-04T13:19:01.540","CR","sonar","Knudsen","tx pulse","8, tx power 1"]
["2016-04-04T03:07:46.350","2016-04-04T15:07:46.350","MP","XBT",null,null,"#50"]
["2016-04-04T03:09:18.620","2016-04-04T15:09:18.620","MP","XBT",null,null,"#50 applied to line 0423"]
["2016-04-04T03:44:20.410","2016-04-04T15:44:20.410","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-04-04T03:44:56.540","2016-04-04T15:44:56.540","DF","sonar","multibeam","Along Direction Pitch",-3]
["2016-04-04T03:48:11.470","2016-04-04T15:48:11.470","DF","sonar","multibeam","Along Direction Pitch",-4]
["2016-04-04T04:04:19.790","2016-04-04T16:04:19.790","DF","sonar","multibeam","New Line","begin turn line 0425"]
["2016-04-04T04:11:21.640","2016-04-04T16:11:21.640","DF","sonar","multibeam","Max Angle","60/40"]
["2016-04-04T04:20:32.070","2016-04-04T16:20:32.070","BG","sonar","multibeam","New Line","begin survey line 0426"]
["2016-04-04T04:22:46.380","2016-04-04T16:22:46.380","DF","sonar","multibeam","Max Angle","55/38"]
["2016-04-04T04:29:46.420","2016-04-04T16:29:46.420","DF","sonar","multibeam","Max Angle","55/45"]
["2016-04-04T04:32:39.660",{"$f":"IF(ISBLANK(A1537),\" \",((A1537)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-04T16:32:39.660"},"DF","sonar","multibeam","Max Angle","55/35"]
["2016-04-04T04:33:58.520","2016-04-04T16:33:58.520","DF","sonar","multibeam","Max Angle","55/45"]
["2016-04-04T04:52:12.180","2016-04-04T16:52:12.180","DF","sonar","multibeam","New Line","begin turn line 0427, turning to north to try different trackline for better ride and data"]
["2016-04-04T05:22:01.670","2016-04-04T17:22:01.670","DF","sonar","multibeam","New Line","begin new altered test survey line 0428"]
["2016-04-04T05:31:36.950","2016-04-04T17:31:36.950","DF","sonar","multibeam","Along Direction Pitch",-5]
["2016-04-04T05:32:54.470","2016-04-04T17:32:54.470","DF","sonar","multibeam","Along Direction Pitch",-6]
["2016-04-04T05:34:03.880","2016-04-04T17:34:03.880","DF","sonar","multibeam",null,"50/40, ping mode to very deep"]
["2016-04-04T05:36:08.920","2016-04-04T17:36:08.920","DF","sonar","multibeam","Along Direction Pitch",-7]
["2016-04-04T05:36:46.960","2016-04-04T17:36:46.960","DF","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-04T05:53:20.470","2016-04-04T17:53:20.470","BG","sonar","knudsen","Tx Power",2]
["2016-04-04T05:57:46.440","2016-04-04T17:57:46.440","BG","sonar","knudsen","Tx Power",3]
["2016-04-04T06:02:53.310","2016-04-04T18:02:53.310","BG","sonar","knudsen","Tx Pulse","16 ms"]
["2016-04-04T06:11:35.280","2016-04-04T18:11:35.280","DF","sonar","knudsen","tx pulse","8 ms"]
["2016-04-04T06:26:33.010","2016-04-04T18:26:33.010","df","sonar","knudsen","Gain Value",38]
["2016-04-04T06:27:24.070","2016-04-04T18:27:24.070","df","sonar","ek",null,"stopped loging and pinging to secure 70, 120, 300 kHz ek's. Started pinging and loging again after they were secured"]
["2016-04-04T06:34:30.960","2016-04-04T18:34:30.960","DF","sonar","multibeam","Along Direction Pitch",-5]
["2016-04-04T06:54:30.180","2016-04-04T18:54:30.180","DF","Weather",null,null,"swell still 7-9 ft, wind waves - 5-7 ft out of 020. "]
["2016-04-04T06:55:45.440","2016-04-04T18:55:45.440","DF","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-04T06:57:42.890","2016-04-04T18:57:42.890","DF","sonar","knudsen","Gain Value",40]
["2016-04-04T07:02:49.610","2016-04-04T19:02:49.610","DF","sonar","multibeam","Max Angle","33/28"]
["2016-04-04T07:03:39.430","2016-04-04T19:03:39.430","DF","sonar","knudsen",null,"tx pulse to 4 ms, gain to 42 dB"]
["2016-04-04T07:04:59.270","2016-04-04T19:04:59.270","DF","sonar","multibeam","Max Angle","35/30"]
["2016-04-04T07:17:20.650","2016-04-04T19:17:20.650","DF","sonar","multibeam","Max Angle","25/25, cannot maintain bottom"]
["2016-04-04T07:25:43.030","2016-04-04T19:25:43.030","DF","sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-04T07:35:11.670","2016-04-04T19:35:11.670","DF","sonar","knudsen","Gain Value",40]
["2016-04-04T07:39:28.090","2016-04-04T19:39:28.090","DF","Sonar","multibeam","Ping Mode","Extra Deep"]
["2016-04-04T07:40:28.240","2016-04-04T19:40:28.240","DS","Sonar","knudsen",null,"phase range 4000-5000, tx pulse 16 ms"]
["2016-04-04T07:46:38.820","2016-04-04T19:46:38.820","DF","sonar","multibeam","new line","begin turn line 0431"]
["2016-04-04T07:47:17.860","2016-04-04T19:47:17.860","DF","sonar","knudsen","tx pulse",8]
["2016-04-04T07:54:00.310","2016-04-04T19:54:00.310","DF","sonar","multibeam","Along Direction Pitch",-3]
["2016-04-04T07:55:23.960","2016-04-04T19:55:23.960","DF","sonar","multibeam",null,"auto tilt"]
["2016-04-04T08:00:57.190","2016-04-04T20:00:57.190","DF","Sonar","multibeam","new line","begin survey line 0432"]
["2016-04-04T08:07:11.230","2016-04-04T20:07:11.230","DF","Sonar","multibeam",null,"auto ping mode, expanding swath angles"]
["2016-04-04T08:09:07.630","2016-04-04T20:09:07.630","DF","sonar","multibeam","Max Angle","40/45"]
["2016-04-04T08:09:24.330","2016-04-04T20:09:24.330","BG","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-04T08:11:11.490","2016-04-04T20:11:11.490","DF","sonar","multibeam","Max Angle","40/50"]
["2016-04-04T08:19:52.830","2016-04-04T20:19:52.830","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-04T08:31:15.390","2016-04-04T20:31:15.390","BG","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-04T08:37:36.090","2016-04-04T20:37:36.090","DF","sonar","multibeam","Max Angle","50/60"]
["2016-04-04T08:45:59.870","2016-04-04T20:45:59.870","DF","sonar","multibeam","Max Angle","45/60"]
["2016-04-04T08:46:37.650","2016-04-04T20:46:37.650","DF","sonar","multibeam","Aeration Filter (On/Off)","off"]
["2016-04-04T08:47:33.070","2016-04-04T20:47:33.070","DF","sonar","multibeam","Max Angle","45/55"]
["2016-04-04T08:49:25.950","2016-04-04T20:49:25.950","DF","sonar","multibeam","Ping Mode","very deep"]
["2016-04-04T08:50:48.400","2016-04-04T20:50:48.400","DF","sonar","multibeam","Max Angle","55/55"]
["2016-04-04T08:59:26.890","2016-04-04T20:59:26.890","DF","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-04T09:03:09.220","2016-04-04T21:03:09.220","Df","sonar","multibeam",null,"ping mode to deep, max angles at 60"]
["2016-04-04T09:05:11.790","2016-04-04T21:05:11.790","DF","sonar","knudsen",null,"tx pulse to 4 ms, power to 2"]
["2016-04-04T09:08:52.140","2016-04-04T21:08:52.140","DF","xbt",null,null,"cast 051 collected"]
["2016-04-04T09:09:06.810","2016-04-04T21:09:06.810","DF","sonar","knudsen",null,"tx power to 1, tx pulse to 2 ms"]
["2016-04-04T09:15:25.880","2016-04-04T21:15:25.880","DF","xbt",null,null,"cast 051 applied to line 0433"]
["2016-04-04T09:40:51.390","2016-04-04T21:40:51.390","SM","sonar","knudsen","Gain Value","36 dB"]
["2016-04-04T09:48:47.710","2016-04-04T21:48:47.710","DF","sonar","multibeam","Max Angle","50/60"]
["2016-04-04T09:57:20.520","2016-04-04T21:57:20.520","DF","sonar","multibeam","Max Angle","60/60"]
["2016-04-04T10:02:50.960","2016-04-04T22:02:50.960","DS","Sonar","Multibeam","New Line","start turn line 0435, turning to east to fill a nearby holiday before proceeding to next waypoint. "]
["2016-04-04T10:16:01.120","2016-04-04T22:16:01.120","DF","sonar","knudsen","Tx Power",2]
["2016-04-04T10:30:07.710","2016-04-04T22:30:07.710","DF","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-04T10:30:36.670","2016-04-04T22:30:36.670","DF","sonar","knudsen",null,"tx power to 3, tx pulse to 4"]
["2016-04-04T10:33:38.730","2016-04-04T22:33:38.730","DF","sonar","multibeam","Ping Mode","very deep"]
["2016-04-04T10:35:29.350","2016-04-04T22:35:29.350","DF","sonar","knudsen","tx pulse",8]
["2016-04-04T10:37:31.470","2016-04-04T22:37:31.470","DF","sonar","multibeam","Aeration Filter (On/Off)","on"]
["2016-04-04T10:40:13.490","2016-04-04T22:40:13.490","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-04T10:42:06.660","2016-04-04T22:42:06.660","DF","sonar","multibeam","Max Angle","30/30"]
["2016-04-04T10:42:45.430","2016-04-04T22:42:45.430","DF","sonar","multibeam","Max Angle","25/25"]
["2016-04-04T10:45:59.810","2016-04-04T22:45:59.810","DF","sonar","multibeam","Ping Mode","auto"]
["2016-04-04T10:55:52.840",{"$f":"IF(ISBLANK(A1601),\" \",((A1601)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-04T22:55:52.840"},"DF","sonar","multibeam","Max Angle","35/35"]
["2016-04-04T10:57:09.280","2016-04-04T22:57:09.280","DF","sonar","multibeam","new line","begin new survey line 0436, fill line for hole"]
["2016-04-04T11:01:21.400","2016-04-04T23:01:21.400","DF","sonar","multibeam","Max Angle","40/35"]
["2016-04-04T11:11:39.490","2016-04-04T23:11:39.490","DF","sonar","multibeam","new line","end survey line"]
["2016-04-04T11:13:16.300","2016-04-04T23:13:16.300","DF","sonar","multibeam","Max Angle","35/35"]
["2016-04-04T11:14:22.830","2016-04-04T23:14:22.830","DF","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-04T11:27:42.130","2016-04-04T23:27:42.130","DF","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-04T11:28:10.510","2016-04-04T23:28:10.510","DF","sonar","Knudsen",null,"tx pulse to 2, tx power to 1"]
["2016-04-04T11:32:27.450","2016-04-04T23:32:27.450","BG","sonar","multibeam","new line","begin survey line 0438"]
["2016-04-04T23:50:43","2016-04-05T11:50:43","AB","sonar","multibeam","new line","0439"]
["2016-04-04T12:50:45","2016-04-05T00:50:45","AB","sonar","multibeam","new line","0440"]
["2016-04-04T13:32:49.670","2016-04-05T01:32:49.670","AB","Sonar","knudsen","Tx Power","2, Phase Range 2000-3000m"]
["2016-04-04T13:52:40.130","2016-04-05T01:52:40.130","AB","Sonar","multibeam","new line","0441"]
["2016-04-04T13:54:33.540","2016-04-05T01:54:33.540","AB","sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-04T14:04:31.560","2016-04-05T02:04:31.560","AB","sonar","knudsen","Tx Pulse","8, Power 3, Phase Range 3000-4000m"]
["2016-04-04T14:20:16.100","2016-04-05T02:20:16.100","AB","sonar","knudsen","Phase Range","4000-5000m"]
["2016-04-04T14:22:49.920","2016-04-05T02:22:49.920","AB","sonar","multibeam","new line","0442 - turn, Ping Mode Very Deep"]
["2016-04-04T14:33:16.930","2016-04-05T02:33:16.930","AB","Sonar",null,null,"New lines started for EK60 and Knudsen"]
["2016-04-04T14:37:22.600","2016-04-05T02:37:22.600","AB","Sonar","multibeam","New Line","0443"]
["2016-04-04T14:39:01.430","2016-04-05T02:39:01.430","AB","sonar","knudsen","Phase Range","3500-4500m"]
["2016-04-04T14:49:56.530","2016-04-05T02:49:56.530","AB","sonar","knudsen","Phase Range","3000-4000m"]
["2016-04-04T14:57:34.620","2016-04-05T02:57:34.620","AB","sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-04T14:57:46.490","2016-04-05T02:57:46.490","AB","sonar","multibeam","Ping Mode","Deep, Max Angles 55/55"]
["2016-04-04T15:04:14.080","2016-04-05T03:04:14.080","AB","sonar","knudsen","Phase Range","2000-3000m, Power 2, Pulse 4 "]
["2016-04-04T15:09:53.400","2016-04-05T03:09:53.400","AB","xbt",null,null,"Xbt #52 applied to line 0444"]
["2016-04-04T15:11:39.860","2016-04-05T03:11:39.860","AB","sonar","multibeam","Max Angle","60/60"]
["2016-04-04T15:15:27.300","2016-04-05T03:15:27.300","AB","sonar","knudsen","Phase Range","1500-2500m"]
["2016-04-04T15:32:20.150","2016-04-05T03:32:20.150","AB","sonar","knudsen","Tx Power","1, Pulse 2, Phase Range 1000-2000m"]
["2016-04-04T16:53:06.830","2016-04-05T04:53:06.830","AB","sonar","multibeam","New Line","0447 - turn"]
["2016-04-04T16:58:38.520","2016-04-05T04:58:38.520","AB","sonar","multibeam","New Line","0448, max angl;e 45/40"]
["2016-04-04T18:31:42.930","2016-04-05T06:31:42.930","AB","sonar","multibeam","Max Angle","30/30"]
["2016-04-04T19:01:14.480","2016-04-05T07:01:14.480","AB","sonar","knudsen","Tx Power","2, Pulse 2, Gain 37, Phase 1500-2500m"]
["2016-04-04T19:00:10","2016-04-05T07:00:10","AB","sonar","multibeam","New Line","0450"]
["2016-04-04T19:14:30.110","2016-04-05T07:14:30.110","AB","sonar","knudsen","Phase Range","2000-3000m, Power 2, Pulse 4, Gain 39dB"]
["2016-04-04T19:44:59.260","2016-04-05T07:44:59.260","WP","Other",null,null,"watch change"]
["2016-04-04T19:45:24.470","2016-04-05T07:45:24.470","wp","sonar","knudsen","Phase Range","2500-3500, pulse 4.0, power 3, gain 38."]
["2016-04-04T19:56:34.830","2016-04-05T07:56:34.830","wp","sonar","knudsen","phase range","3500-4500, pulse 16, power 3, gain 39."]
["2016-04-04T20:18:50.570","2016-04-05T08:18:50.570","wp","sonar","multibeam","new line","begin turn, new line 0452"]
["2016-04-04T20:35:55.030","2016-04-05T08:35:55.030","wp","sonar","multibeam","New Line","begin survey, new line 0453"]
["2016-04-04T20:38:19.480","2016-04-05T08:38:19.480","wp","sonar","knudsen","Start Pinging","Began New line. Pulse 16, power 3, gain 39, range 3000-4000"]
["2016-04-04T20:50:49.310","2016-04-05T08:50:49.310","wp","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-04T21:04:20.160","2016-04-05T09:04:20.160","wp","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-04T21:30:59.670","2016-04-05T09:30:59.670","CR","sonar","knudsen","Tx Power",1]
["2016-04-04T21:50:49.360","2016-04-05T09:50:49.360","MP","sonar","knudsen","Phase Range","1000-2000"]
["2016-04-04T22:11:22.760","2016-04-05T10:11:22.760","MP","sonar","knudsen","Gain Value",33]
["2016-04-04T22:56:56.510","2016-04-05T10:56:56.510","MP","sonar","multibeam","New Line","Begin turn, new line 0456"]
["2016-04-04T23:11:23.630","2016-04-05T11:11:23.630","wp","sonar","multibeam","New Line","begin survey line, new line 0457"]
["2016-04-04T23:25:01.360","2016-04-05T11:25:01.360","MP","sonar","knudsen","Tx Pulse","16, power 2"]
["2016-04-04T23:45:55.540","2016-04-05T11:45:55.540","MP","sonar","knudsen","Gain Value",31]
["2016-04-05T00:44:46.540","2016-04-05T12:44:46.540","CR","sonar","knudsen","Gain Value",32]
["2016-04-05T00:56:02.010","2016-04-05T12:56:02.010","CR","sonar","knudsen","phase range","1500-2500, Tx Power3, Gain Value 34dB"]
["2016-04-05T01:01:43.250","2016-04-05T13:01:43.250","CR","sonar","knudsen","phase range","2000-3000"]
["2016-04-05T01:29:37.560","2016-04-05T13:29:37.560","CR","sonar","knudsen","Tx Pulse","32; gain value 38"]
["2016-04-05T01:44:18.320","2016-04-05T13:44:18.320","MP","sonar","knudsen","Phase Range","2500-3500, gain value 41dB"]
["2016-04-05T01:52:12.820","2016-04-05T13:52:12.820","MP","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-05T02:02:39.670","2016-04-05T14:02:39.670","WP","Sonar","multibeam","New Line","Begin Turn, new line 0460"]
["2016-04-05T02:19:21.540","2016-04-05T14:19:21.540","WP","Sonar","multibeam","New Line","begin survey line, new line 0461."]
["2016-04-05T02:22:57.270","2016-04-05T14:22:57.270","MP","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-05T02:27:57.420","2016-04-05T14:27:57.420","MP","sonar","knudsen","Phase Range","2000-3000, gain 39dB"]
["2016-04-05T02:33:46.450","2016-04-05T14:33:46.450","CR","sonar","knudsen","Gain Value","34; Tx Power 2; Phase Range 1500-2500"]
["2016-04-05T02:34:49.390","2016-04-05T14:34:49.390","CR","XBT",null,null,"#54 (1st Cast cancelled) 2nd Cast Attempt Complete"]
["2016-04-05T02:38:17.980","2016-04-05T14:38:17.980","wp","xbt",null,null,"xbt 54 applied to line 461"]
["2016-04-05T02:41:11.150","2016-04-05T14:41:11.150","MP","sonar","knudsen","Tx Pulse","16, gain 32dB"]
["2016-04-05T02:59:56.460","2016-04-05T14:59:56.460","DS","Ship",null,null,"requested bridge reduce speed by half a knot. "]
["2016-04-05T03:07:14.500",{"$f":"IF(ISBLANK(A1665),\" \",((A1665)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-05T15:07:14.500"},"CR","sonar","knudsen","Tx Pulse",8]
["2016-04-05T03:09:59.210","2016-04-05T15:09:59.210","CR","sonar","knudsen","tx power",1]
["2016-04-05T03:10:53.180","2016-04-05T15:10:53.180","CR","sonar","knudsen","Phase Range","1000-2000"]
["2016-04-05T03:30:45.720","2016-04-05T15:30:45.720","DF","sonar","multibeam","Along Direction Pitch",-1]
["2016-04-05T03:31:49.010","2016-04-05T15:31:49.010","DF","sonar","multibeam","Along Direction Pitch",-2]
["2016-04-05T04:26:49.380","2016-04-05T16:26:49.380","DF","sonar","multibeam","New Line","begin turn line 0464"]
["2016-04-05T04:37:14.650","2016-04-05T16:37:14.650","DF","sonar","knudsen","Tx Power",2]
["2016-04-05T04:39:32.270","2016-04-05T16:39:32.270","DF","sonar","multibeam","New Line","begin test survey line 0465, trying new line plan heading"]
["2016-04-05T04:45:33.290","2016-04-05T16:45:33.290","DF","sonar","multibeam","Max Angle","60/65"]
["2016-04-05T04:46:54.610","2016-04-05T16:46:54.610","DF","sonar","knudsen","tx pulse",32]
["2016-04-05T04:48:23.850","2016-04-05T16:48:23.850","DF","sonar","multibeam","Along Direction Pitch",0]
["2016-04-05T04:56:21.620","2016-04-05T16:56:21.620","DS","Ship",null,null,"staying with new heading line plan for now, requested 500m shift to the north (stbd)"]
["2016-04-05T05:00:55.590","2016-04-05T17:00:55.590","DF","sonar","multibeam","Max Angle","55/60"]
["2016-04-05T05:11:47.030","2016-04-05T17:11:47.030","DF","sonar","multibeam","Max Angle","60/63"]
["2016-04-05T05:22:41.100","2016-04-05T17:22:41.100","DF","sonar","knudsen","Tx Power",1]
["2016-04-05T05:44:40.240","2016-04-05T17:44:40.240","DS","Ship",null,null,"requested bridge to move 300 m starboard (north)"]
["2016-04-05T06:02:03.720","2016-04-05T18:02:03.720","DF","sonar","multibeam","Spike Filter Strength","medium"]
["2016-04-05T06:03:12.710","2016-04-05T18:03:12.710","DF","sonar","multibeam","Max Angle","65/65"]
["2016-04-05T06:05:10.560","2016-04-05T18:05:10.560","DF","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-05T06:09:05.820","2016-04-05T18:09:05.820","DF","sonar","knudsen",null,"tx power to 2, tx pulse to 8"]
["2016-04-05T06:11:43.490","2016-04-05T18:11:43.490","BG","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-05T06:13:00.240","2016-04-05T18:13:00.240","DF","sonar","knudsen","tx power",3]
["2016-04-05T06:14:15.400","2016-04-05T18:14:15.400","DF","sonar","multibeam","Max Angle","60/65"]
["2016-04-05T06:16:23.030","2016-04-05T18:16:23.030","DF","sonar","multibeam","Along Direction Pitch",-2]
["2016-04-05T06:21:17.740","2016-04-05T18:21:17.740","DF","sonar","multibeam","Max Angle","50/60"]
["2016-04-05T06:22:36.630","2016-04-05T18:22:36.630","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-05T06:31:37.780","2016-04-05T18:31:37.780","BG","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-05T06:51:03.630","2016-04-05T18:51:03.630","BG","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-05T06:59:22.690","2016-04-05T18:59:22.690","DF","sonar","multibeam","Max Angle","50/50"]
["2016-04-05T07:09:14.390","2016-04-05T19:09:14.390","DF","sonar","knudsen","Gain Value","34 dB"]
["2016-04-05T07:11:29.210","2016-04-05T19:11:29.210","DF","sonar","multibeam","Max Angle","45/45"]
["2016-04-05T07:21:19.990","2016-04-05T19:21:19.990","DF","sonar","multibeam","New Line","begin turn line 0468"]
["2016-04-05T07:22:06.940","2016-04-05T19:22:06.940","DF","sonar","knudsen","phase range","4000-5000"]
["2016-04-05T07:32:39.940","2016-04-05T19:32:39.940","BG","sonar","knudsen","phase range","4500-5500"]
["2016-04-05T07:33:57.780","2016-04-05T19:33:57.780","SM","sonar","knudsen","phase range","4000-5000"]
["2016-04-05T07:35:00.400","2016-04-05T19:35:00.400","SM","sonar","knudsen","Tx Pulse","8 ms"]
["2016-04-05T07:40:13.450","2016-04-05T19:40:13.450","DF","sonar","multibeam","Max Angle","35/35"]
["2016-04-05T07:47:36.650","2016-04-05T19:47:36.650","DF","sonar","multibeam","Max Angle","40/40"]
["2016-04-05T07:51:01.090","2016-04-05T19:51:01.090","DS","Sonar","Knudsen","Tx Pulse","increased from 8 to 32 ms"]
["2016-04-05T07:52:30.730","2016-04-05T19:52:30.730","DF","sonar","multibeam","Max Angle","35/45"]
["2016-04-05T08:00:29.790","2016-04-05T20:00:29.790","DF","sonar","knudsen","Tx Pulse",16]
["2016-04-05T08:01:12.560","2016-04-05T20:01:12.560","DF","Sonar","multibeam","Along Direction Pitch",0]
["2016-04-05T08:04:01.690","2016-04-05T20:04:01.690","BG","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-05T08:07:53.490","2016-04-05T20:07:53.490","DF","sonar","multibeam","Max Angle","35/40"]
["2016-04-05T08:18:38.450","2016-04-05T20:18:38.450","DF","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-05T08:35:47.900","2016-04-05T20:35:47.900","DF","sonar","multibeam","Max Angle","30/30"]
["2016-04-05T08:41:40.200","2016-04-05T20:41:40.200","DF","sonar","multibeam",null,"40/40, ping mode to very deep"]
["2016-04-05T08:42:48.470","2016-04-05T20:42:48.470","DF","sonar","multibeam","Max Angle","45/40"]
["2016-04-05T08:43:40.890","2016-04-05T20:43:40.890","DF","sonar","multibeam","Along Direction Pitch",1]
["2016-04-05T08:52:55.250","2016-04-05T20:52:55.250","DF","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-05T08:57:28.430","2016-04-05T20:57:28.430","DF","sonar","multibeam","Ping Mode","auto"]
["2016-04-05T08:58:14.700","2016-04-05T20:58:14.700","DF","sonar","multibeam","Max Angle","55/55"]
["2016-04-05T09:01:53.220","2016-04-05T21:01:53.220","DF","sonar","multibeam","Max Angle","65/65"]
["2016-04-05T09:04:54.560","2016-04-05T21:04:54.560","DF","sonar","multibeam","Max Angle","60/65"]
["2016-04-05T09:07:22.170","2016-04-05T21:07:22.170","DF","sonar","multibeam","Max Angle","60/55"]
["2016-04-05T09:10:50.980","2016-04-05T21:10:50.980","DF","xbt",null,null,"cast 055 collected"]
["2016-04-05T09:13:46.470","2016-04-05T21:13:46.470","BG","xbt",null,null,"cast applied to line 0469"]
["2016-04-05T09:15:53.390","2016-04-05T21:15:53.390","SM","sonar","knudsen","Tx Power","1900-01-01"]
["2016-04-05T09:19:11.670","2016-04-05T21:19:11.670","SM","sonar","knudsen","Phase Range","1000-2000"]
["2016-04-05T09:26:41.080","2016-04-05T21:26:41.080","DF","sonar","knudsen","tx pulse","64, gain to 34"]
["2016-04-05T09:33:59.080","2016-04-05T21:33:59.080","DF","sonar","multibeam","Max Angle","50/50"]
["2016-04-05T09:34:39.070","2016-04-05T21:34:39.070","DF","sonar","multibeam","Spike Filter Strength","strong"]
["2016-04-05T09:36:34.170","2016-04-05T21:36:34.170","DF","sonar","multibeam","Along Direction Pitch",-1]
["2016-04-05T09:40:29.020","2016-04-05T21:40:29.020","DF","sonar","multibeam","Max Angle","35/35"]
["2016-04-05T09:41:01.960",{"$f":"IF(ISBLANK(A1729),\" \",((A1729)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-05T21:41:01.960"},"DF","sonar","multibeam","Along Direction Pitch",-2]
["2016-04-05T09:42:53.060","2016-04-05T21:42:53.060","DF","sonar","multibeam","Max Angle","45/45"]
["2016-04-05T09:44:11.550","2016-04-05T21:44:11.550","DF","sonar","multibeam","Max Angle","50/50"]
["2016-04-05T09:46:24.450","2016-04-05T21:46:24.450","DF","sonar","multibeam","Max Angle","45/45"]
["2016-04-05T09:48:51.760","2016-04-05T21:48:51.760","DF","sonar","knudsen","Tx Pulse",16]
["2016-04-05T09:50:21.940","2016-04-05T21:50:21.940","DF","sonar","multibeam","Max Angle","45/50"]
["2016-04-05T10:05:01.210","2016-04-05T22:05:01.210","DF","sonar","multibeam","Max Angle","45/60"]
["2016-04-05T10:28:12.160","2016-04-05T22:28:12.160","DF","sonar","multibeam","New Line","begin turn line 0472"]
["2016-04-05T10:39:20.310","2016-04-05T22:39:20.310","DF","sonar","multibeam","Max Angle","50/60"]
["2016-04-05T10:39:46.930","2016-04-05T22:39:46.930","DF","sonar","multibeam","New Line","begin survey line 0473"]
["2016-04-05T10:45:02.560","2016-04-05T22:45:02.560","DF","sonar","multibeam","Max Angle","45/55"]
["2016-04-05T10:45:20.560","2016-04-05T22:45:20.560","DF","sonar","multibeam","Max Angle","45/50"]
["2016-04-05T10:53:39.790","2016-04-05T22:53:39.790","DF","sonar","multibeam","Spike Filter Strength","medium"]
["2016-04-05T11:05:58.850","2016-04-05T23:05:58.850","DF","sonar","multibeam","Max Angle","60/60"]
["2016-04-05T11:18:45.290","2016-04-05T23:18:45.290","DF","sonar","multibeam","Along Direction Pitch",0]
["2016-04-05T11:39:46.660","2016-04-05T23:39:46.660","AB","sonar","knudsen","Tx Pulse","2, New Line"]
["2016-04-05T12:40:26","2016-04-06T00:40:26","AB","sonar","multibeam","New Line","0475, spike filter strong"]
["2016-04-05T12:51:01.460","2016-04-06T00:51:01.460","AB","sonar","knudsen","Range","1000m, Power 2, Pulse 2, Phase Range 1500-2500m"]
["2016-04-05T12:54:17.740","2016-04-06T00:54:17.740","AB","sonar","knudsen","phase range","2000-3000m"]
["2016-04-05T12:57:49.530","2016-04-06T00:57:49.530","AB","sonar","multibeam","Max Angle","55/55"]
["2016-04-05T13:07:49.580","2016-04-06T01:07:49.580","AB","sonar","knudsen","Tx Pulse","4, Phase Range 2500-3500m"]
["2016-04-05T13:16:44.550","2016-04-06T01:16:44.550","AB","sonar","knudsen","Tx Pulse","8, Power 3, Phase Range 3000-4000m"]
["2016-04-05T13:25:44.850","2016-04-06T01:25:44.850","AB","sonar","Knudsen","Phase Range","3000-4000m"]
["2016-04-05T13:26:23.870","2016-04-06T01:26:23.870","AB","sonar","multibeam","Ping Mode","Auto: Very Deep "]
["2016-04-05T13:47:53.660","2016-04-06T01:47:53.660","SM","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-05T14:07:20.480","2016-04-06T02:07:20.480","AB","sonar","knudsen","Phase Range","3000-4000m"]
["2016-04-05T14:16:47.320","2016-04-06T02:16:47.320","AB","sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-05T14:20:47.230","2016-04-06T02:20:47.230","AB","Sonar","multibeam","Ping Mode","Deep, Max Angles 60/60"]
["2016-04-05T14:23:16.440","2016-04-06T02:23:16.440","AB","sonar","knudsen","Phase Range","2000-3000m"]
["2016-04-05T14:28:43.990","2016-04-06T02:28:43.990","AB","sonar","knudsen","Phase Range","1500-2500m"]
["2016-04-05T14:33:05.430","2016-04-06T02:33:05.430","AB","sonar","multibeam","Max Angle","65/65, along track -2.0"]
["2016-04-05T14:33:48.080","2016-04-06T02:33:48.080","AB","sonar","knudsen","Phase Range","1000-2000m, Gain 36dB, Pulse 2, Power 1"]
["2016-04-05T14:49:39.670","2016-04-06T02:49:39.670","AB","sonar","knudsen","Phase Range","1500-2500m, Power 2 "]
["2016-04-05T15:03:29.510","2016-04-06T03:03:29.510","Ab","xbt",null,null,"#56 - canceled at ~450m"]
["2016-04-05T15:07:42.800","2016-04-06T03:07:42.800","AB","xbt",null,null,"#57 - canceled at 75m, Use #56"]
["2016-04-05T15:10:55.980","2016-04-06T03:10:55.980","AB","xbt",null,null,"#56 applied to line 0478"]
["2016-04-05T15:14:45.210","2016-04-06T03:14:45.210","AB","sonar","knudsen","Phase Range","2500-3500m, Power 3, Pulse 8"]
["2016-04-05T15:18:49.400","2016-04-06T03:18:49.400","AB","sonar","multibeam","Ping Mode","Very Deep, Max angles 52/52"]
["2016-04-05T15:39:49.960","2016-04-06T03:39:49.960","AB","sonar","knudsen","Phase Range","4500-5500m, Pulse 16"]
["2016-04-05T15:51:51.420","2016-04-06T03:51:51.420","AB","sonar","multibeam","Ping Mode","Extra Deep, Max angle 35/35"]
["2016-04-05T15:52:06.090","2016-04-06T03:52:06.090","AB","sonar","knudsen","Phase Range","5000-6000m"]
["2016-04-05T16:35:21.880","2016-04-06T04:35:21.880","AB","sonar","multibeam","New Line","0480 - turn"]
["2016-04-05T16:37:36.040","2016-04-06T04:37:36.040","AB","sonar","multibeam","New Line","0481"]
["2016-04-05T17:15:06.580","2016-04-06T05:15:06.580","AB","sonar","multibeam",null,"Sonar lost bottom due to steep rise on seamount"]
["2016-04-05T17:17:25.920","2016-04-06T05:17:25.920","AB","sonar","multibeam","Ping Mode","Auto: Very Deep; Max Angle 45/50 "]
["2016-04-05T17:18:46.370","2016-04-06T05:18:46.370","AB","sonar","knudsen","phase range","3500-4500m "]
["2016-04-05T17:44:41.760","2016-04-06T05:44:41.760","AB","sonar","multibeam","Ping Mode","Auto: Extra Deep "]
["2016-04-05T18:30:00.620","2016-04-06T06:30:00.620","AB","sonar","multibeam","New Line","0438 - turn"]
["2016-04-05T18:32:14.500","2016-04-06T06:32:14.500","AB","sonar","multibeam","New Line","0484"]
["2016-04-05T19:43:53.660","2016-04-06T07:43:53.660","MP","sonar","knudsen","Tx Pulse",32]
["2016-04-05T19:45:15.490","2016-04-06T07:45:15.490","DS","Ship",null,null,"asked ship to slow to 8-8.8 knots"]
["2016-04-05T19:53:03.240","2016-04-06T07:53:03.240","wp",null,null,null,"watch change"]
["2016-04-05T20:02:12.130","2016-04-06T08:02:12.130","MP","sonar","knudsen","Tx Pulse","16, gain 42dB"]
["2016-04-05T20:11:07.170","2016-04-06T08:11:07.170","MP","sonar","knudsen","Phase Range","4000-5000"]
["2016-04-05T20:14:18.770","2016-04-06T08:14:18.770","DS","Ship",null,null,"slowing to 7.5-8"]
["2016-04-05T20:20:10.950","2016-04-06T08:20:10.950","DS","Ship",null,null,"slowing to 6-6.5"]
["2016-04-05T20:23:59.930","2016-04-06T08:23:59.930","DS","Ship",null,null,"Return ships speed to between 7.5 and 8.0 kts"]
["2016-04-05T20:31:17.730","2016-04-06T08:31:17.730","CR","sonar","knudsen","Phase Range","2500-3500; Gain Value 47"]
["2016-04-05T20:39:48.720","2016-04-06T08:39:48.720","CR","sonar","knudsen","Gain Value",43]
["2016-04-05T20:52:13.870","2016-04-06T08:52:13.870","WP","sonar","Knudsen","phase range","2000-3000, pulse 8, power 2, gain 32."]
["2016-04-05T21:17:14.560","2016-04-06T09:17:14.560","WP","Sonar","Knudsen","Phase range","2500-3500, Pulse 4.0, Power 2, gain 34."]
["2016-04-05T21:19:25.470","2016-04-06T09:19:25.470","CR","XBT",null,null,"XBT 058 complete, stopped collecting data at 600m"]
["2016-04-05T21:22:05.160","2016-04-06T09:22:05.160","WP","XBT",null,null,"XBT 058 applied to line 0486",null,null,null,null,"xb"]
["2016-04-05T21:26:19.640","2016-04-06T09:26:19.640","WP","sonar","knudsen","phase range","2500-3500, power 3.0, pulse 16, gain 41."]
["2016-04-05T21:37:35.560",{"$f":"IF(ISBLANK(A1793),\" \",((A1793)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-06T09:37:35.560"},"WP","sonar","knudsen","phase range","3500-4500"]
["2016-04-05T21:53:05.570","2016-04-06T09:53:05.570","WP","sonar","knudsen","phase range","3000-4000, pulse 2.0, power 3, gain 34"]
["2016-04-05T22:08:02.040","2016-04-06T10:08:02.040","MP","sonar","multibeam","New Line","begin turn, line 0489"]
["2016-04-05T22:17:09.390","2016-04-06T10:17:09.390","MP","sonar","knudsen","Tx Pulse","16, gain 36dB"]
["2016-04-05T22:17:39.520","2016-04-06T10:17:39.520","MP","sonar","multibeam","New Line","begin survey line 0490"]
["2016-04-05T22:20:53.710","2016-04-06T10:20:53.710","MP","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-05T22:24:55.570","2016-04-06T10:24:55.570","WP","Sonar","multibeam","New Line","Survey line advanced a second time by accident, new line 0491"]
["2016-04-05T22:33:12.840","2016-04-06T10:33:12.840","MP","sonar","knudsen","Tx Pulse","2, gain value 30dB, power 2"]
["2016-04-05T22:46:40.810","2016-04-06T10:46:40.810","MP","sonar","Knudsen","Tx Pulse","16, power 3, gain 32dB, phase range 2000-3000"]
["2016-04-05T22:57:05.700","2016-04-06T10:57:05.700","MP","sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-05T23:01:26.730","2016-04-06T11:01:26.730","WP","Sonar","Knudsen","Phase Range","1500-2500, Pulse 8.0, Power 2.0, gain 31"]
["2016-04-05T23:04:19.840","2016-04-06T11:04:19.840","WP","sonar","knudsen","Phase Range","1000-2000, Pulse 2, power 2, gain 29"]
["2016-04-05T23:22:12.650","2016-04-06T11:22:12.650","MP","sonar","knudsen","Tx Pulse",2]
["2016-04-05T23:28:37.400","2016-04-06T11:28:37.400","MP","Sonar","knudsen","Tx Power",1]
["2016-04-06T00:08:23.400","2016-04-06T12:08:23.400","CR","sonar","knudsen","Phase Range","1500-2500"]
["2016-04-06T00:16:56.200","2016-04-06T12:16:56.200","CR","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-06T00:24:44.270","2016-04-06T12:24:44.270","MP","sonar","knudsen","Tx Pulse","32, gain value 38dB, 2500-3500"]
["2016-04-06T00:33:29.450","2016-04-06T12:33:29.450","MP","sonar","knudsen","Phase Range","3000-4000, gain value 41dB"]
["2016-04-06T00:40:13.780","2016-04-06T12:40:13.780","MP","sonar","multibeam","New Line","begin turn, line 0494"]
["2016-04-06T00:41:19.970","2016-04-06T12:41:19.970","MP","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-06T01:04:28.720","2016-04-06T13:04:28.720","wp","sonar","multibeam","New Line","begin survey line, new line 0495"]
["2016-04-06T01:31:07.850","2016-04-06T13:31:07.850","CR","sonar","knudsen","tx power",2]
["2016-04-06T01:35:37.470","2016-04-06T13:35:37.470","CR","sonar","knudsen","phase range","2500-3500"]
["2016-04-06T01:41:59.950","2016-04-06T13:41:59.950","CR","sonar","knudsen","phase range","2000-3000"]
["2016-04-06T02:02:35.690","2016-04-06T14:02:35.690","CR","sonar","knudsen","phase range","1000-2000"]
["2016-04-06T02:41:41.250","2016-04-06T14:41:41.250","CR","sonar","knudsen","phase range","2000-3000"]
["2016-04-06T02:54:54.810","2016-04-06T14:54:54.810","CR","sonar","knudsen","tx power",3]
["2016-04-06T02:58:39.530","2016-04-06T14:58:39.530","CR","sonar","knudsen","phase range","1500-2500"]
["2016-04-06T03:05:48.110","2016-04-06T15:05:48.110","CR","sonar","knudsen","phase range","2000-3000"]
["2016-04-06T03:09:46","2016-04-06T15:09:46","DF","xbt",null,null,"cast 059 collected and applied 0497"]
["2016-04-06T03:25:27.030","2016-04-06T15:25:27.030","BG","sonar","knudsen","phase range","2500-3500"]
["2016-04-06T03:37:54.950","2016-04-06T15:37:54.950","DF","watch change",null,null,"Dan and Breezy on watch"]
["2016-04-06T03:39:40.390","2016-04-06T15:39:40.390","DF","sonar","multibeam","Aeration Filter (On/Off)","off"]
["2016-04-06T03:40:08.010","2016-04-06T15:40:08.010","DF","sonar","multibeam","New Line","begin turn line 0498"]
["2016-04-06T03:41:15.530","2016-04-06T15:41:15.530","DF","sonar","multibeam","Max Angle","48/48"]
["2016-04-06T03:46:09.790","2016-04-06T15:46:09.790","DF","sonar","knudsen","Tx Pulse",32]
["2016-04-06T03:46:29.530","2016-04-06T15:46:29.530","DF","sonar","multibeam","Max Angle","48/50"]
["2016-04-06T03:49:31.510","2016-04-06T15:49:31.510","DF","sonar","multibeam","Max Angle","48/52"]
["2016-04-06T03:52:55.540","2016-04-06T15:52:55.540","DF","sonar","multibeam","Max Angle","48/55"]
["2016-04-06T04:00:55.960","2016-04-06T16:00:55.960","DF","sonar","multibeam","Max Angle","52/48"]
["2016-04-06T04:03:47.090","2016-04-06T16:03:47.090","DF","sonar","multibeam","New Line","begin survey trackline 0499"]
["2016-04-06T04:05:20.800","2016-04-06T16:05:20.800","DF","sonar","multibeam","Max Angle","48/52"]
["2016-04-06T04:06:36.740","2016-04-06T16:06:36.740","DF","sonar","multibeam","Max Angle","46/52"]
["2016-04-06T04:07:39.200","2016-04-06T16:07:39.200","DF","sonar","multibeam","Max Angle","45/70"]
["2016-04-06T04:08:53.300","2016-04-06T16:08:53.300","DF","ship",null,null,"requested 1000 m move to stbd"]
["2016-04-06T04:10:20.510","2016-04-06T16:10:20.510","DF","sonar","multibeam","New Line","new line for trackline shift to stbd (turn spoking)"]
["2016-04-06T04:12:29.500","2016-04-06T16:12:29.500","DF","Sonar","multibeam","Max Angle","60/70"]
["2016-04-06T04:17:26.690","2016-04-06T16:17:26.690","DF","sonar","multibeam","Max Angle","45/70"]
["2016-04-06T04:21:22.670","2016-04-06T16:21:22.670","DF","sonar","multibeam","Max Angle","48/55"]
["2016-04-06T04:22:00.280","2016-04-06T16:22:00.280","DF","sonar","knudsen","phase range","2000-3000"]
["2016-04-06T04:22:31.340","2016-04-06T16:22:31.340","DF","sonar","multibeam","Max Angle","45/52"]
["2016-04-06T04:26:16.850","2016-04-06T16:26:16.850","DF","sonar","multibeam","New Line","begin new survey line 0501, after line shifts and turns"]
["2016-04-06T04:27:18.740","2016-04-06T16:27:18.740","DF","ship",null,null,"requested gradual 700 m move to PORT"]
["2016-04-06T04:35:58.640","2016-04-06T16:35:58.640","DF","sonar","multibeam","Max Angle","42/65"]
["2016-04-06T04:43:27.750","2016-04-06T16:43:27.750","DF","sonar","multibeam","Max Angle","45/60"]
["2016-04-06T04:44:53.750","2016-04-06T16:44:53.750","DF","sonar","multibeam","Max Angle","45/57"]
["2016-04-06T04:45:36.220","2016-04-06T16:45:36.220","DF","Sonar","knudsen","Phase Range","2500-3500"]
["2016-04-06T04:46:09.210","2016-04-06T16:46:09.210","DF","sonar","multibeam","Max Angle","45/60"]
["2016-04-06T04:47:01.330","2016-04-06T16:47:01.330","DF","sonar","multibeam","Max Angle","43/60"]
["2016-04-06T04:48:23.480","2016-04-06T16:48:23.480","DF","sonar","multibeam","Max Angle","40/60"]
["2016-04-06T04:48:47.760","2016-04-06T16:48:47.760","DF","Sonar","multibeam","Spike Filter Strength","strong"]
["2016-04-06T04:49:53.870","2016-04-06T16:49:53.870","DF","sonar","multibeam","Max Angle","35/65"]
["2016-04-06T05:02:54.680","2016-04-06T17:02:54.680","DF","sonar","knudsen",null,"phase range to 2000-3000, tx pulse to 16"]
["2016-04-06T05:08:40.820","2016-04-06T17:08:40.820","DF","Sonar","multibeam","Max Angle","30/60"]
["2016-04-06T05:22:51.370",{"$f":"IF(ISBLANK(A1857),\" \",((A1857)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-06T17:22:51.370"},"DF","sonar","multibeam","Max Angle","32/62"]
["2016-04-06T05:23:22.030","2016-04-06T17:23:22.030","DF","sonar","multibeam","Max Angle","35/65"]
["2016-04-06T05:23:57.550","2016-04-06T17:23:57.550","DF","sonar","multibeam","Max Angle","38/68"]
["2016-04-06T05:26:17.750","2016-04-06T17:26:17.750","DF","sonar","multibeam","Max Angle","40/70"]
["2016-04-06T05:28:03.610","2016-04-06T17:28:03.610","DF","sonar","multibeam","Max Angle","42/70"]
["2016-04-06T05:30:32.500","2016-04-06T17:30:32.500","DF","sonar","multibeam","Max Angle","45/70"]
["2016-04-06T05:32:54.620","2016-04-06T17:32:54.620","DF","sonar","knudsen","tx power",2]
["2016-04-06T05:38:48.350","2016-04-06T17:38:48.350","DS","Sonar","Multibeam","Max Angle","50/70"]
["2016-04-06T05:47:53.720","2016-04-06T17:47:53.720","DS","Sonar","Multibeam","Spike Filter Strength","from strong to medium"]
["2016-04-06T05:53:17.580","2016-04-06T17:53:17.580","BG","sonar","knudsen","phase range","2500-3500"]
["2016-04-06T05:58:55.630","2016-04-06T17:58:55.630","BG","sonar","knudsen","phase range","3000-4000"]
["2016-04-06T06:09:45.340","2016-04-06T18:09:45.340","BG","sonar","knudsen","phase range","3500-4500"]
["2016-04-06T06:33:29.870","2016-04-06T18:33:29.870","DF","sonar","multibeam","Max Angle","42/42"]
["2016-04-06T06:33:36.450","2016-04-06T18:33:36.450","DF","sonar","knudsen","phase range","4000-5000"]
["2016-04-06T06:51:37.330","2016-04-06T18:51:37.330","DF","sonar","multibeam","Max Angle","35/35"]
["2016-04-06T07:20:14.680","2016-04-06T19:20:14.680","DF","sonar","multibeam","New Line","begin turn line 0504"]
["2016-04-06T07:32:06.800","2016-04-06T19:32:06.800","BG","sonar","knudsen","phase range","3500-4500"]
["2016-04-06T07:34:42.540","2016-04-06T19:34:42.540","DF","sonar","multibeam","Max Angle","50/50"]
["2016-04-06T07:36:01.990","2016-04-06T19:36:01.990","DF","sonar","multibeam","Max Angle","48/48"]
["2016-04-06T07:38:08.590","2016-04-06T19:38:08.590","BG","sonar","knudsen","phase range","3000-4000"]
["2016-04-06T07:40:36.490","2016-04-06T19:40:36.490","DF","sonar","multibeam","Max Angle","46/46"]
["2016-04-06T07:44:03.580","2016-04-06T19:44:03.580","DF","sonar","multibeam","Max Angle","70/70"]
["2016-04-06T07:58:16.190","2016-04-06T19:58:16.190","DF","sonar","knudsen","phase range","2500-3500"]
["2016-04-06T08:12:02.830","2016-04-06T20:12:02.830","DF","sonar","knudsen","phase range","1500-2500"]
["2016-04-06T08:17:29.450","2016-04-06T20:17:29.450","DF","sonar","knudsen","phase range","1000-2000"]
["2016-04-06T08:18:43.830","2016-04-06T20:18:43.830","DF","sonar","knudsen",null,"tx pulse to 2, tx power to 1"]
["2016-04-06T09:21:33.820","2016-04-06T21:21:33.820","SM","XBT",null,null,"Cast 060"]
["2016-04-06T09:21:57.430","2016-04-06T21:21:57.430","SM","XBT",null,null,"Cast 060 applied to line 0506"]
["2016-04-06T09:23:06.510","2016-04-06T21:23:06.510","SM","sonar","knudsen","phase range","1500-2500"]
["2016-04-06T09:38:30.770","2016-04-06T21:38:30.770","BG","sonar","knudsen","phase range","2000-3000"]
["2016-04-06T09:42:11.640","2016-04-06T21:42:11.640","DF","sonar","knudsen","Tx Power",2]
["2016-04-06T09:43:54.760","2016-04-06T21:43:54.760","DF","sonar","knudsen","phase range","2500-3500"]
["2016-04-06T09:59:53.080","2016-04-06T21:59:53.080","DF","Sonar","knudsen",null,"tx pulse to 8ms, tx power to 3"]
["2016-04-06T11:24:06.140","2016-04-06T23:24:06.140","BG","sonar","knudsen","phase range","3000-4000"]
["2016-04-06T11:35:14.330","2016-04-06T23:35:14.330","DF","sonar","ek",null,"stopping logging and pinging to turn on the 70, 120, and 300 kHz EK's"]
["2016-04-06T11:50:21.720","2016-04-06T23:50:21.720","BG","sonar","knudsen","phase range","3500-4500"]
["2016-04-06T12:02:35.040","2016-04-07T00:02:35.040","BG","sonar","knudsen","Phase Range","4000-5000"]
["2016-04-06T12:10:24.870","2016-04-07T00:10:24.870","BG","sonar","multibeam","New Line","begin turn line 0508"]
["2016-04-06T12:17:55.490","2016-04-07T00:17:55.490","BG","sonar","multibeam","New Line","begin survey line 0509"]
["2016-04-06T13:18:51","2016-04-07T01:18:51","AB","sonar","multibeam","New Line","0510"]
["2016-04-06T13:51:30.830","2016-04-07T01:51:30.830","AB","sonar","knudsen","Phase Range","3500-4500m "]
["2016-04-06T13:56:41.780","2016-04-07T01:56:41.780","AB","sonar","multibeam","Max Angle","52/52"]
["2016-04-06T14:07:12.030","2016-04-07T02:07:12.030","AB","Sonar","multibeam","New Line","0511 - turn"]
["2016-04-06T14:10:28.560","2016-04-07T02:10:28.560","AB","sonar","multibeam","New Line","0512"]
["2016-04-06T14:25:09.280","2016-04-07T02:25:09.280","AB","sonar","knudsen","phase range","3000-4000m"]
["2016-04-06T14:30:33.020","2016-04-07T02:30:33.020","AB","sonar","multibeam","Ping Mode","Deep, Max Angles 60/60"]
["2016-04-06T14:31:10.880","2016-04-07T02:31:10.880","AB","Sonar","knudsen","phase range","2500-3500m"]
["2016-04-06T14:34:54.610","2016-04-07T02:34:54.610","AB","sonar","knudsen","phase range","2000-3000m"]
["2016-04-06T14:47:01.250","2016-04-07T02:47:01.250","AB","sonar","knudsen","phase range","1500-2500m, Power 2, Pulse 4"]
["2016-04-06T14:47:43.310","2016-04-07T02:47:43.310","AB","Sonar","multibeam","Max Angle","65/70"]
["2016-04-06T14:52:26.860","2016-04-07T02:52:26.860","AB","sonar","knudsen","Tx Power","1, Pulse 2"]
["2016-04-06T15:21:54.560","2016-04-07T03:21:54.560","AB","sonar","knudsen","phase range","2000-3000m, Power 2, Pulse 2"]
["2016-04-06T15:22:43.270","2016-04-07T03:22:43.270","AB","sonar","multibeam","Max Angle","60/60"]
["2016-04-06T15:29:22.530","2016-04-07T03:29:22.530","AB","sonar","knudsen","Tx Power","3, Pulse 8"]
["2016-04-06T15:34:28.100","2016-04-07T03:34:28.100","AB","sonar","knudsen","phase range","3000-4000m"]
["2016-04-06T15:45:31.900","2016-04-07T03:45:31.900","CA","sonar","knudsen","phase range","3500-4500m "]
["2016-04-06T15:53:46.920","2016-04-07T03:53:46.920","AB","sonar","knudsen","phase range","4000-5000m"]
["2016-04-06T15:58:16","2016-04-07T03:58:16","AB","Sonar","Multibeam","Max Angle","40/40"]
["2016-04-06T16:00:33.060","2016-04-07T04:00:33.060","AB","Sonar","knudsen","phase range","4500-5500m"]
["2016-04-06T16:03:58.860","2016-04-07T04:03:58.860","AB","sonar","multibeam","Ping Mode","Auto: Extra Deep "]
["2016-04-06T16:06:12.680","2016-04-07T04:06:12.680","AB","XBT",null,null,"#61"]
["2016-04-06T16:11:02.250","2016-04-07T04:11:02.250","AB","XBT",null,null,"#61 added to new line 0515."]
["2016-04-06T16:38:30.360","2016-04-07T04:38:30.360","AB","sonar","multibeam","New Line","0516"]
["2016-04-06T16:52:22.720","2016-04-07T04:52:22.720","AB","sonar","multibeam","Ping Mode","Very Deep, Max angles 52/52"]
["2016-04-06T16:53:32.510",{"$f":"IF(ISBLANK(A1921),\" \",((A1921)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-04-07T04:53:32.510"},"AB","sonar","knudsen","phase range","4000-5000m"]
["2016-04-06T17:32:59.390","2016-04-07T05:32:59.390","AB","sonar","multibeam","Ping Mode","Deep, Max Angles 60/60"]
["2016-04-06T17:33:45.330","2016-04-07T05:33:45.330","CA","sonar","knudsen","phase range","2000-3000m"]
["2016-04-06T17:50:35.750","2016-04-07T05:50:35.750","AB","sonar","multibeam","Max Angle","70/60"]
["2016-04-06T18:46:15.270","2016-04-07T06:46:15.270","AB","sonar","multibeam","New Line","0520 - turn"]
["2016-04-06T18:51:32.400","2016-04-07T06:51:32.400","AB","sonar","multibeam","New Line","0521"]
["2016-04-06T19:25:43.600","2016-04-07T07:25:43.600","CA","sonar","knudsen","phase range","2500-3500m"]
["2016-04-06T19:32:50.150","2016-04-07T07:32:50.150","CA","sonar","multibeam","Ping Mode","Deep, Max Angles 60/60"]
["2016-04-06T19:38:56.100","2016-04-07T07:38:56.100","AB","sonar","knudsen","phase range","2000-3000m, Power 2, Pulse 4"]
["2016-04-06T20:00:32.120","2016-04-07T08:00:32.120","AB","sonar","multibeam","Max Angle","65/75"]
["2016-04-06T20:01:12.830","2016-04-07T08:01:12.830","AB","sonar","knudsen","Tx Power","1, Pulse 1, Gain 35dB"]
["2016-04-06T20:09:28.600","2016-04-07T08:09:28.600","AB","sonar","multibeam","Max Angle","75/75"]
["2016-04-06T20:42:55.270","2016-04-07T08:42:55.270","wp","other",null,null,"Watch Change"]
["2016-04-06T21:55:35.170","2016-04-07T09:55:35.170","MP","XBT",null,null,"#62 abnormal profile, deleted  (first attempt failed at 158m)"]
["2016-04-06T21:59:36.210","2016-04-07T09:59:36.210","MP","sonar","knudsen","Tx Power","3, pulse 16, gain value 34dB, phase range 1500-2500"]
["2016-04-06T22:08:20.770","2016-04-07T10:08:20.770","MP","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-06T22:08:42.170","2016-04-07T10:08:42.170","MP","XBT",null,null,"#62 retaken, profile useable"]
["2016-04-06T22:12:00.340","2016-04-07T10:12:00.340","CR","XBT",null,null,"#62 XBT Profile applied to line 524"]
["2016-04-06T22:20:32.410","2016-04-07T10:20:32.410","MP","Sonar","knudsen","Phase Range","2500-3500, gain value 31dB"]
["2016-04-06T22:29:21.160","2016-04-07T10:29:21.160","MP","sonar","knudsen","Tx Pulse","16, gain value 36dB"]
["2016-04-06T22:46:29.910","2016-04-07T10:46:29.910","WP","sonar","knudsen","Tx Pulse","Pulse 4.0, Power 2, gain 32, range 2000-3000 (depth 2500 m+/-)"]
["2016-04-06T23:00:09.760","2016-04-07T11:00:09.760","WP","sonar","knudsen","phase range","1000-2000"]
["2016-04-06T23:10:30.740","2016-04-07T11:10:30.740","MP","sonar","knudsen","Tx Pulse","16, gain value 31dB"]
["2016-04-06T23:18:02.850","2016-04-07T11:18:02.850","MP","sonar","knudsen","Phase Range","1500-2500, gain value 36dB"]
["2016-04-06T23:27:44.320","2016-04-07T11:27:44.320","MP","sonar","knudsen","Tx Power",3]
["2016-04-06T23:58:25.070","2016-04-07T11:58:25.070","MP","sonar","knudsen","Phase Range","4000-5000"]
["2016-04-07T00:00:58.070","2016-04-07T12:00:58.070","WP","sonar","knudsen","Tx Pulse","Pulse 32.0, Power 3, gain 34, Phase 4000-5000"]
["2016-04-07T00:19:16.730","2016-04-07T12:19:16.730","MP","sonar","knudsen","Gain Value","40dB"]
["2016-04-07T00:24:14.350","2016-04-07T12:24:14.350","MP","Sonar","knudsen","Gain Value","36dB"]
["2016-04-07T00:32:38.270","2016-04-07T12:32:38.270","MP","Sonar","Knudsen","Phase Range","3500-4500, gain 41dB"]
["2016-04-07T00:37:51.820","2016-04-07T12:37:51.820","MP","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-07T00:43:40.550","2016-04-07T12:43:40.550","MP","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-07T00:50:13.710","2016-04-07T12:50:13.710","MP","Sonar","knudsen","Phase Range","2000-3000"]
["2016-04-07T00:57:56.080","2016-04-07T12:57:56.080","WP","Sonar","knudsen","phase range","1500-2500, pulse 4.0, power 3, gain 31"]
["2016-04-07T01:04:28","2016-04-07T13:04:28","WP","sonar","knudsen","phase range","1000-2000"]
["2016-04-07T01:09:15.810","2016-04-07T13:09:15.810","WP","Sonar","knudsen","Tx Power","2, pulse 2.0, gain 26"]
["2016-04-07T01:21:53.690","2016-04-07T13:21:53.690","WP","sonar","knudsen","phase range","1500-2500, Pulse 16.0, Power 3.0, Gain 31"]
["2016-04-07T01:25:54.390","2016-04-07T13:25:54.390","WP","Sonar","Knudsen","phase range","2000-3000, Tx Pulse 32, Power 3, Gain 41"]
["2016-04-07T01:35:10.380","2016-04-07T13:35:10.380","WP","sonar","knudsen","phase range","3000-4000"]
["2016-04-07T01:44:37.920","2016-04-07T13:44:37.920","DS","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-07T01:53:14.290","2016-04-07T13:53:14.290","WP","Sonar","knudsen","phase range","4000-5000"]
["2016-04-07T02:00:54.590","2016-04-07T14:00:54.590","WP","Sonar","knudsen","phase range","4500-5500"]
["2016-04-07T02:17:18.270","2016-04-07T14:17:18.270","WP","Sonar","Multibeam","New Line"," begin turn, new line 0529"]
["2016-04-07T02:26:07.740","2016-04-07T14:26:07.740","MP","Sonar","Multibeam","New Line","begin new survey line 0530"]
["2016-04-07T02:42:02.300","2016-04-07T14:42:02.300","MP","Sonar","knudsen","Gain Value","35dB"]
["2016-04-07T03:28:22.070","2016-04-07T15:28:22.070","MP","sonar","knudsen","Gain Value","33dB"]
["2016-04-07T03:41:10.950","2016-04-07T15:41:10.950","WP","Sonar","Knudsen","Tx Pulse","8.0, Power 3, gain 31, phase range 4500-5500"]
["2016-04-07T03:55:48.660","2016-04-07T15:55:48.660","CR","XBT",null,null,"XBT #63 applied to line 531"]
["2016-04-07T04:36:16.930","2016-04-07T16:36:16.930","DF","watch change",null,null,"Dan and Breezy on watch"]
["2016-04-07T04:51:27.830","2016-04-07T16:51:27.830","DF","sonar","knudsen",null,"tx pulse to 16, gain to 34"]
["2016-04-07T08:39:43.510","2016-04-07T20:39:43.510","SM","sonar","knudsen","phase range","4000-5000"]
["2016-04-07T09:09:21.910","2016-04-07T21:09:21.910","DF","sonar","knudsen","phase range","3500-4500"]
["2016-04-07T09:12:39.320","2016-04-07T21:12:39.320","DF","sonar","knudsen","phase range","3000-4000"]
["2016-04-07T09:19:40.010","2016-04-07T21:19:40.010","DF","sonar","knudsen","Tx Pulse",8]
["2016-04-07T09:23:20.550","2016-04-07T21:23:20.550","BG","sonar","knudsen","phase range","2500-3500"]
["2016-04-07T09:38:38.400","2016-04-07T21:38:38.400","BG","sonar","knudsen","phase range","2000-3000"]
["2016-04-07T09:50:27.830","2016-04-07T21:50:27.830","DF","sonar","multibeam","Max Angle","60/62"]
["2016-04-07T10:12:16.360","2016-04-07T22:12:16.360","BG","sonar","knudsen","phase range","1500-2500"]
["2016-04-07T10:17:45.420","2016-04-07T22:17:45.420","BG","sonar","knudsen","phase range","1000-2000"]
["2016-04-07T10:21:31.580","2016-04-07T22:21:31.580",null,"xbt",null,null,"conducted XBT 064, 3rd launch was successful, first canceled at 400m, second canceled at 200m"]
["2016-04-07T10:25:34.580","2016-04-07T22:25:34.580","DF","sonar","multibeam","Max Angle","70/70"]
["2016-04-07T10:28:22.920","2016-04-07T22:28:22.920","BG","xbt",null,null,"applied xbt 064 to line 0538"]
["2016-04-07T10:29:43.160","2016-04-07T22:29:43.160","BG","sonar","knudsen","Tx Power",2]
["2016-04-07T10:33:20.730","2016-04-07T22:33:20.730","DF","sonar","knudsen",null,"tx power to 1, tx pulse to 2 ms"]
["2016-04-07T11:00:00",{"$f":"IF(ISBLANK(A1985),\" \",((A1985)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-04-07T22:00:00"},"DF","Ship",null,null,"Time change minus 1 hr"]
["2016-04-07T11:04:05",{"$f":"IF(ISBLANK(A1986),\" \",((A1986)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-04-07T22:04:05"},"DF","sonar","Multibeam","Max Angle","75/75"]
["2016-04-07T11:51:46","2016-04-07T22:51:46","DF","sonar","knudsen","Phase Range","2000-3000"]
["2016-04-07T12:01:03","2016-04-07T23:01:03","DF","Sonar","knudsen","tx pulse","4 ms"]
["2016-04-07T12:01:29","2016-04-07T23:01:29","DF","Sonar","knudsen","Gain Value","36 dB"]
["2016-04-07T12:05:24.070","2016-04-07T23:05:24.070","BG","Sonar","knudsen","Phase Range","2500-3500"]
["2016-04-07T12:14:31.230","2016-04-07T23:14:31.230","BG","sonar","knudsen","phase range","3000-4000"]
["2016-04-07T12:40:55.900","2016-04-07T23:40:55.900","AB","sonar","Multibeam","New Line","0542"]
["2016-04-07T12:42:18.700","2016-04-07T23:42:18.700","AB","sonar","knudsen","phase range","4000-5000m, Power 3, Pulse 8, Gain 36dB"]
["2016-04-07T13:03:06.840","2016-04-08T00:03:06.840","CA","sonar","knudsen","Phase Range","4500-5500m"]
["2016-04-07T13:04:54.910","2016-04-08T00:04:54.910","AB","sonar","knudsen","Tx Pulse",16]
["2016-04-07T13:18:10.660","2016-04-08T00:18:10.660","AB","sonar","knudsen","Phase Range","5000-6000m"]
["2016-04-07T13:28:35.360","2016-04-08T00:28:35.360","AB","sonar","knudsen","Gain Value","40dB"]
["2016-04-07T14:43:14.180","2016-04-08T01:43:14.180","AB","sonar","Multibeam","New Line","0545 - turn"]
["2016-04-07T14:46:14.900","2016-04-08T01:46:14.900","AB","sonar","Multibeam","New Line","0546"]
["2016-04-07T14:54:54.970","2016-04-08T01:54:54.970","AB","Sonar","knudsen","Phase Range","4500-5500m"]
["2016-04-07T15:00:07","2016-04-08T02:00:07","AB","XBT",null,null,"#65"]
["2016-04-07T15:03:20.380","2016-04-08T02:03:20.380","AB","XBT",null,null,"Applied #65 to new line 0547"]
["2016-04-07T15:09:04.520","2016-04-08T02:09:04.520","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max angles 52/52"]
["2016-04-07T15:12:29.580","2016-04-08T02:12:29.580","AB","Sonar","knudsen","Phase Range","4000-5000m"]
["2016-04-07T15:23:40.320","2016-04-08T02:23:40.320","AB","Sonar","knudsen","phase range","3500-4500m "]
["2016-04-07T15:32:55.850","2016-04-08T02:32:55.850","AB","sonar","knudsen","phase range","3000-4000m"]
["2016-04-07T15:36:45.790","2016-04-08T02:36:45.790","AB","Sonar","knudsen","phase range","2500-3500m"]
["2016-04-07T15:37:21.170","2016-04-08T02:37:21.170","AB","sonar","Multibeam","Ping Mode","Deep, Max Angles 60/60"]
["2016-04-07T15:40:23.680","2016-04-08T02:40:23.680","AB","Sonar","Knudsen","phase range","2000-3000m"]
["2016-04-07T15:46:14.210","2016-04-08T02:46:14.210","AB","sonar","knudsen","phase range","1500-2500m, Power 2, Pulse 4"]
["2016-04-07T15:49:33.210","2016-04-08T02:49:33.210","AB","Sonar","Knudsen","Phase Range","1000-2000m, Power 1, Pulse 2"]
["2016-04-07T15:53:01.140","2016-04-08T02:53:01.140","AB","Sonar","Multibeam","Max Angle","75/75"]
["2016-04-07T15:58:01.420","2016-04-08T02:58:01.420","AB","Sonar","knudsen","phase range","500-1500m"]
["2016-04-07T16:00:58.100","2016-04-08T03:00:58.100","AB","Sonar","knudsen","phase range","1000-2000m"]
["2016-04-07T16:03:36.960","2016-04-08T03:03:36.960","AB","Sonar","knudsen","Tx Power","2, Pulse 2, Gain 36dB"]
["2016-04-07T16:06:06.430","2016-04-08T03:06:06.430","AB","Sonar","knudsen","phase range","1500-2500m, Power 2, Pulse"]
["2016-04-07T16:07:46.580","2016-04-08T03:07:46.580","AB","sonar","knudsen","phase range","2000-3000m"]
["2016-04-07T16:11:43.860","2016-04-08T03:11:43.860","AB","Sonar","Knudsen","phase range","2500-3500m, Power 3, Pulse 8"]
["2016-04-07T16:15:50.410","2016-04-08T03:15:50.410","AB","sonar","knudsen","phase range","3000-4000m"]
["2016-04-07T16:20:06.340","2016-04-08T03:20:06.340","AB","sonar","knudsen","phase range","3500-4500m "]
["2016-04-07T16:27:19.490","2016-04-08T03:27:19.490","AB","sonar","knudsen","phase range","4000-5000m"]
["2016-04-07T16:46:43.910","2016-04-08T03:46:43.910","CA","sonar","knudsen","phase range","4500-5500m"]
["2016-04-07T18:09:17.200","2016-04-08T05:09:17.200","AB","sonar","knudsen","phase range","4000-5000m"]
["2016-04-07T18:09:50.720","2016-04-08T05:09:50.720","AB","sonar","multibeam","Ping Mode","Very Deep, Max angles 52/52"]
["2016-04-07T18:17:34.820","2016-04-08T05:17:34.820","AB","sonar","knudsen","phase range","3500-4500m "]
["2016-04-07T18:20:03.190","2016-04-08T05:20:03.190","AB","sonar","knudsen","phase range","3000-4000m"]
["2016-04-07T18:40:01.530","2016-04-08T05:40:01.530","AB","sonar","knudsen","phase range","4000-5000m"]
["2016-04-07T18:45:50.600","2016-04-08T05:45:50.600","AB","sonar","multibeam","Ping Mode","Auto: Extra Deep 35/35"]
["2016-04-07T18:55:58.770","2016-04-08T05:55:58.770","AB","sonar","knudsen","phase range","5000-6000m"]
["2016-04-07T20:23:57.020","2016-04-08T07:23:57.020","MP","Sonar","Multibeam","New Line","Begin turn, new line 0553"]
["2016-04-07T20:30:25.870","2016-04-08T07:30:25.870","MP","sonar","multibeam","New Line","Begin survey line 0554"]
["2016-04-07T20:30:57.490","2016-04-08T07:30:57.490","MP","Watch Change"]
["2016-04-07T21:05:20.650","2016-04-08T08:05:20.650","MP","XBT",null,null,"#66, cast ended early at 490m but still using profile"]
["2016-04-07T21:07:24.170","2016-04-08T08:07:24.170","WP","XBT",null,null,"XBT Cast 066 applied to line 0554"]
["2016-04-07T23:03:44.990","2016-04-08T10:03:44.990","WP","sonar","knudsen","Phase Range","4500-5500"]
["2016-04-07T23:33:47.800","2016-04-08T10:33:47.800","CR","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-07T23:41:13.300","2016-04-08T10:41:13.300","CR","sonar","knudsen","tx pulse","32; gain value 43"]
["2016-04-07T23:46:06.690","2016-04-08T10:46:06.690","CR","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-07T23:53:27.180","2016-04-08T10:53:27.180","wp","sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-08T00:08:18.570","2016-04-08T11:08:18.570","wp","sonar","knudsen","tx pulse","8.0, tx power 3, gain 34"]
["2016-04-08T00:09:32.840","2016-04-08T11:09:32.840","wp","sonar ","knudsen","phase range","2000-3000"]
["2016-04-08T00:18:59.490","2016-04-08T11:18:59.490","wp","sonar","knudsen","phase range","1500-2500, pulse 4.0, power 2.0, gain 31."]
["2016-04-08T00:29:24.580","2016-04-08T11:29:24.580","MP","Sonar","knudsen","Phase Range","1000-2000"]
["2016-04-08T00:34:10.830","2016-04-08T11:34:10.830","MP","Sonar","knudsen","Gain Value","28dB, power 2"]
["2016-04-08T01:00:49.380","2016-04-08T12:00:49.380","MP","Sonar","knudsen","Phase Range","1500-2500, pulse 16, power 3"]
["2016-04-08T01:01:54.520","2016-04-08T12:01:54.520","MP","Ship",null,null,"Resumes 8.7 knots"]
["2016-04-08T01:09:31.010","2016-04-08T12:09:31.010","wp","sonar","knudsen","phase range","2000-3000, gain to 34"]
["2016-04-08T01:14:47.320","2016-04-08T12:14:47.320","wp","sonar","knudsen","Phase Range","2500-3500"]
["2016-04-08T01:32:05.100","2016-04-08T12:32:05.100","WP","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-08T01:35:59.830",{"$f":"IF(ISBLANK(A2050),\" \",((A2050)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-04-08T12:35:59.830"},"WP","Sonar","knudsen","Tx Pulse","32, Power 3, Gain 41, Phase Range 3500-4500"]
["2016-04-08T02:00:09.610","2016-04-08T13:00:09.610","WP","Sonar","knudsen","Phase Range","4500-5000"]
["2016-04-08T02:13:49.120","2016-04-08T13:13:49.120","DS","Sonar","Knudsen","Tx Pulse","pulse 64, gain 48, power 3"]
["2016-04-08T02:47:16.190","2016-04-08T13:47:16.190","MP","Sonar","knudsen","Phase Range","5000-6000"]
["2016-04-08T03:16:24.740","2016-04-08T14:16:24.740","MP","XBT",null,null,"#67 taken"]
["2016-04-08T03:18:05.250","2016-04-08T14:18:05.250","MP","XBT",null,null,"#67 applied to line 0560"]
["2016-04-08T03:41:30.150","2016-04-08T14:41:30.150","WP","sonar","Knudsen","phase range","5000-6000, tx pulse 16, power 3, gain 37."]
["2016-04-08T04:16:40.710","2016-04-08T15:16:40.710","CR","sonar","Multibeam","new line","new line 0562, turn begin"]
["2016-04-08T04:21:11.640","2016-04-08T15:21:11.640","CR","sonar","Multibeam","new line","new line 053, turn end"]
["2016-04-08T04:32:00.940","2016-04-08T15:32:00.940","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-04-08T05:01:40.010","2016-04-08T16:01:40.010","DS","Sonar",null,null,"turned on ADCP wh300 "]
["2016-04-08T05:03:44.040","2016-04-08T16:03:44.040","DF","Sonar","Multibeam","Max Angle","70/25"]
["2016-04-08T05:05:37.610","2016-04-08T16:05:37.610","DF","Sonar","Multibeam","Max Angle","70/70"]
["2016-04-08T05:06:36.920","2016-04-08T16:06:36.920","DS","Sonar","ADCP",null,"secured adcp, causing artifact in mb wcd in stbd outter sector"]
["2016-04-08T05:41:25.710","2016-04-08T16:41:25.710","DF","Sonar","multibeam","Aeration Filter (On/Off)","on"]
["2016-04-08T05:45:41.180","2016-04-08T16:45:41.180","DF","Sonar","knudsen","Gain Value",44]
["2016-04-08T05:46:58.550","2016-04-08T16:46:58.550","DF","Sonar","multibeam","Spike Filter Strength","strong"]
["2016-04-08T06:28:53.340","2016-04-08T17:28:53.340","DS","Sonar","Multibeam","Aeration Filter (On/Off)","tried off. Seemed to worsen deep artefacts, turned it on"]
["2016-04-08T06:36:54.120","2016-04-08T17:36:54.120","DS","Sonar","Multibeam","Max Angle","22/22 to clean up the swath edges, avoid occasional artefacts"]
["2016-04-08T06:49:12.730","2016-04-08T17:49:12.730","DF","Sonar","multibeam","Along Direction Pitch",1.5]
["2016-04-08T06:52:07.470","2016-04-08T17:52:07.470","DF","Sonar","multibeam","Along Direction Pitch",2]
["2016-04-08T09:12:38.310","2016-04-08T20:12:38.310","DF","xbt",null,null,"cast 068 collected"]
["2016-04-08T09:17:32.390","2016-04-08T20:17:32.390","DF","xbt",null,null,"cast 068 applied to line 0568"]
["2016-04-08T09:26:38.560","2016-04-08T20:26:38.560","DF","Sonar","knudsen","tx pulse",16]
["2016-04-08T10:27:20.520","2016-04-08T21:27:20.520","DF","Sonar","multibeam","Along Direction Pitch",1.5]
["2016-04-08T11:58:14.760","2016-04-08T22:58:14.760","DF","sonar","multibeam","Along Direction Pitch",1]
["2016-04-08T12:30:13","2016-04-08T23:30:13","AB","Watch Change",null,null,"Watch Change"]
["2016-04-08T15:09:41.770","2016-04-09T02:09:41.770","AB","XBT",null,null,"#65"]
["2016-04-08T15:15:40.840","2016-04-09T02:15:40.840","AB","XBT",null,null,"#65 applied to new line 0575"]
["2016-04-08T15:15:49","2016-04-09T02:15:49","AB","Sonar","Multibeam","New Line","0575"]
["2016-04-08T16:15:42","2016-04-09T03:15:42","AB","Sonar","Multibeam","New Line","0576"]
["2016-04-08T17:15:38","2016-04-09T04:15:38","AB","Sonar","multibeam","New Line","0577"]
["2016-04-08T18:03:51.450","2016-04-09T05:03:51.450","AB","Sonar","Multibeam","new line","0578 - turn"]
["2016-04-08T18:05:59.160","2016-04-09T05:05:59.160","AB","Sonar","Multibeam","new line","0579"]
["2016-04-08T19:06:25","2016-04-09T06:06:25","AB","Sonar","Multibeam","new line","0580"]
["2016-04-08T20:06:53.570","2016-04-09T07:06:53.570","AB","Sonar","Multibeam","new line","0581"]
["2016-04-08T20:19:38.380","2016-04-09T07:19:38.380","AB","Sonar","Multibeam","Max Angle","35/30"]
["2016-04-08T21:00:53.990","2016-04-09T08:00:53.990","CR","sonar","knudsen","phase range","3500-4500; pulse 32; gain value 48"]
["2016-04-08T21:22:43.760","2016-04-09T08:22:43.760","MP","Sona","knudsen","Phase Range","3000-4000"]
["2016-04-08T21:23:18.290","2016-04-09T08:23:18.290","MP","XBT",null,null,"#70"]
["2016-04-08T21:23:31.570","2016-04-09T08:23:31.570","MP","XBT",null,null,"#70 applied to line 0582"]
["2016-04-08T21:40:29.590","2016-04-09T08:40:29.590","CR","sonar","knudsen","phase range","3500-4500"]
["2016-04-08T21:47:56.220","2016-04-09T08:47:56.220","wp","sonar","knudsen","phase range","4400-5000, Pulse 16, Power 3, gain 38"]
["2016-04-08T22:01:56.140","2016-04-09T09:01:56.140","MP","Sonar","Knudsen","Tx Pulse",32]
["2016-04-08T22:08:57.580","2016-04-09T09:08:57.580","MP","Sonar","Knudsen","Gain Value","46dB, 4500-5500"]
["2016-04-08T22:15:13.860","2016-04-09T09:15:13.860","MP","Sonar","Knudsen","Phase Range","5000-6000"]
["2016-04-08T22:37:46.590","2016-04-09T09:37:46.590","MP","Sonar","Knudsen","Tx Pulse","16, gain value 36dB"]
["2016-04-08T23:15:36.260","2016-04-09T10:15:36.260","MP","Sonar","Knudsen","Tx Pulse","32, gain value 38dB"]
["2016-04-08T23:32:26.550","2016-04-09T10:32:26.550","wp","Sonar","knudsen","Gain Value",38]
["2016-04-09T00:15:37.500","2016-04-09T11:15:37.500","wp","sonar","Multibeam","new line","begin turn, new line 0586"]
["2016-04-09T00:19:36.850","2016-04-09T11:19:36.850","wp","sonar","multibeam","new line","begin survey line, new line 0587"]
["2016-04-09T01:33:13.440","2016-04-09T12:33:13.440","MP","Sonar","knudsen","Gain Value","40dB"]
["2016-04-09T03:03:47.860","2016-04-09T14:03:47.860","CR","xBT",null,null,"#71 applied to line 589"]
["2016-04-09T03:55:36.950","2016-04-09T14:55:36.950","CR","sonar","multibeam","new line","begin turn, new line 591"]
["2016-04-09T04:02:23.190","2016-04-09T15:02:23.190","CR","sonar","multibeam","new line","end turn, new line 592"]
["2016-04-09T04:30:00","2016-04-09T15:30:00","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-04-09T05:14:31.560","2016-04-09T16:14:31.560","DS","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-04-09T06:13:32.440","2016-04-09T17:13:32.440","DF","Sonar","knudsen","phase range","4000-5000"]
["2016-04-09T06:14:37.940","2016-04-09T17:14:37.940","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-04-09T06:34:33.710","2016-04-09T17:34:33.710","DF","Sonar","knudsen","phase range","3500-4500"]
["2016-04-09T06:38:40.710","2016-04-09T17:38:40.710","BG","sonar","knudsen","phase range","3000-4000"]
["2016-04-09T06:48:59.450","2016-04-09T17:48:59.450","BG","sonar","knudsen","phase range","2500-3500"]
["2016-04-09T06:56:58.860","2016-04-09T17:56:58.860","BG","sonar","knudsen","phase range","2000-3000"]
["2016-04-09T07:03:35.820","2016-04-09T18:03:35.820","BG","sonar","knudsen","phase range","1500-2500"]
["2016-04-09T07:07:38.440","2016-04-09T18:07:38.440","BG","sonar","knudsen","phase range","1000-2000"]
["2016-04-09T07:08:02.120",{"$f":"IF(ISBLANK(A2115),\" \",((A2115)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-04-09T18:08:02.120"},"BG","sonar","knudsen","Tx Power",2]
["2016-04-09T07:09:06.590","2016-04-09T18:09:06.590","DF","sonar","knudsen","tx pulse",4]
["2016-04-09T07:10:12.640","2016-04-09T18:10:12.640","DF","sonar","Multibeam","Spike Filter Strength","medium"]
["2016-04-09T07:58:50.820","2016-04-09T18:58:50.820","DF","sonar","knudsen","Gain Value",34]
["2016-04-09T08:17:25.210","2016-04-09T19:17:25.210","BG","sonar","knudsen","Gain Value",30]
["2016-04-09T08:21:05.010","2016-04-09T19:21:05.010","BG","Sonar","knudsen","Gain Value",33]
["2016-04-09T09:29:52.840","2016-04-09T20:29:52.840","SM","Sonar","knudsen","phase range","1500-2500"]
["2016-04-09T09:39:27.650","2016-04-09T20:39:27.650","SM","XBT",null,null,"Cast 072"]
["2016-04-09T09:39:52.030","2016-04-09T20:39:52.030","SM","XBT",null,null,"Cast 072 applied to line 0597"]
["2016-04-09T09:45:18.310","2016-04-09T20:45:18.310","BG","sonar","knudsen","Tx Power",2]
["2016-04-09T10:14:58.560","2016-04-09T21:14:58.560","BG","sonar","knudsen","phase range","2000-3000"]
["2016-04-09T10:25:10.550","2016-04-09T21:25:10.550","BG","sonar","knudsen","phase range","2500-3500"]
["2016-04-09T10:56:28.410","2016-04-09T21:56:28.410","BG","sonar","knudsen","phase range","3000-4000"]
["2016-04-09T11:00:33.560","2016-04-09T22:00:33.560","BG","sonar","knudsen","Tx Power",3]
["2016-04-09T11:01:12.090","2016-04-09T22:01:12.090","BG","sonar","knudsen","phase range","3500-4500"]
["2016-04-09T11:07:19.460","2016-04-09T22:07:19.460","BG","sonar","knudsen",null,"phase range 4000-5000, tx pulse 4 ms"]
["2016-04-09T11:30:09.020","2016-04-09T22:30:09.020","BG","sonar","knudsen","phase range","4500-5500"]
["2016-04-09T11:52:02.770","2016-04-09T22:52:02.770","BG","sonar","knudsen","phase range","5000-6000"]
["2016-04-09T12:09:30.740","2016-04-09T23:09:30.740","DF","sonar","knudsen",null,"tx pulse to 16, gain to 38"]
["2016-04-09T12:33:46.610","2016-04-09T23:33:46.610","AB",null,null,null,"Watch Change"]
["2016-04-09T12:58:24.710","2016-04-09T23:58:24.710","AB","Sonar","knudsen","Gain Value","40dB"]
["2016-04-09T13:02:44","2016-04-10T00:02:44","AB","Sonar","Multibeam","new line","0600"]
["2016-04-09T14:02:59","2016-04-10T01:02:59","AB","Sonar","Multibeam","new line","0602"]
["2016-04-09T14:33:32.710","2016-04-10T01:33:32.710","AB","Sonar","knudsen","Gain Value","36dB"]
["2016-04-09T15:04:10.710","2016-04-10T02:04:10.710","AB","XBT",null,null,"#73"]
["2016-04-09T15:07:02.770","2016-04-10T02:07:02.770","AB","Sonar","knudsen","Gain Value","35dB"]
["2016-04-09T15:11:21.860","2016-04-10T02:11:21.860","AB","XBT",null,null,"#73 applied to new line 0604"]
["2016-04-09T18:11:15","2016-04-10T05:11:15","AB","Sonar","Multibeam","new line","0607"]
["2016-04-09T20:37:06.250","2016-04-10T07:37:06.250","wp"," other",null,null,"Watch Change"]
["2016-04-09T20:37:55.470","2016-04-10T07:37:55.470","wp","sonar","Knudsen","Phase Range","5000-6000, tx pulse 16, power 3, gain 38."]
["2016-04-09T21:11:06.070","2016-04-10T08:11:06.070","wp","xbt",null,null,"xbt cast 074 applied to line #0610"]
["2016-04-09T23:05:40.730","2016-04-10T10:05:40.730","cr","sonar","Knudsen","Tx Pulse",32]
["2016-04-09T23:10:34.240","2016-04-10T10:10:34.240","cr","sonar","Knudsen","gain Value",40]
["2016-04-09T23:28:24.450","2016-04-10T10:28:24.450","MP","Sonar","knudsen","Phase Range","4500-5500"]
["2016-04-09T23:39:47.900","2016-04-10T10:39:47.900","wp","sonar","knudsen","Phase Range","4000-5000, pulse 16, power 3, gain 38."]
["2016-04-09T23:42:57.790","2016-04-10T10:42:57.790","wp","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-09T23:50:59.920","2016-04-10T10:50:59.920","cr","sonar","Knudsen","gain Value",34]
["2016-04-10T00:00:19.250","2016-04-10T11:00:19.250","cr","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-10T00:10:35.510","2016-04-10T11:10:35.510","wp","sonar","Knudsen","Phase Range","2500-3500, tx pulse 8, power 3, gain 31."]
["2016-04-10T00:20:47.190","2016-04-10T11:20:47.190","wp","sonar","Knudsen","phase range","2000-3000"]
["2016-04-10T00:24:21.160","2016-04-10T11:24:21.160","MP","Sonar","Knudsen","Phase Range","1500-2500, pulse 32"]
["2016-04-10T00:29:08.440","2016-04-10T11:29:08.440","MP","Sonar","Knudsen","Phase Range","1000-2000"]
["2016-04-10T00:40:09.960","2016-04-10T11:40:09.960","CR","Sonar","knudsen","Tx Pulse","8, power 2, gain valuwe 31dB"]
["2016-04-10T00:44:16.310","2016-04-10T11:44:16.310","CR","Sonar","Knudsen","Tx Power","1, gain value 28dB"]
["2016-04-10T01:01:29.690","2016-04-10T12:01:29.690","MP","Sonar","Knudsen","Tx Power","3; Pulse 16; Range 1500-2500"]
["2016-04-10T01:06:13.980","2016-04-10T12:06:13.980","CR","Sonar","Knudsen","phase range","2000-3000"]
["2016-04-10T01:06:37.070","2016-04-10T12:06:37.070","CR","Sonar","Knudsen","gain value","36dB"]
["2016-04-10T01:09:50.470","2016-04-10T12:09:50.470","CR","Sonar","Knudsen","phase range","2500-3500"]
["2016-04-10T01:25:32.060","2016-04-10T12:25:32.060","MP","Sonar","Knudsen","Phase Range","3500-4500, gain vaule 41dB"]
["2016-04-10T01:53:29.470","2016-04-10T12:53:29.470","MP","Sonar","knudsen","Gain Value","38dB"]
["2016-04-10T01:55:22.890","2016-04-10T12:55:22.890","MP","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-04-10T02:21:10.130","2016-04-10T13:21:10.130","CR","Sonar","Knudsen","Phase Range","5000-6000"]
["2016-04-10T02:21:32.400","2016-04-10T13:21:32.400","MP","Sonar","Knudsen","Gain Value",41]
["2016-04-10T02:44:11.440","2016-04-10T13:44:11.440","CR","Sonar","Knudsen","Phase Range","5500-6500"]
["2016-04-10T03:24:28.870","2016-04-10T14:24:28.870","CR","XBT",null,null,"cast 75 applied to Line 616"]
["2016-04-10T03:26:25.260","2016-04-10T14:26:25.260","CR","Sonar","Multibeam","New Line","begin turn, line 06178"]
["2016-04-10T03:36:35.990","2016-04-10T14:36:35.990","MP","Sonar","Multibeam","New Line","new survey line 0618"]
["2016-04-10T03:49:55.960","2016-04-10T14:49:55.960","CR","Sonar","Knudsen","Gain value",37]
["2016-04-10T04:28:18.050","2016-04-10T15:28:18.050","DF","Sonar","Multibeam",null,"Aeration filter on, spike filter strength to strong, max angles 22/18"]
["2016-04-10T04:30:24.340","2016-04-10T15:30:24.340","MP","Sonar","Multibeam",null,"Needle-gunning line 0618"]
["2016-04-10T04:34:37","2016-04-10T15:34:37","DF","sonar","knudsen","Gain Value","40 dB"]
["2016-04-10T04:52:36.440","2016-04-10T15:52:36.440","DF","sonar","Multibeam","Max Angle","30/30"]
["2016-04-10T04:53:51.050",{"$f":"IF(ISBLANK(A2177),\" \",((A2177)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-04-10T15:53:51.050"},"DF","Sonar","Multibeam","Max Angle","26/26"]
["2016-04-10T06:10:02.640","2016-04-10T17:10:02.640","DF","Sonar","Multibeam","Spike Filter Strength","medium"]
["2016-04-10T07:28:09.040",{"$f":"IF(ISBLANK(A2179),\" \",((A2179)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-04-10T18:28:09.040"},"DF","sonar","Multibeam","Max Angle","35/35"]
["2016-04-10T07:35:26.890","2016-04-10T18:35:26.890","DF","sonar","Multibeam","Max Angle","33/33"]
["2016-04-10T09:09:27.430","2016-04-10T20:09:27.430","BG","xbt",null,null,"xbt 075 collected"]
["2016-04-10T09:10:23.500","2016-04-10T20:10:23.500","BG","xbt",null,null,"xbt 075 applied to line 0623"]
["2016-04-10T10:40:53.700","2016-04-10T21:40:53.700","DF","ship",null,null,"requested a increase in speede 8.5-9 knots"]
["2016-04-10T12:31:25","2016-04-10T23:31:25","AB",null,null,null,"Watch Change"]
["2016-04-10T12:43:28.770","2016-04-10T23:43:28.770","AB","Sonar","knudsen","Phase Range","5000-6000m"]
["2016-04-10T13:37:15","2016-04-11T00:37:15","AB","Sonar","Multibeam","new line","0628"]
["2016-04-10T14:37:23","2016-04-11T01:37:23","AB","Sonar","Multibeam","new line","0629"]
["2016-04-10T14:52:50.780","2016-04-11T01:52:50.780","AB","Sonar","Multibeam","new line","0630 - turn"]
["2016-04-10T14:57:40.030","2016-04-11T01:57:40.030","AB","Sonar","Multibeam","new line","0631"]
["2016-04-10T14:59:18.770",{"$f":"IF(ISBLANK(A2190),\" \",((A2190)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-04-11T00:59:18.770"},"AB","Ship",null,null,"Time change minus 1 hr"]
["2016-04-10T15:05:56.240",{"$f":"IF(ISBLANK(A2191),\" \",((A2191)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-04-11T01:05:56.240"},"AB","XBT",null,null,"#77"]
["2016-04-10T15:11:23.790","2016-04-11T01:11:23.790","AB","XBT",null,null," #77 applied to new line 0632"]
["2016-04-10T15:47:23.700","2016-04-11T01:47:23.700","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2016-04-10T15:51:08.130","2016-04-11T01:51:08.130","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max angles 52/52"]
["2016-04-10T15:52:24.130","2016-04-11T01:52:24.130","AB","Sonar","Knudsen","Phase Range","4000-5000m, Gain 40dB"]
["2016-04-10T15:57:50.430","2016-04-11T01:57:50.430","AB","Sonar","Knudsen","Phase Range","3500-4500m "]
["2016-04-10T16:02:38.750","2016-04-11T02:02:38.750","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-04-10T16:07:23","2016-04-11T02:07:23","AB","Sonar","knudsen","Phase Range","2500-3500m"]
["2016-04-10T16:22:33.040","2016-04-11T02:22:33.040","AB","Sonar","Multibeam","Ping Mode","Deep, Max Angles 50/65"]
["2016-04-10T16:24:38.230","2016-04-11T02:24:38.230","AB","Sonar","knudsen","Phase Range","2000-3000m"]
["2016-04-10T17:06:50.200","2016-04-11T03:06:50.200","AB","Sonar","Multibeam","Along Direction Pitch","-2, Ping Mode Auto"]
["2016-04-10T17:07:09.510","2016-04-11T03:07:09.510","AB","Sonar","Knudsen","Phase Range","3000-4000m, Power 3, Pulse 8, Gain 38dB"]
["2016-04-10T17:11:28.290","2016-04-11T03:11:28.290","AB","Sonar","Multibeam","New Line","0634"]
["2016-04-10T17:14:33.760","2016-04-11T03:14:33.760","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max angles 52/52"]
["2016-04-10T17:20:21.090","2016-04-11T03:20:21.090","AB","Sonar","Knudsen","Phase Range","2500-3500m, Pulse 16"]
["2016-04-10T17:26:38.810","2016-04-11T03:26:38.810","AB","Sonar","Knudsen","Phase Range","3500-4500m , Gain 38dB"]
["2016-04-10T17:37:33.500","2016-04-11T03:37:33.500","AB","Sonar","knudsen","phase range","4000-5000m"]
["2016-04-10T17:46:54.570","2016-04-11T03:46:54.570","AB","Sonar","Knudsen","phase range","4500-5500m"]
["2016-04-10T17:53:37.660","2016-04-11T03:53:37.660","AB","Sonar","Multibeam","Ping Mode","Extra Deep, Along direction 0 degrees"]
["2016-04-10T18:10:01.450","2016-04-11T04:10:01.450","AB","Sonar","Knudsen","phase range","5000-6000m"]
["2016-04-10T19:37:24.790","2016-04-11T05:37:24.790","AB","Sonar","Multibeam","New Line","0637 - turn"]
["2016-04-10T19:39:18.510","2016-04-11T05:39:18.510","AB","Sonar","Multibeam","New Line","0638"]
["2016-04-10T20:01:54.100","2016-04-11T06:01:54.100","AB","Sonar","Multibeam","Max Angle","25/25, Spike filter strong, aeration on, slope on, sector tracking on, alongtrack +2. Southern line direction."]
["2016-04-10T21:50:22.100","2016-04-11T07:50:22.100","MP","XBT",null,null,"#78 taken"]
["2016-04-10T21:51:27.740","2016-04-11T07:51:27.740","MP","XBT",null,null,"4/10/2016  9:55:48 PM, XBT 078 applied to line #0640"]
["2016-04-10T21:55:52.130","2016-04-11T07:55:52.130","wp","other",null,null,"watch change"]
["2016-04-10T23:55:31.650","2016-04-11T09:55:31.650","MP","Sonar","Knudsen","Tx Pulse","32, gain value 39dB"]
["2016-04-11T00:17:15.470","2016-04-11T10:17:15.470","wp","sonar","Multibeam","New Line","begin turn, new line 0643"]
["2016-04-11T00:21:59.180","2016-04-11T10:21:59.180","wp","sonar","Multibeam","new line","begin survey line, new line 0644"]
["2016-04-11T00:31:17.140","2016-04-11T10:31:17.140","MP","Sonar","Knudsen","Gain Value","37dB"]
["2016-04-11T00:35:30.260","2016-04-11T10:35:30.260","wp","sonar","Knudsen","Phase Range","4500-5000, gain to 39"]
["2016-04-11T00:52:45.800","2016-04-11T10:52:45.800","MP","Sonar","Knudsen","Phase Range","4000-5000, gain value 42dB"]
["2016-04-11T01:03:09.520","2016-04-11T11:03:09.520","MP","Sonar","Knudsen","Phase Range","4500-5500, gaim value 41dB"]
["2016-04-11T01:15:28.980","2016-04-11T11:15:28.980","MP","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-04-11T01:39:19.770","2016-04-11T11:39:19.770","wp","sonar","knudsen","Phase Range","3500-4500, pulse 8, power 3, gain 34"]
["2016-04-11T01:47:29.750","2016-04-11T11:47:29.750","wp","sonar","knudsen","Tx Pulse","16, gain to 35"]
["2016-04-11T01:54:04.410","2016-04-11T11:54:04.410","MP","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-11T02:00:14.790","2016-04-11T12:00:14.790","MP","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-11T02:02:29.370","2016-04-11T12:02:29.370","MP","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-11T02:06:11.100","2016-04-11T12:06:11.100","MP","Sonar","Knudsen","Gain Value","37dB, pulse 16"]
["2016-04-11T02:10:52.310","2016-04-11T12:10:52.310","wp","sonar","knudsen","phase range","1500-2500, tx pulse 2.0, power 2.0, gasin 29"]
["2016-04-11T02:32:23.480","2016-04-11T12:32:23.480","wp","sonar","knudsen","Phase Range","3000-4000, pulse 16, power 3, gain 39"]
["2016-04-11T02:45:21.430","2016-04-11T12:45:21.430","wp","sonar","knudsen","phase range","3500-4500"]
["2016-04-11T02:57:45.030","2016-04-11T12:57:45.030","wp","sonar","knudsen","phase range","4000-5000"]
["2016-04-11T03:04:03.790","2016-04-11T13:04:03.790","MP","XBT",null,null,"#79 taken"]
["2016-04-11T03:07:01.760","2016-04-11T13:07:01.760","MP","Sonar","Knudsen","Phase Range","4500-5500"]
["2016-04-11T03:09:21.450","2016-04-11T13:09:21.450","MP","XBT",null,null,"#79 applied to line 0646"]
["2016-04-11T03:17:46.500","2016-04-11T13:17:46.500","wp","sonar","Knudsen","Gain Value",35]
["2016-04-11T03:28:05.230","2016-04-11T13:28:05.230","wp","sonar","knudsen","Phase Range","5000-6000, gsin 36"]
["2016-04-11T04:30:24.160","2016-04-11T14:30:24.160","DF","Watch Change",null,null,"Dan and Breezy on watch"]
["2016-04-11T04:31:09.020","2016-04-11T14:31:09.020","DF","Sonar","Multibeam","Max Angle","26/32"]
["2016-04-11T04:41:18.430","2016-04-11T14:41:18.430","DF","sonar","Multibeam","Max Angle","52/52"]
["2016-04-11T04:51:30.260","2016-04-11T14:51:30.260","DF","Sonar","Multibeam","Max Angle","26/32"]
["2016-04-11T05:23:27.150","2016-04-11T15:23:27.150","DF","Sonar","Multibeam","Max Angle","25/25"]
["2016-04-11T05:29:14.370","2016-04-11T15:29:14.370","DF","Sonar","Multibeam","Max Angle","22/22"]
["2016-04-11T05:30:06.300","2016-04-11T15:30:06.300","DF","sonar","Multibeam","Along Direction Pitch",2.5]
["2016-04-11T05:30:14.910","2016-04-11T15:30:14.910","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-04-11T05:39:49.310","2016-04-11T15:39:49.310","DF","sonar","Multibeam","Aeration Filter (On/Off)","on, sector artifacts keep popping up - have reduced in quantity but still there"]
["2016-04-11T06:36:54.920","2016-04-11T16:36:54.920","DS","Sonar","Knudsen","Gain Value","increased to 39 dB"]
["2016-04-11T06:51:41.970","2016-04-11T16:51:41.970","DS","Sonar","Multibeam",null,"increased max depth to 7000 - data was getting clipped. Much better. Tilt to 1. "]
["2016-04-11T06:58:04.420","2016-04-11T16:58:04.420","DS","Sonar","Multibeam","Max Angle","changed 25/25 to 70/70"]
["2016-04-11T07:14:36.810","2016-04-11T17:14:36.810","DF","Sonar","Knudsen","Tx Pulse","8 ms"]
["2016-04-11T07:29:08.780","2016-04-11T17:29:08.780","DF","Sonar","Multibeam","New Line","begin turn line 0653"]
["2016-04-11T07:30:54.140","2016-04-11T17:30:54.140","BG","sonar","Knudsen","Phase Range","4000-5000"]
["2016-04-11T07:40:50.940",{"$f":"IF(ISBLANK(A2255),\" \",((A2255)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-04-11T17:40:50.940"},"DF","sonar","Multibeam","New Line","begin survey trackline 0654"]
["2016-04-11T08:11:12","2016-04-11T18:11:12","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-11T08:16:15.270","2016-04-11T18:16:15.270","BG","xbt",null,null,"cast 080 collected"]
["2016-04-11T08:19:10.750","2016-04-11T18:19:10.750","BG","xbt",null,null,"cast 080 applied to line 0654"]
["2016-04-11T08:24:13.490","2016-04-11T18:24:13.490","DF","ship",null,null,"asked bridge to slow to 8-8.5"]
["2016-04-11T08:29:12.730","2016-04-11T18:29:12.730","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-04-11T08:29:49.050","2016-04-11T18:29:49.050","BG","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-11T08:36:05.270","2016-04-11T18:36:05.270","DF","Sonar","Multibeam","Spike Filter Strength","medium"]
["2016-04-11T09:18:57.550","2016-04-11T19:18:57.550","BG","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-11T09:32:10.750","2016-04-11T19:32:10.750","DF","Sonar","Multibeam","Ping Mode","deep"]
["2016-04-11T09:33:35.590","2016-04-11T19:33:35.590","DF","Sonar","Multibeam","Max Angle","50/70"]
["2016-04-11T09:47:33.200","2016-04-11T19:47:33.200","bg","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-04-11T09:48:52.120","2016-04-11T19:48:52.120","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2016-04-11T10:11:13.740","2016-04-11T20:11:13.740","DF","sonar","Knudsen",null,"tx power to 2, gain value to 36"]
["2016-04-11T10:20:13.540","2016-04-11T20:20:13.540","DF","sonar","Knudsen","Gain Value",38]
["2016-04-11T10:20:45.390","2016-04-11T20:20:45.390","DF","Sonar","Knudsen",null,"3, tx pulse to 4"]
["2016-04-11T10:25:21.480","2016-04-11T20:25:21.480","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-11T10:45:26.760","2016-04-11T20:45:26.760","DF","Ship",null,null,"Asked bridge to run 5 min past waypoint to extend line slighty"]
["2016-04-11T10:52:44.150","2016-04-11T20:52:44.150","DF","Sonar","Multibeam","New Line","begin turn line 0658"]
["2016-04-11T10:53:31.220","2016-04-11T20:53:31.220","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-11T10:58:16.050","2016-04-11T20:58:16.050","BG","sonar","knudsen","Phase Range","3500-4500"]
["2016-04-11T11:19:40.050","2016-04-11T21:19:40.050","DF","sonar","Multibeam","New Line","begin survey trackline 0659"]
["2016-04-11T11:25:26.860","2016-04-11T21:25:26.860","DF","sonar","Multibeam","Max Angle","70/70"]
["2016-04-11T11:26:07.780","2016-04-11T21:26:07.780","BG","sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-11T11:27:25.740","2016-04-11T21:27:25.740","DF","sonar","Multibeam","Spike Filter Strength","medium"]
["2016-04-11T12:29:58.010","2016-04-11T22:29:58.010","BG","sonar","Knudsen","phase range","2500-3500"]
["2016-04-11T12:34:15.770","2016-04-11T22:34:15.770","BG","sonar","knudsen","phase range","2000-3000"]
["2016-04-11T12:43:58.640","2016-04-11T22:43:58.640","BG","sonar","knudsen","Tx Power",2]
["2016-04-11T12:45:43.190","2016-04-11T22:45:43.190","DF","Sonar","Multibeam","Max Angle","50/60, rough ride on trackline heading so pulled in the swath"]
["2016-04-11T13:10:59.280","2016-04-11T23:10:59.280","DF","Sonar","Multibeam","Max Angle","50/68"]
["2016-04-11T13:11:47.130","2016-04-11T23:11:47.130","DF","Sonar","Knudsen","Gain Value",36]
["2016-04-11T13:13:02.640","2016-04-11T23:13:02.640","DF","sonar","Multibeam","Max Angle","62/63"]
["2016-04-11T13:13:52.360","2016-04-11T23:13:52.360","DF","sonar","Multibeam","Max Angle","62/62"]
["2016-04-11T13:22:06.030","2016-04-11T23:22:06.030","BG","sonar","Knudsen","Phase Range","1500-2500"]
["2016-04-11T13:30:27","2016-04-11T23:30:27","AB",null,null,null,"watch change"]
["2016-04-11T13:45:20.820","2016-04-11T23:45:20.820","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-04-11T14:07:49.740","2016-04-12T00:07:49.740","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-04-11T14:48:50.700","2016-04-12T00:48:50.700","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-04-11T14:59:50.370","2016-04-12T00:59:50.370","AB","Sonar","Multibeam","Ping Mode","Auto: Very Deep, Max Angles 52/52"]
["2016-04-11T15:06:51.270","2016-04-12T01:06:51.270","AB","XBT",null,null,"#81"]
["2016-04-11T15:07:36.220","2016-04-12T01:07:36.220","AB","Sonar","Knudsen","Tx Pulse","8, Power 3, Gain 38dB"]
["2016-04-11T15:12:51.180","2016-04-12T01:12:51.180","AB","XBT",null,null,"#81 applied to new line 0662"]
["2016-04-11T15:14:18.180","2016-04-12T01:14:18.180","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-04-11T15:15:08.590","2016-04-12T01:15:08.590","AB","sonar","Multibeam","New Line","0663 - turn"]
["2016-04-11T15:34:58.270","2016-04-12T01:34:58.270","AB","Sonar","Multibeam","New Line","0664"]
["2016-04-11T15:35:36.170","2016-04-12T01:35:36.170","AB","Sonar","Knudsen","Phase Range","3000-4000m, new line"]
["2016-04-11T15:53:57.580","2016-04-12T01:53:57.580","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-04-11T16:36:19.870","2016-04-12T02:36:19.870","CA","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-04-11T16:37:02.620","2016-04-12T02:37:02.620","AB","Sonar","Multibeam","Max Angle","70/65; Ping Mode Deep"]
["2016-04-11T17:11:36.970","2016-04-12T03:11:36.970","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2016-04-11T17:37:04.610","2016-04-12T03:37:04.610","AB","sonar","Knudsen","Phase Range","2000-3000m"]
["2016-04-11T17:49:07.380","2016-04-12T03:49:07.380","AB","Sonar","Knudsen","Tx Power","2, Pulse 4. Gain 33dB"]
["2016-04-11T18:07:25.470","2016-04-12T04:07:25.470","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-04-11T18:13:44.290","2016-04-12T04:13:44.290","AB","Sonar","Knudsen","Tx Power","3, Pulse 8, Gain 35dB"]
["2016-04-11T18:17:53.280","2016-04-12T04:17:53.280","AB","Sonar","Knudsen","Phase Range","3000-4000m, Gain 38dB"]
["2016-04-11T18:18:23.700","2016-04-12T04:18:23.700","AB","Sonar","Multibeam","Ping Mode","Auto: Very Deep, Max Angles 52/52"]
["2016-04-11T18:25:14.640","2016-04-12T04:25:14.640","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-04-11T18:34:39.360","2016-04-12T04:34:39.360","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-04-11T18:49:48.330","2016-04-12T04:49:48.330","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2016-04-11T18:50:08.160","2016-04-12T04:50:08.160","AB","Sonar","Multibeam","Ping Mode","Auto: Extra Deep, Max Angles 35/35"]
["2016-04-11T18:59:43.860","2016-04-12T04:59:43.860","AB","Sonar","Knudsen","Phase Range","5000-6000m, Pulse 16"]
["2016-04-11T19:26:22.940","2016-04-12T05:26:22.940","AB","Sonar","Knudsen","Phase Range","5500-6500m, Gain 40db"]
["2016-04-11T19:34:56.030","2016-04-12T05:34:56.030","AB","Sonar","Multibeam","Max Angle","25/25"]
["2016-04-11T19:53:07.100","2016-04-12T05:53:07.100","AB","sonar","Multibeam","New Line","0669 - turn"]
["2016-04-11T19:56:49.170",{"$f":"IF(ISBLANK(A2319),\" \",((A2319)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-04-12T05:56:49.170"},"AB","sonar","Multibeam","New Line","0670"]
["2016-04-11T20:16:10.680","2016-04-12T06:16:10.680","AB","Sonar","Knudsen","Phase Range","6000-7000m, Pulse 32"]
["2016-04-11T20:25:14.570","2016-04-12T06:25:14.570","AB","Sonar","EK","Change Range","7500m "]
["2016-04-11T20:58:20.870","2016-04-12T06:58:20.870","AB","XBT",null,null,"#82"]
["2016-04-11T21:03:55.520","2016-04-12T07:03:55.520","AB","XBT",null,null,"#82 applied to new line 0672"]
["2016-04-11T21:04:56.580","2016-04-12T07:04:56.580","AB","Sonar","EK","Change Range","8000m "]
["2016-04-11T21:16:06.520","2016-04-12T07:16:06.520","AB","sonar","knudsen","Phase Range","6500-7500m, Gain 44dB"]
["2016-04-11T21:23:20.020","2016-04-12T07:23:20.020","AB","sonar","Multibeam","Max Angle","18/18 (6900 meters)"]
["2016-04-11T21:28:51.930","2016-04-12T07:28:51.930","AB","Sonar","Multibeam","Max Angle","15/15"]
["2016-04-11T21:36:17.550","2016-04-12T07:36:17.550","wp","other",null,null,"watch change"]
["2016-04-11T21:54:54.640","2016-04-12T07:54:54.640","DS","Sonar","Multibeam","Max Angle","10 and 10"]
["2016-04-11T22:08:59.260","2016-04-12T08:08:59.260","wp","sonar","Knudsen","phase range","6000-7000"]
["2016-04-11T22:54:13.270","2016-04-12T08:54:13.270","CR","sonar","knudsen","phase range","6500-7500"]
["2016-04-11T23:09:33.420","2016-04-12T09:09:33.420","CR","sonar","knudsen","phase range","7000-8000"]
["2016-04-11T23:10:34.040","2016-04-12T09:10:34.040","CR","sonar","knudsen","Tx Power",4]
["2016-04-11T23:49:32.230","2016-04-12T09:49:32.230","MP","Sonar","Knudsen","Phase Range","8000-9000"]
["2016-04-11T23:52:02.480","2016-04-12T09:52:02.480","MP","EK",null,"Change Range",12000]
["2016-04-11T23:53:56.250","2016-04-12T09:53:56.250","MP","Sonar","Knudsen","Gain Value","48dB"]
["2016-04-12T00:00:26.220","2016-04-12T10:00:26.220","MP","Sonar","Knudsen","Phase Range","8500-9500"]
["2016-04-12T00:15:06.350","2016-04-12T10:15:06.350","MP","Sonar","Knudsen","Phase Range","9000-10000"]
["2016-04-12T00:34:41.210","2016-04-12T10:34:41.210",null,"Sonar","Knudsen","Phase Range","8500-9500"]
["2016-04-12T00:58:48.350","2016-04-12T10:58:48.350","MP","Sonar","Knudsen","Phase Range","8000-9000"]
["2016-04-12T01:14:22.430","2016-04-12T11:14:22.430","wp","sonar","Knudsen","Phase Range","7500-8500"]
["2016-04-12T01:39:21.240","2016-04-12T11:39:21.240","MP","Sonar","Knudsen","Phase Range","7500-8500"]
["2016-04-12T01:50:59.090","2016-04-12T11:50:59.090","wp","sonar","Knudsen","Phase Range","7000-8000"]
["2016-04-12T02:26:38.950","2016-04-12T12:26:38.950","MP","Sonar","Knudsen","Phase Range","7500-8500"]
["2016-04-12T02:38:51.740","2016-04-12T12:38:51.740","MP","Sonar","Knudsen","Phase Range","7000-8000, gain value 48dB"]
["2016-04-12T02:46:14.760","2016-04-12T12:46:14.760","MP","Sonar","Knudsen","Phase Range","6500-7500"]
["2016-04-12T02:47:45.850","2016-04-12T12:47:45.850","MP","XBT",null,null,"#83"]
["2016-04-12T02:52:41.960","2016-04-12T12:52:41.960","MP","XBT",null,null,"#83 applied to line 0677"]
["2016-04-12T03:07:38.730","2016-04-12T13:07:38.730","DS","Sonar","Multibeam","Max Angle","tried 15/15 but too much, 11/12"]
["2016-04-12T03:09:07.780","2016-04-12T13:09:07.780","DS","Sonar","EK",null,"Changed file range to 7100, still getting 10 second timeout warnings"]
["2016-04-12T03:18:33.190","2016-04-12T13:18:33.190","MP","Sonar","Knudsen","Phase Range","6000-7000"]
["2016-04-12T03:36:38.980","2016-04-12T13:36:38.980","CR","Sonar","Knudsen","Tx Power",2]
["2016-04-12T03:36:55.400","2016-04-12T13:36:55.400","CR","Sonar","Knudsen","Tx Power",44]
["2016-04-12T04:44:33.160","2016-04-12T14:44:33.160","CR","Sonar","Knudsen","Tx Power",3]
["2016-04-12T04:48:08.420","2016-04-12T14:48:08.420","CR","Sonar","Knudsen","Phase Range","5000-6000"]
["2016-04-12T04:51:23.970","2016-04-12T14:51:23.970","CR","Sonar","Knudsen","Tx Power",2]
["2016-04-12T05:06:07.120","2016-04-12T15:06:07.120","DS","Sonar","Multibeam","Max Angle","30/70"]
["2016-04-12T06:01:25.740","2016-04-12T16:01:25.740","DF","SHip",null,null,"begin new line because ship is going to slow to stop and do DP test, all sonars left pinging and recording, 0681"]
["2016-04-12T06:13:57.420","2016-04-12T16:13:57.420","DF","Ship",null,null,"begin new line because the DP test is over and we are starting on the trackline again 0682"]
["2016-04-12T06:35:00.310","2016-04-12T16:35:00.310","BG","Sonar","Knudsen","Phase Range","4000-5000"]
["2016-04-12T06:38:17.740","2016-04-12T16:38:17.740","DF","Sonar","Multibeam","Max Angle","70/70"]
["2016-04-12T06:47:05.120","2016-04-12T16:47:05.120","BG","sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-12T07:00:19.760","2016-04-12T17:00:19.760","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-12T07:14:13.820","2016-04-12T17:14:13.820","DF","Sonar","Multibeam","Ping Mode","forced into deep mode"]
["2016-04-12T07:18:36.510","2016-04-12T17:18:36.510","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2016-04-12T07:27:50.260","2016-04-12T17:27:50.260","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2016-04-12T07:31:46.970","2016-04-12T17:31:46.970","DS","Sonar","Multibeam","Ping Mode","switched back to auto"]
["2016-04-12T07:56:33.920","2016-04-12T17:56:33.920","DS","Sonar","Knudsen","Phase Range","3500-4500"]
["2016-04-12T08:26:21.070","2016-04-12T18:26:21.070","DF","sonar","Multibeam","Max Angle","40/42"]
["2016-04-12T08:33:55.670","2016-04-12T18:33:55.670","DF","Sonar","Multibeam","Along Direction Pitch",1.5]
["2016-04-12T08:34:10.870","2016-04-12T18:34:10.870","DF","Sonar","Multibeam","Aeration Filter (On/Off)","off"]
["2016-04-12T09:13:35.950","2016-04-12T19:13:35.950","DF","xbt",null,null,"cast 084 collected"]
["2016-04-12T09:16:33.110","2016-04-12T19:16:33.110","DF","xbt",null,null,"cast 084 applied to line 0685"]
["2016-04-12T09:29:24.010","2016-04-12T19:29:24.010","DF","Sonar","Multibeam","Max Angle","52/52"]
["2016-04-12T09:44:34.220","2016-04-12T19:44:34.220","DF","sonar","knudsen","Phase Range","3000-4000"]
["2016-04-12T10:24:00.700","2016-04-12T20:24:00.700","DF","sonar","Knudsen","phase range","2500-3500"]
["2016-04-12T11:04:40.270","2016-04-12T21:04:40.270","DF","Sonar","Knudsen","Tx Pulse",8]
["2016-04-12T11:11:35.510","2016-04-12T21:11:35.510","BG","sonar","Knudsen","phase range","2000-3000"]
["2016-04-12T11:29:53.670","2016-04-12T21:29:53.670","DF","Sonar","Multibeam","Max Angle","55/55"]
["2016-04-12T12:08:54.340","2016-04-12T22:08:54.340","DF","sonar","Knudsen","phase range","1500-2500"]
["2016-04-12T12:09:16.140","2016-04-12T22:09:16.140","DF","sonar","knudsen","Gain Value",40]
["2016-04-12T12:09:30.880","2016-04-12T22:09:30.880","DF","sonar","Multibeam","Max Angle","70/70"]
["2016-04-12T12:12:30.160",{"$f":"IF(ISBLANK(A2383),\" \",((A2383)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-04-12T22:12:30.160"},"DF","sonar","Multibeam","Max Angle","60/60"]
["2016-04-12T13:05:57.090","2016-04-12T23:05:57.090","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2016-04-12T13:06:25.340","2016-04-12T23:06:25.340","DF","Sonar","Multibeam","Max Angle","70/70"]
["2016-04-12T13:12:01.180","2016-04-12T23:12:01.180","DF","Sonar","Multibeam","Along Direction Pitch",1]
["2016-04-12T13:41:42.390","2016-04-12T23:41:42.390","CA","Sonar","Knudsen","Phase Range","1000-2000m"]
["2016-04-12T14:09:04.730","2016-04-13T00:09:04.730","CA","Sonar","Knudsen","Phase Range","500-1500m"]
["2016-04-12T14:17:03.150","2016-04-13T00:17:03.150","AB","Sonar","Multibeam","New line","0690; Max Angle 75/75"]
["2016-04-12T14:24:39.250","2016-04-13T00:24:39.250","AB","Sonar","Knudsen","Range","500m , Pulse 1, Power 1, Gain 35dB"]
["2016-04-12T14:32:07","2016-04-13T00:32:07","AB","Sonar","Knudsen","Phase Range","250-750m, Gain 33dB, "]
["2016-04-12T15:11:26.270","2016-04-13T01:11:26.270","AB","XBT",null,null,"#85"]
["2016-04-12T15:18:26.440","2016-04-13T01:18:26.440","AB","XBT",null,null,"#85 applied to new line 0692"]
["2016-04-12T15:40:05.130","2016-04-13T01:40:05.130","AB","Sonar","Knudsen","Phase Range","750-1250m, Gain 36dB"]
["2016-04-12T15:46:45.020","2016-04-13T01:46:45.020","AB","Sonar","Knudsen","Tx Pulse","2, Power 2, Gain 30dB"]
["2016-04-12T15:49:59.250","2016-04-13T01:49:59.250","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2016-04-12T16:04:44.810","2016-04-13T02:04:44.810","AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2016-04-12T16:21:31.960","2016-04-13T02:21:31.960","AB","Sonar","Multibeam","New line","0694"]
["2016-04-12T16:23:46.900","2016-04-13T02:23:46.900","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2016-04-12T17:16:27.840","2016-04-13T03:16:27.840","AB","Sonar","Multibeam","New line","0695"]
["2016-04-12T17:21:55.940","2016-04-13T03:21:55.940","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2016-04-12T17:34:32.860","2016-04-13T03:34:32.860","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2016-04-12T17:41:36.640","2016-04-13T03:41:36.640","AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2016-04-12T17:47:52.900","2016-04-13T03:47:52.900","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2016-04-12T17:48:38.090","2016-04-13T03:48:38.090","AB","Sonar","Knudsen","Range","1000m; Phase Range 1500-2500m, Pulse 4, Gain 36dB"]
["2016-04-12T17:52:32.070","2016-04-13T03:52:32.070","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-04-12T18:16:31","2016-04-13T04:16:31","AB","Sonar","Multibeam","New line","0696"]
["2016-04-12T18:30:53.700","2016-04-13T04:30:53.700","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2016-04-12T19:00:01","2016-04-13T05:00:01","AB","Sonar","Multibeam","New line","0697"]
["2016-04-12T19:38:46.180","2016-04-13T05:38:46.180","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-04-12T20:22:35.030","2016-04-13T06:22:35.030","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2016-04-12T20:31:14.380","2016-04-13T06:31:14.380","AB","Ship",null,null,"Reducing speed to do propulsion testing prior to Guam approach"]
["2016-04-12T20:34:26.180","2016-04-13T06:34:26.180","AB","Sonar","Multibeam","New line","0699 - propulsion testing"]
["2016-04-12T21:12:02.780","2016-04-13T07:12:02.780","CA","Sonar","Knudsen","Phase Range","1000-2000m"]
["2016-04-12T21:12:34.780","2016-04-13T07:12:34.780","AB","Sonar","Multibeam","New line","0700 propulsion testing complete"]
["2016-04-12T21:50:44.190","2016-04-13T07:50:44.190","2016-04-12T21:50:44.190","Sonar","All","Secure","Arrival in Guam, All Sonar equipment is secure."]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2447),\" \",((A2447)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2511),\" \",((A2511)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2575),\" \",((A2575)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2639),\" \",((A2639)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2703),\" \",((A2703)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2767),\" \",((A2767)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2831),\" \",((A2831)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2895),\" \",((A2895)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A2959),\" \",((A2959)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A3023),\" \",((A3023)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A3087),\" \",((A3087)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["DS","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DF","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["BG","Weather","Knudsen","New Line","Secure","Gain Mode"]
["AB","Watch Change","All","Max Angle",null,"Gain Value"]
["SM","XBT","ADCP","Spike Filter Strength",null,"Process Shift"]
["CA","Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
["MP","Other",null,"Aeration Filter (On/Off)",null,"Range"]
["CR",null,null,"Interference Filter (On/Off)",null,"Phase Mode"]
["WP",null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]