{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Log","Dropdowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":13,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Log","index":0,"n_rows":2000,"n_cols":8,"rows_kept":2000,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1903L2","UTC to Local: ",-4,"UTC 2","UTC 3","UTC 4","Cruise Details: 06 20 -07 12"]
["2019-07-05T21:07:09.890"]
[null,null,"WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2019-06-19T21:52:07.080",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-19T17:52:07.080"},"SH","Sonar","Multibeam","start up sis","Boot up SIS. Ran BIST. ALL PASSED"]
["2019-06-19T22:44:11.900",{"$f":"IF(ISBLANK(A6),\" \",((A6)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-19T18:44:11.900"},"SH","Sonar","EK","Start Pinging","Set Up Survey. Start Pinging"]
["2019-06-19T22:44:37.200",{"$f":"IF(ISBLANK(A7),\" \",((A7)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-19T18:44:37.200"},"SH","Sonar","EK","Start Recording","Recording Test file to test new storange drive."]
["2019-06-19T23:06:14.930","2019-06-19T19:06:14.930","SH","Sonar","Knudsen","Start Pinging","Test Pinging"]
["2019-06-20T14:55:58.430","2019-06-20T10:55:58.430","KJ","Ship",null,null,"fueling"]
["2019-06-20T14:57:29.390","2019-06-20T10:57:29.390","DP",null,null,null,"added Danielle to watchstander list"]
["2019-06-20T19:42:08.190","2019-06-20T15:42:08.190","SH","Ship",null,null,"secure speed log"]
["2019-06-20T19:42:19.670","2019-06-20T15:42:19.670","SH","Sonar","Multibeam","BIST","Run BIST"]
["2019-06-20T19:47:30.740","2019-06-20T15:47:30.740","SH","Sonar","EK",null,"Set sound speed to TSG 1539"]
["2019-06-20T19:59:41.580","2019-06-20T15:59:41.580","SH","Sonar","EK","Start Pinging"]
["2019-06-20T20:00:30.190","2019-06-20T16:00:30.190","SH","Sonar","Multibeam","BIST","All passed"]
["2019-06-20T20:04:14.370","2019-06-20T16:04:14.370","DP","Sonar","Multibeam","Start Pinging","Set KSYNC and started pinging"]
["2019-06-20T21:53:58.330","2019-06-20T17:53:58.330","SH","Sonar","All",null,"Start recording all sonars"]
["2019-06-20T22:02:44.820","2019-06-20T18:02:44.820","SH","XBT",null,null,"XBT 001 launched"]
["2019-06-20T22:15:21.800","2019-06-20T18:15:21.800","SH","Sonar","Multibeam","XBT Applied","XBT 001 applied to line 001"]
["2019-06-20T23:41:20.210","2019-06-20T19:41:20.210","KJ","Sonar","EK",null,"Disabled EK in Ksync to test possible source of interference in EM302 (regular striping in backscatter every "]
["2019-06-20T23:51:51.400","2019-06-20T19:51:51.400","KJ","Sonar","Multibeam",null,"TX power from -20 to Max, seems to have fixed the regular interference issue (not quite sure why, but the depth and BS data look OK)"]
["2019-06-20T23:53:52.860","2019-06-20T19:53:52.860","KJ","Sonar","Multibeam","New Line","0003 for full powah"]
["2019-06-21T00:32:12.430","2019-06-20T20:32:12.430","KJ","Sonar","EK","Stop Recording","Stopped logging, stopped pinging, \"uninstalled\" 38 transceiver"]
["2019-06-21T00:33:43.890","2019-06-20T20:33:43.890","KJ","Sonar","EK",null,"First file sans 38 is D20190621-T003237"]
["2019-06-21T00:40:31.900","2019-06-20T20:40:31.900","DP","XBT",null,null,"XBT 002 Launched"]
["2019-06-21T00:53:23.140","2019-06-20T20:53:23.140","DP","XBT",null,"XBT Applied","XBT 002 applied to line 0004"]
["2019-06-21T01:13:20.800","2019-06-20T21:13:20.800","DP","Sonar","EK",null,"Split file"]
["2019-06-21T01:13:53.170","2019-06-20T21:13:53.170","DP","Sonar","Knudsen",null,"Split File"]
["2019-06-21T01:14:16.010","2019-06-20T21:14:16.010","DP","Sonar","Multibeam",null,"End Line 0004/Start line 0005"]
["2019-06-21T01:32:58.920","2019-06-20T21:32:58.920","DP","Sonar","Multibeam",null,"End Line 0005/Start line 0006"]
["2019-06-21T01:33:24.700","2019-06-20T21:33:24.700","DP","Sonar","EK",null,"New Line"]
["2019-06-21T01:33:51.500","2019-06-20T21:33:51.500","DP","Sonar","Knudsen",null,"New Line"]
["2019-06-21T03:15:53.240","2019-06-20T23:15:53.240","DP","Sonar","Multibeam",null,"End Line 0008/Start line 0009"]
["2019-06-21T03:16:43.840","2019-06-20T23:16:43.840","DP","Sonar","EK",null,"New Line"]
["2019-06-21T03:16:47.190","2019-06-20T23:16:47.190","DP","Sonar","Knudsen",null,"New Line"]
["2019-06-21T03:23:00.220","2019-06-20T23:23:00.220","DP","Sonar","Multibeam",null,"End Line 0009/Start Line 0010"]
["2019-06-21T03:23:40.880","2019-06-20T23:23:40.880","DP","Sonar","EK",null,"New Line"]
["2019-06-21T03:23:44.110","2019-06-20T23:23:44.110","DP","Sonar","Knudsen",null,"New Line"]
["2019-06-21T03:28:28.770","2019-06-20T23:28:28.770","DP","XBT",null,"XBT Launch","XBT 003 Launched"]
["2019-06-21T03:34:59.690","2019-06-20T23:34:59.690","DP","Sonar","Multibeam","XBT Applied","XBT 003 Applied to 0010"]
["2019-06-21T04:43:26.690","2019-06-21T00:43:26.690","KJ","Sonar","Multibeam","New Line","End line 0011/Start turn line 0012"]
["2019-06-21T04:43:34.020","2019-06-21T00:43:34.020","DP","Sonar","EK",null,"New Line"]
["2019-06-21T04:43:44.850","2019-06-21T00:43:44.850","DP","Sonar","Knudsen",null,"New Line"]
["2019-06-21T04:59:20.860","2019-06-21T00:59:20.860","KJ","Sonar","Multibeam","New Line","End Turn line 0012/ Start Line 0013"]
["2019-06-21T04:59:31.190","2019-06-21T00:59:31.190","DP","Sonar","EK",null,"New Line"]
["2019-06-21T04:59:52.910","2019-06-21T00:59:52.910","DP","Sonar","Knudsen",null,"New Line"]
["2019-06-21T05:04:59.270","2019-06-21T01:04:59.270","KJ","XBT",null,"XBT Launch","Launch XBT 004"]
["2019-06-21T05:10:25.070","2019-06-21T01:10:25.070","KJ","Sonar","Multibeam","XBT Applied","XBT Applied to line 0013"]
["2019-06-21T06:47:27.290","2019-06-21T02:47:27.290","DP","XBT",null,"XBT Launch","Launch XBT 005"]
["2019-06-21T06:52:04.380","2019-06-21T02:52:04.380","DP","Sonar","Multibeam","XBT Applied","XBT Applied to line 0014"]
["2019-06-21T07:04:22.720","2019-06-21T03:04:22.720","KJ","Sonar","Multibeam","New Line","0016 for turn"]
["2019-06-21T07:44:04.460","2019-06-21T03:44:04.460","KJ","Sonar","Multibeam","New Line","0017 for survey line"]
["2019-06-21T08:31:07.760","2019-06-21T04:31:07.760","KJ","Sonar","Multibeam","New Line","0018 for transit to dive site"]
["2019-06-21T08:34:39.870","2019-06-21T04:34:39.870","KJ","XBT",null,null,"AXBT006 initial launch failed from tube 6 - no splash detected; try again with tube 7, worked with no issue"]
["2019-06-21T08:47:28.110","2019-06-21T04:47:28.110","KJ","XBT",null,null,"AXBT006 applied in line 0018"]
["2019-06-21T10:01:51.080","2019-06-21T06:01:51.080","SH","Sonar","All","Secure","Secure all for Dive 01. Bridge turned on speed log. "]
["2019-06-21T10:03:00.660","2019-06-21T06:03:00.660","SH","Sonar","ADCP",null,"Turned on ADCP for Dive 01"]
["2019-06-21T10:05:03.630","2019-06-21T06:05:03.630","SH",null,null,null,"Switched Pos Configuration"]
["2019-06-21T13:25:55.610","2019-06-21T09:25:55.610","SH","Sonar","EK","Start Pinging","Start Pinging and Recording Eks. Recording 18,70,120, and 200. 70 in CW mode! In this mode throughout dive."]
["2019-06-21T21:00:28.300","2019-06-21T17:00:28.300","SH","Sonar","ADCP","secure","Secured after Dive 01"]
["2019-06-21T21:01:41.630","2019-06-21T17:01:41.630","SH","Sonar","SpeedLog","secure"]
["2019-06-21T21:07:37.840","2019-06-21T17:07:37.840","SH","Sonar","All",null,"Start Pinging all sonars. Multibeam started in Marine Mammal Mode"]
["2019-06-21T21:37:20.820","2019-06-21T17:37:20.820","SH","Sonar","EK","Start Recording"]
["2019-06-21T21:39:20.390","2019-06-21T17:39:20.390","SH","Sonar","Multibeam",null,"EX1903L2_DIVE01_20190621_ROVCTD.cnv applied to line 0021"]
["2019-06-21T21:40:15.730","2019-06-21T17:40:15.730","SH","Sonar","Multibeam",null,"Start Line 0021"]
["2019-06-21T22:19:29.370","2019-06-21T18:19:29.370","DP","XBT",null,"XBT Launch","Launch XBT 007"]
["2019-06-21T22:25:51.380","2019-06-21T18:25:51.380","DP","Sonar","Multibeam","XBT Applied","Applied XBT 007 to line 0021"]
["2019-06-21T22:53:51.980","2019-06-21T18:53:51.980","DP","Sonar","Multibeam","New Line","End 0022 for turn line"]
["2019-06-21T23:01:25.630","2019-06-21T19:01:25.630","DP","Sonar","Multibeam","New Line","End Turn Line 0023/ Start survey line"]
["2019-06-22T00:17:01.850",{"$f":"IF(ISBLANK(A70),\" \",((A70)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-21T20:17:01.850"},"DP","XBT",null,"XBT Launch","Launch XBT 008"]
["2019-06-22T00:17:35.140","2019-06-21T20:17:35.140","DP","Sonar","Multibeam","New Line","End Line 0025 Start line 0026"]
["2019-06-22T00:21:11.210","2019-06-21T20:21:11.210","DP","Sonar","Multibeam","XBT Applied","XBT 008 Applied to line 0026"]
["2019-06-22T02:09:48.540","2019-06-21T22:09:48.540","KJ","XBT",null,"XBT Launch","AXBT009 launched"]
["2019-06-22T02:24:01.970","2019-06-21T22:24:01.970","DP","Sonar","Multibeam","XBT Applied","AXBT009 applied to line 0028"]
["2019-06-22T03:13:43.450","2019-06-21T23:13:43.450","DP","Sonar","Multibeam",null,"Survey Speed increased to 10.7 knots for lines 0026 to 0028"]
["2019-06-22T03:17:42.670","2019-06-21T23:17:42.670","DP","Sonar","Multibeam","New Line","End Line 0028 Start Line 0029"]
["2019-06-22T04:18:38.720","2019-06-22T00:18:38.720","DP","XBT",null,"XBT Launch","AXBT010 Launched"]
["2019-06-22T04:25:00.850","2019-06-22T00:25:00.850","DP","Sonar","Multibeam","XBT Applied","AXBT010 applied to line 0031"]
["2019-06-22T04:51:13.310","2019-06-22T00:51:13.310","DP","Sonar","Multibeam","New Line","End Line 0031 for turn line 0032"]
["2019-06-22T05:16:53.850","2019-06-22T01:16:53.850","DP","Sonar","Multibeam","New Line","End Turn Line 0032 / Start Survey Line 0033"]
["2019-06-22T06:17:19.710","2019-06-22T02:17:19.710","DP","XBT",null,"XBT Launch","AXBT011 Launched"]
["2019-06-22T06:20:00.670","2019-06-22T02:20:00.670","DP","Sonar","Multibeam","XBT Applied","AXBT011 applied to line 0034"]
["2019-06-22T07:03:48.190","2019-06-22T03:03:48.190","KJ","Sonar","Multibeam","New Line","0035 start transit to dive site"]
["2019-06-22T08:08:23.340","2019-06-22T04:08:23.340","KJ","XBT",null,null,"AXBT012 launched"]
["2019-06-22T08:15:05.950","2019-06-22T04:15:05.950","KJ","Sonar","Multibeam","XBT Applied","AXBT012 applied in line 0036"]
["2019-06-22T10:01:33.330","2019-06-22T06:01:33.330","KJ","Sonar","All","Secure","arriving on site for drift test with speed log on"]
["2019-06-22T10:02:19.110","2019-06-22T06:02:19.110","KJ","XBT",null,null,"AXBT013 launched"]
["2019-06-22T10:20:16.330","2019-06-22T06:20:16.330","KJ","Sonar","Multibeam","XBT Applied","AXBT013 applied in line 0040 (0039 and 0040 are short files on dive site, just to get the ASVP file into the Qimera processing path; files may be missing POS data because this had been switched to DP mode)"]
["2019-06-22T12:19:09.050","2019-06-22T08:19:09.050","SH","Sonar","EK","Start Pinging","Start Pinging and Recording Eks. Recording 18,70,120, and 200. 70 in CW mode! In this mode throughout dive."]
["2019-06-22T14:01:14.870","2019-06-22T10:01:14.870","SH","Sonar","EK",null,"Saw massive multiple in EK 60 18 kHz. We figured out that it was just perfect conditions after we turned off the Multibeam and the ping rate subsequently changed."]
["2019-06-22T17:31:51.670","2019-06-22T13:31:51.670","SH","Sonar","EK","Stop Recording","Stop recording to change output to Manual and 2000 m"]
["2019-06-22T17:31:54.470","2019-06-22T13:31:54.470","SH","Sonar","EK",null,"Change Recording Range to Manual 2000 m"]
["2019-06-22T17:32:38.740","2019-06-22T13:32:38.740","SH","Sonar","EK","Start Pinging"]
["2019-06-22T17:32:55.040","2019-06-22T13:32:55.040","SH","Sonar","EK",null,"change ping mode to maximum"]
["2019-06-22T19:20:35.520","2019-06-22T15:20:35.520","SH","Sonar","EK","Stop Recording","Stop pinging and recording. Setting up for Dive 02 Midwater transect"]
["2019-06-22T19:22:47.370","2019-06-22T15:22:47.370","SH","Sonar","EK",null,"38 kHz Installed"]
["2019-06-22T19:23:02.960","2019-06-22T15:23:02.960","SH","Sonar","EK",null,"Set to Midwater Mode. 18 = 1.024 ms, 2000 W. 70 = 1.024ms, 750 W, CW. 120 = 1.024 ms, 250 W,  200 = 1.024 ms, 150 W."]
["2019-06-22T19:23:55.980","2019-06-22T15:23:55.980","SH","Sonar","EK",null,"Start Pinging EK 38 kHz"]
["2019-06-22T19:25:21.190","2019-06-22T15:25:21.190","SH","Sonar","EK",null,"Put EK 38 in Active Mode"]
["2019-06-22T19:37:37.780","2019-06-22T15:37:37.780","SH","Sonar","EK",null,"Uninstalled 38 kHz. Start Pinging and recording for Midwater transects. Speed log secured."]
["2019-06-22T22:47:10.370","2019-06-22T18:47:10.370","SH","Sonar","EK",null,"Stop Pinging and recording. Changing settings back to normal operations"]
["2019-06-22T22:52:53.140","2019-06-22T18:52:53.140","SH","Sonar","EK",null,"EK set to be slave to Ksync"]
["2019-06-22T22:56:36.640","2019-06-22T18:56:36.640","SH","POS",null,null,"Switched Pos Configuration"]
["2019-06-22T22:56:59.650","2019-06-22T18:56:59.650","SH","Sonar","ADCP","Secure"]
["2019-06-22T22:57:30.900","2019-06-22T18:57:30.900","SH","Sonar","EK","Start Pinging","Start Pinging and Recording EKS. Normal Mode. 18 = 4 ms, 2000 W. 70 = 2 ms, 750 W, CW. 120 = 1.024 ms, 250 W,  200 = 1.024 ms, 150 W."]
["2019-06-22T22:59:14.940","2019-06-22T18:59:14.940","SH","Sonar","Knudsen","Start Pinging","Start Pinging and Recording"]
["2019-06-22T23:00:45.810","2019-06-22T19:00:45.810","SH","Sonar","Multibeam","Start Pinging","Start Pinging and Recording in Marine Mammal Mode: -20 dB"]
["2019-06-22T23:01:26.120","2019-06-22T19:01:26.120","SH","Sonar","SpeedLog","secure"]
["2019-06-22T23:05:31.710","2019-06-22T19:05:31.710","SH","Sonar","EK",null,"Turn EK 70 pulse length back to 1 ms"]
["2019-06-22T23:06:20.990","2019-06-22T19:06:20.990","SH","Sonar","Multibeam",null,"Brought multibeam up to max power"]
["2019-06-22T23:10:45.340","2019-06-22T19:10:45.340","SH","Sonar","Multibeam",null,"Applied Dive 02 CTD  002 from ROVCTD. Downcast due to midwater transit"]
["2019-06-22T23:12:30.630","2019-06-22T19:12:30.630","SH","Sonar","ADCP","start pinging","starting ADCPs to troubleshoot ek noise"]
["2019-06-22T23:24:37.480","2019-06-22T19:24:37.480","SH","Sonar","ADCP","secure"]
["2019-06-22T23:25:37.460","2019-06-22T19:25:37.460","SH","Sonar","Multibeam","Start Pinging","start pinging after noise test"]
["2019-06-22T23:29:32.470","2019-06-22T19:29:32.470","DP","Sonar","Multibeam","Start Logging","Start logging"]
["2019-06-23T00:47:51.280","2019-06-22T20:47:51.280","KJ","Sonar","EK",null,"Stopped logging, stopped pinging, changed 70 kHz from 1 ms CW to 2 ms FM (LFM up, 45-90 kHz) and changed logging range from common 2000 m (from midwater dive) to auto logging; note that the recording range for each system will depend on the window display range, not necessarily the bottom detection depth; 18 kHz is 4 ms, 38 is secure, 120 and 200 are 1 ms, all at highest power settings in CW; started pinging and logging after changes"]
["2019-06-23T01:07:04.460","2019-06-22T21:07:04.460","DP","Sonar","Multibeam","New Line","End 0042 for turn line"]
["2019-06-23T01:12:47.170","2019-06-22T21:12:47.170","DP","Sonar","Multibeam","New Line","End 0043 for Survey Line"]
["2019-06-23T01:19:31.910","2019-06-22T21:19:31.910","DP","XBT",null,"XBT Launch","AXBT0014 Launched"]
["2019-06-23T01:21:10.590","2019-06-22T21:21:10.590","DP","Sonar","Multibeam","XBT Applied","AXBT0014 applied to 0044"]
["2019-06-23T01:29:12.510","2019-06-22T21:29:12.510","DP","Sonar","Multibeam",null,"Had bridge shift to starboard to cover a holiday in previous data"]
["2019-06-23T03:03:23.500","2019-06-22T23:03:23.500","DP","XBT",null,"XBT Launch","AXBT015 Launched"]
["2019-06-23T03:11:53.980","2019-06-22T23:11:53.980","DP","Sonar","Multibeam","XBT Applied","AXBT Applied to 0045"]
["2019-06-23T05:03:12.540","2019-06-23T01:03:12.540","DP","XBT",null,"XBT Launch","AXBT016 Launched"]
["2019-06-23T05:10:16.150","2019-06-23T01:10:16.150","DP","Sonar","Multibeam","XBT Applied","AXBT016 Applied to 0047"]
["2019-06-23T05:46:57.740","2019-06-23T01:46:57.740","DP","Sonar","Multibeam","New Line","Turn onto Survey Line 0049"]
["2019-06-23T07:02:07.430","2019-06-23T03:02:07.430","KJ","Sonar","Multibeam","New Line","Start turn line 0051"]
["2019-06-23T07:18:48.850",{"$f":"IF(ISBLANK(A128),\" \",((A128)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-23T03:18:48.850"},"KJ","Sonar","Multibeam","New Line","Start Survey Line 0052"]
["2019-06-23T07:22:13.650","2019-06-23T03:22:13.650","KJ","XBT",null,"XBT Launch","AXBT017 Launched"]
["2019-06-23T07:30:47.990","2019-06-23T03:30:47.990","KJ","Sonar","Multibeam","XBT Applied","AXBT017 Applied to 0052"]
["2019-06-23T07:44:19.390","2019-06-23T03:44:19.390","KJ","Sonar","Multibeam","New Line","0053 for transit to dive site"]
["2019-06-23T08:17:26.420","2019-06-23T04:17:26.420","KJ","Ship",null,null,"diverting around very strong squall"]
["2019-06-23T08:18:39.070","2019-06-23T04:18:39.070","KJ","Sonar","All",null,"Data affected by severe rain/wind/lightning"]
["2019-06-23T09:27:44.090",{"$f":"IF(ISBLANK(A134),\" \",((A134)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-23T05:27:44.090"},"KJ","XBT",null,null,"AXBT018 launched"]
["2019-06-23T09:35:09.370","2019-06-23T05:35:09.370","KJ","Sonar","Multibeam",null,"AXBT018 applied in line 0055"]
["2019-06-23T09:55:46.140","2019-06-23T05:55:46.140","KJ","Sonar","All","Secure","Arriving on dive site"]
["2019-06-23T10:08:13.340","2019-06-23T06:08:13.340","SH","Sonar","Multibeam","Secure"]
["2019-06-23T10:08:26.060","2019-06-23T06:08:26.060","SH","Sonar","Knudsen",null,"Stop Pinging"]
["2019-06-23T10:12:27.800","2019-06-23T06:12:27.800","SH","POS",null,null,"Switched Pos Configuration"]
["2019-06-23T10:13:31.840","2019-06-23T06:13:31.840","SH","Sonar","EK",null,"70 put into CW mode"]
["2019-06-23T20:00:02.220","2019-06-23T16:00:02.220","SH","Sonar","EK","Start Recording","Start Recording"]
["2019-06-23T21:01:54.720","2019-06-23T17:01:54.720","SH","POS",null,null,"Switched Pos Configuration"]
["2019-06-23T21:03:35.610","2019-06-23T17:03:35.610","SH","Sonar","ADCP","secure","Secured after Dive 03"]
["2019-06-23T21:05:06.980","2019-06-23T17:05:06.980","SH","Sonar","EK",null,"Changed synchronization to slave. Changed 70 from CW to FM. "]
["2019-06-23T21:05:44.660","2019-06-23T17:05:44.660","SH","Sonar","SpeedLog","secure"]
["2019-06-23T21:06:49.610","2019-06-23T17:06:49.610","SH","Sonar","Knudsen",null,"Start Pinging Knudsen. And recording"]
["2019-06-23T21:07:25.020","2019-06-23T17:07:25.020","SH","Sonar","Multibeam","Start Pinging","Start pinging in marine mammal mode -20"]
["2019-06-23T21:11:38.140","2019-06-23T17:11:38.140","SH","Sonar",null,"Start Logging","Start logging SMD"]
["2019-06-23T21:18:15.120","2019-06-23T17:18:15.120","DP","Sonar","Multibeam",null,"Pinging in full power"]
["2019-06-23T21:24:03.840","2019-06-23T17:24:03.840","DP","Sonar","Multibeam",null,"Applied CPCTD003 to line 0057"]
["2019-06-23T21:24:29.620","2019-06-23T17:24:29.620","DP","Sonar","Multibeam","Start Logging","Start Logging Multibeam"]
["2019-06-23T23:03:59.540","2019-06-23T19:03:59.540","SH","Sonar","Multibeam","New Line","New Line for Turn (yaw Stabilization OFF) TURN =0059"]
["2019-06-23T23:19:58.200","2019-06-23T19:19:58.200","SH","Sonar","Multibeam","New Line","Start 0060"]
["2019-06-23T23:20:15.580","2019-06-23T19:20:15.580","SH","XBT",null,null,"Failed Launch. Spike at 90 meters"]
["2019-06-23T23:21:22.960","2019-06-23T19:21:22.960","SH","XBT",null,null,"Re launching XBT 0019"]
["2019-06-23T23:23:55.990","2019-06-23T19:23:55.990","SH","XBT",null,null,"Good Profile"]
["2019-06-23T23:29:03.220","2019-06-23T19:29:03.220","SH","Sonar","Multibeam",null,"AXBT0019 asvp profile applied to Line 0061"]
["2019-06-23T23:53:48.250","2019-06-23T19:53:48.250","KJ","Sonar","Multibeam","New Line","0062 turn"]
["2019-06-24T00:04:38.720","2019-06-23T20:04:38.720","KJ","XBT",null,null,"AXBT020 launched"]
["2019-06-24T00:07:19.860","2019-06-23T20:07:19.860","KJ","Sonar","Multibeam",null,"AXBT020 applied in line 0062"]
["2019-06-24T01:59:22.260","2019-06-23T21:59:22.260","KJ","XBT",null,null,"AXBT021 launched"]
["2019-06-24T02:08:50.740","2019-06-23T22:08:50.740","KJ","Sonar","Multibeam",null,"AXBT021 applied in line 0064"]
["2019-06-24T03:25:28.440","2019-06-23T23:25:28.440","KJ","XBT",null,null,"AXBT022 launched"]
["2019-06-24T03:30:26.010","2019-06-23T23:30:26.010","KJ","Sonar","Multibeam",null,"qa"]
["2019-06-24T03:35:48.010","2019-06-23T23:35:48.010","KJ","Sonar","Multibeam","Along Direction Pitch","changed from 0 to -1 to try to reduce Erik's Horns and penetration at nadir, seems to have helped"]
["2019-06-24T04:09:18.390","2019-06-24T00:09:18.390","DP","Sonar","Multibeam","New Line","End survey line for turn line 0067"]
["2019-06-24T04:15:52.940","2019-06-24T00:15:52.940","DP","Sonar","Multibeam","New Line","End turn line for survey line 0068"]
["2019-06-24T05:29:15.590","2019-06-24T01:29:15.590","DP","XBT",null,"XBT Launch","Launch AXBT023"]
["2019-06-24T05:34:47.680","2019-06-24T01:34:47.680","DP","Sonar","Multibeam","XBT Applied","Applied AXBT023 to line 0069"]
["2019-06-24T06:06:12.680","2019-06-24T02:06:12.680","DP","Sonar","Multibeam","New Line","End Survey Line for turn line 0070"]
["2019-06-24T06:27:12.790","2019-06-24T02:27:12.790","DP","Sonar","Multibeam","New Line","End turn line for survey line 0071"]
["2019-06-24T07:22:14.780","2019-06-24T03:22:14.780","KJ","XBT",null,null,"Launch AXBT024"]
["2019-06-24T07:28:46.690","2019-06-24T03:28:46.690","KJ","Sonar","Multibeam","New Line","0073 turn"]
["2019-06-24T07:29:11.790","2019-06-24T03:29:11.790","KJ","Sonar","Multibeam","XBT Applied","AXBT024 applied to line 0073"]
["2019-06-24T07:44:48.660","2019-06-24T03:44:48.660","KJ","Sonar","Multibeam","New Line","0074 survey line"]
["2019-06-24T09:03:52.220","2019-06-24T05:03:52.220","KJ","Sonar","EK",null,"changed 70 kHz window range from 1000 to 750 m to test whether window range determines recording range when file output recording length is set to 'auto / common'"]
["2019-06-24T09:11:31.450","2019-06-24T05:11:31.450","KJ","Sonar","EK",null,"turned 70 kHz window range back to 1000 m"]
["2019-06-24T09:26:02.690","2019-06-24T05:26:02.690","KJ","XBT",null,null,"AXBT025 launched"]
["2019-06-24T09:34:00.850","2019-06-24T05:34:00.850","KJ","Sonar","Multibeam",null,"AXBT025 applied in 0075"]
["2019-06-24T09:48:17.040","2019-06-24T05:48:17.040","KJ","Sonar","Multibeam",null,"Secure for drift test; speed log coming on; ADCPs on; interference in 70 kHz EK in FM mode migrating through water column due to slightly different ping intervals"]
["2019-06-24T09:49:53.990","2019-06-24T05:49:53.990","KJ","Sonar","EK",null,"EK 18 kHz showed multiple return when pinging in maximum; set to 1 sec intervaland multiple has disappeared"]
["2019-06-24T10:52:24.350","2019-06-24T06:52:24.350","SH","Sonar","EK",null,"EK 70kHz set to CW"]
["2019-06-24T20:57:15.140","2019-06-24T16:57:15.140","DP","POS",null,null,"Switched Pos Configuration"]
["2019-06-24T20:57:16.900","2019-06-24T16:57:16.900","DP","Sonar","ADCP","Secure","Secure ADCP"]
["2019-06-24T20:57:44.820","2019-06-24T16:57:44.820","DP","Sonar","SpeedLog","Secure","Secure SpeedLog"]
["2019-06-24T20:58:35.900","2019-06-24T16:58:35.900","SH","Sonar","EK",null,"Switching EK to slave, 70 from CW to FM, Interval to Max ping mode"]
["2019-06-24T20:59:04.150","2019-06-24T16:59:04.150","SH","Sonar","EK","Start Pinging","Start Pinging and Recording"]
["2019-06-24T20:59:06.500","2019-06-24T16:59:06.500","SH","Sonar","Knudsen","Start Pinging","Start Pinging and Recording"]
["2019-06-24T20:59:36.800","2019-06-24T16:59:36.800","SH","Sonar","Multibeam","Start Pinging","Start pinging in marine mammal mode -20"]
["2019-06-24T21:01:10.710","2019-06-24T17:01:10.710","SH","Sonar",null,null,"Start recording SMD"]
["2019-06-24T21:09:14.010","2019-06-24T17:09:14.010","DP","Sonar","Multibeam",null,"CPCTD004 applied to 0077"]
["2019-06-24T21:10:00.490","2019-06-24T17:10:00.490","DP","Sonar","Multibeam","Start Pinging","Start Pinging in MAX POWAH"]
["2019-06-24T21:15:18.260","2019-06-24T17:15:18.260","DP","Sonar","Multibeam","Start Logging","Start Logging Multibeam"]
["2019-06-24T21:52:59.930","2019-06-24T17:52:59.930","SH","Sonar","Multibeam","Start Line","Turn line 0078. yaw stabilization off"]
["2019-06-24T21:55:13.750","2019-06-24T17:55:13.750","SH","Sonar","Multibeam","Start Line","End turn line. "]
["2019-06-24T22:21:27.920","2019-06-24T18:21:27.920","SH","Sonar","Multibeam",null,"Start Turn Line 0080"]
["2019-06-24T22:22:44.920","2019-06-24T18:22:44.920","SH","Sonar","Multibeam",null,"Start Survey Line 0081"]
["2019-06-24T22:28:45.620","2019-06-24T18:28:45.620","DP","XBT",null,"XBT Launch","Launch AXBT026"]
["2019-06-24T22:34:41.460",{"$f":"IF(ISBLANK(A199),\" \",((A199)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-24T18:34:41.460"},"DP","Sonar","Multibeam","XBT Applied","AXBT Applied to 0081"]
["2019-06-24T22:40:09","2019-06-24T18:40:09","DP","Sonar","Multibeam",null,"Shifting 300 meters to port to increase overlap with existing data"]
["2019-06-25T00:18:27.460","2019-06-24T20:18:27.460","KJ","Sonar","Multibeam","New Line","0083 turn"]
["2019-06-25T00:21:55.470","2019-06-24T20:21:55.470","KJ","Sonar","Multibeam","Along Direction Pitch","0 to -1"]
["2019-06-25T00:26:54.720","2019-06-24T20:26:54.720","KJ","Sonar","Knudsen","Range","from 200 to 100 m over very flat terrain"]
["2019-06-25T00:35:40.160","2019-06-24T20:35:40.160","DP","Sonar","Multibeam","New Line","Start survey line 0084"]
["2019-06-25T00:38:28.910","2019-06-24T20:38:28.910","KJ","XBT",null,null,"AXBT027 launched"]
["2019-06-25T01:10:23.880","2019-06-24T21:10:23.880","DP","Sonar","Multibeam","XBT Applied","AXBT 027 applied to 0084"]
["2019-06-25T02:25:40.150","2019-06-24T22:25:40.150","KJ","XBT",null,null,"AXBT028 launched"]
["2019-06-25T02:31:02.380","2019-06-24T22:31:02.380","KJ","Sonar","Multibeam","XBT Applied","AXBT028 applied in line 0085"]
["2019-06-25T04:16:53.180","2019-06-25T00:16:53.180","DP","XBT",null,"XBT Launch","Launch AXBT 29"]
["2019-06-25T04:23:12.310","2019-06-25T00:23:12.310","DP","Sonar","Multibeam","XBT Applied","AXBT029 applied in line 0088"]
["2019-06-25T06:10:52.040","2019-06-25T02:10:52.040","DP","XBT",null,"XBT Launch","AXBT030 launched"]
["2019-06-25T06:16:21.090","2019-06-25T02:16:21.090","DP","Sonar","Multibeam","XBT Applied","AXBT030 applied in line 0090"]
["2019-06-25T08:11:40.780","2019-06-25T04:11:40.780","KJ","XBT",null,null,"AXBT031 launched"]
["2019-06-25T08:14:51.830","2019-06-25T04:14:51.830","KJ","Sonar","Multibeam","XBT Applied","AXBT031 applied in line 0092"]
["2019-06-25T09:31:47.890","2019-06-25T05:31:47.890","KJ","XBT",null,null,"AXBT032 launched"]
["2019-06-25T09:37:58.940","2019-06-25T05:37:58.940","KJ","Sonar","Multibeam","XBT Applied","AXBT032 applied in line 0095"]
["2019-06-25T09:55:08.490","2019-06-25T05:55:08.490","KJ","Sonar","All","Secure","on site for drift test; switching POS MV to DP config"]
["2019-06-25T09:55:35.360","2019-06-25T05:55:35.360","KJ","Sonar","EK",null,"70 kHz from FM to CW; all but 38 kHz pinging and logging at dive site"]
["2019-06-25T09:56:18.560","2019-06-25T05:56:18.560","KJ","Sonar","ADCP",null,"started pinging"]
["2019-06-25T09:58:36.370","2019-06-25T05:58:36.370","KJ","Sonar","EK",null,"changed from maximum to interval ping mode; adjusted to 3 sec interval to avoid multiple returns"]
["2019-06-25T18:33:51.810","2019-06-25T14:33:51.810","SH","Ship",null,null,"Pulling up ROV early and heading to Jacksonville to drop off a personnel for medical issue. Will be transit mapping over the next 48 hours."]
["2019-06-25T18:57:48.650","2019-06-25T14:57:48.650","DP","Sonar","ADCP",null,"secure ADCP"]
["2019-06-25T18:58:04.090","2019-06-25T14:58:04.090","SH","POS",null,null,"Change POS settings"]
["2019-06-25T18:58:46.840","2019-06-25T14:58:46.840","SH","Sonar","EK",null,"Switch EK to max ping and CW mode / Stop then Start recording"]
["2019-06-25T18:59:19.480","2019-06-25T14:59:19.480","SH","Sonar","Knudsen","Start Pinging","Knudsen Pinging"]
["2019-06-25T19:00:10.950","2019-06-25T15:00:10.950","SH","Sonar","Multibeam","Start Pinging","Start EM in MMM"]
["2019-06-25T19:00:39.430","2019-06-25T15:00:39.430","SH","Sonar","Knudsen","Start Recording","Start recording Knudsen"]
["2019-06-25T19:05:07.950","2019-06-25T15:05:07.950","SH","Sonar","SpeedLog","secure"]
["2019-06-25T19:06:08.890","2019-06-25T15:06:08.890","SH","Sonar","Multibeam",null,"Brought multibeam up to -10 dB"]
["2019-06-25T19:10:03.550","2019-06-25T15:10:03.550","DP","Sonar","Multibeam",null,"Max Power and CPCTD Up cast loaded in to 0096"]
["2019-06-25T19:27:06.900","2019-06-25T15:27:06.900","DP","Sonar","Multibeam","Start Logging","Start Logging EM302"]
["2019-06-25T22:24:49.450","2019-06-25T18:24:49.450","DP","XBT",null,"XBT Launch","Launch AXBT033"]
["2019-06-25T22:30:42.780","2019-06-25T18:30:42.780","DP","Sonar","Multibeam","XBT Applied","Apply AXBT033 to line 0099"]
["2019-06-25T23:42:40.800","2019-06-25T19:42:40.800","DP","XBT",null,"XBT Launch","Launch AXBT034"]
["2019-06-25T23:48:13.380","2019-06-25T19:48:13.380","DP","Sonar","Multibeam","XBT Applied","Apply AXBT034 to line 0100"]
["2019-06-25T23:57:07.050","2019-06-25T19:57:07.050","KJ","Sonar","Knudsen","Range","Changed from 100 m to 200 m recording range over more variable terrain"]
["2019-06-26T00:45:06.370","2019-06-25T20:45:06.370","KJ","Issue/Problem",null,null,"MBPROC2 frozen; hard restarting"]
["2019-06-26T00:52:31.080","2019-06-25T20:52:31.080","KJ","XBT",null,null,"AXBT035 launched early, lots of refraction crossing the gulf stream"]
["2019-06-26T00:57:07.930","2019-06-25T20:57:07.930","KJ","Sonar","Multibeam",null,"AXBT035 applied in line 101"]
["2019-06-26T01:13:19.770","2019-06-25T21:13:19.770","KJ","Sonar","EK","Pulse Duration Change","changed 18 kHz from 4 ms to 1 ms for seep survey in relatively shallow water (800 m)"]
["2019-06-26T02:30:43.200","2019-06-25T22:30:43.200","KJ","Ship",null,null,"No seeps observed in real time, coming back up to transit speed"]
["2019-06-26T02:32:58.480","2019-06-25T22:32:58.480","KJ","XBT",null,null,"AXBT036 launched near alleged seep site"]
["2019-06-26T02:39:07.220","2019-06-25T22:39:07.220","Kj","Sonar","Multibeam",null,"AXBT036 applied in line 103"]
["2019-06-26T04:06:49.250","2019-06-26T00:06:49.250","DP","XBT",null,"XBT Launch","Launch AXBT037"]
["2019-06-26T04:12:27.250","2019-06-26T00:12:27.250","DP","Sonar","Multibeam","XBT Applied","AXBT037 applied in line 0104"]
["2019-06-26T04:49:42.960","2019-06-26T00:49:42.960","DP","XBT",null,"XBT Launch","Launch AXBT038"]
["2019-06-26T04:54:00.840","2019-06-26T00:54:00.840","DP","Sonar","Multibeam","XBT Applied","AXBT038 Applied in line 0105"]
["2019-06-26T05:12:40.150","2019-06-26T01:12:40.150","KJ","XBT",null,"XBT Launch","AXBT039 launched"]
["2019-06-26T05:17:27.260","2019-06-26T01:17:27.260","DP","Sonar","Multibeam","XBT Applied","AXBT039 applied in line 0105"]
["2019-06-26T05:33:09.180","2019-06-26T01:33:09.180","KJ","XBT",null,"XBT Launch","AXBT040 launched"]
["2019-06-26T05:36:39.540","2019-06-26T01:36:39.540","KJ","Sonar","Multibeam","XBT Applied","AXBT040 applied in line 106"]
["2019-06-26T05:38:33.240","2019-06-26T01:38:33.240","DP","Sonar","Multibeam","Secure","Stop Logging and Pinging EM302"]
["2019-06-26T05:38:37.610","2019-06-26T01:38:53","KJ","Sonar","EK","Secure","Secure EK60"]
["2019-06-26T05:38:55.740","2019-06-26T01:38:55.740","KJ","Sonar","Knudsen","Secure","Secure Knudsen"]
["2019-06-26T05:39:14.950","2019-06-26T01:39:14.950","KJ","Ship",null,null,"inform bridge that multibeam is secure, they can use fathometer, etc."]
["2019-06-26T20:21:52.990","2019-06-26T16:21:52.990","SH","Sonar","Multibeam","Start Logging","Start logging EM at 120m"]
["2019-06-26T20:22:10.810","2019-06-26T16:22:10.810","SH","Sonar","Knudsen","Start Pinging","Start Pinging  "]
["2019-06-26T20:22:44.840","2019-06-26T16:22:44.840","SH","Sonar","EK",null,"18kHz back up to 4ms"]
["2019-06-26T20:24:05.690","2019-06-26T16:24:05.690","SH","Sonar","EK","Start Recording"]
["2019-06-26T20:24:09.880","2019-06-26T16:24:09.880","SH","Sonar","Knudsen","Start Recording"]
["2019-06-26T20:26:36.320","2019-06-26T16:26:36.320","SH","XBT",null,"XBT Launch","AXBT041 Launch"]
["2019-06-26T20:27:26.010","2019-06-26T16:27:26.010","SH","Sonar",null,null,"Start recording SMD"]
["2019-06-26T20:32:04.480",{"$f":"IF(ISBLANK(A263),\" \",((A263)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-26T16:32:04.480"},"SH","Sonar","Multibeam","XBT Applied","Apply AXBT041 in line 0107"]
["2019-06-26T21:32:52.800","2019-06-26T17:32:52.800","DP","XBT",null,"XBT Launch","AXBT042 Launched"]
["2019-06-26T21:36:53.390","2019-06-26T17:36:53.390","DP","Sonar","Multibeam","XBT Applied","Apply AXBT042 In line 0108"]
["2019-06-26T21:40:30.010","2019-06-26T17:40:30.010","DP","Sonar","Multibeam","New Line","Start turn line 0109"]
["2019-06-26T21:44:19.850","2019-06-26T17:44:19.850","DP","Sonar","Multibeam","New Line","Start survey line 0110"]
["2019-06-26T22:28:18.520","2019-06-26T18:28:18.520","DP","Sonar","Multibeam","New Line","Start Turn Line 0111"]
["2019-06-26T22:39:42.150","2019-06-26T18:39:42.150","DP","Sonar","Multibeam","New Line","Start Survey Line 0112 (Lines moved closer together to achieve ideal overlap)"]
["2019-06-26T22:44:45.220","2019-06-26T18:44:45.220","SH","Sonar","Multibeam",null,"Yaw stabilization turned back on"]
["2019-06-26T23:28:36.550","2019-06-26T19:28:36.550","KJ","XBT",null,null,"AXBT043 launched"]
["2019-06-26T23:35:13.020","2019-06-26T19:35:13.020","KJ","Sonar","Multibeam","XBT Applied","AXBT043 applied in line 0112"]
["2019-06-27T00:57:32.610","2019-06-26T20:57:32.610","KJ","XBT",null,null,"AXBT044 launched"]
["2019-06-27T01:02:12.030","2019-06-26T21:02:12.030","KJ","Sonar","Multibeam","XBT Applied","AXBT044 applied in line 0115"]
["2019-06-27T01:07:44.350","2019-06-26T21:07:44.350","KJ","Ship",null,null,"starting slow line plan shift 300 m to port for coverage"]
["2019-06-27T02:27:06.100","2019-06-26T22:27:06.100","SH","Sonar","Multibeam",null,"Changed file for turn and turned off yaw stabilization"]
["2019-06-27T02:54:33.510","2019-06-26T22:54:33.510","DP","XBT",null,"XBT Launch","AXBT045 launched"]
["2019-06-27T02:59:06.660","2019-06-26T22:59:06.660","DP","Sonar","Multibeam","XBT Applied","AXBT045 applied in line 0118"]
["2019-06-27T03:10:13.550","2019-06-26T23:10:13.550","KJ","Ship",null,null,"passing vessel, had slowed down to 3.5 kts for last half hour, now speeding back up and returning to shifted line plan"]
["2019-06-27T03:23:51.440","2019-06-26T23:23:51.440","KJ","Ship",null,null,"moving over 300 m further to west for coverage"]
["2019-06-27T04:49:38.580","2019-06-27T00:49:38.580","KJ","Sonar","Multibeam",null,"Ending gap-filling survey, starting transit to seep survey site at max speed"]
["2019-06-27T04:53:27.900","2019-06-27T00:53:27.900","KJ","XBT",null,"XBT Launch","AXBT046 launched"]
["2019-06-27T04:58:54.270","2019-06-27T00:58:54.270","KJ","Sonar","Multibeam","XBT Applied","AXBT046 applied"]
["2019-06-27T05:27:11.290","2019-06-27T01:27:11.290","KJ","Ship",null,null,"slowing down momentarily for traffic"]
["2019-06-27T06:45:30.520","2019-06-27T02:45:30.520","KJ","Sonar","Knudsen",null,"Range changed from 100 to 200 m"]
["2019-06-27T06:46:00.960","2019-06-27T02:46:00.960","KJ","Sonar","Multibeam","New Line","starting seep survey in line 124"]
["2019-06-27T06:47:48.240","2019-06-27T02:47:48.240","KJ","XBT",null,"XBT Launch","AXBT047 launched"]
["2019-06-27T06:53:11.020","2019-06-27T02:53:11.020","KJ","Sonar","Multibeam","XBT Applied","AXBT047 applied in line 124"]
["2019-06-27T07:00:25.050","2019-06-27T03:00:25.050","KJ","Sonar","EK","Pulse Duration Change","18 kHz from 4 ms to 1 ms"]
["2019-06-27T08:04:02.340","2019-06-27T04:04:02.340","KJ","XBT",null,null,"AXBT048 launched"]
["2019-06-27T08:12:45.600","2019-06-27T04:12:45.600","KJ","Sonar","Multibeam","XBT Applied","AXBT048 applied in line 0126"]
["2019-06-27T08:15:33.730","2019-06-27T04:15:33.730","KJ",null,null,null,"extremely thin / faint WC targets in stbd multibeam swath, worth checking in FM Midwater"]
["2019-06-27T09:31:43.610","2019-06-27T05:31:43.610","KJ","XBT",null,"XBT Launch","AXBT049 launched"]
["2019-06-27T09:37:37.330","2019-06-27T05:37:37.330","KJ","Sonar","Multibeam","XBT Applied","AXBT049 applied in line 0128"]
["2019-06-27T09:56:09.090","2019-06-27T05:56:09.090","KJ","Sonar","All",null,"Arriving on dive site; EM and Knudsen secure; ADCPs on; EKs all 1 ms CW"]
["2019-06-27T10:04:25.950","2019-06-27T06:04:25.950","KJ","Sonar","EK",null,"changed interval from max to 3 sec to reduce multiple returns"]
["2019-06-27T11:00:16.990","2019-06-27T07:00:16.990","KJ","Issue/Problem",null,null,"MBPROC1 frozen; hard restarting"]
["2019-06-27T12:17:14.580","2019-06-27T08:17:14.580","SH","Sonar","EK",null,"Reset 18 to 4ms and 70 to 2 ms"]
["2019-06-27T19:04:34.500","2019-06-27T15:04:34.500","SH","Sonar","EK",null,"Stop Recording. Install 38 kHz. Set Ping Mode to maximum"]
["2019-06-27T19:12:01.460","2019-06-27T15:12:01.460","SH","Sonar","EK",null,"Start Pinging 38 kHz"]
["2019-06-27T19:25:24.400","2019-06-27T15:25:24.400","SH","Sonar","EK",null,"Stop Pinging 38 KHz"]
["2019-06-27T19:26:07.250","2019-06-27T15:26:07.250","SH","Sonar","EK",null,"Uninstalled 38 kHz."]
["2019-06-27T19:29:37.910","2019-06-27T15:29:37.910","SH","Sonar","EK",null,"Set to Midwater Mode. 18 = 1.024 ms, 2000 W. 70 = 1.024ms, 750 W, CW. 120 = 1.024 ms, 250 W,  200 = 1.024 ms, 150 W."]
["2019-06-27T19:34:14.430","2019-06-27T15:34:14.430","SH","Sonar","EK",null,"Set range recording to Manual: 2000m"]
["2019-06-27T19:35:51.820","2019-06-27T15:35:51.820","SH","Sonar","EK",null,"Set range recording to Manual: 1500m"]
["2019-06-27T19:36:50.060","2019-06-27T15:36:50.060","SH","Sonar","SpeedLog","secure"]
["2019-06-27T19:38:18.830","2019-06-27T15:38:18.830","SH","Sonar","EK","Start Pinging"]
["2019-06-27T19:39:12.190","2019-06-27T15:39:12.190","SH","Sonar","EK","Start Recording"]
["2019-06-27T19:53:53.850","2019-06-27T15:53:53.850","SH","Sonar","EK",null,"set minimum bottom detection on EK 18 to 500 meters in hopes to improve bottom track with USBL noise"]
[null," ","SH","Sonar","SpeedLog","Start","Start Pinging (22:18)"]
["2019-06-27T22:27:26.570","2019-06-27T18:27:26.570","SH","Sonar","EK",null,"Midwater Transects ended. Switching to normal ops. "]
["2019-06-27T22:28:05.990","2019-06-27T18:28:05.990","SH","Sonar","EK","Stop Recording","Stop Pinging and Recording"]
["2019-06-27T22:29:31.090","2019-06-27T18:29:31.090","SH","Sonar","EK",null,"Start Pinging in \"normal\" pulse lengths"]
["2019-06-27T22:30:42.430","2019-06-27T18:30:42.430","SH","Sonar","EK","Start Recording","Start Recording"]
["2019-06-27T22:32:01.530","2019-06-27T18:32:01.530","SH","Sonar","EK",null,"Output range set to AUTO"]
["2019-06-27T23:12:24.790","2019-06-27T19:12:24.790","SH","POS",null,null,"Change to mapping config"]
["2019-06-27T23:12:38.550","2019-06-27T19:12:38.550","DP","Sonar","ADCP","secure","Secure"]
["2019-06-27T23:13:07.960","2019-06-27T19:13:07.960","SH","Sonar","Knudsen","Start Pinging","Start Pinging and recording"]
["2019-06-27T23:13:43.010","2019-06-27T19:13:43.010","SH","Sonar","Multibeam","Start Pinging","Start Pinging in MMP"]
["2019-06-27T23:21:50.940","2019-06-27T19:21:50.940","DP","Sonar","SpeedLog","secure","Secure Speed Log"]
["2019-06-27T23:24:03.180","2019-06-27T19:24:03.180","DP","Sonar","Multibeam",null,"Apply ROV CTD Down Cast in line 0129"]
["2019-06-27T23:24:12.460","2019-06-27T19:24:12.460","DP","Sonar","Multibeam",null,"Start Pinging in Full Power"]
["2019-06-27T23:48:21.380","2019-06-27T19:48:21.380","DP","Sonar","Multibeam","Start Logging","Start Logging"]
["2019-06-28T00:09:29.840","2019-06-27T20:09:29.840","KJ","Sonar","EK",null,"Changed 70 kHz from CW to FM, 45-90 kHz, maintaining 2 ms at full power"]
["2019-06-28T00:28:02.980","2019-06-27T20:28:02.980","SH","Sonar",null,"Start Logging","Started Logging SMD"]
["2019-06-28T00:42:31.380","2019-06-27T20:42:31.380","KJ","Sonar","Multibeam","New Line","0130 start survey transit"]
["2019-06-28T01:38:33.680",{"$f":"IF(ISBLANK(A327),\" \",((A327)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-27T21:38:33.680"},"KJ","Sonar","Multibeam","New Line","0131 start turn line"]
["2019-06-28T01:43:59.580","2019-06-27T21:43:59.580","DP","XBT",null,"XBT Launch","AXBT050 launched"]
["2019-06-28T01:48:38.380","2019-06-27T21:48:38.380","DP","Sonar","Multibeam","XBT Applied","AXBT050 applied to line 131"]
["2019-06-28T03:58:01.080","2019-06-27T23:58:01.080","DP","XBT",null,"XBT Launch","AXBT051 launched"]
["2019-06-28T03:58:24.380","2019-06-27T23:58:24.380","KJ","Sonar","Multibeam","XBT Applied","AXBT051 applied in line 0134"]
["2019-06-28T05:35:49.780","2019-06-28T01:35:49.780","DP","XBT",null,"XBT Launch","AXBT052 launched"]
["2019-06-28T05:41:17.590","2019-06-28T01:41:17.590","DP","Sonar","Multibeam","XBT Applied","AXBT052 applied in line 136"]
["2019-06-28T08:19:27.990","2019-06-28T04:19:27.990","KJ","XBT",null,"XBT Launch","AXBT053 launched"]
["2019-06-28T08:25:09.700","2019-06-28T04:25:09.700","KJ","Sonar","Multibeam","XBT Applied","AXBT053 applied in line 140"]
["2019-06-28T08:26:45.550","2019-06-28T04:26:45.550","KJ","Ship",null,null,"we will be skipping the small dogleg to port in the line plan in order to arrive on site with time for a brief, slow pass over with the multibeam"]
["2019-06-28T08:53:14.940","2019-06-28T04:53:14.940","KJ","Sonar","Multibeam",null,"start of RESTRICTED data, new file 0141"]
["2019-06-28T08:54:48.330","2019-06-28T04:54:48.330","KJ","Sonar","EK",null,"start of RESTRICTED data, new file D20190628-T05616"]
["2019-06-28T09:02:04.420","2019-06-28T05:02:04.420","KJ","Sonar","Knudsen",null,"start of RESTRICTED data, new file 0077_2019_179_0854"]
["2019-06-28T09:02:18.010","2019-06-28T05:02:18.010","KJ","Ship",null,null,"securing AIS transmission"]
["2019-06-28T09:33:37.760","2019-06-28T05:33:37.760","KJ","XBT",null,"XBT Launch","AXBT054 launched"]
["2019-06-28T09:42:25.640","2019-06-28T05:42:25.640","KJ","Sonar","Multibeam","XBT Applied","AXBT054 aplied in line 0142"]
["2019-06-28T09:48:19.170","2019-06-28T05:48:19.170","KJ","Sonar","Multibeam",null,"changed penetration filter from weak to medium"]
["2019-06-28T10:00:36.910","2019-06-28T06:00:36.910","KJ","Sonar","All","Secure","arriving on site for drift test with speed log on; MB last file before drift test is 0142"]
["2019-06-28T10:03:39.170","2019-06-28T06:03:39.170","KJ","Sonar","EK",null,"EK 70 kHz from FM to CW, still 2 ms at full power; interval changed from maximum to 2 sec to avoid multiple returns; bottom detection max range set to 750 m"]
["2019-06-28T20:49:12.830","2019-06-28T16:49:12.830","DP","Ship",null,null,"No shipwreck found, no files partitioned"]
["2019-06-28T21:21:45.460","2019-06-28T17:21:45.460","DP","POS",null,null,"Switch to mapping config"]
["2019-06-28T21:22:11.680","2019-06-28T17:22:11.680","DP","Sonar","ADCP","secure","Secure ADCP"]
["2019-06-28T21:22:19.540","2019-06-28T17:22:19.540","SH","Sonar","EK",null,"Changing interval to max, stop recording to switch from CW to FM then start recording again"]
["2019-06-28T21:23:08.710","2019-06-28T17:23:08.710","SH","Sonar","Knudsen","Start Pinging"]
["2019-06-28T21:23:39.190","2019-06-28T17:23:39.190","SH","Sonar","Knudsen","Start Recording"]
["2019-06-28T21:24:08.620","2019-06-28T17:24:08.620","SH","Sonar","SpeedLog","secure","Secure Speedlog"]
["2019-06-28T21:25:39.080","2019-06-28T17:25:39.080","SH","Sonar","Multibeam","Start Pinging","Pinging in MMP"]
["2019-06-28T21:31:44.010","2019-06-28T17:31:44.010","SH","Sonar","Multibeam","Start Pinging","Pinging in full power"]
["2019-06-28T21:37:27.750","2019-06-28T17:37:27.750","DP","Sonar","Multibeam",null,"Apply CP CTD UP cast in line 0143"]
["2019-06-28T22:06:10.340","2019-06-28T18:06:10.340","DP","Sonar","Multibeam","Start Logging"]
["2019-06-28T22:12:22.790","2019-06-28T18:12:22.790","DP","Sonar",null,null,"Start logging SMD"]
["2019-06-28T23:32:41.590","2019-06-28T19:32:41.590","KJ","Sonar","All",null,"moved data from RESTRICTED folders to regular raw data folders after confirming non-UCH dive site"]
["2019-06-28T23:33:21.430","2019-06-28T19:33:21.430","KJ","XBT",null,"XBT Launch","AXBT055 launched"]
["2019-06-28T23:38:00.420","2019-06-28T19:38:00.420","KJ","Issue/Problem",null,null,"SSM crash during import of AXBT055; fix was to switch the profile direction (under input settings) from 'up' (used for CTD processing earlier) back to 'down' for XBT processing"]
["2019-06-28T23:43:06.380","2019-06-28T19:43:06.380","KJ","Sonar","Multibeam","XBT Applied","AXBT055 applied in line 144"]
["2019-06-29T01:43:35.770","2019-06-28T21:43:35.770","DP","XBT",null,"XBT Launch","AXBT056 launched"]
["2019-06-29T01:49:11.390","2019-06-28T21:49:11.390","DP","Sonar","Multibeam","XBT Applied","AXBT056 applied in line 0146"]
["2019-06-29T02:55:36.310","2019-06-28T22:55:36.310","DP","Sonar","Multibeam","New Line","Start turn line 0148"]
["2019-06-29T03:04:24.990","2019-06-28T23:04:24.990","DP","Sonar","Multibeam","New Line","Start survey line 0149"]
["2019-06-29T03:31:44.080","2019-06-28T23:31:44.080","DP","XBT",null,"XBT Launch","AXBT057 launched"]
["2019-06-29T03:38:02.390","2019-06-28T23:38:02.390","DP","Sonar","Multibeam","XBT Applied","AXBT057 applied in line 0149"]
["2019-06-29T03:58:54.080","2019-06-28T23:58:54.080","DP","Sonar","Multibeam","New Line","Start turn line 0150"]
["2019-06-29T04:11:16.640","2019-06-29T00:11:16.640","DP","Sonar","Multibeam","New Line","Start survey line 0151"]
["2019-06-29T04:20:31.600","2019-06-29T00:20:31.600","KJ","Ship",null,null,"Adjusting line plan 300 m to port"]
["2019-06-29T05:44:44.350","2019-06-29T01:44:44.350","KJ","XBT",null,"XBT Launch","AXBT058 launched"]
["2019-06-29T05:56:27.010","2019-06-29T01:56:27.010","KJ","Sonar","Multibeam","XBT Applied","AXBT058 applied in line 153"]
["2019-06-29T07:41:17.640","2019-06-29T03:41:17.640","KJ","XBT",null,"XBT Launch","AXBT059 launched"]
["2019-06-29T07:49:31.040","2019-06-29T03:49:31.040","KJ","Sonar","Multibeam","XBT Applied","AXBT059 applied in line 0157"]
["2019-06-29T09:42:47.230","2019-06-29T05:42:47.230","KJ","XBT",null,"XBT Launch","AXBT060 launched"]
["2019-06-29T09:48:46.260","2019-06-29T05:48:46.260","KJ","Sonar","Multibeam","XBT Applied","AXBT060 applied in line 159"]
["2019-06-29T10:01:18.570","2019-06-29T06:01:18.570","KJ","Sonar","All","Secure"]
["2019-06-29T10:02:42.920","2019-06-29T06:02:42.920","KJ","Sonar","EK","2019-07-05T21:07:17.360","EK 70 kHz from FM to CW, still 2 ms at full power; interval changed from maximum to 2 sec to avoid multiple returns; bottom detection max range set to 1200 m"]
["2019-06-29T18:35:35.300","2019-06-29T14:35:35.300","SH","Sonar","EK","Stop Recording","Stop Pinging. Stop Recording. Install 38 kHz"]
["2019-06-29T18:39:52.370","2019-06-29T14:39:52.370","SH","Sonar","EK","Start Pinging","EK 38 kHz"]
["2019-06-29T18:40:34.480","2019-06-29T14:40:34.480","SH","Sonar","SpeedLog","Secure"]
["2019-06-29T18:44:29.730","2019-06-29T14:44:29.730","SH","Sonar","EK",null,"Stop pinging uninstall 38 kHz"]
["2019-06-29T18:46:38.840","2019-06-29T14:46:38.840","SH","Sonar","EK","Start Recording","Set up for MidWater Transects. 1 ms pulse on all frequencies. Range recording set to 2000. ping mode set to maximum."]
["2019-06-29T18:55:49.880","2019-06-29T14:55:49.880","SH","Sonar","EK",null,"Change Ping Mode to Interval: 1000 ms"]
["2019-06-29T18:59:07.640","2019-06-29T14:59:07.640","SH","Sonar","EK",null,"Split File to account for ping interval"]
["2019-06-29T18:59:25.740","2019-06-29T14:59:25.740","SH","Sonar","EK",null,"Change bottom detection to min 800 to try to limit USBL bottom pics"]
["2019-06-29T19:01:25.220","2019-06-29T15:01:25.220","SH","Sonar","EK",null,"change ping mode to maximum. Split file."]
["2019-06-29T19:03:13.740","2019-06-29T15:03:13.740","SH","Sonar","EK",null,"change ping interval back to 1000 ms and split file"]
["2019-06-29T19:04:52.020","2019-06-29T15:04:52.020","SH","Sonar","EK",null,"Set bottom range to 1000 and ping interval to maximum"]
["2019-06-29T19:10:26.250","2019-06-29T15:10:26.250","SH","Sonar","EK",null,"Set bottom range to 2000 and ping to 1000 ms"]
["2019-06-29T20:23:55.230",{"$f":"IF(ISBLANK(A391),\" \",((A391)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-29T16:23:55.230"},"SH","Sonar","EK",null,"Change back to normal mapping mode. Range = Auto. 18 and 70 kHz back to 4 and 2 ms. 70 set to FM"]
["2019-06-29T20:25:38.120","2019-06-29T16:25:38.120","SH","Sonar","EK","Start Recording"]
["2019-06-29T20:31:11.250","2019-06-29T16:31:11.250","SH","Sonar","EK",null,"Change 70 to CW due to EM 302 FM interference"]
["2019-06-29T20:47:42.730","2019-06-29T16:47:42.730","SH","POS",null,null,"Change to mapping config"]
["2019-06-29T20:48:15.220","2019-06-29T16:48:15.220","DP","Sonar","ADCP","secure","Secure ADCP"]
["2019-06-29T20:48:17.720","2019-06-29T16:48:17.720","SH","Sonar","Multibeam","Start Pinging","Start Pinging in MMP"]
["2019-06-29T20:49:32","2019-06-29T16:49:32","SH","Sonar","EK","Start Recording","Start recording"]
["2019-06-29T20:49:44.570","2019-06-29T16:49:44.570","SH","Sonar","Knudsen","Start Pinging","Started pinging and recording"]
["2019-06-29T20:57:16.750","2019-06-29T16:57:16.750","DP","Sonar","Multibeam",null,"Pinging in full power"]
["2019-06-29T20:57:50.300","2019-06-29T16:57:50.300","DP","Sonar","Multibeam",null,"Apply ROV CTD Down Cast 08 in line 0160"]
["2019-06-29T21:06:12.050","2019-06-29T17:06:12.050","SH","Sonar","SpeedLog","secure"]
["2019-06-29T21:14:48.660","2019-06-29T17:14:48.660","SH","Sonar","Multibeam","Start Logging"]
["2019-06-29T21:57:57.930","2019-06-29T17:57:57.930","DP","Sonar","Multibeam","New Line","Start turn line 0161"]
["2019-06-29T22:10:34.700","2019-06-29T18:10:34.700","DP","Sonar","Multibeam","New Line","Start survey line 0162"]
["2019-06-29T22:13:04.600","2019-06-29T18:13:04.600","DP","XBT",null,"XBT Launch","AXBT061 launched"]
["2019-06-29T22:18:42.910","2019-06-29T18:18:42.910","DP","Sonar","Multibeam","XBT Applied","AXBT061 applied in line 0162"]
["2019-06-29T23:40:42.500","2019-06-29T19:40:42.500","SH","Sonar","Multibeam",null,"Turn Line 0164"]
["2019-06-30T00:21:17.200","2019-06-29T20:21:17.200","KJ","XBT",null,"XBT Launch","AXBT062 launched"]
["2019-06-30T00:27:51.570","2019-06-29T20:27:51.570","KJ","Sonar","Multibeam","XBT Applied","AXBT062 applied in line 0165"]
["2019-06-30T00:38:41.810","2019-06-29T20:38:41.810","KJ","Ship",null,null,"slowing down from transit speed to 9 kt for edge matching survey"]
["2019-06-30T01:17:31.580","2019-06-29T21:17:31.580","KJ","Ship",null,null,"shifting line plan 300 m to port for coverage"]
["2019-06-30T02:15:58.300","2019-06-29T22:15:58.300","DP","XBT",null,"XBT Launch","AXBT063 launched"]
["2019-06-30T02:24:07.770","2019-06-29T22:24:07.770","DP","Sonar","Multibeam","XBT Applied","AXBT063 applied in line 0167"]
["2019-06-30T03:26:31.080","2019-06-29T23:26:31.080","KJ","Sonar","Multibeam",null,"interference causing strong 'railroad track' artifact, bridge confirmed no echosounders active; TX tilt adjusted to -2 and penetration filter adjusted from medium to weak to balance out these two issues over soft sediment"]
["2019-06-30T04:23:39.480","2019-06-30T00:23:39.480","KJ","XBT",null,"XBT Launch","attempted to launch AXBT064 from tube 2, but no launch detected; launched successfully from tube 3"]
["2019-06-30T04:32:54.070","2019-06-30T00:32:54.070","KJ","Sonar","Multibeam","XBT Applied","AXBT064 applied in line 169"]
["2019-06-30T06:37:59.400","2019-06-30T02:37:59.400","KJ","XBT",null,"XBT Launch","AXBT065"]
["2019-06-30T06:44:28.060","2019-06-30T02:44:28.060","KJ","Sonar","Multibeam","XBT Applied","AXBT065 applied in line 173"]
["2019-06-30T08:31:33.890","2019-06-30T04:31:33.890","KJ","Ship",null,null,"slowing to 6 kts for on time arrival"]
["2019-06-30T09:02:02.210","2019-06-30T05:02:02.210","KJ","XBT",null,"XBT Launch","AXBT066 launched"]
["2019-06-30T09:08:17.990","2019-06-30T05:08:17.990","KJ","Sonar","Multibeam","XBT Applied","AXBT066 applied in line 176"]
["2019-06-30T09:55:45.940","2019-06-30T05:55:45.940","SH","Sonar","Multibeam","New Line","Start Trun Line 0179. Yaw stabilization OFF"]
["2019-06-30T10:03:38.380","2019-06-30T06:03:38.380","SH","Sonar","Multibeam",null,"stop pinging. Arrived at dive site"]
["2019-06-30T10:04:28.580","2019-06-30T06:04:28.580","SH","Sonar","SpeedLog","Secure"]
["2019-06-30T10:05:48.560","2019-06-30T06:05:48.560","SH","Sonar","ADCP","Start Pinging"]
["2019-06-30T10:06:14.420","2019-06-30T06:06:14.420","SH","POS",null,null,"Change config to ROV"]
["2019-06-30T10:07:25.010","2019-06-30T06:07:25.010","SH","Sonar","Knudsen","Stop Recording"]
["2019-06-30T19:25:46.300","2019-06-30T15:25:46.300","SH","Sonar","EK","Stop Recording","Stop recordinga and setting up for midwater transects"]
["2019-06-30T19:27:24.710","2019-06-30T15:27:24.710","SH","Sonar","EK",null,"Install 38 kHz"]
["2019-06-30T19:29:24.290","2019-06-30T15:29:24.290","SH","Sonar","EK","Start Pinging","Start Pinging 38 kHz"]
["2019-06-30T19:35:48.380","2019-06-30T15:35:48.380","SH","Sonar","EK",null,"Stop Pinging and Uninstall 38 kHz"]
["2019-06-30T19:46:17.970","2019-06-30T15:46:17.970","SH","Sonar","EK","Start Recording","Start recording in midwater mode. Range = 2000m. Ping Rate = Interval (2000 ms) - minimizing bottom multiple. All frequencies set to 1 ms pulse and max power. Bottom detection gates tight to improve bottom tracking with USBL"]
["2019-06-30T22:42:14.190","2019-06-30T18:42:14.190","SH","Sonar","EK","Stop Recording","Putting back to 'normal' mode. End of midwater transects. Range = AUTO. 18 = 4 ms, 70 = 2 ms. Ping Mode = MAXIMUM"]
["2019-06-30T22:44:03.850","2019-06-30T18:44:03.850","SH","Sonar","EK","Start Recording"]
["2019-06-30T22:48:05.750","2019-06-30T18:48:05.750","DP","POS",null,null,"Change to mapping config"]
["2019-06-30T22:48:14.160","2019-06-30T18:48:14.160","DP","Sonar","ADCP","secure"]
["2019-06-30T22:48:36.390","2019-06-30T18:48:36.390","KJ","Sonar","Knudsen","Start Pinging"]
["2019-06-30T22:49:19.250","2019-06-30T18:49:19.250","KJ","Sonar","Knudsen","Start Recording"]
["2019-06-30T22:50:14.110","2019-06-30T18:50:14.110","KJ","Sonar","Multibeam","Start Pinging","In MMP"]
["2019-06-30T22:51:45.360","2019-06-30T18:51:45.360","KJ","Sonar","Multibeam",null,"Restart SIS, start pinging at -20 dB"]
["2019-06-30T22:54:52.340","2019-06-30T18:54:52.340","SH","Sonar",null,null,"Start logging SMD"]
["2019-06-30T22:55:35.630","2019-06-30T18:55:35.630","DP","Sonar","SpeedLog","secure"]
["2019-06-30T23:02:48.380","2019-06-30T19:02:48.380","DP","Sonar","Multibeam",null,"Apply ROV CTD Down Cast in line 0180"]
["2019-06-30T23:06:18.830","2019-06-30T19:06:18.830","KJ","Sonar","Multibeam",null,"TX power to -10 dB"]
["2019-06-30T23:10:06.970","2019-06-30T19:10:06.970","KJ","Sonar","Multibeam",null,"TX power to max"]
["2019-06-30T23:11:04.350","2019-06-30T19:11:04.350","KJ","Sonar","Multibeam","Start Logging","Start Logging line 0180"]
["2019-07-01T00:27:30.480","2019-06-30T20:27:30.480","KJ","XBT",null,"XBT Launch","AXBT066 launched"]
["2019-07-01T00:35:52.170","2019-06-30T20:35:52.170","KJ","Sonar","Multibeam","XBT Applied","AXBT067 applied in line 0181"]
["2019-07-01T00:45:42.540","2019-06-30T20:45:42.540","KJ","Issue/Problem",null,null,"MBPROC1 keyboard not responding on any KVM; Roland is troubleshooting; previously required restart of MBPROC machine"]
["2019-07-01T02:26:10.910","2019-06-30T22:26:10.910","DP","XBT",null,"XBT Launch","AXBT 068 Launched"]
["2019-07-01T02:32:09.050","2019-06-30T22:32:09.050","DP","Sonar","Multibeam","XBT Applied","AXBT068 applied in line 0183"]
["2019-07-01T03:11:57.700","2019-06-30T23:11:57.700","DP","Sonar","Multibeam","New Line","Start Turn line 0185"]
["2019-07-01T03:16:14.510","2019-06-30T23:16:14.510","DP","Sonar","Multibeam","New Line","Start Survey line 0186"]
["2019-07-01T03:24:42.090","2019-06-30T23:24:42.090","KJ","XBT",null,"XBT Launch","AXBT069 launched"]
["2019-07-01T03:30:18.490",{"$f":"IF(ISBLANK(A455),\" \",((A455)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-06-30T23:30:18.490"},"KJ","Sonar","Multibeam","XBT Applied","AXBT069 applied in line 186"]
["2019-07-01T04:18:21.830","2019-07-01T00:18:21.830","KJ","Sonar","EK",null,"Changed 70 kHz from CW to FM, 45-90 kHz, maintaining 2 ms at full power"]
["2019-07-01T04:27:16.480","2019-07-01T00:27:16.480","KJ","Sonar","EK",null,"started logging (had secured logging for the change from CW to FM)"]
["2019-07-01T04:40:01.770","2019-07-01T00:40:01.770","KJ","XBT",null,"XBT Launch","AXBT070 launched"]
["2019-07-01T04:44:04.870","2019-07-01T00:44:04.870","KJ","Sonar",null,"XBT Applied","AXBT070 applied in line 0188"]
["2019-07-01T05:39:47.250","2019-07-01T01:39:47.250","DP","Sonar","Multibeam","New Line","Start turn line 0190"]
["2019-07-01T05:50:45.540","2019-07-01T01:50:45.540","DP","Sonar","Multibeam","New Line","Start survey line 0191"]
["2019-07-01T06:02:12.580","2019-07-01T02:02:12.580","KJ","XBT",null,"XBT Launch","AXBT071"]
["2019-07-01T06:07:47.010","2019-07-01T02:07:47.010","KJ","Sonar","Multibeam","XBT Applied","AXBT071 applied in line 191"]
["2019-07-01T06:35:54.690","2019-07-01T02:35:54.690","KJ","Sonar","Multibeam","New Line","Start turn line 0192"]
["2019-07-01T06:43:27.330","2019-07-01T02:43:27.330","KJ","Sonar","Multibeam","New Line","Start Survey Line 0193"]
["2019-07-01T07:18:56.080","2019-07-01T03:18:56.080","KJ","XBT",null,"XBT Launch","AXBT072"]
["2019-07-01T07:23:51.600","2019-07-01T03:23:51.600","KJ","Sonar","Multibeam","XBT Applied","AXBT072 applied in line 193"]
["2019-07-01T08:58:31.430","2019-07-01T04:58:31.430","SH","XBT",null,"XBT Launch","AXBT073 "]
["2019-07-01T09:10:32.080","2019-07-01T05:10:32.080","SH","Sonar","Multibeam","XBT Applied","AXBT073 applied to line 0196"]
["2019-07-01T09:47:49.700","2019-07-01T05:47:49.700","SH","Sonar","Multibeam",null,"stop pinging. Arrived at dive site"]
["2019-07-01T09:48:46.720","2019-07-01T05:48:46.720","SH","Sonar","Knudsen",null,"stop pinging and recording"]
["2019-07-01T09:49:28.990","2019-07-01T05:49:28.990","SH","Sonar","EK",null,"stop pinging and recording. Switch 70 to CW for dive.switched ping mode to interval = 2000ms to remove bottom multiple"]
["2019-07-01T09:51:00.450","2019-07-01T05:51:00.450","SH","Sonar","EK",null,"Start Recording"]
["2019-07-01T09:51:30.050","2019-07-01T05:51:30.050","SH","Sonar","ADCP","start pinging"]
["2019-07-01T09:56:13.600","2019-07-01T05:56:13.600","SH","POS",null,null,"Switched Pos Configuration"]
["2019-07-01T09:59:13.980","2019-07-01T05:59:13.980","SH","Sonar","SpeedLog","Start"]
["2019-07-01T20:56:00","2019-07-01T16:56:00","DP","Sonar","ADCP","secure","ADCP Secure"]
["2019-07-01T20:56:00","2019-07-01T16:56:00","DP","POS",null,null,"POS Config swapped to mapping"]
["2019-07-01T20:57:00","2019-07-01T16:57:00","DP","Sonar","Knudsen","Start Pinging","Start Pinging and recording Knudsen"]
["2019-07-01T20:58:00","2019-07-01T16:58:00","DP","Sonar","Multibeam","Start Pinging","Start Pinging in MMP"]
["2019-07-01T21:02:00","2019-07-01T17:02:00","KJ","Sonar","SpeedLog","secure","Secure Speedlog"]
["2019-07-01T21:03:00","2019-07-01T17:03:00","KJ","Sonar","Multibeam",null,"CPCTD UP Cast 10 applied in line 0198"]
["2019-07-01T21:08:00","2019-07-01T17:08:00","KJ","Sonar","Multibeam",null,"TX Max Power"]
["2019-07-01T21:12:00","2019-07-01T17:12:00","KJ","Sonar","Multibeam","Start Logging","Start Logging"]
["2019-07-01T21:48:32.760",{"$f":"IF(ISBLANK(A485),\" \",((A485)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-01T17:48:32.760"},"DP","Sonar","Multibeam","New Line","Line 0199"]
["2019-07-01T22:10:57.960","2019-07-01T18:10:57.960","KJ","Sonar","Multibeam","New Line","Start turn line 0200"]
["2019-07-01T22:20:56.570","2019-07-01T18:20:56.570","KJ","Sonar","Multibeam","New Line","Start survey line 0201"]
["2019-07-01T23:14:28.520","2019-07-01T19:14:28.520","KJ","XBT",null,"XBT Launch","AXBT074 launched"]
["2019-07-01T23:18:59.800","2019-07-01T19:18:59.800","DP","Sonar","Multibeam","XBT Applied","AXBT074 applied in 0204"]
["2019-07-01T23:33:07.240","2019-07-01T19:33:07.240","SH","Sonar","EK",null,"SVP Probe appled to Transducer Face enviornment in EK software. "]
["2019-07-01T23:39:39.220","2019-07-01T19:39:39.220","SH","Sonar","EK",null,"Changed Watercolumn Sound Speed to 1500 m/s"]
["2019-07-02T00:26:03.570","2019-07-01T20:26:03.570","KJ","Sonar","Multibeam","New Line","Start turn line 0206"]
["2019-07-02T00:29:27.880","2019-07-01T20:29:27.880","KJ","XBT",null,"XBT Launch","AXBT075 launched"]
["2019-07-02T00:32:42.300","2019-07-01T20:32:42.300","KJ","Sonar","Multibeam","XBT Applied","AXBT075 applied in line 0206"]
["2019-07-02T00:39:41.510","2019-07-01T20:39:41.510","KJ","Sonar","Multibeam","New Line","Start survey line 0207"]
["2019-07-02T01:55:32.590","2019-07-01T21:55:32.590","KJ","XBT",null,"XBT Launch","AXBT076"]
["2019-07-02T02:01:01.410","2019-07-01T22:01:01.410","KJ","Sonar","Multibeam","XBT Applied","AXBT076 applied in line 208"]
["2019-07-02T02:14:38.180","2019-07-01T22:14:38.180","DP","Sonar","Multibeam","New Line","Start Turn Line 0209"]
["2019-07-02T02:27:11.950","2019-07-01T22:27:11.950","DP","Sonar","Multibeam","New Line","Start Survey Line 0210"]
["2019-07-02T03:35:41.960","2019-07-01T23:35:41.960","DP","XBT",null,"XBT Launch","AXBT077 launched"]
["2019-07-02T03:41:26.190","2019-07-01T23:41:26.190","DP","Sonar","Multibeam","XBT Applied","AXBT077 applied in line 0211"]
["2019-07-02T03:44:52.070","2019-07-01T23:44:52.070","DP","Sonar","Multibeam","New Line","Start turn line 0212"]
["2019-07-02T04:00:13.310","2019-07-02T00:00:13.310","DP","Sonar","Multibeam","New Line","Start survey line 0213"]
["2019-07-02T05:32:25.170","2019-07-02T01:32:25.170","DP","Sonar","Multibeam","New Line","Start Turn Line 0215"]
["2019-07-02T05:40:34.720","2019-07-02T01:40:34.720","DP","XBT",null,"XBT Launch","AXBT078 launched"]
["2019-07-02T05:43:59.230","2019-07-02T01:43:59.230","DP","Sonar","Multibeam","XBT Applied","AXBT078 applied in line 0215"]
["2019-07-02T05:45:23.050","2019-07-02T01:45:23.050","DP","Sonar","Multibeam","New Line","Start survey line 0216"]
["2019-07-02T07:06:23.090","2019-07-02T03:06:23.090","KJ","XBT",null,"XBT Launch","AXBT079 launched"]
["2019-07-02T07:10:24.070","2019-07-02T03:10:24.070","KJ","Sonar","Multibeam","XBT Applied","AXBT079 applied in line 217"]
["2019-07-02T07:15:56.660","2019-07-02T03:15:56.660","KJ","Issue/Problem",null,null,"Qimera froze while filtering and updating surface; required hard restart"]
["2019-07-02T08:46:08.730","2019-07-02T04:46:08.730","KJ","XBT",null,"XBT Launch","AXBT080 launched"]
["2019-07-02T08:54:26.490","2019-07-02T04:54:26.490","KJ","Sonar","Multibeam","XBT Applied","AXBT080 applied in line 219"]
["2019-07-02T09:24:31.940","2019-07-02T05:24:31.940","SH","Sonar","All",null,"increase line for turn"]
["2019-07-02T09:42:54.760","2019-07-02T05:42:54.760","SH","Sonar","Multibeam","Secure","Arriving at dive site"]
["2019-07-02T09:44:13.140","2019-07-02T05:44:13.140","SH","Sonar","ADCP","start pinging"]
["2019-07-02T09:44:25.550","2019-07-02T05:44:25.550","SH","Sonar","SpeedLog","Start"]
["2019-07-02T09:44:43.950","2019-07-02T05:44:43.950","SH","POS",null,null,"Switch Pos Configuration"]
["2019-07-02T09:46:31.820","2019-07-02T05:46:31.820","SH","Sonar","Knudsen","Stop Recording","Stop pingin and reording"]
["2019-07-02T09:47:34.620",{"$f":"IF(ISBLANK(A519),\" \",((A519)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-02T05:47:34.620"},"SH","Sonar","EK",null,"70 set to CW. Ping Mode = Interval 1000 ms"]
["2019-07-02T12:36:22.490","2019-07-02T08:36:22.490","SH","Sonar","ADCP","secure","Now transiting to Deep Pamlico and mapping. Currents too strong"]
["2019-07-02T12:36:53.580","2019-07-02T08:36:53.580","SH","Sonar","SpeedLog","secure"]
["2019-07-02T12:37:18.230","2019-07-02T08:37:18.230","SH","POS",null,null,"POS Config swapped to mapping"]
["2019-07-02T12:38:17.100","2019-07-02T08:38:17.100","SH","Sonar","Multibeam",null,"Start Pinging Multibeam"]
["2019-07-02T12:38:54.820","2019-07-02T08:38:54.820","SH","Sonar","Knudsen","Start Recording","Start Pinging and Recording Knudsen"]
["2019-07-02T12:39:39.510","2019-07-02T08:39:39.510","SH","Sonar","EK",null,"Set EK to Maximum Pinging and 70 kHz mode to FM"]
["2019-07-02T12:40:12.490","2019-07-02T08:40:12.490","SH","Sonar","Multibeam",null,"Start Recording Multibeam Line 0222"]
["2019-07-02T12:42:48.680","2019-07-02T08:42:48.680","SH","XBT",null,null,"Launch AXBT081"]
["2019-07-02T12:48:35.770","2019-07-02T08:48:35.770","SH","Sonar","Multibeam","XBT Applied","XABT 081 appliedto line 0222"]
["2019-07-02T13:45:11.070","2019-07-02T09:45:11.070","SH","XBT",null,null,"Launch AXBT082"]
["2019-07-02T13:50:27.830","2019-07-02T09:50:27.830","SH","Sonar","Multibeam","XBT Applied","AXBT 082 applied to line 0223"]
["2019-07-02T14:09:01.090","2019-07-02T10:09:01.090","SH","Sonar","Multibeam",null,"Increase line for Turn"]
["2019-07-02T14:58:16.930","2019-07-02T10:58:16.930","SH","Sonar","Multibeam","Start Line",225]
["2019-07-02T15:59:46.520","2019-07-02T11:59:46.520","SH","Sonar","Multibeam","XBT Applied","AXBT 083 applied to line 0226"]
["2019-07-02T16:09:40.370","2019-07-02T12:09:40.370","SH","Sonar","Knudsen","Gain Value","Gain value decreased to 16"]
["2019-07-02T17:58:30.850","2019-07-02T13:58:30.850","SH","XBT",null,null,"AXBT 084 Launched"]
["2019-07-02T18:10:45.300","2019-07-02T14:10:45.300","SH","Sonar","Multibeam","XBT Applied","AXBT 084 Applied to line 0228"]
["2019-07-02T20:15:04.010","2019-07-02T16:15:04.010","DP","XBT",null,"XBT Launch","AXBT085 launched"]
["2019-07-02T20:15:52.560","2019-07-02T16:15:52.560","DP","Ship",null,null,"Decrease speed for traffic situation"]
["2019-07-02T20:19:16.570","2019-07-02T16:19:16.570","DP","Sonar","Multibeam","XBT Applied","AXBT085 applied in line 0230"]
["2019-07-02T20:20:22.380","2019-07-02T16:20:22.380","DP","Ship",null,null,"Coming back up to speed"]
["2019-07-02T20:38:07.710","2019-07-02T16:38:07.710","KJ","Sonar","Multibeam",null,"turned yaw stabilization on RMH"]
["2019-07-02T22:42:11.540","2019-07-02T18:42:11.540","DP","XBT",null,"XBT Launch","AXBT086 launched"]
["2019-07-03T00:22:34.780","2019-07-02T20:22:34.780","DP","Sonar","Multibeam","XBT Applied","AXBT086 Applied in line 0232"]
["2019-07-03T00:23:17.020","2019-07-02T20:23:17.020","DP","XBT",null,"XBT Launch","AXBT087 launched"]
["2019-07-03T01:59:44.320","2019-07-02T21:59:44.320","DP","Sonar","Multibeam","XBT Applied","AXBT087 applied in line 0234"]
["2019-07-03T02:00:24.300","2019-07-02T22:00:24.300","DP","XBT",null,"XBT Launch","AXBT088 launched"]
["2019-07-03T02:04:46.740","2019-07-02T22:04:46.740","DP","Sonar","Multibeam","XBT Applied","AXBT088 applied in line 0236"]
["2019-07-03T03:19:29.140","2019-07-02T23:19:29.140","DP","XBT",null,"XBT Launch","AXBT089 launched"]
["2019-07-03T04:54:59.260","2019-07-03T00:54:59.260","DP","Sonar","Multibeam","XBT Applied","AXBT089 Applied in line 0237"]
["2019-07-03T04:57:23.390","2019-07-03T00:57:23.390","DP","XBT",null,"XBT Launched","AXBT090 launched"]
["2019-07-03T05:02:21.730","2019-07-03T01:02:21.730","DP","Sonar","Multibeam","XBT Applied","AXBT090 applied in line 0239"]
["2019-07-03T05:16:20.130","2019-07-03T01:16:20.130","DP","Sonar","Knudsen",null,"Changed knudsen range from 200 m to 500 m"]
["2019-07-03T06:53:45.600","2019-07-03T02:53:45.600","KJ","XBT",null,"XBT Launched","AXBT091"]
["2019-07-03T07:00:20.300","2019-07-03T03:00:20.300","KJ","Sonar","Multibeam","XBT Applied","AXBT091 applied in line 241"]
["2019-07-03T07:12:45.590","2019-07-03T03:12:45.590","KJ","Sonar","EK",null,"changed 70 kHz from FM to CW while EM uses FM pulse forms in deeper modes"]
["2019-07-03T09:15:41","2019-07-03T05:15:41","SH","XBT",null,"XBT Launched","AXBT092 launched"]
["2019-07-03T09:21:45.740","2019-07-03T05:21:45.740","SH","Sonar","Multibeam","XBT Applied","AXBT092 applied in line 0243"]
["2019-07-03T09:37:45.340","2019-07-03T05:37:45.340","SH","Sonar","Multibeam",null,"New line. Turning to dive site."]
["2019-07-03T09:53:20.380","2019-07-03T05:53:20.380","SH","Sonar","Multibeam","Secure","Arriving at dive site"]
["2019-07-03T09:54:04.480","2019-07-03T05:54:04.480","SH","Sonar","ADCP","start pinging","Turn on"]
["2019-07-03T09:54:39.610","2019-07-03T05:54:39.610","SH","Sonar","SpeedLog","start"]
["2019-07-03T09:54:52.830","2019-07-03T05:54:52.830","SH","Sonar","Knudsen","secure"]
["2019-07-03T09:55:09.110","2019-07-03T05:55:09.110","SH","POS",null,null,"Switch Pos Configuration"]
["2019-07-03T11:22:59.560","2019-07-03T07:22:59.560","SH","Sonar","Multibeam","BIST","Ran a BIST test. ALL PASSED"]
["2019-07-03T13:51:39.850","2019-07-03T09:51:39.850","SH","Sonar","EK",null,"Switched from CW to FM in hopes to image seeps"]
["2019-07-03T14:53:12.080","2019-07-03T10:53:12.080","SH","Sonar","EK",null,"Start Recording EK"]
["2019-07-03T23:11:15.550","2019-07-03T19:11:15.550","SH","Sonar","EK",null,"Switching pulse lengths to normal (was in 1 ms for each during dive). Switching EK 70 to CW"]
["2019-07-04T00:00:34.450","2019-07-03T20:00:34.450","DP","POS",null,null,"Switch Pos Configuration"]
["2019-07-04T00:00:36.470","2019-07-03T20:00:36.470","SH","Sonar","ADCP","secure"]
["2019-07-04T00:00:56.640","2019-07-03T20:00:56.640","SH","Sonar","Multibeam","start pinging","Start pinging in MMP"]
["2019-07-04T00:01:30.080","2019-07-03T20:01:30.080","DP","Sonar","Knudsen","start pinging"]
["2019-07-04T00:02:09.050","2019-07-03T20:02:09.050","DP","Sonar","Knudsen","Start Recording"]
["2019-07-04T00:07:24.040","2019-07-03T20:07:24.040","KJ","Ship",null,null,"Bridge's speed log secured"]
["2019-07-04T00:10:47.850","2019-07-03T20:10:47.850","KJ","Sonar","Multibeam",null,"Max power"]
["2019-07-04T00:14:37.330","2019-07-03T20:14:37.330","KJ","Sonar","Multibeam","XBT Applied","CPCTD dive 11 downcast applied in line 0246 (not logging yet)"]
["2019-07-04T00:18:09.840","2019-07-03T20:18:09.840","KJ","Sonar","Multibeam","New Line","0246 start of seep survey with yaw stab OFF, max angles 60/60 to increase ping rate"]
["2019-07-04T00:41:22.660","2019-07-03T20:41:22.660","DP","Sonar","Multibeam",null,"Starting Seep Survey in line 0247"]
["2019-07-04T00:46:23.340","2019-07-03T20:46:23.340","DP","Sonar","Multibeam","New Line","start turn line 0248"]
["2019-07-04T00:56:40.180","2019-07-03T20:56:40.180","DP","Sonar","Multibeam","New Line","Start new seep survey line 0249"]
["2019-07-04T01:06:45.740","2019-07-03T21:06:45.740","DP","Sonar","Multibeam","New Line","Start Transit Line"]
["2019-07-04T01:13:16.690","2019-07-03T21:13:16.690","KJ","Sonar","Multibeam",null,"Bumped out the swath to 75/75 and turned on yaw stabilization "]
["2019-07-04T01:58:34.820","2019-07-03T21:58:34.820","DP","XBT",null,"XBT Launched","AXBT093 launched"]
["2019-07-04T02:05:12.350",{"$f":"IF(ISBLANK(A583),\" \",((A583)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-03T22:05:12.350"},"KJ","Sonar","Multibeam","XBT Applied","AXBT093 applied in line 0250"]
["2019-07-04T02:59:58.910","2019-07-03T22:59:58.910","KJ","Sonar","Multibeam",null,"changed penetration filter from weak to off to prevent mistracking at nadir over steep canyons with hard sediments"]
["2019-07-04T03:10:00","2019-07-03T23:10:00","KJ","Sonar","EK",null,"disabled in KSYNC and stopped logging to update transducer offsets from the API survey (2018); waterline will be set to match EM302 waterline (measured +down in meters from the granite block, currently set to 2.2 m based on updates in 2018)"]
["2019-07-04T03:25:24.990","2019-07-03T23:25:24.990","KJ","Sonar","EK",null,"Resumed pinging and logging"]
["2019-07-04T04:14:32.980","2019-07-04T00:14:32.980","DP","XBT",null,"XBT Launched","AXBT 094 launched"]
["2019-07-04T04:20:48.540","2019-07-04T00:20:48.540","DP","Sonar","Multibeam","XBT Applied","AXBT 094 applied in line 0253"]
["2019-07-04T04:43:11.030","2019-07-04T00:43:11.030","DP","Sonar","Multibeam","New Line","Start of \"shipwreck\" line 0254"]
["2019-07-04T06:08:32.620","2019-07-04T02:08:32.620","DP","XBT",null,"XBT Launched","AXBT 095 launched"]
["2019-07-04T06:14:06.430","2019-07-04T02:14:06.430","DP","Sonar","Multibeam","XBT Applied","AXBT095 applied in line 0255"]
["2019-07-04T07:57:36.540","2019-07-04T03:57:36.540","KJ","XBT",null,"XBT Launched","AXBT096 launched"]
["2019-07-04T08:07:13.350",{"$f":"IF(ISBLANK(A593),\" \",((A593)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-04T04:07:13.350"},"KJ","Sonar","Multibeam","XBT Applied","AXBT096 applied in line 257"]
["2019-07-04T08:07:33.420","2019-07-04T04:07:33.420","KJ","Sonar","Multibeam",null,"interference from unknown source occasionally causing severe bottom detection issues"]
["2019-07-04T09:30:58.690","2019-07-04T05:30:58.690","KJ","XBT",null,"XBT Launched","AXBT097 launched"]
["2019-07-04T09:54:32.920","2019-07-04T05:54:32.920","SH","Sonar","Multibeam","XBT Applied","AXBT097 applied to line 0259"]
["2019-07-04T09:55:56.160","2019-07-04T05:55:56.160","SH","Sonar","Multibeam","secure"]
["2019-07-04T09:56:19.890","2019-07-04T05:56:19.890","SH","Sonar","Knudsen","secure"]
["2019-07-04T09:56:37.580","2019-07-04T05:56:37.580","SH","Sonar","ADCP","start pinging"]
["2019-07-04T09:57:16.480","2019-07-04T05:57:16.480","SH","POS",null,null,"switched pos configuration"]
["2019-07-04T20:58:48.560","2019-07-04T16:58:48.560","SH","POS",null,null,"Switched POS configuration"]
["2019-07-04T20:58:55.580","2019-07-04T16:58:55.580","DP","Sonar","ADCP","Secure"]
["2019-07-04T20:59:47.470","2019-07-04T16:59:47.470","SH","Sonar","Multibeam","start pinging","Start Pinging in MMP"]
["2019-07-04T20:59:59.620","2019-07-04T16:59:59.620","DP","Sonar","Knudsen","Start Pinging","Start pinging and recording"]
["2019-07-04T21:01:57.550","2019-07-04T17:01:57.550","SH","Sonar","SpeedLog","Secure"]
["2019-07-04T21:06:22.500","2019-07-04T17:06:22.500","DP","Sonar","Multibeam","start pinging","Start pinging in full power"]
["2019-07-04T21:22:01.710","2019-07-04T17:22:01.710","KJ","Sonar","Multibeam",null,"merging onto first line that will be used as roll calibration line 2 (line 1 from approach to dive site); there is a fishing vessel ~2-3 miles away that may be source of occasional interference in EM302"]
["2019-07-04T21:25:06.590","2019-07-04T17:25:06.590","KJ","Sonar","Multibeam","start logging","260 departure from dive site, roll cal line 2"]
["2019-07-04T22:15:05.280","2019-07-04T18:15:05.280","SH","XBT",null,null,"AXBT Launched 098"]
["2019-07-04T22:18:09.240","2019-07-04T18:18:09.240","KJ","Sonar","Multibeam",null,"changed mode to Deep to try to increase swath width beyond 52/52 in Very Deep, but reverted back to Auto after a few pings to maintain better soundings"]
["2019-07-04T22:21:24.900","2019-07-04T18:21:24.900","KJ","Sonar","Multibeam","XBT Applied","applied AXBT098 in line 0260"]
["2019-07-05T00:27:31.950","2019-07-04T20:27:31.950","KJ","XBT",null,"XBT Launched","AXBT099 launched"]
["2019-07-05T00:34:51.740","2019-07-04T20:34:51.740","KJ","Sonar","Multibeam","XBT Applied","AXBT099 applied in line 264"]
["2019-07-05T00:55:47.610","2019-07-04T20:55:47.610","KJ","Ship",null,null,"moved 300 m to starboard for coverage"]
["2019-07-05T01:10:58.740","2019-07-04T21:10:58.740","KJ","Sonar","Multibeam",null,"grid engine not updating…"]
["2019-07-05T02:00:09.820","2019-07-04T22:00:09.820","KJ","Ship",null,null,"starting an additional 500 m shift to stbd"]
["2019-07-05T02:08:23.450","2019-07-04T22:08:23.450","KJ","Ship",null,null,"requested another 500 m to stbd, for a total of 1300 m off original line plan"]
["2019-07-05T02:28:11.840","2019-07-04T22:28:11.840","KJ","XBT",null,"XBT launched","AXBT100 launched"]
["2019-07-05T02:28:30.210","2019-07-04T22:28:30.210","KJ","Ship",null,null,"reverting back to original line plan and dropping speed from 13 to 10 kts with Gulf Stream on the stern…"]
["2019-07-05T02:35:10.180","2019-07-04T22:35:10.180","KJ","Sonar","Multibeam","XBT Applied","AXBT100 applied in line 0266"]
["2019-07-05T02:43:02.100","2019-07-04T22:43:02.100","KJ","Sonar","Knudsen",null,"changed TX pulse from 1 ms to 0.5 ms and range from 200 m to 50 m , then back to 100 m over shallow, variable terrain"]
["2019-07-05T02:51:08.360","2019-07-04T22:51:08.360","KJ","Sonar","Knudsen",null,"Secure over highly variable terrain (high ping rate, low data quality)"]
["2019-07-05T03:04:08.550","2019-07-04T23:04:08.550","KJ","Sonar","EK",null,"changed 70 kHz from CW to FM, 45-90 kHz, all systems set to 1 ms in 50-100 m water depths"]
["2019-07-05T03:12:27.220","2019-07-04T23:12:27.220","DP","XBT",null,"XBT Launch","AXBT101 launched"]
["2019-07-05T03:12:50.540","2019-07-04T23:12:50.540","DP","Sonar","Multibeam","XBT Applied","AXBT101 applied in line 0267"]
["2019-07-05T03:57:39.420","2019-07-04T23:57:39.420","KJ","Ship",null,null,"reducing speed to 7 kts for shipwreck survey"]
["2019-07-05T04:06:12.520","2019-07-05T00:06:12.520","KJ","XBT",null,"XBT Launched","AXBT102 launched"]
["2019-07-05T04:11:54.010","2019-07-05T00:11:54.010","KJ","Sonar","Multibeam","XBT Applied","AXBT102 applied in line 268"]
["2019-07-05T04:16:29.740","2019-07-05T00:16:29.740","KJ","Sonar","Multibeam",null,"starting seep survey at 4 kts"]
["2019-07-05T04:19:39.840","2019-07-05T00:19:39.840","KJ","Sonar","All",null,"seeps in multibeam line 268, EK data"]
["2019-07-05T05:58:45.810","2019-07-05T01:58:45.810","DP","XBT",null,"XBT Launch","AXBT103 launched"]
["2019-07-05T06:02:39.020","2019-07-05T02:02:39.020","DP","Sonar","Multibeam","XBT Applied","AXBT103 applied in line0271"]
["2019-07-05T08:09:02.360","2019-07-05T04:09:02.360","KJ","XBT",null,"XBT launched","AXBT104 launched"]
["2019-07-05T08:13:21.420","2019-07-05T04:13:21.420","KJ","Sonar","Multibeam","XBT Applied","AXBT104 applied in line 275"]
["2019-07-05T08:27:24.220","2019-07-05T04:27:24.220","KJ","Ship",null,null,"starting 200 m shift to stbd for coverage"]
["2019-07-05T09:46:52.670","2019-07-05T05:46:52.670","KJ","Sonar",null,null,"bridge reported whales possible off the port bow; all sonars secure and ship coming to drift until whales move out of the way"]
["2019-07-05T09:56:02.850","2019-07-05T05:56:02.850","SH","Sonar","ADCP","start pinging"]
["2019-07-05T09:57:37.770","2019-07-05T05:57:37.770","SH","POS",null,null,"switched pos configuration"]
["2019-07-05T09:58:20.480","2019-07-05T05:58:20.480","SH","Sonar","EK","Start Recording","70 in CW"]
["2019-07-05T20:56:26.280","2019-07-05T16:56:26.280","DP","POS",null,null,"Switch Pos Configuration"]
["2019-07-05T20:56:49.960","2019-07-05T16:56:49.960","DP","Sonar","ADCP","secure"]
["2019-07-05T20:58:02.070","2019-07-05T16:58:02.070","KJ","Sonar","EK",null,"Switch to FM, switch pulse length to 1ms for all, start pinging"]
["2019-07-05T20:58:42.480","2019-07-05T16:58:42.480","KJ","Sonar","Knudsen","Start Pinging"]
["2019-07-05T20:59:14.230","2019-07-05T16:59:14.230","KJ","Sonar","Multibeam","start pinging","Start pinging in MMP"]
["2019-07-05T21:00:02.430","2019-07-05T17:00:02.430","KJ","Sonar","Knudsen","Start Recording"]
["2019-07-05T21:00:27.100","2019-07-05T17:00:27.100","KJ","Sonar","EK","Start Recording"]
["2019-07-05T21:05:14.280",{"$f":"IF(ISBLANK(A647),\" \",((A647)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-05T17:05:14.280"},"KJ","Sonar","Multibeam",null,"power to -10 dB"]
["2019-07-05T21:13:56.760","2019-07-05T17:13:56.760","KJ","Sonar","Multibeam",null,"Max power"]
["2019-07-05T21:33:55.710","2019-07-05T17:33:55.710","SH","Sonar","SpeedLog","Secure"]
["2019-07-05T21:35:36.320","2019-07-05T17:35:36.320","SH","Sonar","Multibeam","Start Logging","Turning to survey"]
["2019-07-05T21:41:45.870","2019-07-05T17:41:45.870","SH","Sonar","Multibeam",null,"Dive 13 CP CTD applied to 0278"]
["2019-07-05T21:51:12.690","2019-07-05T17:51:12.690","SH","Sonar","Multibeam",null,"Starting shipwreck"]
["2019-07-05T22:55:57.880","2019-07-05T18:55:57.880","DP","Sonar","Multibeam","New Line","Starting end cap turn line 0281"]
["2019-07-05T23:03:12.950","2019-07-05T19:03:12.950","DP","Sonar","Knudsen","Secure","Securing for pilot whales"]
["2019-07-05T23:10:24.620","2019-07-05T19:10:24.620","DP","Sonar","Multibeam","New Line","Start of survey line 0282"]
["2019-07-05T23:44:36.410","2019-07-05T19:44:36.410","DP","XBT",null,"XBT Launch","AXBT105 launched"]
["2019-07-05T23:51:36.580","2019-07-05T19:51:36.580","DP","Sonar","Multibeam","XBT Applied","AXBT105 applied in line 0282"]
["2019-07-06T00:26:43.960","2019-07-05T20:26:43.960","DP","Sonar","Knudsen","Start Pinging","Resume pinging after not seeing any more whales"]
["2019-07-06T02:06:13.870","2019-07-05T22:06:13.870","DP","XBT",null,"XBT Launch","AXBT106 launched"]
["2019-07-06T02:11:58.320","2019-07-05T22:11:58.320","DP","Sonar","Multibeam","XBT Applied","AXBT106 applied in line 0288"]
["2019-07-06T04:02:14.010","2019-07-06T00:02:14.010","DP","XBT",null,"XBT Launch","AXBT107 launched"]
["2019-07-06T04:07:05.610","2019-07-06T00:07:05.610","DP","Sonar","Multibeam","XBT Applied","AXBT107 applied in line 0293"]
["2019-07-06T06:24:41.660","2019-07-06T02:24:41.660","DP","XBT",null,"XBT Launch","AXBT108 launched"]
["2019-07-06T06:29:28.790","2019-07-06T02:29:28.790","KJ","Sonar","Multibeam","XBT Applied","AXBT applied in line 0299"]
["2019-07-06T08:10:11.800","2019-07-06T04:10:11.800","KJ","Ship",null,null,"breaking off line plan to head straight to seep survey site"]
["2019-07-06T08:47:57.230","2019-07-06T04:47:57.230","KJ","XBT",null,"XBT launched","AXBT109 launched"]
["2019-07-06T08:54:01.840","2019-07-06T04:54:01.840","KJ","Sonar","Multibeam","XBT Applied","AXBT109 applied in line 303"]
["2019-07-06T09:12:24.590","2019-07-06T05:12:24.590","SH","Sonar","Multibeam",null,"Begin Seep Survey 0304"]
["2019-07-06T09:12:47.720","2019-07-06T05:12:47.720","SH","XBT",null,null,"AXBT110 Launched"]
["2019-07-06T09:18:11.470","2019-07-06T05:18:11.470","SH","Sonar","Multibeam","XBT Applied","AXBT110 appliedto 0304"]
["2019-07-06T09:23:28.620","2019-07-06T05:23:28.620","SH","Sonar","Multibeam",null,"brought angles to 60/60"]
["2019-07-06T10:03:32.350","2019-07-06T06:03:32.350","SH","Sonar","Multibeam","secure"]
["2019-07-06T10:03:41.390","2019-07-06T06:03:41.390","SH","Sonar","ADCP","start pinging"]
["2019-07-06T10:03:51.790","2019-07-06T06:03:51.790","SH","Sonar","speedlog","start"]
["2019-07-06T10:04:03.860","2019-07-06T06:04:03.860","SH","POS",null,null,"Switch Pos Configuration"]
["2019-07-06T10:05:16.760","2019-07-06T06:05:16.760","SH","Sonar","EK",null,"stop recording. Change 70 to CW. Start recording"]
["2019-07-06T20:15:32.170","2019-07-06T16:15:32.170","SH",null,null,null,"setting up for midwater transects"]
["2019-07-06T20:16:32.200","2019-07-06T16:16:32.200","SH","Sonar","EK",null,"stop pinging and recording"]
["2019-07-06T20:22:24.720","2019-07-06T16:22:24.720","SH","Sonar","EK",null,"Install 38 kHz and start pinging"," "]
["2019-07-06T20:27:42.150","2019-07-06T16:27:42.150","SH","Sonar","EK",null,"stop pinging. Uninstalling 38 transducer"]
["2019-07-06T20:30:14.750","2019-07-06T16:30:14.750","SH","Sonar","EK",null,"start pinging"]
["2019-07-06T20:30:57.460","2019-07-06T16:30:57.460","SH","Sonar","EK",null,"set recording range to 500m"]
["2019-07-06T20:31:19.620","2019-07-06T16:31:19.620","SH","Sonar","EK",null,"start pinging  and recording"]
["2019-07-06T22:20:29.010","2019-07-06T18:20:29.010","SH","Sonar","EK",null,"end midwater transects"]
["2019-07-06T22:20:49.300","2019-07-06T18:20:49.300","SH","Sonar","EK",null,"stop pinging and recording"]
["2019-07-06T22:21:34.740","2019-07-06T18:21:34.740","SH","Sonar","EK",null,"70 to FM. All set to 1ms for seep survey"]
["2019-07-06T22:22:32.840","2019-07-06T18:22:32.840","SH","Sonar","EK",null,"start pinging and recording"]
["2019-07-06T22:42:59.230","2019-07-06T18:42:59.230","DP","POS",null,null,"Change POS settings"]
["2019-07-06T22:43:37.250","2019-07-06T18:43:37.250","DP","Sonar","ADCP","secure"]
["2019-07-06T22:44:13.410","2019-07-06T18:44:13.410","DP","Sonar","Knudsen","Start Pinging","Start pinging and recording"]
["2019-07-06T22:44:49.470","2019-07-06T18:44:49.470","DP","Sonar","SpeedLog","Secure"]
["2019-07-06T22:45:43.170","2019-07-06T18:45:43.170","DP","Sonar","Multibeam","Start Pinging","Start Pinging at max power"]
["2019-07-06T22:47:11.830","2019-07-06T18:47:11.830","DP","Sonar","Multibeam","Start Logging","Start logging for seeeeeeeeeeeeeps"]
["2019-07-06T23:16:48.010","2019-07-06T19:16:48.010","DP","Sonar","Multibeam","New Line","Start of survey line 0313"]
["2019-07-06T23:21:55.680","2019-07-06T19:21:55.680","DP","Sonar","Multibeam",null,"CPCTD 14 applied in line 0313"]
["2019-07-06T23:45:04.780","2019-07-06T19:45:04.780","DP","XBT",null,"XBT Launch","AXBT111 launched"]
["2019-07-06T23:48:23.070","2019-07-06T19:48:23.070","DP","Sonar","Multibeam","XBT Applied","AXBT111 applied in line 0314"]
["2019-07-06T23:54:07.720","2019-07-06T19:54:07.720","DP","Sonar","Multibeam","New Line","Line cut for ROV going into the garage"]
["2019-07-07T00:21:13.150","2019-07-06T20:21:13.150","DP","Sonar","Multibeam","New Line","Start of return to survey"]
["2019-07-07T01:10:14.030","2019-07-06T21:10:14.030","KJ","Ship",null,null,"shift 200 m to port for coverage"]
["2019-07-07T01:29:36.070","2019-07-06T21:29:36.070","KJ","Ship",null,null,"shift 500 m to port for coverage"]
["2019-07-07T01:48:39.140","2019-07-06T21:48:39.140","DP","XBT",null,"XBT Launch","AXBT112 Launched"]
["2019-07-07T01:52:53.960","2019-07-06T21:52:53.960","DP","Sonar","Multibeam","XBT Applied","AXBT112 applied in line 0317"]
["2019-07-07T03:57:53.560","2019-07-06T23:57:53.560","KJ","XBT",null,"XBT Launched","AXB113 launched"]
["2019-07-07T03:58:14.210","2019-07-06T23:58:14.210","KJ","ship",null,null,"slowing to 4 kts for deep shipwreck survey"]
["2019-07-07T04:05:19.340","2019-07-07T00:05:19.340","KJ","Sonar","Multibeam","XBT Applied","AXBT113 applied in line 320"]
["2019-07-07T05:36:28.530","2019-07-07T01:36:28.530","KJ","XBT",null,"XBT launched","AXBT114 launched"]
["2019-07-07T05:43:25.220","2019-07-07T01:43:25.220","KJ","Sonar","Multibeam","XBT Applied","AXBT114 applied in line 321"]
["2019-07-07T06:33:06.260","2019-07-07T02:33:06.260","DP","Ship",null,null,"Thunderstorm affecting acquisition of bathymetric data"]
["2019-07-07T07:41:30.930","2019-07-07T03:41:30.930","KJ","XBT",null,"XBT Launched","AXBT launched, failed in high wind with lightning all around; will try again when storm settles a little bit"]
["2019-07-07T09:56:10.880",{"$f":"IF(ISBLANK(A711),\" \",((A711)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-07T05:56:10.880"},"SH","Sonar","Multibeam","secure","Arriving at dive site"]
["2019-07-07T09:56:26.360","2019-07-07T05:56:26.360","SH","Sonar","ADCP","start pinging"]
["2019-07-07T09:56:59.680","2019-07-07T05:56:59.680","SH","POS",null,null,"switch configuration"]
["2019-07-07T09:58:46.500","2019-07-07T05:58:46.500","SH","Sonar","Knudsen","secure"]
["2019-07-07T09:59:19.290","2019-07-07T05:59:19.290","SH","Sonar","EK",null,"switch 70 to CW. And put pulse lengths back to standard mode 4,2,1,1 ms"]
["2019-07-07T20:58:18.850","2019-07-07T16:58:18.850","DP","POS",null,null,"Switch POS settings"]
["2019-07-07T20:58:41.530","2019-07-07T16:58:41.530","DP","Sonar","ADCP","secure"]
["2019-07-07T21:00:53.490","2019-07-07T17:00:53.490","DP","Sonar","EK","Stop Recording","Stop recording to change to FM "]
["2019-07-07T21:00:56.020","2019-07-07T17:00:56.020","DP","Sonar","EK","Start Recording","Resume Recording"]
["2019-07-07T21:01:20.650","2019-07-07T17:01:20.650","DP","Sonar","Knudsen","start pinging"]
["2019-07-07T21:01:44.400","2019-07-07T17:01:44.400","DP","Sonar","Knudsen","Start Recording"]
["2019-07-07T21:02:26.550","2019-07-07T17:02:26.550","DP","Sonar","speedlog","secure"]
["2019-07-07T21:02:47.840","2019-07-07T17:02:47.840","DP","Sonar","Multibeam","start pinging"]
["2019-07-07T21:13:14.180","2019-07-07T17:13:14.180","KJ","Sonar","Multibeam","start logging","0329 leaving dive site"]
["2019-07-07T21:14:13.470","2019-07-07T17:14:13.470","KJ","Sonar","Multibeam",null,"Dive 15 CP CTD applied to line 329"]
["2019-07-07T21:19:37.270","2019-07-07T17:19:37.270","KJ","Ship",null,null,"mapping at 1.5 kts in DP, waiting 20-30 minutes for engineer to be available to shift out of DP..."]
["2019-07-07T21:23:56.020","2019-07-07T17:23:56.020","KJ","Sonar","EK",null,"changed 70 kHz from FM to CW while EM uses FM pulse forms in deeper modes"]
["2019-07-07T21:39:44.550","2019-07-07T17:39:44.550","DP","Ship",null,null,"Comng up to speed on line 0329"]
["2019-07-07T22:04:04.050","2019-07-07T18:04:04.050","KJ","Sonar","Multibeam","New Line","Turn onto line 0330, slowing to 4 kts for shipwreck survey"]
["2019-07-07T22:49:13.130","2019-07-07T18:49:13.130","DP","Sonar","Multibeam","New Line","Start turn line 0331"]
["2019-07-07T22:58:01.700","2019-07-07T18:58:01.700","DP","Sonar","Multibeam","New Line","Start survey line 0332"]
["2019-07-07T23:57:07.880","2019-07-07T19:57:07.880","KJ","Sonar","Multibeam",null,"lines 332 and 333 have a small target of interest off to stbd before turn, near nadir after turn"]
["2019-07-08T00:16:36.780","2019-07-07T20:16:36.780","DP","XBT",null,"XBT Launch","AXBT115 launched"]
["2019-07-08T00:21:50.550","2019-07-07T20:21:50.550","DP","Sonar","Multibeam","XBT Applied","AXBT115 applied in line 0336"]
["2019-07-08T01:15:51.840","2019-07-07T21:15:51.840","KJ","Ship",null,null,"coming up to speed to get out of severe thunderstorm; shipwreck hunting is impacted by weather"]
["2019-07-08T01:55:44.790","2019-07-07T21:55:44.790","DP","Sonar","Knudsen",null,"changed recording range from 200 to 100 m"]
["2019-07-08T02:21:15.700","2019-07-07T22:21:15.700","DP","XBT",null,"XBT Launch","AXBT116 launched"]
["2019-07-08T02:25:05.090","2019-07-07T22:25:05.090","DP","Sonar","Multibeam","XBT Applied","AXBT116 applied in line 0339"]
["2019-07-08T05:07:34.230","2019-07-08T01:07:34.230","KJ","XBT",null,null,"AXBT117 launched"]
["2019-07-08T05:14:32.480","2019-07-08T01:14:32.480","KJ","Sonar","Multibeam","XBT Applied","AXBT117 applied in line 0342"]
["2019-07-08T06:23:38.570","2019-07-08T02:23:38.570","KJ","Ship",null,null,"diverting off line for fishing vessel, line 334"]
["2019-07-08T07:20:27.310","2019-07-08T03:20:27.310","KJ","Ship",null,null,"rejoined the transit line near seep survey, slowing to 6 kts"]
["2019-07-08T07:27:05.630","2019-07-08T03:27:05.630","KJ","XBT",null,"XBT Launched","AXBT118 launched"]
["2019-07-08T07:30:47.650","2019-07-08T03:30:47.650","KJ","Sonar","Multibeam","XBT Applied","AXBT118 applied in line 0345"]
["2019-07-08T07:54:26.810","2019-07-08T03:54:26.810","KJ","Sonar","All",null,"start Washington Canyon survey; line 346; seep possible near end of line 345/start of 346"]
["2019-07-08T07:57:08.100","2019-07-08T03:57:08.100","KJ","Sonar","Multibeam",null,"lots of interference, unknown source"]
["2019-07-08T07:57:45.570","2019-07-08T03:57:45.570","KJ","Sonar","Knudsen",null,"restarted logging after range change a few minutes ago"]
["2019-07-08T08:02:36.870","2019-07-08T04:02:36.870","KJ","Sonar","Knudsen",null,"changed range from 200 to 500 over steep canyon"]
["2019-07-08T08:21:58.060","2019-07-08T04:21:58.060","KJ","Sonar","Multibeam",null,"seeps in multibeam in 346 over canyon and 347 turn line"]
["2019-07-08T09:14:19.170","2019-07-08T05:14:19.170","KJ","Sonar","Knudsen",null,"Secure over highly variable terrain (high ping rate, low data quality)"]
["2019-07-08T09:51:09.290","2019-07-08T05:51:09.290","KJ","XBT",null,"XBT launched","AXBT119 launched"]
["2019-07-08T09:58:07.150","2019-07-08T05:58:07.150","KJ","Sonar","Multibeam","XBT Applied","AXBT119 applied in line 351"]
["2019-07-08T09:59:06.390","2019-07-08T05:59:06.390","SH","Sonar","ADCP","start pinging"]
["2019-07-08T09:59:55.290","2019-07-08T05:59:55.290","SH","Sonar","EK",null,"Change to CW"]
["2019-07-08T20:47:02.880","2019-07-08T16:47:02.880","DP","POS",null,null,"Change POS settings"]
["2019-07-08T20:48:27.030","2019-07-08T16:48:27.030","DP","Sonar","ADCP","secure"]
["2019-07-08T20:48:55.520","2019-07-08T16:48:55.520","KJ","Sonar","Knudsen","start pinging","Starting the Knudsen pinging"]
["2019-07-08T20:49:57.480","2019-07-08T16:49:57.480","DP","Sonar","Multibeam","Start Pinging","Start Pinging "]
["2019-07-08T20:52:26.430","2019-07-08T16:52:26.430","KJ","Sonar","Knudsen","Start recording"]
["2019-07-08T20:55:53.600","2019-07-08T16:55:53.600","KJ","Issue/Problem",null,null,"Waiting for an engineer for another 35 minutes to get out of DP and start survey line"]
["2019-07-08T21:02:34.750","2019-07-08T17:02:34.750","KJ","Sonar","Multibeam",null,"CPCTD Upcast 16 applied in line 0352"]
["2019-07-08T21:03:06.270","2019-07-08T17:03:06.270","KJ","Sonar","Multibeam","start logging","underway, line 352"]
["2019-07-08T21:12:43.580","2019-07-08T17:12:43.580","KJ","Sonar","Multibeam",null,"Second version of CPCTD upcast 16 applied in line 0352 (reprocessed the upper water column to match surface sound speed value over slightly wider range of depths as ship heaves a bit)"]
["2019-07-08T21:39:04.180","2019-07-08T17:39:04.180","KJ","Sonar","Knudsen",null,"TX power from 1 to 2, range from 500 m to 200 m, still 1 ms for subbottom profiling line up Washington Canyon"]
["2019-07-08T21:43:12.520","2019-07-08T17:43:12.520","KJ","Sonar","Multibeam",null,"forced into VERY DEEP to track bottom while heading into swell"]
["2019-07-08T21:56:25.010","2019-07-08T17:56:25.010","DP","Sonar","Multibeam","New Line","Turn Line 0354"]
["2019-07-08T21:59:11.480","2019-07-08T17:59:11.480","KJ","Sonar","Multibeam","New Line","Kevin cut the line again like a silly goose"]
["2019-07-08T22:02:38.430","2019-07-08T18:02:38.430","KJ","Sonar","Multibeam","New Line","Start survey line 0356, Knudsen line 194"]
["2019-07-08T22:18:07.810","2019-07-08T18:18:07.810","KJ","XBT",null,"XBT launched","AXBT120"]
["2019-07-08T22:25:09.320","2019-07-08T18:25:09.320","KJ","Sonar","Multibeam","XBT Applied","AXBT120 applied in line 356; using CTD salinity as reference"]
["2019-07-08T23:20:40.130","2019-07-08T19:20:40.130","KJ","Sonar","Multibeam",null,"PPS occasionally dropping out"]
["2019-07-08T23:24:04.790","2019-07-08T19:24:04.790","KJ","Sonar","Multibeam",null,"interference, possibly from cetaceans"]
["2019-07-08T23:40:40.970","2019-07-08T19:40:40.970","KJ","XBT",null,"XBT launched","AXBT121"]
["2019-07-08T23:45:12.950","2019-07-08T19:45:12.950","KJ","Sonar","Multibeam","XBT Applied","AXBT121 applied in line 359"]
["2019-07-09T00:02:57.340",{"$f":"IF(ISBLANK(A775),\" \",((A775)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-08T20:02:57.340"},"KJ","Sonar","Multibeam",null,"Stop recording Ek to change all pulses to 1ms then resume recording"]
["2019-07-09T00:16:50.250","2019-07-08T20:16:50.250","KJ","Sonar","Knudsen",null,"Changed range to 100m"]
["2019-07-09T00:23:32.910","2019-07-08T20:23:32.910","DP","Sonar","Knudsen",null,"Stop recording, change power to 1, start recording"]
["2019-07-09T01:31:57.080","2019-07-08T21:31:57.080","DP","XBT",null,"XBT Launched","AXBT122"]
["2019-07-09T01:36:02.200","2019-07-08T21:36:02.200","DP","Sonar","Multibeam","XBT Applied","AXBT122 applied in line 361"]
["2019-07-09T03:35:17.490","2019-07-08T23:35:17.490","DP","XBT",null,"XBT Launched","AXBT123"]
["2019-07-09T03:42:26.400","2019-07-08T23:42:26.400","DP","Sonar","Multibeam","XBT Applied","AXBT123 applied in line 363 (CTD salinity used for this cast but reverted back to WOA13 for future casts)"]
["2019-07-09T04:17:49.110","2019-07-09T00:17:49.110","DP","Sonar","Multibeam","New Line","Cut line for shipwreck hunt 0364"]
["2019-07-09T05:06:13.070","2019-07-09T01:06:13.070","DP","Sonar","Multibeam","New Line","End of shipwreck line 364"]
["2019-07-09T05:24:24.950","2019-07-09T01:24:24.950","DP","XBT",null,"XBT Launch","AXBT124 launched"]
["2019-07-09T05:28:25.540","2019-07-09T01:28:25.540","KJ","Sonar","Multibeam","XBT Applied","AXBT124 applied in line 0365"]
["2019-07-09T07:22:27.010","2019-07-09T03:22:27.010","KJ","XBT",null,"XBT Launched","AXBT125"]
["2019-07-09T07:28:42.340","2019-07-09T03:28:42.340","KJ","Sonar","Multibeam","XBT Applied","AXBT125 applied in line 367"]
["2019-07-09T09:44:47.990","2019-07-09T05:44:47.990","SH","Sonar","Multibeam","secure","Arriving at dive site"]
["2019-07-09T09:46:10.810","2019-07-09T05:46:10.810","SH","Sonar","ADCP","start pinging"]
["2019-07-09T09:47:18.330","2019-07-09T05:47:18.330","SH","Sonar","Knudsen","secure"]
["2019-07-09T09:49:54.210","2019-07-09T05:49:54.210","SH","Sonar","EK",null,"Pulse lengths set to normal (4, 2, 1, 1)"]
["2019-07-09T20:52:54.120","2019-07-09T16:52:54.120","DP","POS",null,null,"Change POS Config"]
["2019-07-09T20:53:04.440","2019-07-09T16:53:04.440","DP","Sonar","ADCP","secure"]
["2019-07-09T20:53:59.050","2019-07-09T16:53:59.050","DP","Sonar","Knudsen","start pinging"]
["2019-07-09T20:54:16.480","2019-07-09T16:54:16.480","DP","Sonar","Knudsen","Start recording"]
["2019-07-09T20:55:08.660","2019-07-09T16:55:08.660","DP","Sonar","Multibeam","Start Pinging"]
["2019-07-09T20:57:20.290","2019-07-09T16:57:20.290","DP","Sonar","speedlog","secure"]
["2019-07-09T21:06:57.190","2019-07-09T17:06:57.190","DP","Sonar","Multibeam",null,"CPCTD UP Cast 17 applied in line 0371"]
["2019-07-09T21:13:27.530","2019-07-09T17:13:27.530","KJ","Sonar","Multibeam","start logging",371]
["2019-07-09T21:15:00.960","2019-07-09T17:15:00.960","KJ","Sonar","Knudsen","Tx Power","changed TX power from 1 to 2, keeping 1 ms, same settings as last night for subbottom profile survey lines"]
["2019-07-09T21:33:14.200","2019-07-09T17:33:14.200","DP","Ship",null,null,"Coming out of DP and up to speed"]
["2019-07-09T22:20:24.330","2019-07-09T18:20:24.330","DP","XBT",null,"XBT Launch","AXBT126 launched"]
["2019-07-09T22:27:05.610","2019-07-09T18:27:05.610","DP","Sonar","Multibeam","XBT Applied","AXBT126 applied in line 0372"]
["2019-07-09T22:27:36.310","2019-07-09T18:27:36.310","DP","Sonar","Multibeam","New Line","Kevin recut my already cut line. Ignore line 0373"]
["2019-07-09T22:29:06.680","2019-07-09T18:29:06.680","DP","Sonar","Knudsen",null,"Range down to 200 for subbottom line, accidentally made a really small file by starting recording before remembering to adjust the range"]
["2019-07-09T23:46:10.140","2019-07-09T19:46:10.140","KJ","XBT",null,"XBT launched","AXBT127"]
["2019-07-09T23:54:46.770","2019-07-09T19:54:46.770","KJ","Sonar","Multibeam","XBT Applied","AXBT127 applied in line 376"]
["2019-07-10T00:46:07.490","2019-07-09T20:46:07.490","KJ","Sonar","Knudsen",null,"subbottom survey #1 is file 0205, subbottom survey #2 is file 208"]
["2019-07-10T02:12:36.080","2019-07-09T22:12:36.080","DP","XBT",null,"XBT Launch","AXBT128 launch failed"]
["2019-07-10T02:16:21.890","2019-07-09T22:16:21.890","DP","XBT",null,"XBT Launch","AXBT128 launch  "]
["2019-07-10T02:22:26.360","2019-07-09T22:22:26.360","DP","Sonar","Multibeam","XBT Applied","AXBT128 applied in line 0381"]
["2019-07-10T03:37:59.190","2019-07-09T23:37:59.190","DP","Sonar","Knudsen",null,"Subbottom line 211 started for survey #3"]
["2019-07-10T04:26:54.060","2019-07-10T00:26:54.060","DP","XBT",null,"XBT Launch","AXBT129 launched"]
["2019-07-10T04:32:17.590","2019-07-10T00:32:17.590","DP","Sonar","Multibeam","XBT Applied","AXBT129 applied in line 0384"]
["2019-07-10T04:39:07.640","2019-07-10T00:39:07.640","KJ","Sonar","Knudsen",null,"Subbottom line 212 for second part of survey #3 up canyon"]
["2019-07-10T05:41:08.850","2019-07-10T01:41:08.850","KJ","XBT",null,"XBT launched","AXBT130"]
["2019-07-10T05:48:54.380","2019-07-10T01:48:54.380","KJ","Sonar","Multibeam","XBT Applied","AXBT130 applied in line 386"]
["2019-07-10T05:59:09.080","2019-07-10T01:59:09.080","KJ","Sonar","Knudsen",null,"Subbottom line 213 for third part of survey #3 up canyon"]
["2019-07-10T06:55:05.510","2019-07-10T02:55:05.510","KJ","Ship",null,null,"Turning around because we are surrounded by a giant U-shape arrangement of fish traps and buoys; we will not be able to complete the subbottom survey lines to the north"]
["2019-07-10T07:01:09.750","2019-07-10T03:01:09.750","KJ","Sonar","Knudsen",null,"file 215 for reciprocal course down the canyon back toward the dive site, offset by a few hundred meters to the east from file 213"]
["2019-07-10T07:15:01.970","2019-07-10T03:15:01.970","KJ","XBT",null,"XBT launched","AXBT131"]
["2019-07-10T07:15:32.660","2019-07-10T03:15:32.660","KJ","Sonar","Multibeam",null,"interesting backscatter target near nadir a few minutes ago in file 389"]
["2019-07-10T07:21:19.310","2019-07-10T03:21:19.310","KJ","Sonar","Multibeam","XBT Applied","AXBT131 applied in line 389"]
["2019-07-10T08:08:15.900","2019-07-10T04:08:15.900","KJ","Sonar","Knudsen",null,"file 216 for reciprocal line of middle segment of Baltimore canyon subbottom survey"]
["2019-07-10T08:53:54.170","2019-07-10T04:53:54.170","KJ","Sonar","Knudsen",null,"file 218 for return toward dive site, offset 200 m to SW from original line plan"]
["2019-07-10T09:12:55.480","2019-07-10T05:12:55.480","KJ","XBT",null,"XBT launched","attempted to launch AXBT from tubes 8 and 1, both failed to detect launch; Shannon checking pins; metal retaining pins have been pulled, but the launcher pin on tube 8 was retracted half way"]
["2019-07-10T09:30:03.570","2019-07-10T05:30:03.570","KJ","XBT",null,"XBT launched","AXBT132 launched from tube 8 after rechecking the tube and trying to launch again"]
["2019-07-10T09:35:09.250","2019-07-10T05:35:09.250","KJ","Sonar","Multibeam","XBT Applied","AXBT132 applied in line 395"]
["2019-07-10T09:35:28.040","2019-07-10T05:35:28.040","KJ","Ship",null,null,"maneuvering around fishing vessels near dive site"]
["2019-07-10T09:37:22.650","2019-07-10T05:37:22.650","KJ","Sonar","EK",null,"change from CW to FM on 70 kHz"]
["2019-07-10T09:47:40.150","2019-07-10T05:47:40.150","KJ","Sonar","EK",null,"changed 18 kHz from 4 ms to 1 ms, 70 kHz FM from 2 ms to 1 ms"]
["2019-07-10T09:51:38.720","2019-07-10T05:51:38.720","KJ","Sonar","EK",null,"70 kHz back to 1 ms CW"]
["2019-07-10T09:54:34.090","2019-07-10T05:54:34.090","KJ","Sonar","Multibeam",null,"Knudsen and multibeam secure"]
["2019-07-10T09:55:15.400","2019-07-10T05:55:15.400","KJ","Sonar","ADCP",null,"on for arrival at dive site"]
["2019-07-10T09:56:31.860","2019-07-10T05:56:31.860","KJ","POS",null,null,"switched to ROV mode"]
["2019-07-10T20:56:11.400","2019-07-10T16:56:11.400","DP","POS",null,null,"Switched to mapping mode"]
["2019-07-10T20:57:43.170","2019-07-10T16:57:43.170","DP","Sonar","EK",null,"Stop recording, change pulse to 4,2,1,1, put it in FM, and start recording again"]
["2019-07-10T20:58:24.340","2019-07-10T16:58:24.340","DP","Sonar","Knudsen","Start pinging"]
["2019-07-10T20:58:32.490",{"$f":"IF(ISBLANK(A839),\" \",((A839)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-10T16:58:32.490"},"DP","Sonar","Knudsen","Start recording"]
["2019-07-10T20:59:16.600","2019-07-10T16:59:16.600","DP","Sonar","Multibeam","start pinging"]
["2019-07-10T21:06:30.220","2019-07-10T17:06:30.220","DP","Sonar","speedlog","secure"]
["2019-07-10T21:11:21.970","2019-07-10T17:11:21.970","DP","Sonar","Multibeam",null,"CPCTD 18 UP cast applied in line 0398"]
["2019-07-10T21:16:32.060","2019-07-10T17:16:32.060","KJ","Sonar","EK",null,"changed ping interval from 1 sec to maximum, did not fix interference in EM302"]
["2019-07-10T21:24:01.370","2019-07-10T17:24:01.370","KJ","Sonar","Multibeam","start logging",398]
["2019-07-10T21:31:53.100","2019-07-10T17:31:53.100","KJ","Sonar","ADCP",null,"ADCP machine has been restarted to troubleshoot lost comms; interference in EM302 from ADCPs; ADCPs shut off at the breaker, interference went away in EM302"]
["2019-07-10T21:58:30.890","2019-07-10T17:58:30.890","KJ","Sonar","Knudsen",null,"power from 2 to 1 in shallow water, still 1 ms"]
["2019-07-10T21:58:46.280","2019-07-10T17:58:46.280","KJ","Sonar","ADCP",null,"breaker turned back on; no interference in EM302; still troubleshooting"]
["2019-07-10T22:01:19.960","2019-07-10T18:01:19.960","KJ","XBT",null,"XBT launched","AXBT133"]
["2019-07-10T22:07:43","2019-07-10T18:07:43","KJ","Sonar",null,"XBT Applied","AXBT133 applied in line 0398"]
["2019-07-11T00:45:01.460","2019-07-10T20:45:01.460","DP","XBT",null,"XBT Launch","AXBT134 launched"]
["2019-07-11T00:50:31.110","2019-07-10T20:50:31.110","DP","Sonar","Multibeam","XBT Applied","AXBT134 applied in line 0404"]
["2019-07-11T01:00:25.980","2019-07-10T21:00:25.980","DP","Sonar","Knudsen",null,"Change range to 500m"]
["2019-07-11T02:06:39.820","2019-07-10T22:06:39.820","DP","XBT",null,"XBT Launch","AXBT135 launched"]
["2019-07-11T02:13:05.070","2019-07-10T22:13:05.070","DP","Sonar","Multibeam","XBT Applied","AXBT135 applied in line 0406"]
["2019-07-11T05:01:20.440","2019-07-11T01:01:20.440","DP","XBT",null,"XBT Launch","AXBT136 launched"]
["2019-07-11T05:07:34.320","2019-07-11T01:07:34.320","DP","Sonar","Multibeam","XBT Applied","AXBT136 applied in line 0409"]
["2019-07-11T06:19:59.840","2019-07-11T02:19:59.840","KJ","Sonar","All",null,"Seep survey pass 1 at 3-4 kts, MB line 411; EK 18 kHz 4 ms CW, 70 kHz 2 ms FM 45-90 kHz, 120 and 200 kHz 1 ms CW"]
["2019-07-11T06:21:04.250","2019-07-11T02:21:04.250","KJ","Sonar","Multibeam",null,"swath angles from 70/70 to 65/65 for seep survey"]
["2019-07-11T06:48:59.170","2019-07-11T02:48:59.170","KJ","Sonar","Knudsen",null,"changed range from 500 to 200 for seep site survey"]
["2019-07-11T07:01:10.770","2019-07-11T03:01:10.770","KJ","Sonar","All",null,"seep survey pass 2, MB line 413"]
["2019-07-11T07:08:05.890","2019-07-11T03:08:05.890","KJ","XBT",null,"XBT launched","AXBT137 launched"]
["2019-07-11T07:15:54.720","2019-07-11T03:15:54.720","KJ","Sonar","Multibeam","XBT Applied","AXBT137 applied in line 413"]
["2019-07-11T07:36:45","2019-07-11T03:36:45","KJ","Sonar","All",null,"seep survey pass 3, MB line 415"]
["2019-07-11T08:22:40.860","2019-07-11T04:22:40.860","KJ","Sonar","All",null,"seep survey pass 4, MB line 417"]
["2019-07-11T08:43:32.630","2019-07-11T04:43:32.630","KJ","Sonar","All",null,"seep survey pass 5, MB line 419"]
["2019-07-11T09:01:04.240","2019-07-11T05:01:04.240","KJ","Sonar","Multibeam",null,"backscatter blowout "]
["2019-07-11T09:21:20.030","2019-07-11T05:21:20.030","KJ","Sonar","Multibeam",null,"seep survey pass 6, MB line 421"]
["2019-07-11T09:42:04.850","2019-07-11T05:42:04.850","KJ","XBT",null,"XBT Launched","AXBT138"]
["2019-07-11T09:49:03.170","2019-07-11T05:49:03.170","SH","Sonar","Multibeam","XBT Applied","AXBT138 applied to line 0422"]
["2019-07-11T10:02:02.580","2019-07-11T06:02:02.580","SH","Sonar",null,null,"Setup for Dive (ADCPS,POS, secure, etc.)"]
["2019-07-11T20:52:14.660","2019-07-11T16:52:14.660","SH","Sonar","EK",null,"Changed pulse to 4,2,1,1"]
["2019-07-11T20:57:08.800","2019-07-11T16:57:08.800","DP","POS",null,null,"Switch to mapping mode"]
["2019-07-11T20:57:29.680","2019-07-11T16:57:29.680","DP","Sonar","ADCP","secure"]
["2019-07-11T20:59:10.380","2019-07-11T16:59:10.380","KJ","Sonar","EK","secure","Secure for speed noise testing"]
["2019-07-11T21:16:33.050","2019-07-11T17:16:33.050","DP","Sonar","speedlog","secure"]
["2019-07-11T21:37:48.730","2019-07-11T17:37:48.730","KJ","Sonar","Multibeam",null,"RX noise and spectrum BIST vs. speed testing from drifting to full speed in 2 kt increments; generators 1, 3, 4 are on; all echosounders secure; sea state is mild/calm, 1-2 ft waves and 2 ft swell, winds 15 kt from 170, will be on the stern for all tests after drifting as we steam toward the transit to Norfolk"]
["2019-07-11T21:45:01.620","2019-07-11T17:45:01.620","KJ","Sonar","Multibeam",null,"start 2 kt speed noise test"]
["2019-07-11T22:08:11.330","2019-07-11T18:08:11.330","KJ","Sonar","Multibeam",null,"Noise and Spectrum test failing, restarting TRU"]
["2019-07-11T22:11:20.140","2019-07-11T18:11:20.140","KJ","Sonar","Multibeam",null,"TRUs turned back on"]
["2019-07-11T22:20:51.570","2019-07-11T18:20:51.570","KJ","Sonar","Multibeam",null,"BIST all passed"]
["2019-07-11T23:10:40.830","2019-07-11T19:10:40.830","KJ","Sonar","Multibeam",null,"Completed all testing beginning mapping operations"]
["2019-07-11T23:11:55.720","2019-07-11T19:11:55.720","KJ","Sonar","Multibeam","Start pinging","start in MMM"]
["2019-07-11T23:13:04.200","2019-07-11T19:13:04.200","DP","XBT",null,"XBT Launch","AXBT139 launched"]
["2019-07-11T23:13:12.150","2019-07-11T19:13:12.150","KJ","Sonar","EK","Start Pinging"]
["2019-07-11T23:13:50.170","2019-07-11T19:13:50.170","KJ","Sonar","EK","Start recording"]
["2019-07-11T23:14:13.680","2019-07-11T19:14:13.680","KJ","Sonar","Knudsen","Start Pinging"]
["2019-07-11T23:14:35.170","2019-07-11T19:14:35.170","KJ","Sonar","Knudsen","Start recording"]
["2019-07-11T23:15:21.700","2019-07-11T19:15:21.700","KJ","Sonar","Multibeam",null,"power to -10 dB"]
["2019-07-11T23:17:51.490","2019-07-11T19:17:51.490","KJ","Sonar","Multibeam",null,"Max power"]
["2019-07-11T23:18:30.300","2019-07-11T19:18:30.300","KJ","Sonar","Multibeam","XBT Applied","AXBT139 applied in line 0423"]
["2019-07-11T23:18:36.200","2019-07-11T19:18:36.200","KJ","Sonar","Multibeam","start logging"]
["2019-07-11T23:40:24.480","2019-07-11T19:40:24.480","KJ","Sonar","All",null,"start of 5 kt subbottom line 241 up Norfolk Canyon, 1 ms pulse with TX power at 2, all Eks in CW with 18 at 4 ms, 70 at 2 ms, 120 and 200 at 1 ms, MB file 425"]
["2019-07-12T00:18:09.710","2019-07-11T20:18:09.710","SH","POS",null,null,"POS position was red for a bit (15 seconds??)"]
["2019-07-12T00:22:20.050","2019-07-11T20:22:20.050","KJ","Sonar","Multibeam",null,"interference in EM302 from unknown source"]
["2019-07-12T01:03:49.350","2019-07-11T21:03:49.350","DP","Sonar","Knudsen",null,"Turn onto line 242 for second part of sub bottom survey"]
["2019-07-12T01:30:13.100","2019-07-11T21:30:13.100","KJ","XBT",null,"XBT launched","AXBT140"]
["2019-07-12T01:36:55.360","2019-07-11T21:36:55.360","KJ","Sonar","Multibeam","XBT Applied","AXBT140 applied in line 428"]
["2019-07-12T01:55:20.910","2019-07-11T21:55:20.910","KJ","Sonar","Knudsen",null,"turn onto line 243 for third part of subbottom survey"]
["2019-07-12T01:58:11.630","2019-07-11T21:58:11.630","KJ","Sonar","All",null,"small swell is causing bubbles that occasionally wipe out all sonars"]
["2019-07-12T02:19:12.340","2019-07-11T22:19:12.340","KJ","Sonar","Knudsen",null,"turn onto line 244 for fourth and last part of subbottom survey up Norfolk Canyon"]
["2019-07-12T02:37:27.390","2019-07-11T22:37:27.390","KJ","XBT",null,"XBT launched","AXBT141"]
["2019-07-12T02:41:21.790","2019-07-11T22:41:21.790","KJ","Sonar","Multibeam","XBT Applied","AXBT141 applied in line 0432"]
["2019-07-12T02:41:45.240",{"$f":"IF(ISBLANK(A903),\" \",((A903)-DATE(1970,1,1))+25569+($C$1/24))","v":"2019-07-11T22:41:45.240"},"KJ","Sonar","Multibeam","secure"]
["2019-07-12T02:41:53.660","2019-07-11T22:41:53.660","DP","Sonar","Knudsen","secure"]
["2019-07-12T02:42:09.700","2019-07-11T22:42:09.700","DP","Sonar","EK","secure"]
["2019-07-12T14:20:47.850","2019-07-12T10:20:47.850","SH","Sonar","ADCP","secure"]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A967),\" \",((A967)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1031),\" \",((A1031)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1095),\" \",((A1095)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1159),\" \",((A1159)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1223),\" \",((A1223)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1287),\" \",((A1287)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1351),\" \",((A1351)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1415),\" \",((A1415)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1479),\" \",((A1479)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1543),\" \",((A1543)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1607),\" \",((A1607)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1671),\" \",((A1671)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1735),\" \",((A1735)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1799),\" \",((A1799)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1863),\" \",((A1863)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1927),\" \",((A1927)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1991),\" \",((A1991)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"Dropdowns","index":1,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Item","Sonar","Multibeam","EK","Knudsen","All","ADCP","Ksync","SpeedLog"]
["NB","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up","start pinging","Running","Secure"]
["CW","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure","secure","Paused","Start"]
["DS","Weather","Knudsen","New Line","Secure","Gain Mode","New Lines",null,"Configuration Change"]
["SH","Watch Change","All","Max Angle","Bottom Detection","Gain Value",null,null,"EK Enabled"]
["KJ","XBT","ADCP","Spike Filter Strength","Start Recording","Process Shift",null,null,"EK Disabled"]
["JD","Issue/Problem","Ksync","Slope Filter (On/Off)","Stop Recording","Tx Blanking",null,null,"Knudsen Enabled"]
["JM","POS","SpeedLog","Aeration Filter (On/Off)","Pulse Duration Change","Range",null,null,"Knudsen Disabled"]
["MW","Other",null,"Interference Filter (On/Off)",null,"Phase Mode",null,null,"MB Enabled"]
["ML","Multibeam",null,"Start Pinging",null,"Start Pinging",null,null,"MB Disabled"]
["DP","EK",null,"Secure",null,"Secure",null,null,"Group Change"]
[null,"Knudsen",null,"Start Logging",null,null,null,null,"ADCP Enabled"]
[null,"All",null,"BIST",null,"Start Recording",null,null,"ADCP Disabled"]
[null,"ADCP",null,"XBT Applied",null,"Stop Recording"]
[null,"Ksync"]
[null,"SpeedLog"]