{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["EX1602_Mapping_LogBook"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":20,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EX1602_Mapping_LogBook","index":0,"n_rows":135,"n_cols":7,"rows_kept":135,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1602",null,"ROV/Mapping Shakedown - Feb 12 to Feb 17, 2016",null,"UTC to Local: ",-10]
["UTC Time","Ship Time","WatchStander","Item","Sonar","Variable","Note"]
["2016-02-13T03:56:49.080",{"$f":"IF(ISBLANK(A3),\" \",((A3)-DATE(1970,1,1))+25569+(F1/24))","v":"2016-02-12T17:56:49.080"},"DF","Sonar","EK_18kHz","Start Pinging","Started pinging EK60 - 18,70, 120, 200 kHz and recording; Dan and Bill on watch"]
["2016-02-13T03:58:01.680",{"$f":"IF(ISBLANK(A4),\" \",((A4)-DATE(1970,1,1))+25569+(-10/24))","v":"2016-02-12T17:58:01.680"},"DF","Sonar","Multibeam",null,"Scanning for the transducer isnt working, restarting TRU to try and reconnect. LM -- Tried the following troubleshooting to TRU: restart SIS, restart TRU, check all cable and network connections, switched network cards. Confirmed that commands from SIS are going into TRU, but appears nothing is going out. The \"good power\" light is off on the 170V PSU, replaced with spare, but no luck getting TRU to talk to talk with SIS. Shutdown TRU at 2200 ship time, retry in morning. "]
["2016-02-13T04:04:49.170","2016-02-12T18:04:49.170","DF","Sonar","Multibeam",null,"Turned on TRU"]
["2016-02-13T04:09:57.560","2016-02-12T18:09:57.560","WWP","Sonar","Knudsen","Start Pinging","Started recording at 500 m, Range - 1000 m, Phase Range - 500 to 1500, TX Pulse - 1 ms, TX Power - 1, Gain - 32 dB, Max Range - 5000 m"]
["2016-02-13T04:32:17.990","2016-02-12T18:32:17.990","DF","Sonar","EK_18kHz",null,"Ranges all to 2000 m, and max depth range to 2000 m"]
["2016-02-13T04:42:24.580","2016-02-12T18:42:24.580","DF","Sonar","Knudsen","Tx Power","2, TX Pulse to 2 ms"]
["2016-02-13T04:46:18.780","2016-02-12T18:46:18.780","DF","Sonar","EK_18kHz",null,"Ranges all to 2500 m, and max depth range to 2500 m"]
["2016-02-13T04:53:15.690","2016-02-12T18:53:15.690","DF","Sonar","EK_18kHz",null,"Ranges all to 3000 m, and max depth range to 3000 m"]
["2016-02-13T04:55:34.120","2016-02-12T18:55:34.120","DF","Sonar","EK_18kHz",null,"Ranges all to 4000 m, and max depth ranges to 4000 m"]
["2016-02-13T06:01:25.130","2016-02-12T20:01:25.130","DF","Sonar","Knudsen","Phase Range","2000-3000 m"]
["2016-02-13T06:03:33.680","2016-02-12T20:03:33.680","DF","Sonar","Knudsen","Phase Range","1500-2500 m"]
["2016-02-13T06:47:17.690","2016-02-12T20:47:17.690","DF","Sonar","ADCP_300kHz",null,"Power up unit"]
["2016-02-13T06:57:41.710","2016-02-12T20:57:41.710","DF","Sonar","Multibeam",null,"TRU wont connect with SIS, shut down TRU for cold start tomorrow after Lindsay will email Kongsberg"]
["2016-02-13T06:59:36.490","2016-02-12T20:59:36.490","DF","Sonar","ADCP_300kHz",null,"Started new cruise EX1602_01_wh300 and started logging"]
["2016-02-13T07:06:22.900","2016-02-12T21:06:22.900","WWP","Sonar","EK_18kHz",null,"ranges set at 18kHz 4000m, 70 kHz 600m. Bottom Detection 18kHz at 4000m, 70 kHz 600m."]
["2016-02-13T07:11:12.770","2016-02-12T21:11:12.770","DF","Sonar","EK_18kHz",null,"200 kHz sonar secured for running ADCP wh300"]
["2016-02-13T11:33:10.850","2016-02-13T01:33:10.850","WWP","SONAR","EK_18kHz",null,"18 Khz, range, bottom detection and output all changed to 4200m"]
["2016-02-13T11:38:52.330","2016-02-13T01:38:52.330","WWP","Sonar","Knudsen",null,"Txpulse changed to 4.0"]
["2016-02-13T12:07:05.130","2016-02-13T02:07:05.130","WWP","SONAR","EK_18kHz",null,"18 Khz, range, bottom detection and output all changed to 4000 m"]
["2016-02-13T12:16:21.230","2016-02-13T02:16:21.230","WWP","SONAR","Knudsen",null,"Phase changed to; 2500-3500"]
["2016-02-13T12:41:52","2016-02-13T02:41:52","AB","Sonar","Knudsen","Range","500m, New file started"]
["2016-02-13T12:52:25.410","2016-02-13T02:52:25.410","AB","Sonar","Knudsen","Gain Value","37dB"]
["2016-02-13T14:00:49","2016-02-13T04:00:49","AB","Sonar","Knudsen","Phase Range","2750-3250m"]
["2016-02-13T15:03:12.440","2016-02-13T05:03:12.440","AB","Sonar","Knudsen","Phase Range","2250-2750m"]
["2016-02-13T15:05:45.900","2016-02-13T05:05:45.900","AB","Sonar","Knudsen","Phase Range","2500-3000m, Pulse 2.0ms, Gain 35"]
["2016-02-13T15:19:49.450","2016-02-13T05:19:49.450","AB","Sonar","Knudsen","Phase Range","2750-3250m"]
["2016-02-13T15:37:06.650","2016-02-13T05:37:06.650","AB","Ship",null,null,"Increasing speed, heading toward ROV calibration site."]
["2016-02-13T16:11:06.690","2016-02-13T06:11:06.690","AB","Sonar","Knudsen","Phase Range","2500-3000m "]
["2016-02-13T16:24:32.160","2016-02-13T06:24:32.160","AB","Sonar","Knudsen","Phase Range","2250-2750m"]
["2016-02-13T16:27:30.160","2016-02-13T06:27:30.160","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2016-02-13T16:33:51.210","2016-02-13T06:33:51.210","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2016-02-13T16:37:52.290","2016-02-13T06:37:52.290","AB","Sonar","Knudsen","Tx Power","1, Range 1250-1750m, Gain 30db"]
["2016-02-13T16:57:23.440","2016-02-13T06:57:23.440","AB","Sonar","Knudsen","Phase Range","1000-1500m, New line."]
["2016-02-13T17:01:27.660","2016-02-13T07:01:27.660","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2016-02-13T17:12:46.200","2016-02-13T07:12:46.200","Ab","Ship",null,null,"Arriving to ROV cal site. Securing sonars."]
["2016-02-13T17:14:47.530","2016-02-13T07:14:47.530","AB","Sonar","Knudsen","Secure","ADCP Secure, EK60 Secure"]
["2016-02-14T03:55:53.700","2016-02-13T17:55:53.700","DF","Sonar","Multibeam","Start Pinging","Error could not ping and survey wouldn’t show up. So we created a new survey EX1602a, with correct naming protocol"]
["2016-02-14T04:08:54.800","2016-02-13T18:08:54.800","DF","Sonar","Knudsen","Start Pinging","Started pinging and logging "]
["2016-02-14T04:10:41.010","2016-02-13T18:10:41.010","DF","Sonar","EK_18kHz","Start Pinging","Started pinging and recording EK60 18, 70, 120, 200 kHz"]
["2016-02-14T04:11:46.630","2016-02-13T18:11:46.630","DF","Sonar","Multibeam",null,"Lamp 3 sonar head statusn lamp was red but went green when we stopped pinging and opened installation parameters simultaneously, ran BIST"]
["2016-02-14T04:21:17.400","2016-02-13T18:21:17.400","DF","Sonar",null,null,"Secured Knudsen and EK60's "]
["2016-02-14T04:25:54.310","2016-02-13T18:25:54.310","DF","Sonar","Multibeam",null,"Restarted SIS and signed in under survey instead of admin"]
["2016-02-14T04:45:36.460","2016-02-13T18:45:36.460","DF","Sonar","Multibeam","Start Pinging","Started logging and pinging"]
["2016-02-14T04:45:55.220","2016-02-13T18:45:55.220","DF","Sonar","EK_18kHz",null,"Trying 18 and 70 kHz to see if it causes backscatter interference "]
["2016-02-14T04:53:50.730","2016-02-13T18:53:50.730","DF","Sonar","EK_18kHz",null,"Started pinging and recording EK60 18, 70, 120, 200 kHz"]
["2016-02-14T04:58:04.700","2016-02-13T18:58:04.700","DF","Sonar","EK_18kHz",null,"Changed range to 4000 m"]
["2016-02-14T05:17:09.850","2016-02-13T19:17:09.850","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2016-02-14T05:36:14.570","2016-02-13T19:36:14.570","LM","XBT",null,null,"Conduct XBT cast #1"]
["2016-02-14T05:54:55.250","2016-02-13T19:54:55.250","AB","XBT","xbt_","Apply Profile","Applied to line 0002."]
["2016-02-14T06:12:18.610","2016-02-13T20:12:18.610","wwp","sonar","Knudsen","Secure","Secured Knudsen and EK60's "]
["2016-02-14T06:22:41.590","2016-02-13T20:22:41.590","AB","Sonar","Multibeam","Ping Mode","DEEP."]
["2016-02-14T06:35:29.080","2016-02-13T20:35:29.080","AB","Sonar","Multibeam","New Line","0003 First line of target search. (Processed L1)"]
["2016-02-14T07:09:48.570","2016-02-13T21:09:48.570","AB","Sonar","Multibeam","Max Angle","60/55"]
["2016-02-14T07:38:49.470","2016-02-13T21:38:49.470","AB","Sonar","Multibeam","New Line","0004 (Processed L1)"]
["2016-02-14T07:50:56.220","2016-02-13T21:50:56.220","AB","Sonar","Multibeam",null,"Sonar Interference, possible whales"]
["2016-02-14T07:52:15.450","2016-02-13T21:52:15.450","AB","Sonar","Multibeam","New Line","0005 - Turn, Do not process"]
["2016-02-14T08:08:42.880","2016-02-13T22:08:42.880","AB","Sonar","Multibeam","New Line","0006 (Processed L2)"]
["2016-02-14T09:33:55.850","2016-02-13T23:33:55.850","DF","Sonar","Multibeam","New Line","0008 - Turn, Do not process"]
["2016-02-14T09:47:19.090","2016-02-13T23:47:19.090","DF","Sonar","Multibeam","New Line","0009 (Processed L3)"]
["2016-02-14T10:47:29","2016-02-14T00:47:29","AB","Sonar","Multibeam","New Line","0010 (Processed L3)"]
["2016-02-14T10:57:49.620","2016-02-14T00:57:49.620","AB","Sonar","Multibeam",null,"Strong sonar interference. Inference filter ON."]
["2016-02-14T11:06:26.300","2016-02-14T01:06:26.300","wwp","sonar","Multibeam","New line","0011, turn - do not process"]
["2016-02-14T11:17:33.560","2016-02-14T01:17:33.560","AB","Sonar","Multibeam","New Line","0012, interference filter off (Processed L4)"]
["2016-02-14T11:31:22.210","2016-02-14T01:31:22.210","AB","XBT","xbt_","Take Cast","#2"]
["2016-02-14T11:37:57.610","2016-02-14T01:37:57.610","AB","XBT","xbt_","Apply Profile","to line 0013. (Processed L4)"]
["2016-02-14T11:54:26.240",{"$f":"IF(ISBLANK(A68),\" \",((A68)-DATE(1970,1,1))+25569+(-10/24))","v":"2016-02-14T01:54:26.240"},"AB","Sonar","Multibeam","New Line","0014 - turn, do not process."]
["2016-02-14T12:06:59.630","2016-02-14T02:06:59.630","AB","SONAR","Multibeam","New Line","0015 (Processed L5)"]
["2016-02-14T12:51:32.980","2016-02-14T02:51:32.980","AB","Sonar","Multibeam","New Line","0016 - turn, do not process, holding for traffic situation to pass"]
["2016-02-14T13:17:25.630","2016-02-14T03:17:25.630","AB","SONAR","Multibeam","New Line","0017 (Processed L6)"]
["2016-02-14T14:00:46.430","2016-02-14T04:00:46.430","AB","SONAR","Multibeam","New Line","0018 - turn, do not process"]
["2016-02-14T14:14:43.730","2016-02-14T04:14:43.730","AB","Sonar","Multibeam","New Line","0019, possible target (Processed L7)"]
["2016-02-14T14:49:21.150","2016-02-14T04:49:21.150","AB","Sonar","Multibeam","New Line","0020 - turn, do not process"]
["2016-02-14T14:59:02.790","2016-02-14T04:59:02.790","AB","Sonar","Multibeam","New Line","0021 (Processed L8)"]
["2016-02-14T15:51:55.610","2016-02-14T05:51:55.610","AB","Sonar","Multibeam","New Line","0022 - turn, do not process"]
["2016-02-14T15:58:53.340","2016-02-14T05:58:53.340","AB","Sonar","Multibeam","New Line","0023"]
["2016-02-14T15:59:24","2016-02-14T05:59:24","AB","Ship",null,null,"Increase speed to 10 kts to arrive at Dive site."]
["2016-02-14T16:51:34.970","2016-02-14T06:51:34.970","AB","Sonar","Multibeam","New Line","0024"]
["2016-02-14T17:09:44.190","2016-02-14T07:09:44.190","AB","Sonar","Multibeam","Secure","Running BIST03 Test"]
["2016-02-15T00:22:43.150","2016-02-14T14:22:43.150","LM","Sonar","Multibeam","Start Pinging","In marine mammal mode"]
["2016-02-15T00:23:15.330","2016-02-14T14:23:15.330","LM","Sonar","Multibeam",null,"Status lamp on right turned red when pinging started"]
["2016-02-15T00:34:09.830","2016-02-14T14:34:09.830","LM","Sonar","Multibeam",null,"Out of marine mammal mode"]
["2016-02-15T00:35:56.380","2016-02-14T14:35:56.380","LM","Sonar","Multibeam","Max Angle","To 70 degrees"]
["2016-02-15T00:58:09.070","2016-02-14T14:58:09.070","DF","XBT","xbt_","Take Cast","003"]
["2016-02-15T00:59:07.120","2016-02-14T14:59:07.120","DF","XBT","xbt_","Apply Profile","applied to line 0025, started line 0026"]
["2016-02-15T01:00:00.480","2016-02-14T15:00:00.480","DF","Sonar","Multibeam","Ping Mode","Switched to Auto"]
["2016-02-15T01:21:12.880","2016-02-14T15:21:12.880","DF","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-02-15T01:29:45.120","2016-02-14T15:29:45.120","DF","Sonar","Knudsen","Phase Range","1750-2250"]
["2016-02-15T01:44:44.250","2016-02-14T15:44:44.250","DF","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-02-15T02:20:54.650","2016-02-14T16:20:54.650","WWP","Sonar","Knudsen","Phase Range","1750-2250"]
["2016-02-15T02:50:35.790","2016-02-14T16:50:35.790","DF","Sonar","Knudsen","Phase Range","1500-2000"]
["2016-02-15T02:53:03.170","2016-02-14T16:53:03.170","DF","Sonar","Multibeam","Interference Filter (On/Off)","Off"]
["2016-02-15T02:59:57.900","2016-02-14T16:59:57.900","DF","Sonar","Multibeam","Max Angle","75/70"]
["2016-02-15T03:09:57.940","2016-02-14T17:09:57.940","AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2016-02-15T03:11:30.680","2016-02-14T17:11:30.680","AB","Sonar","Multibeam","New Line","0029 - Turn"]
["2016-02-15T03:18:16.420","2016-02-14T17:18:16.420","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2016-02-15T03:22:03.250","2016-02-14T17:22:03.250","AB","Sonar","Multibeam","New Line","0030, Knudsen New line, EK60 New lines after start of turn"]
["2016-02-15T03:23:43.900","2016-02-14T17:23:43.900","AB","Sonar","Knudsen",null,"Tx Pulse 2, TxPower 1, Phase Range 500-100m, Gain 34dB"]
["2016-02-15T03:30:29.050","2016-02-14T17:30:29.050","AB","sonar","Knudsen","Phase Range","750-1250m"]
["2016-02-15T03:32:57.360","2016-02-14T17:32:57.360","DF","sonar","Multibeam","Max Angle","75/75"]
["2016-02-15T03:46:37.630","2016-02-14T17:46:37.630","DF","sonar","Knudsen","Phase Range","1000-1500"]
["2016-02-15T03:54:16.290","2016-02-14T17:54:16.290","DF","Sonar","Knudsen","Phase Range","1250-1750"]
["2016-02-15T03:57:00.050","2016-02-14T17:57:00.050","DF","Ship",null,null,"Asked bridge to move 500 m to STBD to extend coverage"]
["2016-02-15T04:13:59.730","2016-02-14T18:13:59.730","DF","Ship",null,null,"Asked bridge to move 1500 m to STBD to extend coverage"]
["2016-02-15T05:23:38.090","2016-02-14T19:23:38.090","AB","Sonar","Multibeam","New Line","0033 start of turn."]
["2016-02-15T05:35:19.970","2016-02-14T19:35:19.970","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2016-02-15T05:42:59.150","2016-02-14T19:42:59.150","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2016-02-15T06:30:56.880","2016-02-14T20:30:56.880","AB","Sonar","Knudsen","Tx Power",2]
["2016-02-15T06:48:05.220","2016-02-14T20:48:05.220","DF","Sonar","Knudsen","Phase Range","500-1000"]
["2016-02-15T06:55:06.190","2016-02-14T20:55:06.190","DF","Sonar","Knudsen","Tx Power",1]
["2016-02-15T06:55:22.020","2016-02-14T20:55:22.020","DF","Sonar","Knudsen","TX Pulse","1 ms"]
["2016-02-15T07:06:46.380","2016-02-14T21:06:46.380","DF","XBT","xbt_","Take Cast","004"]
["2016-02-15T07:07:11.760","2016-02-14T21:07:11.760","LM","Sonar","Multibeam",null,"Gradual shift -- 500 m to stb"]
["2016-02-15T07:14:49.320","2016-02-14T21:14:49.320","DF","XBT","xbt_","Apply Profile","applied to 0035, started line 0036"]
["2016-02-15T07:43:42.840","2016-02-14T21:43:42.840","DF","Sonar","Knudsen","Phase Range","250-750"]
["2016-02-15T08:39:18.910","2016-02-14T22:39:18.910","AB","Sonar","Knudsen","Phase Range","500-1000"]
["2016-02-15T09:06:10.990","2016-02-14T23:06:10.990","DF","Sonar","Knudsen","Phase Range","750-1250"]
["2016-02-15T09:20:40.190","2016-02-14T23:20:40.190","DF","SONAR","Multibeam",null,"Cont line for turn"]
["2016-02-15T09:22:06.610","2016-02-14T23:22:06.610","DF","Sonar","Knudsen","Phase Range","1000-1500"]
["2016-02-15T09:24:40.570","2016-02-14T23:24:40.570","AB","Sonar","Knudsen","TX Pulse","2 ms"]
["2016-02-15T09:25:03.160","2016-02-14T23:25:03.160","AB","SONAR","Knudsen","TX Power",2]
["2016-02-15T10:04:17.340","2016-02-15T00:04:17.340","DF","Sonar","Knudsen","TX Pulse","1 ms"]
["2016-02-15T10:04:41.400","2016-02-15T00:04:41.400","DF","Sonar","Knudsen","TX Power",1]
["2016-02-15T10:12:12.810","2016-02-15T00:12:12.810","AB","Sonar","Knudsen","Phase Range","500-1000"]
["2016-02-15T10:25:00.330","2016-02-15T00:25:00.330","DF","Sonar","Knudsen","Phase Range","250-750"]
["2016-02-15T10:45:12.500","2016-02-15T00:45:12.500","DF","Sonar","Multibeam",null,"Started new line for turn 0041"]
["2016-02-15T10:56:06.900","2016-02-15T00:56:06.900","DF","Sonar","Multibeam",null,"Started new line for back on trackline"]
["2016-02-15T12:08:07.270","2016-02-15T02:08:07.270","AB","Sonar","Multibeam","New Line","0045 - turn"]
["2016-02-15T12:19:31.130","2016-02-15T02:19:31.130","AB","Sonar","Multibeam","New Line","0046"]
["2016-02-15T13:27:18","2016-02-15T03:27:18","AB","XBT","xbt_","Take Cast","Cast #5"]
["2016-02-15T13:36:09.910",{"$f":"IF(ISBLANK(A132),\" \",((A132)-DATE(1970,1,1))+25569+(-10/24))","v":"2016-02-15T03:36:09.910"},"wp","sonar","Multibeam",null,"Started New Line 0048"]
["2016-02-15T14:05:06.050","2016-02-15T04:05:06.050","AB","Sonar",null,null,"All sonars secured. Transiting to Honolulu"]
["2016-02-15T14:05:54.710","2016-02-15T04:05:54.710","AB","Sonar","Multibeam",null,"BIST Test Completed. All passed"]
["2016-02-15T22:26:14.110","2016-02-15T12:26:14.110","LM","Sonar","Multibeam",null,"Secure TRU"]