{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2000,"n_cols":7,"rows_kept":2000,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1605L3","UTC to Local: ",10,11,12,"UTC 4","Cruise Details: Cruise Dates"]
[null,null,null,null,"2016-06-23T07:11:52.760"]
["2016-07-08T06:36:49.230","Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2016-06-17T02:42:25.770",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-06-17T12:42:25.770"},"DS","Sonar","ADCP",null,"logging since port, ship transitng out of Apra Harbor, Guam, testing for ROV use"]
["2016-06-17T02:44:32.430","2016-06-17T12:44:32.430","DS","Sonar","Multibeam",null,"All BISTs passed"]
["2016-06-17T03:19:50.310","2016-06-17T13:19:50.310","DS","XBT",null,null,"XBT 1 completed "]
["2016-06-17T03:42:07.520","2016-06-17T13:42:07.520","DS","XBT",null,null,"XBT 001 applied to MB line 000 (not logging yet) . MB in softstart for 15 minutes. "]
["2016-06-17T03:48:46.680","2016-06-17T13:48:46.680","DS","Sonar","EK","Start Pinging","Start Line"]
["2016-06-17T03:50:49.680","2016-06-17T13:50:49.680","DS","Sonar","Multibeam","New Line","started logging multibeam, line 000"]
["2016-06-17T04:47:00.360","2016-06-17T14:47:00.360","DS","Sonar","Knudsen",null,"Start Line, delayed start due to survey username password problem (resolved) "]
["2016-06-17T06:04:47.090","2016-06-17T16:04:47.090","DS","Sonar","Multibeam","Max Angle","port reduced to 65 to fill gaps"]
["2016-06-17T06:52:03.380","2016-06-17T16:52:03.380","DS","Sonar","Multibeam","Max Angle","port reduced to 57 stbd opened to 75"]
["2016-06-17T07:28:05.920","2016-06-17T17:28:05.920","JM","Sonar","Multibeam","Max Angle","port opened to 70"]
["2016-06-17T07:35:06.360","2016-06-17T17:35:06.360","JM","Sonar","Multibeam","Max Angle","port opened to 75"]
["2016-06-17T09:26:20.520","2016-06-17T19:26:20.520","JM","XBT",null,null,"XBT 002"]
["2016-06-17T10:04:17.150","2016-06-17T20:04:17.150","JM","XBT",null,null,"XBT 002 applied to line 0006"]
["2016-06-17T11:57:33.240","2016-06-17T21:57:33.240","JM","Other",null,null,"New extended line plan to dive site created"]
["2016-06-17T12:17:24.130","2016-06-17T22:17:24.130","JM","Sonar","Knudsen","Tx Power","Power to 1 due to shallow waters (150m). Range at 200. Started new line"]
["2016-06-17T12:21:39.230","2016-06-17T22:21:39.230","JM","Sonar","Knudsen","Tx Power","Power back to 2, deeper water. Started new line"]
["2016-06-17T12:24:36.910","2016-06-17T22:24:36.910","JM","Sonar","Knudsen","Range","Range to 500. Started new line"]
["2016-06-17T14:07:52.650","2016-06-18T00:07:52.650","JM","Sonar","Knudsen","Gain Value","44dB"]
["2016-06-17T14:16:51.030","2016-06-18T00:16:51.030","JM","Sonar","Knudsen","Gain Value","36dB"]
["2016-06-17T14:24:34.110","2016-06-18T00:24:34.110","JM","Sonar","Knudsen","Tx Power","Power to 1 due to shallow waters. Range 200. Started new line"]
["2016-06-17T14:32:01","2016-06-18T00:32:01","JM","Sonar","Knudsen","Tx Power","Power back to 2, deeper water. Range 500. Gain 24dB. Started new line"]
["2016-06-17T14:33:58.180","2016-06-18T00:33:58.180","JM","Sonar","Knudsen","Gain Value","32dB"]
["2016-06-17T15:08:01.680","2016-06-18T01:08:01.680","JM","XBT",null,null,"XBT 003"]
["2016-06-17T15:18:42.510","2016-06-18T01:18:42.510","JM","XBT",null,null,"XBT 003 applied to line 0011"]
["2016-06-17T16:15:48.240","2016-06-18T02:15:48.240","JM","Sonar","Multibeam","Max Angle","port and stb 70"]
["2016-06-17T16:16:48.230","2016-06-18T02:16:48.230","JM","Sonar","Multibeam","Along Direction Pitch","1 degree to avoid nadir noise"]
["2016-06-17T16:37:43.400","2016-06-18T02:37:43.400","JM","Sonar","Multibeam","Max Angle","port and stb 75"]
["2016-06-17T20:05:00.870","2016-06-18T06:05:00.870","JM","Sonar","All","Secure","Arrived at FDM2 Dive Site. All secure"]
["2016-06-18T05:49:40.880","2016-06-18T15:49:40.880","CW","XBT",null,null,"XBT 004"]
["2016-06-18T06:08:21.490","2016-06-18T16:08:21.490","DS","Sonar","Multibeam",null,"Multibeam not able to find bottom, no water column shown, restarted SIS to fix."]
["2016-06-18T06:20:40.920","2016-06-18T16:20:40.920","DS","Sonar","Multibeam",null,"ADCPs were still on - turned off and EM302 started tracking bottom, started logging MB, EK 60, and Knudsen"]
["2016-06-18T06:41:58.640","2016-06-18T16:41:58.640","CW","Sonar","Knudsen",null,"TX Pulse 15; Power 2; Range 1000"]
["2016-06-18T07:53:42.070","2016-06-18T17:53:42.070","DS","Sonar","Multibeam","Max Angle","reduced stbd max angle to 55. transiting at 10.5-11 knots is making some holes in data. "]
["2016-06-18T07:58:36.760","2016-06-18T17:58:36.760","DS","Sonar","Multibeam","Max Angle","port max to 70 "]
["2016-06-18T08:01:37.570","2016-06-18T18:01:37.570","DS","Sonar","Knudsen","Gain Value","reduced from 38 to 34"]
["2016-06-18T08:59:18.340","2016-06-18T18:59:18.340","JM","Watch Change"]
["2016-06-18T09:00:18.180","2016-06-18T19:00:18.180","DS","Sonar","Knudsen","Tx Pulse","reduced pulse to 2 ms and gain to 30"]
["2016-06-18T09:06:52.540","2016-06-18T19:06:52.540","JM","Sonar","Multibeam","Max Angle","stb max to 70 "]
["2016-06-18T09:11:02.200","2016-06-18T19:11:02.200","JM","Sonar","Multibeam","Max Angle","port max to 75"]
["2016-06-18T09:19:00.330","2016-06-18T19:19:00.330","JM","Sonar","Knudsen","Range","Range 500, started new line"]
["2016-06-18T09:39:16.260","2016-06-18T19:39:16.260","JM","Sonar","Knudsen","Tx Pulse","Pulse to 4ms, gain to 32dB"]
["2016-06-18T10:58:17.910","2016-06-18T20:58:17.910","JM","Sonar","Multibeam","Max Angle","port max to 70 "]
["2016-06-18T11:10:00.200","2016-06-18T21:10:00.200","JM","XBT",null,null,"XBT 005"]
["2016-06-18T11:26:46.530","2016-06-18T21:26:46.530","JM","XBT",null,null,"XBT 005 applied to line 0022"]
["2016-06-18T13:07:43.380","2016-06-18T23:07:43.380","JM","Sonar","Knudsen","Range","Range 200, gain 37dB, started new line"]
["2016-06-18T13:17:12.820","2016-06-18T23:17:12.820","JM","Sonar","Knudsen","Range","Range 500, gain 35dB, started new line"]
["2016-06-18T14:48:40.320","2016-06-19T00:48:40.320","JM","Sonar","Multibeam","Along Direction Pitch","Set to 1, major nadir penetration "]
["2016-06-18T16:02:09.440","2016-06-19T02:02:09.440","JM","Sonar","Multibeam","Max Angle","port/stb max angle to 50. Ship sped up and trying to avoid data holidays"]
["2016-06-18T16:20:25.110","2016-06-19T02:20:25.110","JM","Sonar","Multibeam","Max Angle","port/stb max angle to 52"]
["2016-06-18T16:43:51.740","2016-06-19T02:43:51.740","JM","XBT",null,null,"XBT 006"]
["2016-06-18T16:48:19.670","2016-06-19T02:48:19.670","JM","Sonar","Multibeam","Max Angle","port/stb max angle to 55"]
["2016-06-18T16:53:00.140","2016-06-19T02:53:00.140","JM","XBT",null,null,"XBT 006 applied to line 0027"]
["2016-06-18T17:36:08.970","2016-06-19T03:36:08.970","JM","Sonar","Multibeam","Max Angle","port/stb max angle to 52"]
["2016-06-18T18:55:17.670","2016-06-19T04:55:17.670","JM","Sonar","Knudsen","Gain Value","TVG 10logR, gain value 5dB. Started new line"]
["2016-06-18T19:04:56.800","2016-06-19T05:04:56.800","JM","Sonar","Knudsen","Gain Value","Turned TVG off, didn't improve data. Gain to 35dB. Started new line"]
["2016-06-18T19:07:00.170","2016-06-19T05:07:00.170","JM","Sonar","Multibeam","Max Angle","port max angle to 60, stb 55"]
["2016-06-18T19:42:23.890","2016-06-19T05:42:23.890","JM","Sonar","Multibeam","Max Angle","port max angle to 65 stb 65"]
["2016-06-18T19:48:57.120","2016-06-19T05:48:57.120","JM","Sonar","Multibeam","Max Angle","port max angle to 75 stb 75"]
["2016-06-18T20:06:24.600","2016-06-19T06:06:24.600","JM","Sonar","Knudsen","Tx Power","power to 1. depth shallower than 1000m. Gain 47dB"]
["2016-06-18T20:21:15.360","2016-06-19T06:21:15.360","JM","Sonar","All","Secure","At Pagan dive site"]
["2016-06-19T07:10:44.400","2016-06-19T17:10:44.400","JM","Sonar","Multibeam","Start Pinging","Logging EK60 as well, MB is soft start"]
["2016-06-19T07:18:27.450","2016-06-19T17:18:27.450","DS","XBT",null,null,"XBT 007 collected."]
["2016-06-19T07:25:04.210","2016-06-19T17:25:04.210","DS","XBT",null,null,"XBT 007 applied to line 0031"]
["2016-06-19T07:26:31.420","2016-06-19T17:26:31.420","DS","Sonar","Multibeam",null,"switched off soft start"]
["2016-06-19T07:32:55.790","2016-06-19T17:32:55.790","DS","Sonar","Knudsen","Start Pinging","logging Knudsen. Pulse 4 ms, range 500m, gain 36"]
["2016-06-19T08:45:42.980",{"$f":"IF(ISBLANK(A70),\" \",((A70)-DATE(1970,1,1))+25569+($C$1/24))","v":"2016-06-19T18:45:42.980"},"DS","Sonar","Multibeam",null,"max depth changed to 4000m"]
["2016-06-19T08:47:09.770","2016-06-19T18:47:09.770","JM","Watch Change"]
["2016-06-19T09:27:21.150","2016-06-19T19:27:21.150","JM","Sonar","Knudsen","Gain Value","44"]
["2016-06-19T13:39:46.820","2016-06-19T23:39:46.820","JM","XBT",null,null,"XBT 008"]
["2016-06-19T13:50:10.470","2016-06-19T23:50:10.470","JM","XBT",null,null,"XBT 008 applied to line 0037"]
["2016-06-19T16:51:23.300","2016-06-20T02:51:23.300","JM","Sonar","Knudsen","Gain Value","32"]
["2016-06-19T17:04:45.290","2016-06-20T03:04:45.290","JM","Sonar","Knudsen","Gain Value","37"]
["2016-06-19T19:26:21.820","2016-06-20T05:26:21.820","JM","Sonar","Multibeam","New Line","Turn. Line 0044"]
["2016-06-19T19:31:08.740","2016-06-20T05:31:08.740","JM","Sonar","Multibeam","New Line","End turn. line 0045 "]
["2016-06-19T20:02:52.690","2016-06-20T06:02:52.690","JM","Sonar","Multibeam","New Line","Turn. Line 0046"]
["2016-06-19T20:06:10.790","2016-06-20T06:06:10.790","JM","Sonar","Multibeam","New Line","End turn. line 0047"]
["2016-06-19T20:25:45.020","2016-06-20T06:25:45.020","JM","Sonar","All","Secure","Arrived at Maug Dive Site"]
["2016-06-20T03:43:23.580","2016-06-20T13:43:23.580","DS","Sonar","EK","Start Pinging","Running EK60s to inform ROV mid-water transit depth selection."]
["2016-06-20T07:14:28.310","2016-06-20T17:14:28.310","DS","Sonar","Multibeam","Start Pinging","started in softstart, logging data"]
["2016-06-20T07:24:14.060","2016-06-20T17:24:14.060","DS","XBT",null,null,"XBT 009 conducted"]
["2016-06-20T07:37:25.250","2016-06-20T17:37:25.250","DS","XBT",null,null,"XBT 009 applied to line 0048, softstart turned off"]
["2016-06-20T07:44:14.350","2016-06-20T17:44:14.350","DS","Sonar","Knudsen","Start Pinging","start logging"]
["2016-06-20T07:50:14.580","2016-06-20T17:50:14.580","DS","Sonar",null,null,"chsanged the range on EK60 (70kHz) to 2500m "]
["2016-06-20T09:00:31.920","2016-06-20T19:00:31.920","JM","Watch Change",null,null,"Jason and Charlie on watch"]
["2016-06-20T10:16:35.400","2016-06-20T20:16:35.400","DS","Sonar","Knudsen","Tx Pulse","pulse to 8, gain to 38. "]
["2016-06-20T13:24:11.030","2016-06-20T23:24:11.030","JM","XBT",null,null,"XBT 010"]
["2016-06-20T13:31:25.220","2016-06-20T23:31:25.220","JM","XBT",null,null,"XBT 010 applied to line 0054"]
["2016-06-20T16:11:17.470",{"$f":"IF(ISBLANK(A92),\" \",((A92)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-06-21T03:11:17.470"},"JM","Sonar","Knudsen","Tx Power","Power to 3, Pulse 4, Gain 42, started new line"]
["2016-06-20T18:04:17.650",{"$f":"IF(ISBLANK(A93),\" \",((A93)-DATE(1970,1,1))+25569+($D$1/24))","v":"2016-06-21T05:04:17.650"},"JM","Sonar","Knudsen","Gain Value","51 dB"]
["2016-06-20T18:09:38.390","2016-06-21T05:09:38.390","JM","Sonar","Knudsen","Range","Turn. Range to 1000, Tx pulse to 2, Gain to 42. Started new line"]
["2016-06-20T18:11:11.390","2016-06-21T05:11:11.390","JM","Sonar","Multibeam","New Line","Turn line 0059"]
["2016-06-20T18:20:54.730","2016-06-21T05:20:54.730","JM","Sonar","Multibeam","New Line","Turn line 0060. Also started new Knudsen line"]
["2016-06-20T18:44:00.030","2016-06-21T05:44:00.030","JM","Sonar","Multibeam","New Line","Turn line 0061. Also started new Knudsen line"]
["2016-06-20T18:50:47.510","2016-06-21T05:50:47.510","JM","Sonar","Knudsen","Tx Pulse","8 ms"]
["2016-06-20T19:11:14.510","2016-06-21T06:11:14.510","JM","Sonar","All","Secure","Arrived at Hadal Ridge Dive site"]
["2016-06-20T19:11:59.910","2016-06-21T06:11:59.910","JM","Sonar","ADCP",null,"Start ADCP"]
["2016-06-21T07:59:10.110","2016-06-21T18:59:10.110","DS","Sonar",null,null,"ADCPs secured. MBES started in softstart. EK60s started logging."]
["2016-06-21T08:15:08.750","2016-06-21T19:15:08.750","JM","Watch Change",null,null,"Charlie and Jason on watch"]
["2016-06-21T08:30:06.600","2016-06-21T19:30:06.600","DS","XBT",null,null,"XBT 011 conducted"]
["2016-06-21T08:37:12.390","2016-06-21T19:37:12.390","CW","XBT",null,null,"XBT applied to Line 0062"]
["2016-06-21T08:41:29.400","2016-06-21T19:41:29.400","JM","Sonar","All",null,"All systems pinging and logging"]
["2016-06-21T09:16:16.620","2016-06-21T20:16:16.620","JM","Sonar","Knudsen","Gain Value","42dB"]
["2016-06-21T09:45:17.640","2016-06-21T20:45:17.640","DS","Sonar","Multibeam",null,"min to 500, max to 5500"]
["2016-06-21T10:08:25.740","2016-06-21T21:08:25.740","JM","Sonar","Knudsen","Gain Value","37dB"]
["2016-06-21T10:22:38.910","2016-06-21T21:22:38.910","JM","Sonar","Knudsen","Tx Power","Power to 2- moving shallower, gain 42 dB, started new line"]
["2016-06-21T10:38:33.140","2016-06-21T21:38:33.140","JM","Sonar","Knudsen","Gain Value","37dB"]
["2016-06-21T11:33:50.820","2016-06-21T22:33:50.820","JM","Sonar","Knudsen","Gain Value","42dB"]
["2016-06-21T12:32:16.660","2016-06-21T23:32:16.660","JM","Sonar","Knudsen","Tx Pulse","Pulse to 4 ms, gain to 34 dB"]
["2016-06-21T13:29:44.290","2016-06-22T00:29:44.290","JM","Sonar","Knudsen","Tx Power","Power to 3, Pulse 4, Gain 34, started new line"]
["2016-06-21T14:46:08.480","2016-06-22T01:46:08.480","JM","XBT",null,null,"XBT 012"]
["2016-06-21T14:49:44.660","2016-06-22T01:49:44.660","JM","XBT",null,null,"XBT cast applied to line 0068"]
["2016-06-21T17:00:18.590","2016-06-22T04:00:18.590","JM","Sonar","Knudsen","Tx Power","Power to 2, Pulse 4, Gain 34, started new line"]
["2016-06-21T17:28:19.560","2016-06-22T04:28:19.560","JM","Sonar","Knudsen","Tx Pulse","Pulse to 2 ms, gain to 31 dB, started new line"]
["2016-06-21T19:35:47.750","2016-06-22T06:35:47.750","JM","Sonar","All","Secure","Arrived at Ahyi Dive Site"]
["2016-06-21T19:38:56.950","2016-06-22T06:38:56.950","JM","Sonar","ADCP",null,"Started"]
["2016-06-21T21:59:13.760","2016-06-22T08:59:13.760","DS","Sonar","EK","Start Pinging","EK60s logging over Ahyi dive site to look for water column plumes, turbidity, etc. "]
["2016-06-22T05:59:54.920","2016-06-22T16:59:54.920","DS","Sonar",null,null,"Derek and Charlie on watch. Started pinging MB in softstart. Synced EK 60. "]
["2016-06-22T06:06:49.140","2016-06-22T17:06:49.140","DS","Sonar","Multibeam","Along Direction Pitch","Set to 1, major nadir penetration, logging turn line 0073"]
["2016-06-22T06:23:53.320","2016-06-22T17:23:53.320","DS","Sonar","Multibeam","New Line","Start survey line 0074 over Ahyi summit. "]
["2016-06-22T06:45:48.490","2016-06-22T17:45:48.490","DS","XBT",null,null,"XBT 013 conducted"]
["2016-06-22T06:53:29.480","2016-06-22T17:53:29.480","DS","XBT",null,null,"applied XBT 013 to line 0074"]
["2016-06-22T06:55:23.380","2016-06-22T17:55:23.380","DS","Sonar","Knudsen",null,"power 2, pulse, 8, range 1000, gain  38"]
["2016-06-22T07:28:20.150","2016-06-22T18:28:20.150","DS","Sonar","Knudsen",null,"reduced pulse to 2, gain to 30, file was not logging. Started logging. "]
["2016-06-22T08:01:28.400","2016-06-22T19:01:28.400","JM","Watch Change"]
["2016-06-22T08:28:20.560","2016-06-22T19:28:20.560","JM","Sonar","Knudsen","Gain Value","34 dB"]
["2016-06-22T09:36:14.840","2016-06-22T20:36:14.840","JM","Sonar","Knudsen","Gain Value","32 dB"]
["2016-06-22T10:04:46.820","2016-06-22T21:04:46.820","JM","Sonar","Knudsen","Range","changed to 500m"]
["2016-06-22T10:21:10.820","2016-06-22T21:21:10.820","JM","Sonar","Knudsen","Tx Pulse","4 ms"]
["2016-06-22T11:27:43.480","2016-06-22T22:27:43.480","JM","Sonar","Knudsen",null,"new line for turn"]
["2016-06-22T11:46:02.140","2016-06-22T22:46:02.140","JM","Sonar","Knudsen",null,"new line for turn"]
["2016-06-22T13:15:42.970",{"$f":"IF(ISBLANK(A135),\" \",((A135)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-06-23T01:15:42.970"},"JM","XBT",null,null,"XBT 014"]
["2016-06-22T13:20:44.870",{"$f":"IF(ISBLANK(A136),\" \",((A136)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-06-23T01:20:44.870"},"JM","XBT",null,null,"XBT cast applied to line 0081"]
["2016-06-22T18:07:03.170","2016-06-23T06:07:03.170","JM","Sonar","Multibeam","New Line","Turn. Diverting course to remain out of 12 mile zone until engineering proceedures are complete. Start line 88"]
["2016-06-22T18:15:53.470","2016-06-23T06:15:53.470","JM","Sonar","Multibeam","New Line","Back on track. Start line 89"]
["2016-06-22T18:33:41.550","2016-06-23T06:33:41.550","JM","Sonar","All","Secure","At Supply Reef dive site"]
["2016-06-23T04:51:10","2016-06-23T16:51:10","DS","Sonar","Multibeam","Start Pinging","softstart, Charlie and Derek on watch"]
["2016-06-23T05:11:30.290","2016-06-23T17:11:30.290","DS","Sonar","Multibeam",null,"started logging transit survey line 0090"]
["2016-06-23T05:15:26.930","2016-06-23T17:15:26.930","DS","Sonar",null,null,"logging EK60s and Knudsen"]
["2016-06-23T05:32:08.680","2016-06-23T17:32:08.680","DS","XBT",null,null,"XBT 15 conducted"]
["2016-06-23T05:39:13.910","2016-06-23T17:39:13.910","DS","XBT",null,null,"XBT 15 applied to line 0090"]
["2016-06-23T05:41:35.120","2016-06-23T17:41:35.120","DS","Sonar","Multibeam","Along Direction Pitch","changed to -2 to get rid of nadir shoal artifacts"]
["2016-06-23T06:52:17.960","2016-06-23T18:52:17.960","JM","Watch Change"]
["2016-06-23T07:01:23.810","2016-06-23T19:01:23.810","CW","Sonar","Multibeam","New Line","new line 0092 for turn"]
["2016-06-23T07:12:11.360","2016-06-23T19:12:11.360","CW","Sonar","Multibeam","New Line","new line 0093 for mainscheme"]
["2016-06-23T07:29:05.210","2016-06-23T19:29:05.210","JM","Sonar","Knudsen","Range","Range to 500. Started new line"]
["2016-06-23T07:39:20.780","2016-06-23T19:39:20.780","JM","Sonar","Knudsen","Gain Value","30 dB"]
["2016-06-23T09:58:43.740","2016-06-23T21:58:43.740","CW","Sonar","Multibeam","Along Direction Pitch","Chaged to -2 to grab sudden nadir gap. Then kept at -1. "]
["2016-06-23T10:31:36.540","2016-06-23T22:31:36.540","CW","Sonar","Multibeam","New Line","New line 0097 for turn"]
["2016-06-23T10:52:56.210","2016-06-23T22:52:56.210","JM","Sonar","Multibeam","New Line","New line 0098 resume trackline. Also new Knudsen line"]
["2016-06-23T10:55:39.770","2016-06-23T22:55:39.770","JM","Sonar","Knudsen","Tx Pulse","4 ms, Gain 35 dB"]
["2016-06-23T12:26:54.960","2016-06-24T00:26:54.960","JM","XBT",null,null,"XBT cast 016"]
["2016-06-23T12:36:38.130","2016-06-24T00:36:38.130","JM","XBT",null,null,"XBT applied to Line 0099"]
["2016-06-23T18:20:05.670","2016-06-24T06:20:05.670","JM","Sonar","All","Secure","Arrival at Chammoro Dive Site"]
["2016-06-24T23:30:00","2016-06-25T11:30:00","DS","Sonar","EK","Start Pinging","started EK60s during dive over Chammoro Seamount where some minor hydrothermal vents were discovered. "]
["2016-06-24T04:32:00","2016-06-24T16:32:00","DS","Sonar","EK","Secure","04:32 stopped logging/pinging EK60s over dive site, secured ADCP "]
["2016-06-24T04:49:03.340","2016-06-24T16:49:03.340","DS","Sonar","Multibeam",null,"Derek and Charlie on watch. Multibeam failed two BIST tests. Restarting SIS and TRU. "]
["2016-06-24T05:23:18.850","2016-06-24T17:23:18.850","CW","Sonar","Multibeam","Start Pinging","BIST's passed. Started logging, line 0113"]
["2016-06-24T05:30:18.430","2016-06-24T17:30:18.430","CW","Sonar","Multibeam",null,"Temporery fallout from ADCP being mysteriously restarted. All is well now."]
["2016-06-24T05:34:20.160","2016-06-24T17:34:20.160","DS","Sonar","Knudsen","Start Pinging","started logging"]
["2016-06-24T05:41:22.840","2016-06-24T17:41:22.840","DS","XBT",null,null,"XBT 17 conducted"]
["2016-06-24T05:51:20.480","2016-06-24T17:51:20.480","DS","XBT",null,null,"XBT 17 applied to line 0113"]
["2016-06-24T06:16:55.960","2016-06-24T18:16:55.960","CW","Sonar","Multibeam","Ping Mode","Changed to DEEP mode, Stb ang to 57 to solve sawtooth, -1 Along Direction pitch."]
["2016-06-24T06:40:33.600","2016-06-24T18:40:33.600","DS","Other",null,null,"going 11 knots, asked ship to slow to 10 for better data quality, switched to auto"]
["2016-06-24T06:47:03.880","2016-06-24T18:47:03.880","DS","Other",null,null,"finding new shallow feature (700m), asked ship to slow to 8.5-9. "]
["2016-06-24T06:48:47.170","2016-06-24T18:48:47.170","DS","Sonar","Knudsen","Tx Power","Power 1, pulse 8, gain 40"]
["2016-06-24T07:00:20","2016-06-24T19:00:20","JM","Watch Change"]
["2016-06-24T07:14:56.780","2016-06-24T19:14:56.780","JM","Sonar","Knudsen","Tx Pulse","4 ms, gain 44"]
["2016-06-24T07:25:13.090","2016-06-24T19:25:13.090","JM","Sonar","Knudsen","Tx Power","Power 2, pulse 4, gain 41"]
["2016-06-24T09:09:33.490","2016-06-24T21:09:33.490","JM","Sonar","Knudsen","Gain Value","36 dB"]
["2016-06-24T09:49:28.510","2016-06-24T21:49:28.510","JM","Sonar","Knudsen","Range","200m, power 1, gain 42 dB, approaching summit, new line"]
["2016-06-24T10:01:05.140","2016-06-24T22:01:05.140","JM","Sonar","Knudsen","Range","1000m, past summit, new line"]
["2016-06-24T10:04:16.420","2016-06-24T22:04:16.420","JM","Sonar","Knudsen","Tx Power","power to 2, gain 37 dB"]
["2016-06-24T10:08:24.880","2016-06-24T22:08:24.880","JM","Sonar","Multibeam",null,"Possible plume in water coulmn line 117"]
["2016-06-24T11:20:20.120","2016-06-24T23:20:20.120","JM","XBT",null,null,"XBT cast 018"]
["2016-06-24T11:26:21.910","2016-06-24T23:26:21.910","JM","XBT",null,null,"XBT applied to line 123"]
["2016-06-24T11:31:13.310","2016-06-24T23:31:13.310","JM","Sonar","Knudsen","Range","200m, power 1, gain 42 dB, approaching summit, new line"]
["2016-06-24T12:37:00.430","2016-06-25T00:37:00.430","JM","Sonar","Knudsen","Tx Power","power to 2, gain 37 dB"]
["2016-06-24T18:29:18.680","2016-06-25T06:29:18.680","JM","Sonar","All","Secure","Arrival at Eifuku Dive site"]
["2016-06-25T05:03:28.640","2016-06-25T17:03:28.640","DS","Sonar","Multibeam",null,"BIST failed. Re-starting TRU"]
["2016-06-25T05:23:47.820","2016-06-25T17:23:47.820","DS","Sonar","Multibeam","Start Pinging","softstart, Charlie and Derek on watch, near Eifuku"]
["2016-06-25T05:38:14.580","2016-06-25T17:38:14.580","DS","Sonar","EK","Start Pinging"]
["2016-06-25T05:39:50.910","2016-06-25T17:39:50.910","DS","Sonar","Multibeam",null,"started logging survey line 0136"]
["2016-06-25T05:54:06.270","2016-06-25T17:54:06.270","CW","Sonar","Knudsen","Range","Started Recording: Pulse 4; Power 2; Gain 36"]
["2016-06-25T06:07:48.600","2016-06-25T18:07:48.600","DS","XBT",null,null,"XBT 019 applied to line 0136"]
["2016-06-25T06:37:58.380","2016-06-25T18:37:58.380","JM",null,null,null,"secured multibeam started ADCP"]
["2016-06-25T07:00:19","2016-06-25T19:00:19","JM","Watch Change"]
["2016-06-25T07:44:26.780","2016-06-25T19:44:26.780","DS","Other",null,null,"observed slick near Daifuku hydrothermal plume. Secured ADCPs. Current was NE 067. "]
["2016-06-25T07:45:38.610","2016-06-25T19:45:38.610","DS","Sonar","Multibeam",null,"mulitbeam will not find bottom, BIST failed. Rebooting TRU. "]
["2016-06-25T07:55:09.180","2016-06-25T19:55:09.180","DS","Sonar","Multibeam",null,"Failed second BIST since stopping. Rebooting TRU and SIS operator station. "]
["2016-06-25T08:01:24.740","2016-06-25T20:01:24.740","DS","Sonar",null,null,"pinging/logging Eks and SBPs"]
["2016-06-25T08:19:55.360","2016-06-25T20:19:55.360","CW","Sonar","EK","Secure","Stopped recording"]
["2016-06-25T08:20:49.860","2016-06-25T20:20:49.860","CW","Sonar","Knudsen","Secure","Stopped recording"]
["2016-06-25T08:21:29.440",{"$f":"A198A198=#REF!","v":{"$error":"#NAME?"}},"CW","Sonar","Multibeam",null,"BIST passed!!! Saved as BIST #9"]
["2016-06-25T08:27:19.820","2016-06-25T20:27:19.820","CW","Sonar","Multibeam","Start Pinging","Logging line 0137"]
["2016-06-25T08:28:11.190",{"$f":"IF(ISBLANK(A199),\" \",((A199)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-06-25T20:28:11.190"},"CW","Sonar","EK","Start Pinging","Start Line"]
["2016-06-25T08:29:31","2016-06-25T20:29:31","CW","Sonar","Knudsen","Start Pinging","Started Recording: Pulse 4; Power 2; Gain 38"]
["2016-06-25T09:21:22.020","2016-06-25T21:21:22.020","CW","Sonar","Multibeam","New Line","Turn at beginning of Line 0138"]
["2016-06-25T12:44:53.100","2016-06-26T00:44:53.100","JM","XBT",null,null,"XBT 020 "]
["2016-06-25T12:53:46.380","2016-06-26T00:53:46.380","JM","XBT",null,null,"XBT applied to line 141"]
["2016-06-25T06:15:46","2016-06-25T18:15:46","JM","Sonar","All","Secure","Arrival at Daikoku Dive Site. ADCP logging"]
["2016-06-25T22:06:00",null,"DS","Sonar","EK","Start Pinging","pinging/logging Eks over Daikoku during ROV dive. "]
["2016-06-25T23:27:00",null,"DS","Sonar","EK",null,"changed EK60 file range to 500 (from 5000)"]
["2016-06-26T06:55:09.810","2016-06-26T18:55:09.810","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-06-26T06:57:02.770","2016-06-26T18:57:02.770","CW","Sonar","Multibeam",null,"BIST passed!!! Saved as BIST #10"]
["2016-06-26T06:58:54.650","2016-06-26T18:58:54.650","CW","Sonar","Multibeam","Start Pinging","Start Pinging in Mammal Protection -20"]
["2016-06-26T07:03:03.900","2016-06-26T19:03:03.900","CW","Sonar","Multibeam","Start Logging","Start Line 0149"]
["2016-06-26T07:08:08.510","2016-06-26T19:08:08.510","CW","Sonar","EK","Start Pinging","EK 60 Started"]
["2016-06-26T07:09:18.480","2016-06-26T19:09:18.480","CW","Sonar","Knudsen","Start Pinging","Started Recording: Pulse 4; Power 2; Gain 32"]
["2016-06-26T07:39:08.670","2016-06-26T19:39:08.670","CW","Sonar","Multibeam",null,"Turn Line 0150"]
["2016-06-26T08:06:51.370","2016-06-26T20:06:51.370","CW","Sonar","Multibeam","New Line","Line  0151 for mainscheme"]
["2016-06-26T08:39:20.280","2016-06-26T20:39:20.280","DS","XBT",null,null,"applied XBT 021 to line 0151"]
["2016-06-26T09:39:28.840","2016-06-26T21:39:28.840","JM","Sonar","Multibeam","New Line","Turn line 0153"]
["2016-06-26T10:03:36.660","2016-06-26T22:03:36.660","JM","Sonar","Knudsen","Range","Range to 500. Started new line"]
["2016-06-26T10:12:34.290","2016-06-26T22:12:34.290","JM","Ship",null,null,"Shifting line plan to port 600m to get sufficient overlap coverage"]
["2016-06-26T12:51:48.130","2016-06-27T00:51:48.130","JM","Sonar","Knudsen","Range","Range to 1000. Started new line"]
["2016-06-26T12:55:39.310","2016-06-27T00:55:39.310","JM","Ship",null,null,"Shifting line and additional 400m to port to get sufficient overlap coverage"]
["2016-06-26T13:56:19.010","2016-06-27T01:56:19.010","JM","XBT",null,null,"XBT 022"]
["2016-06-26T14:07:35.330","2016-06-27T02:07:35.330","JM","XBT",null,null,"XBT applied to line 0158"]
["2016-06-26T14:17:18.420","2016-06-27T02:17:18.420","JM","Sonar","Knudsen","Tx Power","Power to 3, Pulse 8 ms, gain 43 dB"]
["2016-06-26T18:28:11.440","2016-06-27T06:28:11.440","JM","Sonar","All","Secure","Arrived at Stega Dive site. Start ADCP"]
["2016-06-27T04:40:37.820","2016-06-27T16:40:37.820","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-06-27T04:45:56.920","2016-06-27T16:45:56.920","CW","Sonar","Multibeam",null,"BIST passed. Saved as BIST11_pass"]
["2016-06-27T04:47:08.150","2016-06-27T16:47:08.150","CW","Sonar","Multibeam","Start Pinging","Pinging in Mammal Mode -20"]
["2016-06-27T05:03:52.580","2016-06-27T17:03:52.580","DS","Sonar","Multibeam","Start Logging","line 0165, started pinging/logging EK60s and SBP"]
["2016-06-27T05:09:59.640","2016-06-27T17:09:59.640","DS","XBT",null,null,"XBT 23 conducted near Stegasaurus dive site"]
["2016-06-27T05:20:23.780","2016-06-27T17:20:23.780","DS","XBT",null,null,"XBT 23 applied to line 0165"]
["2016-06-27T05:26:01.860","2016-06-27T17:26:01.860","DS","Sonar","Multibeam","New Line","started turn line 0166"]
["2016-06-27T05:30:08.680","2016-06-27T17:30:08.680","DS","Sonar","Multibeam","New Line","started survey line 0167"]
["2016-06-27T06:17:27.990","2016-06-27T18:17:27.990","DS","Sonar","Multibeam",null,"max depth to 5500m"]
["2016-06-27T06:45:03.520","2016-06-27T18:45:03.520","DS","Sonar",null,null,"changed ranges on EK60 and SBP to 6000"]
["2016-06-27T06:55:59.410","2016-06-27T18:55:59.410","CW","Sonar","Multibeam","New Line","Turn line 0169"]
["2016-06-27T07:03:52.340","2016-06-27T19:03:52.340","CW","Sonar","Multibeam","New Line","Mainscheme 0170"]
["2016-06-27T07:09:24.090","2016-06-27T19:09:24.090","JM","Sonar","Knudsen","Tx Pulse","16 ms, gain 49 dB, New line. "]
["2016-06-27T08:19:28.860","2016-06-27T20:19:28.860","DS","Sonar","Multibeam","New Line","broke line 0172 for potential dive site, started line 0172, speeding up to 8.5-9 knots"]
["2016-06-27T08:38:53.590","2016-06-27T20:38:53.590","DS","Sonar","Multibeam",null,"min/max depths to 2000/6800"]
["2016-06-27T09:29:35.800","2016-06-27T21:29:35.800","DS","Sonar","Knudsen","Tx Pulse","moved up to 32 ms"]
["2016-06-27T09:34:47.090","2016-06-27T21:34:47.090","JM","Sonar","Multibeam","New Line","Start Line 174, turn"]
["2016-06-27T09:52:25.810","2016-06-27T21:52:25.810","JM","Sonar","Multibeam","New Line","Start Line 175"]
["2016-06-27T12:17:34.950","2016-06-28T00:17:34.950","JM","Sonar","Multibeam","New Line","Start Line 178, turn"]
["2016-06-27T12:45:15.910","2016-06-28T00:45:15.910","JM","Sonar","Knudsen",null,"Start new Line"]
["2016-06-27T13:00:45","2016-06-28T01:00:45","JM","XBT",null,null,"XBT 024 cast"]
["2016-06-27T13:15:55.300","2016-06-28T01:15:55.300","JM","XBT",null,null,"XBT cast applied to line 0179"]
["2016-06-27T15:09:21.640","2016-06-28T03:09:21.640","JM","Sonar","Multibeam","New Line","Start Line 182, turn"]
["2016-06-27T15:09:41.860","2016-06-28T03:09:41.860","JM","Sonar","Knudsen",null,"Start new Line"]
["2016-06-27T15:58:24.070","2016-06-28T03:58:24.070","JM","Sonar","Multibeam","New Line","Start Line 183, turn"]
["2016-06-27T15:58:27","2016-06-28T03:58:27","JM","Sonar","Knudsen",null,"Start new Line"]
["2016-06-27T18:04:28.030","2016-06-28T06:04:28.030","DS","Sonar","All","Secure","ended mapping for night on line 0185, secured Eks and SBP"]
["2016-06-27T18:05:27.020","2016-06-28T06:05:27.020","DS","Sonar","ADCP",null,"started ADCPs over North Forearc dive site"]
["2016-06-28T06:58:05.680","2016-06-28T18:58:05.680","DS","Sonar","Multibeam","Start Pinging","Rx BIST failed, all other pass, started pinging and EM302 worked. Softstart."]
["2016-06-28T07:13:37.700","2016-06-28T19:13:37.700","DS","Sonar","Multibeam","New Line","logging new turn line 0186"]
["2016-06-28T07:17:13.660","2016-06-28T19:17:13.660","DS","Sonar","EK","Start Pinging","started logging EK60 and SBP, Charlie and Jason on watch"]
["2016-06-28T08:55:25.840","2016-06-28T20:55:25.840","JM","Sonar","Knudsen",null,"New line"]
["2016-06-28T11:19:34.920","2016-06-28T23:19:34.920","JM","Sonar","Knudsen",null,"New line"]
["2016-06-28T11:51:06.420","2016-06-28T23:51:06.420","DS","Sonar","Multibeam",null,"asked bridge to slow down from 9 to 8.5"]
["2016-06-28T11:59:16.140","2016-06-28T23:59:16.140","DS","Sonar","Knudsen",null,"reduced pulse to 16, gain to 36, changed pulse back to 16"]
["2016-06-28T13:15:31.950","2016-06-29T01:15:31.950","JM","Sonar","Knudsen",null,"New line"]
["2016-06-28T13:48:20.240","2016-06-29T01:48:20.240","JM","XBT",null,null,"XBT cast 026"]
["2016-06-28T13:52:14.120","2016-06-29T01:52:14.120","JM","XBT",null,null,"XBT apllied to line 196"]
["2016-06-28T17:21:59.490","2016-06-29T05:21:59.490","JM","Sonar","Knudsen",null,"New line. Transect up unnamed forearc seamount"]
["2016-06-28T18:10:27.800","2016-06-29T06:10:27.800","JM","Sonar","All","Secure","Arrived at Unnamed forearc dive site"]
["2016-06-28T18:11:19.830",{"$f":"IF(ISBLANK(A265),\" \",((A265)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-06-29T06:11:19.830"},"JM","Sonar","ADCP",null,"Start logging"]
["2016-06-29T04:31:59.600","2016-06-29T16:31:59.600","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-06-29T04:38:01.680","2016-06-29T16:38:01.680","CW","Sonar","Multibeam",null,"BIST 13 passed"]
["2016-06-29T04:52:32.020","2016-06-29T16:52:32.020","CW","Sonar","Multibeam","Start Pinging","Pinging in Mammal Mode -20"]
["2016-06-29T05:14:37.500","2016-06-29T17:14:37.500","CW","Sonar","Multibeam","Start Logging","Line 0204"]
["2016-06-29T05:28:08.740","2016-06-29T17:28:08.740","DS","XBT",null,null,"XBT 027 conducted"]
["2016-06-29T05:35:39.180","2016-06-29T17:35:39.180","DS","XBT",null,null,"XBT 027 applied to line 0204"]
["2016-06-29T05:45:09.010","2016-06-29T17:45:09.010","DS","Sonar","Multibeam","New Line","started survey line 0205"]
["2016-06-29T05:47:15.370","2016-06-29T17:47:15.370","CW","Sonar","EK","Start Pinging","Range 6000"]
["2016-06-29T05:48:37.250","2016-06-29T17:48:37.250","CW","Sonar","Knudsen","Start Pinging","Pullse 32; Power 3; Gain 43"]
["2016-06-29T06:00:46.060","2016-06-29T18:00:46.060","CW","Ship",null,null,"Slowing to 3 knots for Ceremony"]
["2016-06-29T06:07:37.470","2016-06-29T18:07:37.470","CW","Sonar","Multibeam",null,"Stopped logging for Ceremony, holding position. Will come back on line afterward."]
["2016-06-29T06:38:58.400","2016-06-29T18:38:58.400","CW","Sonar","Multibeam","Start Logging","Start logging, line 0206"]
["2016-06-29T06:39:45.680","2016-06-29T18:39:45.680","CW","Sonar","EK","Start Pinging","Range 6000"]
["2016-06-29T06:40:26.940","2016-06-29T18:40:26.940","CW","Sonar","Knudsen","Start Pinging","Pullse 32; Power 3; Gain 43"]
["2016-06-29T06:58:34.530","2016-06-29T18:58:34.530","CW","Sonar","Multibeam","Max Angle","34 degrees on port to maintain 2800m min coverage for overlap"]
["2016-06-29T07:00:56","2016-06-29T19:00:56","JM","Watch Change"]
["2016-06-29T09:42:03.040","2016-06-29T21:42:03.040","JM","Sonar","Knudsen","Tx Pulse","16 ms, gain 40 dB"]
["2016-06-29T11:35:08","2016-06-29T23:35:08","JM","XBT",null,null,"XBT cast 028"]
["2016-06-29T11:45:19.080","2016-06-29T23:45:19.080","JM","XBT",null,null,"XBT applied to line 0213"]
["2016-06-29T12:11:34.480","2016-06-30T00:11:34.480","JM","Sonar","Knudsen","Tx Pulse","32 ms, gain 45 dB"]
["2016-06-29T18:11:08.630","2016-06-30T06:11:08.630","JM","Sonar","All","Secure","Arrived at Twin Peaks dive site. Started ADCP"]
["2016-06-30T06:54:26.050","2016-06-30T18:54:26.050","DS","Sonar","Multibeam","Start Pinging","softstart, Charlie and Derek on watch, near Twin Peaks dive site"]
["2016-06-30T07:23:38.660","2016-06-30T19:23:38.660","DS","Sonar","Multibeam","Start Logging","logging line 0224, logging Eks and SBP "]
["2016-06-30T07:28:28.810","2016-06-30T19:28:28.810","DS","XBT",null,null,"Applied XBT 29 to line 0224"]
["2016-06-30T09:09:06.840","2016-06-30T21:09:06.840","JM","Sonar","Knudsen","Tx Pulse","16 ms, gain 40 dB, range 500, started new line"]
["2016-06-30T11:33:32.630","2016-06-30T23:33:32.630","JM","Sonar","Knudsen",null,"Start new Line"]
["2016-06-30T12:32:44.680","2016-07-01T00:32:44.680","JM","Ship",null,null,"Shifting trackline to south by 500m to achieve sufficient overlap"]
["2016-06-30T13:08:48.090","2016-07-01T01:08:48.090","JM","Sonar","Knudsen","Tx Pulse","8 ms, gain 34 dB"]
["2016-06-30T13:35:10","2016-07-01T01:35:10","JM","XBT",null,null,"XBT 030"]
["2016-06-30T13:43:36.550","2016-07-01T01:43:36.550","JM","XBT",null,null,"XBT applied to line 0232"]
["2016-06-30T14:07:02.160","2016-07-01T02:07:02.160","JM","Sonar","Knudsen","Tx Power","power to 2, gain 37 dB, new line"]
["2016-06-30T15:59:46.620","2016-07-01T03:59:46.620","JM","Sonar","Knudsen","Tx Pulse","4 ms, gain 28 dB, newe line"]
["2016-06-30T18:12:15.600","2016-07-01T06:12:15.600","JM","Sonar","All","Secure","Arrived at Explorer dive site. Turn ADCP on"]
["2016-07-01T04:29:21.700","2016-07-01T16:29:21.700","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-01T04:36:32.500","2016-07-01T16:36:32.500","CW","Sonar","Multibeam","BIST # pass/fail","BIST 15 passed"]
["2016-07-01T04:54:44.830","2016-07-01T16:54:44.830","CW","Sonar","Multibeam","Start Pinging","Pinging in Mammal Mode -20"]
["2016-07-01T05:04:25.740","2016-07-01T17:04:25.740","DS","Sonar","Multibeam","Start Logging","line 0239 over Explorer Ridge Deep dive site. Started logging EK60s"]
["2016-07-01T05:27:26.710","2016-07-01T17:27:26.710","CW","XBT",null,null,"XBT 31"]
["2016-07-01T05:28:08.590","2016-07-01T17:28:08.590","CW","XBT",null,null,"XBT 31 appliked to line 0239"]
["2016-07-01T05:33:51.680","2016-07-01T17:33:51.680","DS","Sonar","Knudsen","Start Pinging","and logging"]
["2016-07-01T06:19:57.410","2016-07-01T18:19:57.410","DS","Sonar","Knudsen","Tx Power","changed from 2 to 1"]
["2016-07-01T06:47:13.110","2016-07-01T18:47:13.110","DS","Sonar","Knudsen",null,"minimum depth not deep enough map have lost some data"]
["2016-07-01T08:43:55.190","2016-07-01T20:43:55.190","JM","Sonar","Knudsen","Tx Power","power 2, pulse 4, gain 33"]
["2016-07-01T09:01:10.380","2016-07-01T21:01:10.380","JM","Sonar","Knudsen","Tx Pulse","pulse 2 ms, gain 28"]
["2016-07-01T10:07:35.350","2016-07-01T22:07:35.350","JM","Sonar","Knudsen","Tx Power","power 1, pulse 2, gain 37"]
["2016-07-01T11:33:28.590","2016-07-01T23:33:28.590","JM","XBT",null,null,"XBT cast 032"]
["2016-07-01T11:38:11.490","2016-07-01T23:38:11.490","JM","XBT",null,null,"XBT applioed to line 0245"]
["2016-07-01T13:45:49.590","2016-07-02T01:45:49.590","JM","Sonar","Knudsen",null,"Knudsen turned off by itself (transmit off). Turned back on. Started new line"]
["2016-07-01T13:46:33","2016-07-02T01:46:33","JM","Sonar","Knudsen","Tx Pulse","8 ms, gain 40 dB, power 1"]
["2016-07-01T16:35:27.940","2016-07-02T04:35:27.940","JM","Sonar","Multibeam","Secure"]
["2016-07-01T16:45:48","2016-07-02T04:45:48","JM","Sonar","ADCP",null,"Startup"]
["2016-07-01T18:12:44.830","2016-07-02T06:12:44.830","JM","Sonar","All","Secure"]
["2016-07-02T04:28:43.720","2016-07-02T16:28:43.720","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-02T04:34:32.510","2016-07-02T16:34:32.510","CW","Sonar","Multibeam","BIST # pass/fail","BIST 16 sorta passed. RX Noise in reds, possibly due to ADCP running."]
["2016-07-02T04:53:57.060","2016-07-02T16:53:57.060","CW","Sonar","Multibeam","Start Pinging","Pinging in Soft Startup"]
["2016-07-02T05:12:21.750","2016-07-02T17:12:21.750","DS","Sonar","Multibeam","New Line","logging MB line 0252"]
["2016-07-02T05:16:10.650","2016-07-02T17:16:10.650","DS","XBT",null,null,"XBT 33 collected"]
["2016-07-02T05:21:13.020","2016-07-02T17:21:13.020","DS","XBT",null,null,"applied XBT 33 to line 0252"]
["2016-07-02T05:29:38.880","2016-07-02T17:29:38.880","DS","Sonar","EK",null,"logging EK60s "]
["2016-07-02T05:39:28.930","2016-07-02T17:39:28.930","DS","Sonar","Knudsen",null,"started logging, pulse 4, power 2, gain 32 dB, range 500"]
["2016-07-02T07:05:41.520","2016-07-02T19:05:41.520","JM","Watch Change"]
["2016-07-02T07:10:36.960","2016-07-02T19:10:36.960","JM","Sonar","Knudsen","Tx Power","power 3, pulse 8 ms, gain 36 dB, new line"]
["2016-07-02T07:21:24.620",{"$f":"IF(ISBLANK(A328),\" \",((A328)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-07-02T19:21:24.620"},"JM","Sonar","Knudsen","Tx Pulse","4 ms, gain 30 dB"]
["2016-07-02T07:28:39.370","2016-07-02T19:28:39.370","JM","Sonar","Knudsen","Tx Power","power 2, pulse 4 ms, gain 29 dB, new line"]
["2016-07-02T07:49:11.780","2016-07-02T19:49:11.780","JM","Sonar","Knudsen","Tx Pulse","2 ms, gain 34 dB"]
["2016-07-02T11:29:12.200","2016-07-02T23:29:12.200","JM","XBT",null,null,"Cast 034"]
["2016-07-02T11:31:51.030","2016-07-02T23:31:51.030","JM","XBT",null,null,"XBT applied to line 0258"]
["2016-07-02T12:13:14.300","2016-07-03T00:13:14.300","JM","Sonar","Knudsen","Tx Power","power 3, pulse 16 ms, gain 42 dB, new line"]
["2016-07-02T12:47:53.120","2016-07-03T00:47:53.120","JM","Sonar","Knudsen","Range","1000m"]
["2016-07-02T16:21:48.700","2016-07-03T04:21:48.700","JM","Sonar","Knudsen","Tx Pulse","32 ms, gain 42 dB"]
["2016-07-02T18:16:00.290","2016-07-03T06:16:00.290","JM","Sonar","All","Secure","Arrived at Subducting Guyot dive site. ADCP turned on"]
["2016-07-03T03:08:11.300","2016-07-03T15:08:11.300","DS","Sonar","EK","Start Pinging","logging EK60s for mid-water ROV transects over the \"Subducting Guyot 1\" dive site. ADCPs still on. "]
["2016-07-03T06:51:39.580","2016-07-03T18:51:39.580","CW","Sonar","Multibeam","BIST # pass/fail","BIST passed"]
["2016-07-03T06:53:50.150","2016-07-03T18:53:50.150","CW","Sonar","Multibeam","Start Pinging","Pinging in Mammal Mode -20"]
["2016-07-03T06:54:26.600","2016-07-03T18:54:26.600","CW","Sonar","EK","Change Range","Range to 5500, started logging"]
["2016-07-03T06:57:47.640","2016-07-03T18:57:47.640","CW","Sonar","Knudsen","Start Pinging"]
["2016-07-03T07:04:28.890","2016-07-03T19:04:28.890","DS","Sonar","Multibeam","New Line","start logging line 0266"]
["2016-07-03T07:06:00.160","2016-07-03T19:06:00.160","DS","Sonar","Knudsen",null,"start logging"]
["2016-07-03T07:10:46.300","2016-07-03T19:10:46.300","JM","XBT",null,null,"XBT 035"]
["2016-07-03T07:18:11.890","2016-07-03T19:18:11.890","JM","XBT",null,null,"XBT cast applied to line 0266"]
["2016-07-03T09:26:21.280","2016-07-03T21:26:21.280","CW","Sonar","Multibeam","Ping Mode","Shoaling up, changed PM to DEEP, Coverage angle slowly adjusted to  66/65"]
["2016-07-03T09:39:48.370","2016-07-03T21:39:48.370","CW","Sonar","Multibeam","Ping Mode","Back to VERY DEEP "]
["2016-07-03T13:01:42.600","2016-07-04T01:01:42.600","JM","XBT",null,null,"XBT 036"]
["2016-07-03T13:10:39.280","2016-07-04T01:10:39.280","JM","XBT",null,null,"XBT cast applied to line 0272"]
["2016-07-03T18:16:56.180","2016-07-04T06:16:56.180","JM","Sonar","All","Secure","Arrived at Fryer Guyot dive site"]
["2016-07-04T04:27:48.570","2016-07-04T16:27:48.570","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-04T04:40:08.340","2016-07-04T16:40:08.340","CW","Sonar","Multibeam","BIST # pass/fail","BIST 18 had multiple failures. Will run again when ADCP is off."]
["2016-07-04T04:56:14.350","2016-07-04T16:56:14.350","CW","Sonar","Multibeam","BIST # pass/fail","BIST 19 passed! YAY!!! BIST does not like ADCP at all."]
["2016-07-04T05:00:03.630","2016-07-04T17:00:03.630","CW","Sonar","EK","Start Pinging","Recording at 6500"]
["2016-07-04T05:01:05.090","2016-07-04T17:01:05.090","CW","Sonar","Knudsen","Start Pinging","Pulse 2; Power 1; Gasin 35"]
["2016-07-04T05:22:23.110","2016-07-04T17:22:23.110",null,null,null,null,"XBT 037 conducted"]
["2016-07-04T05:26:10.310","2016-07-04T17:26:10.310","DS","XBT",null,null,"XBT 037 applied to line 0281, not yet logging multibeam"]
["2016-07-04T05:31:35.570","2016-07-04T17:31:35.570","DS","Sonar","Multibeam","Start Logging","logging survey line 0281"]
["2016-07-04T06:29:29.330","2016-07-04T18:29:29.330","DS","Sonar","Knudsen","Range","reduced range from 1000 to 200. increased pulse from 2ms to 4ms. Started new line."]
["2016-07-04T07:01:27.080","2016-07-04T19:01:27.080","JM","Watch Change"]
["2016-07-04T07:35:50.110","2016-07-04T19:35:50.110","JM","Sonar","EK","Start Pinging","EK60 was recording but not pinging. Started pinging and new line"]
["2016-07-04T07:38:49.210","2016-07-04T19:38:49.210","JM","Sonar","Knudsen","Range","Range to 500. Started new line"]
["2016-07-04T07:48:49.780","2016-07-04T19:48:49.780","JM","Sonar","Knudsen","Tx Power","set Tx power to 2"]
["2016-07-04T08:35:23.160","2016-07-04T20:35:23.160","JM","Sonar","Knudsen","Tx Power","set Tx power to 3, pulse to 16 ms, gain 39"]
["2016-07-04T09:53:40.900","2016-07-04T21:53:40.900","JM","Sonar","Knudsen","Tx Pulse","set to 16 ms, gain 40 dB"]
["2016-07-04T10:21:22.230","2016-07-04T22:21:22.230","JM","Sonar","Knudsen","Tx Pulse","set to 32 ms, gain 45 dB"]
["2016-07-04T11:53:35.690","2016-07-04T23:53:35.690","JM","XBT",null,null,"XBT cast 038"]
["2016-07-04T12:04:18.590","2016-07-05T00:04:18.590","JM","XBT",null,null,"XBT cast applied to line 0287"]
["2016-07-04T12:30:35.470","2016-07-05T00:30:35.470","JM","Sonar","Knudsen","Range","Range to 200m. Started new line"]
["2016-07-04T14:24:45.180","2016-07-05T02:24:45.180","JM","Sonar","Knudsen","Tx Pulse","set to 64 ms, gain 69 dB"]
["2016-07-04T14:53:22.350","2016-07-05T02:53:22.350","JM","Sonar","Knudsen","Range","Range to 500. Started new line"]
["2016-07-04T16:15:38","2016-07-05T04:15:38","JM","Sonar","Knudsen",null,"New line"]
["2016-07-04T18:20:37.280","2016-07-05T06:20:37.280","JM","Sonar","All","Secure","Arrived at Petite dive site. ADCP turned on"]
["2016-07-05T03:29:00","2016-07-05T15:29:00","DS","Sonar","EK",null,"started logging EK60 data for midwater dives over Petit Spt dive site"]
["2016-07-05T06:35:37.680","2016-07-05T18:35:37.680","DS",null,null,null,"Charlie and Derek on watch "]
["2016-07-05T06:56:23.390","2016-07-05T18:56:23.390","CW","Sonar","Multibeam","BIST # pass/fail","BIST 20 passed"]
["2016-07-05T06:57:11.150","2016-07-05T18:57:11.150","CW","Sonar","Multibeam","Start Pinging","Pinging in Mammal Mode -20"]
["2016-07-05T06:59:24.920","2016-07-05T18:59:24.920","CW","Sonar","EK","Start Pinging","Range 6200"]
["2016-07-05T07:00:07.250","2016-07-05T19:00:07.250","CW","Sonar","Knudsen","Start Pinging","Pulse 8; Power 3; Gain 42"]
["2016-07-05T07:13:36.970","2016-07-05T19:13:36.970","DS","Sonar","Multibeam","Start Logging","start logging line 0296"]
["2016-07-05T07:17:24.930","2016-07-05T19:17:24.930","JM","XBT",null,null,"XBT cast 039"]
["2016-07-05T07:23:39.050","2016-07-05T19:23:39.050","DS","XBT",null,null,"XBT 039 applied to line 0296"]
["2016-07-05T08:29:28.210","2016-07-05T20:29:28.210","JM","Sonar","Knudsen","Range","Range to 1000. Started new line"]
["2016-07-05T13:02:45.430","2016-07-06T01:02:45.430","JM","Sonar","Knudsen","Range","Range to 200. Started new line"]
["2016-07-05T13:32:45.870","2016-07-06T01:32:45.870","JM","XBT",null,null,"XBT cast 040"]
["2016-07-05T13:35:08.210","2016-07-06T01:35:08.210","JM","XBT",null,null,"XBT cast applied to line 0302"]
["2016-07-05T13:36:55.210","2016-07-06T01:36:55.210","JM","Sonar","Knudsen","Range","Range to 500. Started new line"]
["2016-07-05T16:21:30.200","2016-07-06T04:21:30.200","JM","Sonar","Knudsen","Range","Range to 1000. Started new line"]
["2016-07-05T18:15:54","2016-07-06T06:15:54","JM","Sonar","All","Secure","Arrived at Vogt dive site. Started ADCP"]
["2016-07-06T04:13:32.430","2016-07-06T16:13:32.430","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-06T04:59:44.990","2016-07-06T16:59:44.990","DS","Sonar","Multibeam",null,"first BIST (BIST 21) failed RX noise level, RX noise spectrum, BIST 22 passed"]
["2016-07-06T05:15:24.490",{"$f":"IF(ISBLANK(A392),\" \",((A392)-DATE(1970,1,1))+25569+($E$1/24))","v":"2016-07-06T17:15:24.490"},"DS","Sonar","EK","Start Pinging","start logging EK60 data"]
["2016-07-06T05:33:32.750","2016-07-06T17:33:32.750","DS","Sonar","Multibeam","Start Logging","logging multibeam line 0309"]
["2016-07-06T05:39:43.210","2016-07-06T17:39:43.210","DS","XBT",null,null,"XBT 41 conducted"]
["2016-07-06T05:43:56.650","2016-07-06T17:43:56.650","CW","XBT",null,null,"XBT applied to line 0309"]
["2016-07-06T05:45:35.040","2016-07-06T17:45:35.040","DS","Sonar","Knudsen","Start Pinging","start logging"]
["2016-07-06T06:39:09.060","2016-07-06T18:39:09.060","CW","Sonar","Multibeam",null,"Alarm window: Pingers Status Faulty, not pinging. Clicked it off and everything was fine."]
["2016-07-06T06:57:29.540","2016-07-06T18:57:29.540","JM","Watch Change"]
["2016-07-06T07:09:41.300","2016-07-06T19:09:41.300","JM","Sonar","Knudsen","Range","Range to 500m. Started new line"]
["2016-07-06T09:54:46.070","2016-07-06T21:54:46.070","JM","Sonar","Knudsen",null,"Noticed it wasn't transmitting. Appears to turn off on its own occasionally. Started new line."]
["2016-07-06T12:18:21.580","2016-07-07T00:18:21.580","JM","XBT",null,null,"XBT cast 042"]
["2016-07-06T12:20:51.360","2016-07-07T00:20:51.360","JM","XBT",null,null,"XBT cast applied to line 0315"]
["2016-07-06T14:48:39.130","2016-07-07T02:48:39.130","JM","Sonar","Knudsen","Range","Range to 1000. Started new line"]
["2016-07-06T18:06:25.360","2016-07-07T06:06:25.360","JM","Sonar","All","Secure","Arrived at Subducting Guyot dive site #2. Turned on ADCP"]
["2016-07-07T04:30:56.170","2016-07-07T16:30:56.170","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-07T04:53:53.670","2016-07-07T16:53:53.670","CW","Sonar","Multibeam","Start Pinging","BIST 23 passed! Yay!"]
["2016-07-07T05:08:23.460","2016-07-07T17:08:23.460","DS","Sonar","All",null,"start logging all, MB line 0326"]
["2016-07-07T05:15:40.700","2016-07-07T17:15:40.700","DS","XBT",null,null,"XBT cast 043 first attempt terminated early. Second attempt successful. "]
["2016-07-07T05:25:01.570","2016-07-07T17:25:01.570","DS","XBT",null,null,"XBT 043 applied to line 0326"]
["2016-07-07T05:31:15.260","2016-07-07T17:31:15.260","DS","Sonar","Knudsen",null,"can't find bottom at 5660 meters. Timeout errors also on EK60"]
["2016-07-07T05:40:22.380","2016-07-07T17:40:22.380","DS","Sonar","EK",null,"EK60 timing out. Followed SOP for EK60 operation in very deep waters. 18 and 70 kHz changed to passive mode. Logging data. "]
["2016-07-07T05:43:48.560","2016-07-07T17:43:48.560","DS","Sonar","Multibeam","Max Angle","pulled in to 30/30"]
["2016-07-07T06:09:34.700","2016-07-07T18:09:34.700","CW","Sonar","EK","Secure","Stopped pinging due to depth threshold"]
["2016-07-07T06:19:15.920","2016-07-07T18:19:15.920","DS","Sonar","Knudsen",null,"found bottom again, staying with power 3"]
["2016-07-07T06:20:54.160","2016-07-07T18:20:54.160","DS","Sonar","Multibeam","Max Angle","16/16 in 7420 meters"]
["2016-07-07T06:33:13.640","2016-07-07T18:33:13.640","DS","Sonar","EK",null,"EK60 still giving timeout warning with 18 and 70 kHz transducers in passive. Logging data. "]
["2016-07-07T07:00:17.570","2016-07-07T19:00:17.570","DS","Sonar","Multibeam","Max Angle","reduced max starboard angle to 13 - getting too many artifacts"]
["2016-07-07T07:01:31","2016-07-07T19:01:31","JM","Watch Change"]
["2016-07-07T07:18:11.620","2016-07-07T19:18:11.620","DS","Sonar","EK","Secure","EK not working. Secured until we get shallower"]
["2016-07-07T07:19:09.710","2016-07-07T19:19:09.710","DS","Sonar","Multibeam","Max Angle","starboard reduced to 10 to reduce artifacts, port to 12"]
["2016-07-07T07:29:01.080","2016-07-07T19:29:01.080","JM","Sonar","Knudsen","Start Pinging","Had to restart Knudsen computer."]
["2016-07-07T11:39:55.480","2016-07-07T23:39:55.480","JM","XBT",null,null,"XBT cast 044"]
["2016-07-07T11:41:41.700","2016-07-07T23:41:41.700","JM","XBT",null,null,"XBT cast applied to line 0332"]
["2016-07-07T18:12:04.050","2016-07-08T06:12:04.050","JM","Sonar","All","Secure","Arrived at Hadal Wall dive site. Turned on ADCP"]
["2016-07-08T06:36:54.370","2016-07-08T18:36:54.370","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-08T06:57:27.030","2016-07-08T18:57:27.030","CW","Sonar","Multibeam","BIST # pass/fail","BIST 24 passed. Softstart pinging multibeam"]
["2016-07-08T07:13:58.580","2016-07-08T19:13:58.580","DS","Sonar","Multibeam","Start Logging","line 0340"]
["2016-07-08T07:22:25.550","2016-07-08T19:22:25.550","JM","XBT",null,null,"XBT cast 045"]
["2016-07-08T07:28:47.020","2016-07-08T19:28:47.020","JM","XBT",null,null,"XBT cast applied to line 0340"]
["2016-07-08T13:33:36.100","2016-07-09T01:33:36.100","JM","XBT",null,null,"XBT cast 046"]
["2016-07-08T13:35:38.940","2016-07-09T01:35:38.940","JM","XBT",null,null,"XBT cast applied to line 0346"]
["2016-07-08T19:41:19.380","2016-07-09T07:41:19.380","DS","Sonar","Knudsen","Secure","DS relieved JM. close to shore in Saipan and have existing data here on same line. "]
["2016-07-08T20:09:20.860","2016-07-09T08:09:20.860","DS","Sonar","Multibeam",null,"stop logging line 0352 on MB. Stopped logging on EK60 too."]
["2016-07-08T20:13:22.680","2016-07-09T08:13:22.680","DS","Sonar","Multibeam","new line","start survey line 00353. Logging again on EK60 line 201413 (start non-public data)"]
["2016-07-08T20:33:30.970","2016-07-09T08:33:30.970","DS","Sonar","EK","Change Range","file 203321 non-public"]
["2016-07-08T20:52:53.010","2016-07-09T08:52:53.010","DS","Sonar","Multibeam",null,"Secured MB and Eks. Started ADCPs. Turned off MB TRU"]
["2016-07-08T21:06:27.150","2016-07-09T09:06:27.150","DS",null,null,null,"on station for 7/8 dive site"]
["2016-07-09T05:28:09.240","2016-07-09T17:28:09.240","CW","Watch Change",null,null,"Derek and Charlie on watch"]
["2016-07-09T05:28:35.310","2016-07-09T17:28:35.310","CW","Sonar","Multibeam","BIST # pass/fail","BIST 25 failed. Possibly due to lack of TRU warmup. "]
["2016-07-09T05:39:22.150","2016-07-09T17:39:22.150","CW","Sonar","Multibeam","BIST # pass/fail","BIST fail. Not saved. Closed SIS and turened off TRU. Will hard restart and try again. "]
["2016-07-09T06:12:30.660","2016-07-09T18:12:30.660","CW","Sonar","Multibeam","BIST # pass/fail","BIST 26 Fail (Only RX channel) Going ahead"]
["2016-07-09T06:13:19.710","2016-07-09T18:13:19.710","CW","Sonar","Multibeam","Start Pinging","Pinging in Mammal Mode -20"]
["2016-07-09T06:26:15.470","2016-07-09T18:26:15.470","DS","Sonar","Multibeam","Start Logging","started MB line 0354"]
["2016-07-09T06:26:56.790","2016-07-09T18:26:56.790","DS","XBT",null,null,"XBT 47 conducted"]
["2016-07-09T06:30:45.850","2016-07-09T18:30:45.850","DS","XBT",null,null,"XBT 47 applied to line 0354"]
["2016-07-09T06:33:16.740","2016-07-09T18:33:16.740","DS","Sonar",null,null,"Started logging EK60s and SBP"]
["2016-07-09T06:57:55.020","2016-07-09T18:57:55.020","JM","Watch Change"]
["2016-07-09T09:02:54.200","2016-07-09T21:02:54.200","JM","Sonar","Knudsen","Tx Power","Power to 1, pulse 8ms, gain 46dB"]
["2016-07-09T10:48:26.020","2016-07-09T22:48:26.020","JM","Sonar","Knudsen","Tx Pulse","4ms, gain 42dB"]
["2016-07-09T11:12:11.170","2016-07-09T23:12:11.170","DS","Sonar","Knudsen","Tx Blanking","power 2"]
["2016-07-09T12:44:14.910","2016-07-10T00:44:14.910","JM","XBT",null,null,"XBT cast 048"]
["2016-07-09T12:47:33.450","2016-07-10T00:47:33.450","JM","XBT",null,null,"XBT cast applied to line 0360"]
["2016-07-09T19:25:57.940","2016-07-10T07:25:57.940","DS",null,null,null,"watch change. DS on watch"]
["2016-07-09T20:51:50.010","2016-07-10T08:51:50.010","DS","Sonar","All",null,"stopped all sonars, meeting pilot into Guam"]
["2016-07-10T00:11:27.100","2016-07-10T12:11:27.100","DS","Sonar",null,null,"Ran final BIST (all pass), exported PU parameters, secured all sonars with breakers off, cruise complete"]
[null,{"$f":"IF(ISBLANK(A456),\" \",((A456)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A520),\" \",((A520)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A584),\" \",((A584)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A648),\" \",((A648)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A712),\" \",((A712)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A776),\" \",((A776)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A840),\" \",((A840)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A904),\" \",((A904)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A968),\" \",((A968)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1032),\" \",((A1032)-DATE(1970,1,1))+25569+($E$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1085),\" \",((A1085)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1094),\" \",((A1094)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1158),\" \",((A1158)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1222),\" \",((A1222)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1286),\" \",((A1286)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1350),\" \",((A1350)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1414),\" \",((A1414)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1478),\" \",((A1478)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1542),\" \",((A1542)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1606),\" \",((A1606)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1670),\" \",((A1670)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1734),\" \",((A1734)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1798),\" \",((A1798)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1862),\" \",((A1862)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1926),\" \",((A1926)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1990),\" \",((A1990)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["DS","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["CW","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["JM","Weather","Knudsen","New Line","Secure","Gain Mode"]
[null,"Watch Change","All","Max Angle",null,"Gain Value"]
[null,"XBT","ADCP","Spike Filter Strength",null,"Process Shift"]
[null,"Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
[null,"Other",null,"Aeration Filter (On/Off)",null,"Range"]
[null,null,null,"Interference Filter (On/Off)",null,"Phase Mode"]
[null,null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]
[null,null,null,"BIST # pass/fail"]