{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":1996,"n_cols":7,"rows_kept":1996,"cut":false,"hidden":false,"merged":[]}
["2016-12-13T14:30:40.520","UTC to Local: ",10,"UTC 2","UTC 3","UTC 4","Cruise Details: Dec 10th - Dec 16th"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
["2016-12-15T04:54:42.880","Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2016-12-10T22:06:02.720",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-10T12:06:02.720"},"DF","Sonar","Multibeam",null,"started new survey EX1609, ran BIST 01"]
["2016-12-10T22:23:59.850",{"$f":"IF(ISBLANK(A6),\" \",((A6)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-10T12:23:59.850"},"DF","Sonar","Multibeam",null,"BIST 01 TX Channels Fail, will rerun bist"]
["2016-12-10T22:31:46.670","2016-12-10T12:31:46.670","DF","Sonar","Multibeam",null,"BIST 02 TX Channels Fail, restarting TRU"]
["2016-12-10T23:41:18.910","2016-12-10T13:41:18.910","DS","Sonar","ADCP",null,"started ADCP cruise EX1609_01 for bottom tracking data on 300 and 38 kHz ADCPs as we leave Pearl Harbor"]
["2016-12-10T23:41:18.910",{"$f":"IF(ISBLANK(A9),\" \",((A9)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-10T13:41:18.910"},"CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2016-12-11T07:51:26.320","2016-12-10T21:51:26.320","CW","Sonar","Multibeam",null,"Sound Speed 1535.45"]
["2016-12-11T07:52:37.820","2016-12-10T21:52:37.820","CW","XBT",null,null,"XBT 001"]
["2016-12-11T07:55:09.370","2016-12-10T21:55:09.370","CW","Sonar","Multibeam","Start Logging","0000"]
["2016-12-11T07:57:02",{"$f":"IF(ISBLANK(A13),\" \",((A13)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-10T21:57:02"},"CW","Sonar","Multibeam","Along Direction Pitch","-2"]
["2016-12-11T07:57:02","2016-12-10T21:57:02","CW","Sonar","Multibeam",null,"XBT 001 applied to line 0000"]
["2016-12-11T08:16:48.510","2016-12-10T22:16:48.510","CW","Issue/Problem","Multibeam",null,"SIS being a jerkface. TRU lamp went out and red screen of death. Came back in a few seconds w/o intervention. "]
["2016-12-11T08:37:09.550","2016-12-10T22:37:09.550","CW","Issue/Problem","Multibeam",null,"TRU jerkface again. 3 seconds red. Lost a few pings. Fixed itself."]
["2016-12-11T09:29:22.120","2016-12-10T23:29:22.120","CW","Sonar","Multibeam","Max Angle","45/40"]
["2016-12-11T09:33:09.980","2016-12-10T23:33:09.980","CW","Sonar","Knudsen","Start Pinging","Pulse 2; Power 3; Gain 36"]
["2016-12-11T09:34:19.720","2016-12-10T23:34:19.720","CW","Sonar","Knudsen","Phase Mode","3500-4500"]
["2016-12-11T09:38:28.990","2016-12-10T23:38:28.990","CW","Sonar","Multibeam",null,"SV 1534.10"]
["2016-12-11T09:50:50.100","2016-12-10T23:50:50.100","CW","Sonar","Multibeam",null,"SV 1531.8"]
["2016-12-11T09:56:58.190","2016-12-10T23:56:58.190","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2016-12-11T10:00:18.140","2016-12-11T00:00:18.140","CW","Issue/Problem","Multibeam",null,"Lost bottom, then telnet popped uip SW Fuse Tx TimedOut, then the ususal errors on the Slot 14"]
["2016-12-11T10:03:04.610","2016-12-11T00:03:04.610","CW","Sonar","Multibeam",null,"Stopped Logging / Pinging"]
["2016-12-11T10:12:42.980","2016-12-11T00:12:42.980","CW","Sonar","Multibeam",null,"Bist 05 All Pass. "]
["2016-12-11T10:20:56.720","2016-12-11T00:20:56.720","CW","Sonar","Multibeam",null,"No return on pinging. Restarted SIS again."]
["2016-12-11T10:22:26.520","2016-12-11T00:22:26.520","CA","Sonar","Knudsen",null,"Pulse 4.0"]
["2016-12-11T10:29:03.400","2016-12-11T00:29:03.400","CW","Sonar","Multibeam","Start Pinging","It's working! Yay! Data okay."]
["2016-12-11T10:30:36.500","2016-12-11T00:30:36.500","CW","Sonar","Multibeam","Start Logging","Line 0004"]
["2016-12-11T10:31:07.780","2016-12-11T00:31:07.780","CW","Sonar","Multibeam",null,"SV 1531.4"]
["2016-12-11T10:33:28.540","2016-12-11T00:33:28.540","CW","Sonar","Multibeam","Along Direction Pitch","=G30=G32-1"]
["2016-12-11T11:02:33.740","2016-12-11T01:02:33.740","AB","Sonar","Multibeam",null,"Stopped Logging / Pinging, TRU off"]
["2016-12-11T11:27:40.980","2016-12-11T01:27:40.980","AB","Sonar","Multibeam",null,"Restarted System. Pinging. "]
["2016-12-11T11:28:02.270","2016-12-11T01:28:02.270","AB","Sonar","Multibeam",null,"Sound Speed 1534.1"]
["2016-12-11T11:30:54.750","2016-12-11T01:30:54.750","CW","Sonar","Multibeam",null,"Turned off TRU. Reseated TX card 14, and the ones on each side. Reseated all ethernet cables. Let TRU chill out for 15 minutes. Restarted with success. "]
["2016-12-11T11:32:57.110","2016-12-11T01:32:57.110","CW","Sonar","Multibeam","Start Pinging"]
["2016-12-11T11:33:17.520","2016-12-11T01:33:17.520","CW","Sonar","Multibeam","Start Logging","Line 0004"]
["2016-12-11T11:49:57.320","2016-12-11T01:49:57.320","CA","XBT",null,null,"0002 added to line 0004. 7m/s different, use xbt 3."]
["2016-12-11T11:50:15.670","2016-12-11T01:50:15.670","AB","Sonar","Multibeam",null,"Deep Mode, 50/50"]
["2016-12-11T11:55:03.170","2016-12-11T01:55:03.170","AB","Sonar","Knudsen",null,"Pulse 4, Power 2, Gain 38, Range 1000, Phase 2500-3500"]
["2016-12-11T12:06:23.410","2016-12-11T02:06:23.410","AB","Sonar","Multibeam","New Line","0005"]
["2016-12-11T12:21:31.070","2016-12-11T02:21:31.070","CA","XBT",null,null,"xbt 3 added to line 0005. (Cast#2 is bad, reapplied Cast #3 to lines 4 and 5 to removed 90m vertical  data artifact.)"]
["2016-12-11T12:23:00.280","2016-12-11T02:23:00.280","AB","Sonar","Knudsen","Phase Mode","2000-3000m"]
["2016-12-11T12:27:00.500","2016-12-11T02:27:00.500","AB","Sonar","Multibeam","Ping Mode","Very Deep"]
["2016-12-11T13:22:50.080","2016-12-11T03:22:50.080","AB","Sonar","Multibeam","New Line","0006, Ping Mode Deep"]
["2016-12-11T12:56:13.430","2016-12-11T02:56:13.430","AB","Sonar","Multibeam","New Line","0007, turn"]
["2016-12-11T13:01:02.510","2016-12-11T03:01:02.510","AB","Sonar","Multibeam","Sound Velocity Update","TSG 1534.81Psu; PPT 34.31"]
["2016-12-11T13:11:52.520","2016-12-11T03:11:52.520","CA","Sonar","Knudsen","Phase Mode","1500-2500m"]
["2016-12-11T13:22:56.040","2016-12-11T03:22:56.040","AB","Sonar","Multibeam","Max Angle","60/75"]
["2016-12-11T13:23:16.960","2016-12-11T03:23:16.960","AB","Sonar","Knudsen",null,"New line, Pulse 2, Power 1, Gain 34"]
["2016-12-11T13:29:57.730","2016-12-11T03:29:57.730","AB","Sonar","Multibeam","Sound Velocity Update","1535.68 m/s"]
["2016-12-11T13:35:12.070","2016-12-11T03:35:12.070","AB","Sonar","Multibeam","Max Angle","75/75"]
["2016-12-11T13:37:10.770","2016-12-11T03:37:10.770","AB","Sonar","Knudsen","Range","New line, Range 500m, sediment layers developing"]
["2016-12-11T13:55:03.230","2016-12-11T03:55:03.230","AB","Sonar","Multibeam","New Line","0008, turn"]
["2016-12-11T13:55:50.140","2016-12-11T03:55:50.140","AB","Sonar","Knudsen","Phase Range","500-1000m"]
["2016-12-11T13:58:27.810","2016-12-11T03:58:27.810","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2016-12-11T13:59:30.620","2016-12-11T03:59:30.620","AB","Sonar","Multibeam","New Line","0009"]
["2016-12-11T14:24:12.020","2016-12-11T04:24:12.020","AB","Sonar","Multibeam",null,"Coverage 4200m swath at 1028m water depth."]
["2016-12-11T14:42:30.080","2016-12-11T04:42:30.080","AB","Sonar","Multibeam","New Line","0010, turn"]
["2016-12-11T14:42:54.670","2016-12-11T04:42:54.670","AB","Sonar","Knudsen",null,"New line"]
["2016-12-11T14:43:55.720","2016-12-11T04:43:55.720","AB","Sonar","Multibeam","New Line","0011"]
["2016-12-11T15:10:50.740","2016-12-11T05:10:50.740","CA","Sonar","Multibeam","New Line","0012, turn"]
["2016-12-11T15:15:25.330","2016-12-11T05:15:25.330","AB","Sonar","Multibeam","New Line","0013"]
["2016-12-11T15:18:22.100","2016-12-11T05:18:22.100","AB","Sonar","Multibeam","Sound Velocity Update","1536.35 m/s"]
["2016-12-11T15:18:34.750","2016-12-11T05:18:34.750","CA","Sonar","Knudsen","Phase Range","500-1000m"]
["2016-12-11T15:22:46.020","2016-12-11T05:22:46.020","AB","Sonar","Multibeam","New Line","Backscatter adjustment"]
["2016-12-11T15:48:31.540","2016-12-11T05:48:31.540","AB","Sonar","Knudsen","Phase Range","250-750m"]
["2016-12-11T16:00:15.280","2016-12-11T06:00:15.280","AB","Sonar","Multibeam","Ping Mode","Auto: Medium, 2000m swath @ 440m depth"]
["2016-12-11T16:01:30.300","2016-12-11T06:01:30.300","AB","Sonar","Knudsen","Tx Pulse","1"]
["2016-12-11T16:53:24.370","2016-12-11T06:53:24.370","AB","Sonar","Multibeam","New Line","0016"]
["2016-12-11T16:54:53.740",{"$f":"IF(ISBLANK(A71),\" \",((A71)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-11T06:54:53.740"},"AB","Sonar","Knudsen",null,"New line, Pulse 0.5"]
["2016-12-11T17:09:37.250","2016-12-11T07:09:37.250","AB","Sonar","Multibeam","New Line","0017"]
["2016-12-11T17:09:50.130","2016-12-11T07:09:50.130","AB","Sonar","Knudsen","Range","200m, Gain 24, Tx Pulse 0.125"]
["2016-12-11T17:16:58.440","2016-12-11T07:16:58.440","AB","Sonar","Knudsen",null,"Secured <200m depth"]
["2016-12-11T17:17:19.820","2016-12-11T07:17:19.820","AB","Sonar","Multibeam","Ping Mode","Shallow"]
["2016-12-11T17:28:12.490","2016-12-11T07:28:12.490","AB","Sonar","Multibeam",null,"Stop Logging"]
["2016-12-11T18:36:49.510","2016-12-11T08:36:49.510","DS","Sonar","Multibeam","Secure","stopped pinging multibeam"]
["2016-12-11T18:39:00.270","2016-12-11T08:39:00.270","DS","Sonar","ADCP",null,"started logging both ADCPs in bottom track mode for transit from Lanai to EK60 calibration area"]
["2016-12-12T02:09:07.270","2016-12-11T16:09:07.270",null,"Sonar","Multibeam","Start Pinging","Started in mammal protection mode"]
["2016-12-12T02:34:32.870","2016-12-11T16:34:32.870","DF","Sonar","Multibeam","Ping Mode","Auto"]
["2016-12-12T02:37:03.570","2016-12-11T16:37:03.570","MW","Sonar","Multibeam",null,"Full ping strength out of mammal protection mode"]
["2016-12-12T02:39:25.780","2016-12-11T16:39:25.780","DF","Sonar","Multibeam","Start Logging","started logging"]
["2016-12-12T02:49:05.780","2016-12-11T16:49:05.780","MW","XBT",null,null,"Cast 005 added to line 0018"]
["2016-12-12T03:36:57.080","2016-12-11T17:36:57.080","CW","Sonar","Knudsen",null,"started pinging and logging sub bottom"]
["2016-12-12T03:50:34.160","2016-12-11T17:50:34.160","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-12-12T03:55:44.270","2016-12-11T17:55:44.270","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2016-12-12T05:01:45.210","2016-12-11T19:01:45.210","CW","Sonar","Multibeam",null,"SV 1535.0"]
["2016-12-12T05:03:25.820","2016-12-11T19:03:25.820","CW","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-12-12T05:15:12.290","2016-12-11T19:15:12.290","CW","Sonar","Knudsen","Phase Range","3250-3750"]
["2016-12-12T05:20:00.090","2016-12-11T19:20:00.090","CW","Sonar","Multibeam",null,"SV 1534.3"]
["2016-12-12T05:21:13.750","2016-12-11T19:21:13.750","CW","Sonar","Knudsen","Phase Range","3750-4250"]
["2016-12-12T05:21:40.890","2016-12-11T19:21:40.890","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2016-12-12T05:34:05.820","2016-12-11T19:34:05.820","CW","Issue/Problem","Multibeam",null,"TRU jerkface again. 3 seconds red. Lost a few pings. Fixed itself."]
["2016-12-12T05:35:53.060","2016-12-11T19:35:53.060","CW","Sonar","Multibeam","New Line","Turn Line 0021"]
["2016-12-12T05:42:27.230",{"$f":"IF(ISBLANK(A95),\" \",((A95)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-11T19:42:27.230"},"CW","Sonar","Multibeam",null,"SV 1533.4"]
["2016-12-12T05:49:49.720","2016-12-11T19:49:49.720","CW","Sonar","Knudsen","Phase Range","3250-3750"]
["2016-12-12T05:52:23.380","2016-12-11T19:52:23.380","CW","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-12-12T05:54:45.790","2016-12-11T19:54:45.790","CW","Sonar","Multibeam","New Line","Fat fingered for line 0022. Survey Line starts 0023"]
["2016-12-12T05:59:04.190","2016-12-11T19:59:04.190","CW","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2016-12-12T06:00:39.320","2016-12-11T20:00:39.320","CW","Sonar","Multibeam","Along Direction Pitch",0]
["2016-12-12T06:01:00.940","2016-12-11T20:01:00.940","CW","Sonar","Multibeam","Max Angle","35/35"]
["2016-12-12T06:01:42.910","2016-12-11T20:01:42.910","CW","Sonar","Knudsen","Phase Range","3250-3750"]
["2016-12-12T06:07:17.460","2016-12-11T20:07:17.460","CW","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-12-12T06:18:27.170","2016-12-11T20:18:27.170","CW","Issue/Problem",null,null,"WE SHOULD NOT BE HAVING TO RESET KVM's DOZENS OF TIMES ON OUR SHIFTS!!!!!!!!!!!!"]
["2016-12-12T06:20:16.200","2016-12-11T20:20:16.200","CW","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-12-12T06:35:55.430","2016-12-11T20:35:55.430","CW","Sonar","Multibeam",null,"SV 1535.0"]
["2016-12-12T06:38:13.510","2016-12-11T20:38:13.510","CW","Sonar","Multibeam","Max Angle","Slowly brought out to 45/45"]
["2016-12-12T07:39:07.560","2016-12-11T21:39:07.560","mw","XBT",null,null,"XBT 006 "]
["2016-12-12T07:39:36.760","2016-12-11T21:39:36.760","mw","Sonar","Multibeam","New Line","XBT006 applied to new line 0025; turn at beigining of line"]
["2016-12-12T07:46:46.740","2016-12-11T21:46:46.740",null,null,null,"New Line","New Survey Line 0026"]
["2016-12-12T09:02:31.560","2016-12-11T23:02:31.560","CW","Issue/Problem","Multibeam",null,"TRU jerkface again. 3 seconds red. Lost a few pings. Fixed itself."]
["2016-12-12T09:02:34.510","2016-12-11T23:02:34.510","CW","Sonar","Multibeam","Ping Mode","DEEP  "]
["2016-12-12T09:13:15.290","2016-12-11T23:13:15.290","CW","Issue/Problem","Multibeam",null,"TRU jerkface again. 3 seconds red. Lost a few pings. Fixed itself."]
["2016-12-12T09:24:59.820","2016-12-11T23:24:59.820","CW","Sonar","Knudsen","Range","2500-3000"]
["2016-12-12T09:26:22.770","2016-12-11T23:26:22.770","CW","Sonar","Multibeam",null,"SV 1534.60"]
["2016-12-12T09:26:57.580","2016-12-11T23:26:57.580","CW","Sonar","Multibeam",null,"Date just looks inferior. Any tricks are doing little. "]
["2016-12-12T09:30:45.370","2016-12-11T23:30:45.370","CW","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-12-12T09:31:37.490","2016-12-11T23:31:37.490","CW","Sonar","Multibeam","New Line","Turn Line 0028"]
["2016-12-12T10:08:19.500","2016-12-12T00:08:19.500","CW","Sonar","Multibeam","New Line","Survey Line 0029. Had issues coming on to line. Looks like a drunk spider."]
["2016-12-12T10:09:30.540","2016-12-12T00:09:30.540","CW","Sonar","Knudsen","Phase Range","1750-2250"]
["2016-12-12T10:15:36.860","2016-12-12T00:15:36.860","CW","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-12-12T10:58:41.220","2016-12-12T00:58:41.220","AB","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-12-12T11:25:33.840","2016-12-12T01:25:33.840","AB","Sonar","Multibeam","New Line","0031,turn"]
["2016-12-12T11:30:53.090","2016-12-12T01:30:53.090","CA","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-12-12T11:39:37.940","2016-12-12T01:39:37.940","CA","Sonar","Multibeam","New Line",32]
["2016-12-12T11:51:24.990","2016-12-12T01:51:24.990","AB","XBT",null,null,"XBT007"]
["2016-12-12T11:51:58.680","2016-12-12T01:51:58.680","AB","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-12-12T11:59:17.810","2016-12-12T01:59:17.810","AB","XBT","Multibeam",null,"XBT7 added to line 32; SV Update 1535.33; 34.6 psu"]
["2016-12-12T11:59:43.420","2016-12-12T01:59:43.420","AB","Sonar","Multibeam","New Line","0033"]
["2016-12-12T12:01:14.460","2016-12-12T02:01:14.460","AB","Sonar","Multibeam","Max Angle","70/60"]
["2016-12-12T12:08:56.300","2016-12-12T02:08:56.300","AB","Sonar","Knudsen","Phase Range","2000-2500"]
["2016-12-12T12:26:56.830","2016-12-12T02:26:56.830","CA","Sonar","Knudsen","Phase Range","1750-2250"]
["2016-12-12T12:51:54.390","2016-12-12T02:51:54.390","CA","Sonar","Knudsen","Phase Range","1500-2000"]
["2016-12-12T13:04:37.570",{"$f":"IF(ISBLANK(A134),\" \",((A134)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-12T03:04:37.570"},"AB","Sonar","Multibeam","Max Angle","75/65"]
["2016-12-12T13:15:29.970","2016-12-12T03:15:29.970","AB","Sonar","Multibeam","New Line","0035, turn"]
["2016-12-12T13:20:38.390","2016-12-12T03:20:38.390","AB","Sonar","Knudsen","Phase Range","1250-1750, Power 2, Pulse 2, New Line started"]
["2016-12-12T13:31:19.410","2016-12-12T03:31:19.410","AB","Sonar","Multibeam","New Line","0036, Max Angles 65/65. SBP new line. "]
["2016-12-12T13:34:45.310","2016-12-12T03:34:45.310","AB","Sonar","Knudsen","Tx Pulse","1.00ms, Gain 30"]
["2016-12-12T13:39:49.270","2016-12-12T03:39:49.270","AB","Sonar","Multibeam","Swath Check","5600m swath in 1400m"]
["2016-12-12T13:46:40.450","2016-12-12T03:46:40.450","CA","Sonar","Knudsen","Phase Range","1000-1500"]
["2016-12-12T13:53:45.570","2016-12-12T03:53:45.570","CA","Sonar","Knudsen","Phase Range","1250-1750"]
["2016-12-12T13:59:39.250","2016-12-12T03:59:39.250","CA","Sonar","Knudsen","Phase Range","1500-2000"]
["2016-12-12T14:01:34.760","2016-12-12T04:01:34.760","AB","Sonar","Knudsen","Tx Pulse","2, Gain 35, Phase Range 1750-2250m"]
["2016-12-12T14:11:07.880","2016-12-12T04:11:07.880","AB","Sonar","Multibeam","Sound Velocity Update",1535.17]
["2016-12-12T14:21:48.600","2016-12-12T04:21:48.600","CA","Sonar","Multibeam","New Line","0037, turn"]
["2016-12-12T14:25:03.410","2016-12-12T04:25:03.410","AB","Sonar","Multibeam","New Line","Crossline (0038). Max angle 60/60"]
["2016-12-12T14:30:28.900","2016-12-12T04:30:28.900","AB","Sonar","Multibeam","Max Angle","55/55, 5600m swath in 2100m."]
["2016-12-12T14:31:20.260","2016-12-12T04:31:20.260","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2016-12-12T14:43:38.720","2016-12-12T04:43:38.720","AB","Sonar","Knudsen","Phase Range","2250-2750"]
["2016-12-12T15:06:09.810","2016-12-12T05:06:09.810","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max Angles 50/50"]
["2016-12-12T15:36:38.520","2016-12-12T05:36:38.520","AB","Sonar","Multibeam","New Line","0040"]
["2016-12-12T15:41:45.250","2016-12-12T05:41:45.250","AB","Sonar","Knudsen","Phase Range","3500-4000m, Pulse 4, Power 3"]
["2016-12-12T15:43:15.460","2016-12-12T05:43:15.460","AB","Sonar","Multibeam","New Line","0041, Max Angles 50/50"]
["2016-12-12T15:47:30.530","2016-12-12T05:47:30.530","CA","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-12-12T16:06:15.870","2016-12-12T06:06:15.870","AB","Sonar","Knudsen","Phase Range","3000-3500"]
["2016-12-12T16:12:38.730","2016-12-12T06:12:38.730","AB","Sonar","Knudsen","Phase Range","2750-3250"]
["2016-12-12T16:24:22.610","2016-12-12T06:24:22.610","AB","Sonar","Multibeam","Sound Velocity Update","1535.4 m/s"]
["2016-12-12T16:29:04.230","2016-12-12T06:29:04.230","AB","Sonar","Knudsen","Phase Range","2500-3000"]
["2016-12-12T17:18:56.980","2016-12-12T07:18:56.980","AB","Sonar","Multibeam",null,"Stopped Logging, Secured"]
["2016-12-12T17:19:38.920","2016-12-12T07:19:38.920","AB","Sonar","Knudsen",null,"Secured  "]
["2016-12-12T17:24:25.500","2016-12-12T07:24:25.500","AB","Sonar","ADCP",null,"Started new cruise EX1609_02"]
["2016-12-12T17:49:36.990","2016-12-12T07:49:36.990","CA","XBT",null,null,"XBT 08, only 130 meters"]
["2016-12-12T19:00:22","2016-12-12T09:00:22","AB","Sonar","EK",null,"Calibration"]
["2016-12-13T03:56:35.340","2016-12-12T17:56:35.340","mw","sonar","Multibeam",null,"started pinging, warming up"]
["2016-12-13T04:34:31.940","2016-12-12T18:34:31.940","DS","Sonar","Multibeam","Sound Velocity Update","entered manual sound speed of 1535.91"]
["2016-12-13T04:36:41.910","2016-12-12T18:36:41.910","DS","XBT",null,null,"applied XBT 09 just before starting line 0044"]
["2016-12-13T04:37:38.560","2016-12-12T18:37:38.560","DS","Sonar","Multibeam","Start Logging","survey line 0044"]
["2016-12-13T04:51:54.410","2016-12-12T18:51:54.410","CW","Sonar","Knudsen","Start Pinging","Pulse 4; Power 3; Gain 36"]
["2016-12-13T04:57:58.110","2016-12-12T18:57:58.110","CW","Sonar","Knudsen","Range","3500-4000"]
["2016-12-13T05:13:55.770","2016-12-12T19:13:55.770","DS","Sonar","Multibeam",null,"swath coverage about 2000m less than expected. Shifting line plan and taking turn to try again. end turn line 0044, start survey line 0045."]
["2016-12-13T05:44:49.340","2016-12-12T19:44:49.340","CW","Sonar","Multibeam","New Line","Turn on line 0046"]
["2016-12-13T06:42:45.220","2016-12-12T20:42:45.220","DS","Sonar","Multibeam",null,"trying extra deep mode to see effect on swath width, no impact - switched back to Very Deep"]
["2016-12-13T06:48:01.930","2016-12-12T20:48:01.930","DS","Sonar","Knudsen",null,"end line, end pinging to see if it is impacting MBES. No effect"]
["2016-12-13T06:57:40.440","2016-12-12T20:57:40.440","DS","Sonar","Knudsen",null,"turned sub-bottom back on"]
["2016-12-13T07:16:27.290","2016-12-12T21:16:27.290","DS","Sonar","Multibeam","New Line","end survey line 0047, start turn 0048"]
["2016-12-13T07:35:19.820","2016-12-12T21:35:19.820","mw","Sonar","Multibeam","New Line","end turn 0048, started survey line 0049"]
["2016-12-13T08:22:25.730","2016-12-12T22:22:25.730","CW","Sonar","Multibeam",null,"Started losing bottom badly. Switched from Very Deep to Extra Deep and back. Worked well."]
["2016-12-13T08:31:01.780","2016-12-12T22:31:01.780","CW","Sonar","Multibeam","Along Direction Pitch","Zero"]
["2016-12-13T08:57:47.630","2016-12-12T22:57:47.630","CW","Sonar","Knudsen","Range","3750-4250"]
["2016-12-13T08:58:02.210","2016-12-12T22:58:02.210","CW","Sonar","Multibeam",null,"Very Deep is giving off trrbl data. Keeping it in Extra for a little while."]
["2016-12-13T09:04:59.250","2016-12-12T23:04:59.250","CW","Sonar","Multibeam",null,1534.22]
["2016-12-13T09:05:01.520","2016-12-12T23:05:01.520","CW","Sonar","Multibeam","New Line","Turn line 0051"]
["2016-12-13T09:22:23.570","2016-12-12T23:22:23.570","CW","Sonar","Multibeam",null,1535.4]
["2016-12-13T09:24:23.890","2016-12-12T23:24:23.890","CW","Sonar","Multibeam","New Line","Survey Line 0052"]
["2016-12-13T09:50:12.230","2016-12-12T23:50:12.230","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2016-12-13T09:50:28.140","2016-12-12T23:50:28.140","CW","Sonar","Multibeam","Ping Mode","Back to Very Deep. Behaving."]
["2016-12-13T09:53:27.740","2016-12-12T23:53:27.740","CW","Sonar","Multibeam",null,"TRU timing error again. 3 seconds red. Lost a few pings. Fixed itself."]
["2016-12-13T10:19:52.730","2016-12-13T00:19:52.730","CW","Sonar","Knudsen","Range","4250-4750"]
["2016-12-13T10:46:22.560","2016-12-13T00:46:22.560","CA","Sonar","Multibeam","New Line","Turn Line 0054"]
["2016-12-13T10:51:52.970","2016-12-13T00:51:52.970",null,null,null,null,"4000-4500"]
["2016-12-13T10:54:20.360","2016-12-13T00:54:20.360","CW","Sonar","Multibeam","Ping Mode","Losing bottom again. Very Deep to Extra Deep. "]
["2016-12-13T11:04:53.280","2016-12-13T01:04:53.280","CA","Sonar","Multibeam","New Line","End Turn Line 0055"]
["2016-12-13T11:14:18.480","2016-12-13T01:14:18.480","CA","Sonar","Knudsen","Range","4250-4750"]
["2016-12-13T12:00:07.170","2016-12-13T02:00:07.170","CA","Sonar","Knudsen","Range","4000-4500"]
["2016-12-13T12:12:41.150","2016-12-13T02:12:41.150","CA","XBT",null,null,"cast 10 applied to line 0056"]
["2016-12-13T12:20:31.250","2016-12-13T02:20:31.250","AB","Sonar","Multibeam","New Line","0057, turn"]
["2016-12-13T12:35:57.760","2016-12-13T02:35:57.760","AB","Sonar","Multibeam","New Line","0058"]
["2016-12-13T12:38:35.880",{"$f":"IF(ISBLANK(A198),\" \",((A198)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-13T02:38:35.880"},"AB","Sonar","Knudsen","Phase Range","3750-4250m"]
["2016-12-13T12:49:05.760","2016-12-13T02:49:05.760","AB","Sonar","Knudsen","Phase Range","4000-4500m"]
["2016-12-13T12:53:10.250","2016-12-13T02:53:10.250","AB","Sonar","Multibeam","Ping Mode","Very Deep, Max Angles 40/52"]
["2016-12-13T13:05:03.350","2016-12-13T03:05:03.350","CA","Sonar","Knudsen","Phase Range","3750-4250m"]
["2016-12-13T13:08:20.770","2016-12-13T03:08:20.770","CA","Sonar","Knudsen","Phase Range","3500-4000m"]
["2016-12-13T13:27:52.290","2016-12-13T03:27:52.290","AB","Sonar","Multibeam","Swath Check","5600m swath in 3800m"]
["2016-12-13T13:32:27.820","2016-12-13T03:32:27.820","AB","Sonar","Knudsen","Phase Range","3250-3750m, Pulse 8, Power 3, Gain 38"]
["2016-12-13T13:35:46.300","2016-12-13T03:35:46.300","AB","Sonar","Multibeam","New Line","0059"]
["2016-12-13T13:38:14.970","2016-12-13T03:38:14.970","AB","Sonar","Knudsen","Phase Range","3500-4000m"]
["2016-12-13T13:39:40.790","2016-12-13T03:39:40.790","AB","Sonar","Knudsen","Phase Range","3750-4250m"]
["2016-12-13T13:45:41.720","2016-12-13T03:45:41.720","AB","Sonar","Knudsen","Phase Range","4000-4500m"]
["2016-12-13T13:47:56.860","2016-12-13T03:47:56.860","AB","Sonar","Knudsen","Phase Range","4250-4750m"]
["2016-12-13T13:50:32.540","2016-12-13T03:50:32.540","AB","Sonar","Multibeam","New Line","0060, turn, SBP New line"]
["2016-12-13T13:56:52.480","2016-12-13T03:56:52.480","AB","Sonar","Knudsen","Phase Range","4000-4500m"]
["2016-12-13T14:01:48.590","2016-12-13T04:01:48.590","AB","Sonar","Knudsen","Phase Range","3750-4250m"]
["2016-12-13T14:03:07.710","2016-12-13T04:03:07.710","AB","Sonar","Knudsen","Phase Range","3500-4000m, New line"]
["2016-12-13T14:05:03.960","2016-12-13T04:05:03.960","AB","sonar","Multibeam","New Line","0061"]
["2016-12-13T14:08:46.730","2016-12-13T04:08:46.730","AB","Sonar","Multibeam","Ping Mode","Extra Deep, Only getting 31/31 in very Deep. Same in Extra deep."]
["2016-12-13T14:10:18.930","2016-12-13T04:10:18.930","AB","Sonar","Multibeam","Ping Mode","Very Deep, max angles set to 40/52. Cover is 33/31."]
["2016-12-13T14:11:23.100","2016-12-13T04:11:23.100","AB","Sonar","Knudsen","Phase Range","3250-3750m"]
["2016-12-13T14:13:59.510","2016-12-13T04:13:59.510","AB","Sonar","Multibeam","Max Angle","45/52. Coverage 45/35."]
["2016-12-13T14:14:39.920","2016-12-13T04:14:39.920","AB","Sonar","Knudsen","Phase Range","3000-3500m"]
["2016-12-13T14:16:11.260","2016-12-13T04:16:11.260","AB","Sonar","Multibeam","Max Angle","52/52. Coverage 52/35"]
["2016-12-13T14:22:39.280","2016-12-13T04:22:39.280","AB","Sonar","Knudsen","Phase Range","2750-3250m"]
["2016-12-13T14:30:55.780","2016-12-13T04:30:55.780","CA","Sonar","Knudsen","Phase Range","3000-3500m"]
["2016-12-13T14:36:39.950","2016-12-13T04:36:39.950","AB","Sonar","Knudsen","Phase Range","3250-3750m"]
["2016-12-13T15:00:13.310","2016-12-13T05:00:13.310","AB","Sonar","Knudsen","Phase Range","3500-4000m"]
["2016-12-13T15:15:57.740","2016-12-13T05:15:57.740","AB","Sonar","Multibeam","Swath Check","7100m swath in 3800m "]
["2016-12-13T15:17:11.970","2016-12-13T05:17:11.970","AB","Sonar","Multibeam","Sound Velocity Update","1535.81 ppt; 34.75 psu"]
["2016-12-13T15:24:08.150","2016-12-13T05:24:08.150","CA","Sonar","Multibeam","New Line","turn 0063"]
["2016-12-13T15:27:25.030","2016-12-13T05:27:25.030","AB","Sonar","Knudsen","Phase Range","New line, 3250-3750m"]
["2016-12-13T15:33:06.810","2016-12-13T05:33:06.810","AB","Sonar","Knudsen","Phase Range","3000-3500m"]
["2016-12-13T15:37:38.860","2016-12-13T05:37:38.860","AB","Sonar","Knudsen","Phase Range","2750-3250m"]
["2016-12-13T15:46:12.100","2016-12-13T05:46:12.100","AB","Sonar","Multibeam","Ping Mode","Deep, New line 0064 started"]
["2016-12-13T15:48:14.060","2016-12-13T05:48:14.060","AB","Sonar","Multibeam","Ping Mode","Very Deep, Intermittent ping drop outs along swath in Deep mode at 3000m. Full swath restored when switching to Very Deep mode."]
["2016-12-13T15:49:38.320","2016-12-13T05:49:38.320","AB","Sonar","Multibeam","Sound Velocity Update","1536.04ppt, 34.7 psu"]
["2016-12-13T15:51:17.220","2016-12-13T05:51:17.220","AB","Sonar","Knudsen","Phase Range","2500-3000m"]
["2016-12-13T16:01:37.110","2016-12-13T06:01:37.110","AB","Sonar","Multibeam","New Line","0065, Ping Mode changed to Deep at 2600m."]
["2016-12-13T16:05:10.210","2016-12-13T06:05:10.210","AB","Sonar","Multibeam","Max Angle","55/55. Coverage 47/50. Missing along swath pings. Depth 2694m. Ping Hz 0.15. Swath is 5000m in 2694m of water."]
["2016-12-13T16:08:36.040","2016-12-13T06:08:36.040","AB","Sonar","Knudsen","Tx Pulse","4, Power 2, Gain 35dB"]
["2016-12-13T16:16:44.250","2016-12-13T06:16:44.250","AB","Sonar","Knudsen","Tx Pulse","2"]
["2016-12-13T16:35:06.880","2016-12-13T06:35:06.880","AB","Sonar","Multibeam","New Line","0066"]
["2016-12-13T16:42:36.320","2016-12-13T06:42:36.320","AB","Sonar","Knudsen","Phase Range","2250-2750m"]
["2016-12-13T16:46:46.610","2016-12-13T06:46:46.610","AB","Sonar","Multibeam","Max Angle","65/65. Coverage 58/61 in 2426m, Swath is 6500m, Deep Mode switch to Auto:Deep Mode. Improving swath quality on the upslope. Ping Hz 0.13."]
["2016-12-13T16:48:56.260","2016-12-13T06:48:56.260","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2016-12-13T16:51:29.790","2016-12-13T06:51:29.790","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2016-12-13T16:54:37.790","2016-12-13T06:54:37.790","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2016-12-13T16:59:58.420","2016-12-13T06:59:58.420","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2016-12-13T17:00:39.280","2016-12-13T07:00:39.280","AB","Sonar","Multibeam","Max Angle","75/75. Coverage 69/67 Swath 4900m in 1193m"]
["2016-12-13T17:01:29.700","2016-12-13T07:01:29.700","AB","Sonar","Knudsen","Tx Pulse","1, Power 1, New line started."]
["2016-12-13T17:09:58.780","2016-12-13T07:09:58.780","AB","Sonar","Multibeam","New Line","0067, turn to left (270) to avoid ODAS Buoy. Ping 0.20 Hz"]
["2016-12-13T17:14:45.030","2016-12-13T07:14:45.030","AB","Sonar","Multibeam","New Line","0068"]
["2016-12-13T17:33:31.280","2016-12-13T07:33:31.280","DS","Sonar","Knudsen","Secure","almost on station for EK60 18 kHz calibration"]
["2016-12-13T17:42:54.240","2016-12-13T07:42:54.240","mw","sonar","Multibeam","Secure","on station for EK60 calibration, stopped pinging on lkine 0069"]
["2016-12-13T17:46:03.170","2016-12-13T07:46:03.170","DS","Sonar","ADCP",null,"logging to seee what currents are doing. "]
["2016-12-13T19:23:42.750","2016-12-13T09:23:42.750","DS","XBT",null,null,"XBT 11 completed for EK60 18 kHz calibration"]
["2016-12-13T19:24:49.660","2016-12-13T09:24:49.660","DS","Sonar","ADCP",null,"Secured  "]
["2016-12-14T01:49:27.040","2016-12-13T15:49:27.040","mw","sonar","EK","Secure","Secured EK60 post calibration "]
["2016-12-14T02:49:02.500","2016-12-13T16:49:02.500","DS","Sonar","ADCP",null,"started new cruise EX1609_03 to log OS38 bottom track data for several hours south of Lanai"]
["2016-12-14T05:16:30.430",{"$f":"IF(ISBLANK(A257),\" \",((A257)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-13T19:16:30.430"},"mw","kvm",null,null,"kvm froze on MB computers, had to restart manually"]
["2016-12-14T05:24:55.150","2016-12-13T19:24:55.150","mw","Sonar","Multibeam",null,"ran BIST"]
["2016-12-14T05:30:43.660","2016-12-13T19:30:43.660","mw","Sonar","Multibeam",null,"started pinging in mammal protection mode"]
["2016-12-14T05:48:53.080","2016-12-13T19:48:53.080","mw","sonar","Multibeam",null,"started logging line 0068, SVP profile outdated, XBT launcher being worked on, port disconnected"]
["2016-12-14T06:37:49.180","2016-12-13T20:37:49.180","ds","Sonar","ek",null,"started pinging, syncing in EK80 won't work - securing until tomorrow"]
["2016-12-14T07:42:11.120",{"$f":"IF(ISBLANK(A262),\" \",((A262)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-13T21:42:11.120"},"DS","Sonar","Knudsen","Start Pinging","logging Knudsen"]
["2016-12-14T07:49:03.830","2016-12-13T21:49:03.830","DS","XBT",null,null,"XBT 013 applied to line 0070"]
["2016-12-14T07:56:55.630","2016-12-13T21:56:55.630","CW","sonar","Knudsen","Range","2000-3000"]
["2016-12-14T08:05:51.370","2016-12-13T22:05:51.370","mw","Sonar","Multibeam","New Line","end line 0070, started line 0071 for turn"]
["2016-12-14T08:14:20.580","2016-12-13T22:14:20.580","CW","Sonar","Knudsen","Range","2000-3000"]
["2016-12-14T08:28:25.750","2016-12-13T22:28:25.750","CW","Sonar","Multibeam","New Line","Survey Line 0072"]
["2016-12-14T08:51:14.250","2016-12-13T22:51:14.250","CW","Sonar","Knudsen","Range","1500-2000"]
["2016-12-14T11:00:19.300","2016-12-14T01:00:19.300","CW","XBT",null,null,"XBT 014"]
["2016-12-14T11:00:34.490","2016-12-14T01:00:34.490","CW","Sonar","Multibeam","New Line","XBT 014 applied to line 0075"]
["2016-12-14T11:05:24.500","2016-12-14T01:05:24.500","CW","Sonar","Multibeam","New Line","Turn Line 0076"]
["2016-12-14T11:23:57.420","2016-12-14T01:23:57.420","AB","Sonar","Multibeam","New Line","0077, New sbp line"]
["2016-12-14T11:32:19.660","2016-12-14T01:32:19.660","AB","Sonar","Multibeam","Swath Check",".6100m in 2800m of water, Deep mode: second and third sectors of port side have consistent loss of pings at the end of each sector. Max angles 60/60, coverage is 46/60"]
["2016-12-14T11:58:01.720","2016-12-14T01:58:01.720","AB","Sonar","Multibeam","New Line","0078, sector tracking on"]
["2016-12-14T12:09:42.980","2016-12-14T02:09:42.980","AB","Sonar","Multibeam","Max Angle","60/65"]
["2016-12-14T12:44:10.240","2016-12-14T02:44:10.240","AB","Sonar","Multibeam","Max Angle","60/75"]
["2016-12-14T12:50:50","2016-12-14T02:50:50","AB","Sonar","Multibeam","Error Message","Saved on D:\\sisdata\\common\\message. Lost first light of three green on SIS. PU Sensor error COM1 missing. Happened intermittent on last shift.  "]
["2016-12-14T12:57:53.880","2016-12-14T02:57:53.880","CA","Sonar","Knudsen","Phase Range","1500-2500"]
["2016-12-14T13:18:31.250","2016-12-14T03:18:31.250","CA","Sonar","Knudsen","Phase Range","2000-3000"]
["2016-12-14T13:24:49.230","2016-12-14T03:24:49.230","AB","Sonar","Multibeam","Sound Velocity Update","1536.67 ppt, 34.68 psu"]
["2016-12-14T13:30:34","2016-12-14T03:30:34","AB","Sonar","Multibeam","New Line","0081, new sbp line, broke off normal survey lines to head straight for EK cal site."]
["2016-12-14T13:47:32.460","2016-12-14T03:47:32.460","AB","Sonar","Multibeam","Ping Mode","Auto: Very Deep. Max Angles 50/50. Sonar not tracking bottom well."]
["2016-12-14T13:49:38.980","2016-12-14T03:49:38.980","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-12-14T13:53:24.970","2016-12-14T03:53:24.970","AB","Sonar","Multibeam","Ping Mode","Manual:Deep mode, Auto jumping back and for between Very Deep and Deep frequently"]
["2016-12-14T14:09:58.940","2016-12-14T04:09:58.940","AB","Sonar","Knudsen","Phase Range","1000-2000m"]
["2016-12-14T14:15:54.890","2016-12-14T04:15:54.890","AB","Sonar","Multibeam","Error Message","COM1 failure ~10 seconds."]
["2016-12-14T14:29:57.660","2016-12-14T04:29:57.660","AB","Sonar","Knudsen","Phase Range","500-1500m"]
["2016-12-14T14:44:00.460","2016-12-14T04:44:00.460","AB","Sonar","Multibeam","Max Angle","75/75."]
["2016-12-14T14:44:19.300","2016-12-14T04:44:19.300","AB","Sonar","Multibeam","Sound Velocity Update","1536.84 ppt, 34.66 psu"]
["2016-12-14T14:44:46.750","2016-12-14T04:44:46.750","AB","Sonar","Multibeam","Swath Check","4700m swath in 896m of water. Coverage is 72/72."]
["2016-12-14T14:47:11.180","2016-12-14T04:47:11.180","AB","Sonar","Multibeam","Error Message","COM1 failure ~10 seconds."]
["2016-12-14T14:47:40.400","2016-12-14T04:47:40.400","AB","Sonar","Knudsen","Phase Range","0-1000m"]
["2016-12-14T14:48:31","2016-12-14T04:48:31","AB","Sonar","Multibeam","New Line","0082"]
["2016-12-14T14:50:52.200","2016-12-14T04:50:52.200","AB","Sonar","Knudsen","Range","500m, Phase Range 250-750m, Gain 30, TX Pulse 1, Power 1"]
["2016-12-14T14:54:00.480","2016-12-14T04:54:00.480","AB","Sonar","Multibeam","Ping Mode","Medium"]
["2016-12-14T14:58:10.140","2016-12-14T04:58:10.140","AB","Sonar","Multibeam","Error Message","COM1 failure ~10 seconds. Lost pings"]
["2016-12-14T15:01:28.600","2016-12-14T05:01:28.600","AB","Sonar","Multibeam","Error Message","COM1 failure, lost pings, Message Service saved in Cruise Logs and local"]
["2016-12-14T15:21:32.270","2016-12-14T05:21:32.270","AB","Sonar","Multibeam","Error Message","COM1 failure"]
["2016-12-14T15:22:43.280","2016-12-14T05:22:43.280","AB","Sonar","Knudsen","Phase Range","500-1000m"]
["2016-12-14T16:06:53.740","2016-12-14T06:06:53.740","AB","Sonar","Multibeam","New Line","0084, turn"]
["2016-12-14T16:09:15.760","2016-12-14T06:09:15.760","AB","sonar","Multibeam","New Line","0085, New SBP Line"]
["2016-12-14T16:12:52.450","2016-12-14T06:12:52.450","AB","Sonar","Multibeam","Error Message","COM1 Failure, screenshot of result"]
["2016-12-14T16:14:14.870","2016-12-14T06:14:14.870","AB","Ship",null,null,"Altering course directly to drop site for small boat ops."]
["2016-12-14T16:39:04.790","2016-12-14T06:39:04.790","AB","Sonar","Multibeam","Sound Velocity Update","1536.11 ppt, 34.58 psu"]
["2016-12-14T16:39:54.080","2016-12-14T06:39:54.080","AB","sonar","Knudsen","Phase Range","250-750m"]
["2016-12-14T16:53:48.300","2016-12-14T06:53:48.300","DS","Sonar","Knudsen","Secure"]
["2016-12-14T17:08:58.950","2016-12-14T07:08:58.950","DS","Sonar","Multibeam","Secure","getting within a few miles of Lanai. "]
["2016-12-14T18:51:43.330","2016-12-14T08:51:43.330","DS","Sonar","ADCP",null,"started new bottom track survey to test alignment angles entered yesterday by UH. "]
["2016-12-14T21:13:45.360","2016-12-14T11:13:45.360","DS","Sonar","ADCP",null,"started new ADCP survey with bottom track off. EX1609_05"]
["2016-12-15T03:59:03.690","2016-12-14T17:59:03.690","DS","Sonar","Multibeam",null,"secured ADCP, logging multibeam using sound speed profile from the night before for now"]
["2016-12-15T04:54:56.890","2016-12-15T04:54:59.790","mw","xbt",null,null,"XBT 015 "]
["2016-12-15T05:04:44.030","2016-12-14T19:04:44.030","CW","Sonar","Knudsen","Start Pinging","Pulse 4; Power 3; Gain 38"]
["2016-12-15T05:05:35.750","2016-12-14T19:05:35.750","CW","Sonar","Knudsen","Range","3750-4250"]
["2016-12-15T05:10:37.420","2016-12-14T19:10:37.420","CW","Sonar","Multibeam","Sound Velocity Update","SV 1536.4; 34.7 psu"]
["2016-12-15T05:15:23.940","2016-12-14T19:15:23.940","CW","Sonar","Knudsen","Range","4000-4500"]
["2016-12-15T06:04:13.540","2016-12-14T20:04:13.540","DS","Sonar","EK",null,"started logging EK60 data, synchronization appears to be working"]
["2016-12-15T06:11:11.040","2016-12-14T20:11:11.040","CW","Sonar","Knudsen","Range","4250-4750"]
["2016-12-15T06:20:01.510","2016-12-14T20:20:01.510","CW","Sonar","Multibeam","Sound Velocity Update","1533.7 m/sec; 34.84 ppt"]
["2016-12-15T06:26:31.050","2016-12-14T20:26:31.050","CW","Sonar","Multibeam","New Line","Turd Line 0089"]
["2016-12-15T06:46:00.310","2016-12-14T20:46:00.310","CW","Sonar","Multibeam","New Line","Survey Line 0090"]
["2016-12-15T06:49:34.200","2016-12-14T20:49:34.200","CW","Sonar","Multibeam",null,"Bad data at 4500m. Going from Very Deep to Extra Deep. "]
["2016-12-15T07:10:48.760","2016-12-14T21:10:48.760","CW","Sonar","Multibeam","Ping Mode","Not getting very good swath, regardless of mode."]
["2016-12-15T07:21:25.910","2016-12-14T21:21:25.910","CW","Sonar","Knudsen","Range","4000-4500"]
["2016-12-15T07:50:19.840","2016-12-14T21:50:19.840","CW","Sonar","Multibeam","Ping Mode","At 4300m, tried going back to Very Deep; quickly went bad. Back to Extra Deep."]
["2016-12-15T08:02:25.690",{"$f":"IF(ISBLANK(A325),\" \",((A325)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-14T22:02:25.690"},"CW","Sonar","Knudsen","Range","3000-4000"]
["2016-12-15T08:04:27.130","2016-12-14T22:04:27.130","CW","Sonar","Multibeam","Sound Velocity Update","1536.00 m/sec; 34.71 ppt"]
["2016-12-15T08:04:28.730","2016-12-14T22:04:28.730","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2016-12-15T08:19:36.050","2016-12-14T22:19:36.050","CW","Sonar","Knudsen","Range","3000-3500"]
["2016-12-15T08:26:30.910","2016-12-14T22:26:30.910","CW","Sonar","Knudsen","Range","3250-3750"]
["2016-12-15T08:44:10.980","2016-12-14T22:44:10.980","CW","Sonar","Knudsen","Range","2500-3000"]
["2016-12-15T08:47:03.840","2016-12-14T22:47:03.840","CW","Sonar","Knudsen","Range","2250-2750"]
["2016-12-15T08:53:21.580","2016-12-14T22:53:21.580","CW","Sonar","Knudsen","Range","2000-2500"]
["2016-12-15T08:58:13.220","2016-12-14T22:58:13.220","CW","Sonar","Multibeam","New Line","Turn Line 0093"]
["2016-12-15T08:58:39.980","2016-12-14T22:58:39.980","CW","Sonar","Knudsen","Range","1500-2500"]
["2016-12-15T08:59:46.810","2016-12-14T22:59:46.810","CW","Sonar","Knudsen","Tx Power",2]
["2016-12-15T08:59:48.320","2016-12-14T22:59:48.320","CW","Sonar","Knudsen","Tx Pulse",2]
["2016-12-15T09:06:15.180","2016-12-14T23:06:15.180","CW","Sonar","Multibeam","New Line","Bypassing andled coverage line that's making 100% overlap. Line 0093 will be a gigantic U-Turn on to the next main line."]
["2016-12-15T09:18:34.010","2016-12-14T23:18:34.010","CW","Sonar","Knudsen","Range","2000-3000"]
["2016-12-15T09:23:08.650","2016-12-14T23:23:08.650","CW","Sonar","Multibeam","Sound Velocity Update","1535.1 m/sec; 34.78 ppt"]
["2016-12-15T09:32:02.170","2016-12-14T23:32:02.170","CW","Sonar","Multibeam","New Line","Survey Line 0094"]
["2016-12-15T09:51:51.590","2016-12-14T23:51:51.590","CW","Sonar","Knudsen","Range","2500-3000"]
["2016-12-15T10:12:31.940","2016-12-15T00:12:31.940","CW","Sonar","Knudsen","Range","3000-4000"]
["2016-12-15T10:43:43.320","2016-12-15T00:43:43.320","AB","Sonar","Knudsen","Phase Range","4000-5000m, Pulse 4"]
["2016-12-15T11:29:36.210","2016-12-15T01:29:36.210","CA","XBT",null,null,"cast 16 applied to line 0095"]
["2016-12-15T11:39:07.020","2016-12-15T01:39:07.020","AB","Sonar","Knudsen","Phase Range","4000-5000m, Pulse 8"]
["2016-12-15T11:45:15.760","2016-12-15T01:45:15.760","AB","Sonar","Multibeam",null,"Video display issue. Line096 - no screen display, still pinging, still logging. Data processes in Qimera."]
["2016-12-15T11:49:43.330","2016-12-15T01:49:43.330","AB","Sonar","Multibeam","New Line","0098 turn."]
["2016-12-15T12:08:32.880","2016-12-15T02:08:32.880","AB","Sonar","Multibeam","New Line","sbp new line"]
["2016-12-15T12:19:01.740","2016-12-15T02:19:01.740","AB","Sonar","Multibeam","Swath Check","6000m in 4400m of water. Very Deep Mode, 40/38 Coverage. Ping 0.11Hz"]
["2016-12-15T12:45:56.710","2016-12-15T02:45:56.710","AB","Sonar","Knudsen","Phase Range","3500-4500m, Pulse 4"]
["2016-12-15T12:48:36.140","2016-12-15T02:48:36.140","AB","sonar","Multibeam","Swath Check","4700m swath in 4308m of water, coverage 31/30, Ping 0.12 Hz, Very Deep Mode."]
["2016-12-15T13:34:16.960","2016-12-15T03:34:16.960","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-12-15T13:38:42.880","2016-12-15T03:38:42.880","AB","Sonar","Multibeam","Error Message","Com1 Failure - position"]
["2016-12-15T13:52:08.990","2016-12-15T03:52:08.990","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-12-15T14:01:30.330","2016-12-15T04:01:30.330","AB","sonar","Knudsen","Phase Range","3000-4000m"]
["2016-12-15T14:25:30.030","2016-12-15T04:25:30.030","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-12-15T14:52:28.070","2016-12-15T04:52:28.070","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2016-12-15T15:20:10.170","2016-12-15T05:20:10.170","AB","Sonar","Multibeam","New Line","0103, turn line"]
["2016-12-15T15:29:11.790","2016-12-15T05:29:11.790","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2016-12-15T16:03:08.090","2016-12-15T06:03:08.090","AB","Sonar","Multibeam","New Line","0104, new line sbp"]
["2016-12-15T16:11:58.480","2016-12-15T06:11:58.480","AB","Sonar","Multibeam","Max Angle","52/52"]
["2016-12-15T16:13:14.070","2016-12-15T06:13:14.070","AB","Sonar","Multibeam","Sound Velocity Update","1535.53 ppt, 34.81psu"]
["2016-12-15T16:14:27.310","2016-12-15T06:14:27.310","AB","Sonar","Multibeam","Swath Check","Very Deep Mode, 0.12 Hz ping, 52/52 coverage. Swath is 6600m in 3000m of water."]
["2016-12-15T17:02:33.060","2016-12-15T07:02:33.060","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2016-12-15T17:03:27.080","2016-12-15T07:03:27.080","AB","Sonar","Multibeam","New Line","0105"]
["2016-12-15T17:16:46.530","2016-12-15T07:16:46.530","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2016-12-15T18:22:58.230","2016-12-15T08:22:58.230","AB","Sonar","Multibeam","Sound Velocity Update","1534.06 ppt"]
["2016-12-15T18:39:32.460","2016-12-15T08:39:32.460","AB","Sonar","Multibeam","Sound Velocity Update","1533.45 ppt"]
["2016-12-15T18:56:12.850","2016-12-15T08:56:12.850","CA","XBT",null,null,"cast 17 applied to line 0106"]
["2016-12-15T20:18:16.190","2016-12-15T10:18:16.190","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2016-12-15T21:00:26.170","2016-12-15T11:00:26.170","DS","Sonar","Multibeam","New Line","start survey line 0109, multibeam is junk data, called bridge and had deck department stop wirebrush operation near the AC flat. Data improved immediately. Stopped sub-bottom briefly. "]
["2016-12-15T21:25:00.550","2016-12-15T11:25:00.550","DS","Ship",null,null,"requested survey line be moved 900m east. Logging sub-bottom data again. "]
["2016-12-15T22:54:50.770","2016-12-15T12:54:50.770","DS","Sonar",null,null,"secured Knudsens and EK60 and multibeam for CTD cast. "]
["2016-12-15T23:24:00.180","2016-12-15T13:24:00.180","MW","Sonar",null,null,"adcp begin pinging for CTD"]
["2016-12-16T01:12:44.700","2016-12-15T15:12:44.700","CW","Sonar",null,null,"ADCP secure"]
["2016-12-16T01:32:46.620","2016-12-15T15:32:46.620","CW","Sonar","Multibeam","Start Logging","Line 0111"]
["2016-12-16T01:41:41.660","2016-12-15T15:41:41.660","CW","XBT",null,null,"XBT 018, applied to line 0111"]
["2016-12-16T01:44:06.210","2016-12-15T15:44:06.210","CW","Sonar","Multibeam","Sound Velocity Update","1535.8 ppt, 34.73psu"]
["2016-12-16T01:44:37.280","2016-12-15T15:44:37.280","CW","Sonar","Multibeam","Ping Mode","Extra Deep at 4500"]
["2016-12-16T01:45:45.290","2016-12-15T15:45:45.290","CW","Sonar","Multibeam","Max Angle","32/32"]
["2016-12-16T01:50:18.810","2016-12-15T15:50:18.810","DF","Sonar","EK",null,"Started pinging and logging"]
["2016-12-16T02:44:13.060","2016-12-15T16:44:13.060","CW","Sonar","Multibeam","New Line","Turn Line 0113"]
["2016-12-16T02:53:42.420","2016-12-15T16:53:42.420","CW","Issue/Problem","Multibeam",null,"Much more extravagent TRU lamp and num disp red lights, with echo sounder error window. Clicked okay and it resumed pinging, with a few seconds of loss. But it was on a turn, so no big really."]
["2016-12-16T02:58:45.730","2016-12-15T16:58:45.730","CW","Sonar","Multibeam","New Line","Survey Line 0114"]
["2016-12-16T03:14:39.940","2016-12-15T17:14:39.940","DF","Sonar","Multibeam",null,"Position input missing error, lost pinging momentarily"]
["2016-12-16T03:25:20.150","2016-12-15T17:25:20.150","DF","Sonar","Multibeam",null,"TRU Status lamp went red"]
["2016-12-16T05:11:44.810","2016-12-15T19:11:44.810","CW","Sonar","Multibeam","Max Angle","26/26 nice n dapper"]
["2016-12-16T05:13:55.340","2016-12-15T19:13:55.340","CW","Sonar","Multibeam","New Line","Turn Line 0117"]
["2016-12-16T05:33:16.440",{"$f":"IF(ISBLANK(A389),\" \",((A389)-DATE(1970,1,1))+25569-($C$1/24))","v":"2016-12-15T19:33:16.440"},"CW","Sonar","Multibeam","New Line","Survey Line 0118"]
["2016-12-16T05:55:16.390","2016-12-15T19:55:16.390","CW","Sonar","Multibeam","Sound Velocity Update","1534.19 ppt, 34.87psu"]
["2016-12-16T06:10:47.350","2016-12-15T20:10:47.350","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2016-12-16T07:32:29.890","2016-12-15T21:32:29.890","CW","Sonar","Multibeam","Sound Velocity Update","1535.27 ppt, 34.76psu"]
["2016-12-16T07:54:49.120","2016-12-15T21:54:49.120","CW","Sonar","Multibeam","New Line","Turn Line 0121"]
["2016-12-16T07:59:12.120","2016-12-15T21:59:12.120","CW","Sonar","Multibeam","Along Direction Pitch",0]
["2016-12-16T08:11:14.670","2016-12-15T22:11:14.670","CW","Sonar","Multibeam","New Line","Survey Line 0122"]
["2016-12-16T08:40:33.630","2016-12-15T22:40:33.630","CW","XBT",null,null,"XBT 019"]
["2016-12-16T08:41:03.750","2016-12-15T22:41:03.750","CW","Sonar","Multibeam","New Line","XBT 019 applied to line 0123"]
["2016-12-16T08:42:52.870","2016-12-15T22:42:52.870","CW","Sonar","Multibeam","Sound Velocity Update","1534.67 ppt, 34.76psu"]
["2016-12-16T08:43:28.230","2016-12-15T22:43:28.230","CW","Sonar","Multibeam","Max Angle","30/30"]
["2016-12-16T09:47:10.090","2016-12-15T23:47:10.090","CW","Sonar","Multibeam","New Line","Turn Line 0125"]
["2016-12-16T10:10:01.180","2016-12-16T00:10:01.180","CW","Sonar","Multibeam","New Line","Survey Line 0126"]
["2016-12-16T10:11:20.720","2016-12-16T00:11:20.720","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2016-12-16T10:42:43.290","2016-12-16T00:42:43.290","CW","Sonar","Knudsen","Secure","SBP is done, man!"]
["2016-12-16T11:45:35.070","2016-12-16T01:45:35.070","CA","Sonar","Multibeam","New Line","Turn Line 0127"]
["2016-12-16T11:53:54.640","2016-12-16T01:53:54.640","CA","Sonar","Multibeam","Swath Check","Very Deep Mode, 0.12 Hz ping, 45/40 coverage. Swath is 5100m in 3500m of water."]
["2016-12-16T12:21:27.470","2016-12-16T02:21:27.470","AB","Sonar","Multibeam","New Line","Lost bottom over shelf."]
["2016-12-16T12:29:50.560","2016-12-16T02:29:50.560","CA","Sonar","Multibeam","Max Angle","65/65"]
["2016-12-16T12:37:38.790","2016-12-16T02:37:38.790","CA","Sonar","Multibeam","Max Angle","75/75"]
["2016-12-16T12:38:41.400","2016-12-16T02:38:41.400","CA","Sonar","Multibeam","Ping Mode","medium"]
["2016-12-16T12:46:12.180","2016-12-16T02:46:12.180","AB","Sonar","Multibeam","Ping Mode","medium"]
["2016-12-16T13:35:27.540","2016-12-16T03:35:27.540","CA","Sonar","Multibeam","New Line","Turn line 0131"]
["2016-12-16T13:44:35.400","2016-12-16T03:44:35.400","AB","Sonar","Multibeam","New Line",132]
["2016-12-16T13:49:02.700","2016-12-16T03:49:02.700","AB","Sonar","EK",null,"Range change to 600m for 18,38,70"]
["2016-12-16T14:20:08.620","2016-12-16T04:20:08.620","AB","Xbt",null,null,"20 added to new line 133, 1535.13ppt"]
["2016-12-16T14:39:44","2016-12-16T04:39:44","AB","Ship",null,null,"Reducing speed to 6 kts "]
["2016-12-16T14:41:22.370","2016-12-16T04:41:22.370","AB","Sonar","Multibeam","New Line","line 134."]
["2016-12-16T14:42:39.720","2016-12-16T04:42:39.720","AB","Ship",null,null,"Reducing speed to 4 kts"]
["2016-12-16T15:00:52.600","2016-12-16T05:00:52.600","CA","Sonar","Multibeam","New Line","Turn line 0135"]
["2016-12-16T15:11:24.420","2016-12-16T05:11:24.420","CA","Sonar","Multibeam",null,"stopped logging and pinging on EM302 & EK60"]
["2016-12-16T15:29:30.910","2016-12-16T05:29:30.910","AB",null,null,null,"TRU Off, Sonars in closet off, SBP off, TSG secured."]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A454),\" \",((A454)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A518),\" \",((A518)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A582),\" \",((A582)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A646),\" \",((A646)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A710),\" \",((A710)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A774),\" \",((A774)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A838),\" \",((A838)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A902),\" \",((A902)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A966),\" \",((A966)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1001),\" \",((A1001)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1026),\" \",((A1026)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1090),\" \",((A1090)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1154),\" \",((A1154)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1218),\" \",((A1218)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1282),\" \",((A1282)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1346),\" \",((A1346)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1410),\" \",((A1410)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1474),\" \",((A1474)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1538),\" \",((A1538)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1602),\" \",((A1602)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1666),\" \",((A1666)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1730),\" \",((A1730)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1794),\" \",((A1794)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1858),\" \",((A1858)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1922),\" \",((A1922)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1986),\" \",((A1986)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["AB","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DF","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["CW","Weather","Knudsen","New Line","Secure","Gain Mode"]
["DS","Watch Change","All","Max Angle",null,"Gain Value"]
["CA","XBT","ADCP","Spike Filter Strength",null,"Process Shift"]
["MW","Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
[null,"Other",null,"Aeration Filter (On/Off)",null,"Range"]
[null,null,null,"Interference Filter (On/Off)",null,"Phase Mode"]
[null,null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]
[null,null,null,"Sound Velocity Update"]
[null,null,null,"Swath Check"]
[null,null,null,"Error Message"]