

Data Management Plan

Okeanos Explorer (EX1701): Kingman, Palmyra, Jarvis (Mapping)

*OER Data Management Objectives*

*Maintain and monitor normal data pipelines.*

06-Jan-17

Page 1

* 1. **Name and Purpose of the Data Collection Project**

Okeanos Explorer (EX1701): Kingman, Palmyra, Jarvis (Mapping)

* 1. **Summary description of the data to be collected.**

Operations will include the use of the ship’s deep water mapping systems (Kongsberg EM302 multibeam sonar, EK60 split-beam fisheries sonars, ADCPs, and Knudsen 3260 chirp sub-bottom profiler sonar), and the ship’s high- bandwidth satellite connection for real-time ship to shore communications.

* 1. **Keywords or phrases that could be used to enable users to find the data.**

expedition, exploration, explorer, marine education, noaa, ocean, ocean discovery, ocean education, ocean exploration, ocean exploration and research, ocean literacy, ocean research, OER, science, scientific mission, scientific research, sea, stewardship, systematic exploration, technology, transformational research, undersea, underwater, Davisville, mapping survey, multibeam, multibeam backscatter, multibeam sonar, multi-beam sonar, noaa fleet, okeanos, okeanos explorer, R337, Rhode Island, scientific computing system, SCS, single beam sonar, singlebeam sonar, single-beam sonar, sub-bottom profile, water column backscatter, Pago Pago, American Samoa, Pacific Remote Islands Marine National Monument, PRIMNM, Kingman Reef, Palmyra Atoll, Jarvis Island, Phoenix Islands Protected Area, PIPA, Republic of Kiribati, CAPSTONE, biogeographic patterns, Monument and Sanctuaries, habitat surveys, vulnerable marine habitats, Prime Crust Zone, PCZ, deep sea minerals, Central Pacific Seamounts, oceans

* 1. **If this mission is part of a series of missions, what is the series name?**

Okeanos Mapping Cruises

* 1. **Planned or actual temporal coverage of the data.**

Dates:

1/18/2017

to

2/10/2017

**1.6 Planned or actual geographic coverage of the data.**

Latitude Boundaries:

Longitude Boundaries:

0.42

-175.55

to

to

7.2

-161.23

**1.7 What data types will you be creating or capturing and submitting for archive?**

Cruise Plan, Cruise Summary, Data Management Plan, Highlight Images, Quick Look Report, ADCP, CTD (processed), CTD (product), CTD (raw), EK60 Singlebeam Data, Mapping Summary, Multibeam (image), Multibeam (processed), Multibeam (product), Multibeam (raw), SCS Output (compressed), SCS Output (native), Sub-Bottom Profile data, Water Column Backscatter, XBT (raw)

Okeanos Explorer (EX1701): Kingman, Palmyra, Jarvis (Mapping)

**1. General Description of Data to be Managed**

06-Jan-17

**1.8 What platforms will be employed during this mission?**

Deep Discoverer ROV, NOAA Ship Okeanos Explorer, SEIRIOS Camera Sled

Page 2

Overall POC:

Elizabeth Lobecker, Multibeam Mapping Expert, Contractor (ERT, Inc.), NOAA Office of Ocean

Exploration and Research, [elizabeth.lobecker@noaa.gov](mailto:elizabeth.lobecker@noaa.gov) Expedition Coordinator

NOAA Office of Ocean Exploration and Research, UNH CCOM/JHC [elizabeth.lobecker@noaa.gov](mailto:elizabeth.lobecker@noaa.gov)

603-862-1475

Title:

Affiliation/Dept: E-Mail:

Phone:

Data POC Name:

Susan Gottfried (stewardship), Andrew O'Brien (shoreside and onboard (remote) data

management)

Data Manager

[susan.gottfried@noaa.gov,](mailto:susan.gottfried@noaa.gov) [andrew.obrien@tgfoe.org](mailto:andrew.obrien@tgfoe.org)

Title:

E-Mail:

**4.1 Have resources for management of these data been identified?**

True

**4.2 Approximate percentage of the budget devoted to data management. (specify % or "unknown")**

unknown

* 1. **What is the processing workflow from collection to public release?**

SCS data shall be delivered in its native format as well as an archive-ready, documented, and compressed NetCDF3 format to NCEI-MD; multibeam data and metadata will be compressed and delivered in a bagit format to NCEI-CO

* 1. **What quality control procedures will be employed?**

Quality control procedures for the data from the Kongsberg EM302 is handled at UNH CCOM/JHC. Raw (level-0) bathymetry files are cleaned/edited into new data files (level-1) and converted to a variety of products (level-2). Data from sensors monitored through the SCS are archived in their native format and are not quality controlled. Data from CTD casts and XBT firings are archived in their native format. CTDs are post-processed by the data management team as a quality control measure and customized CTD profiles are generated for display on the Okeanos Atlas (explore.noaa.gov/okeanosatlas).

**6.1 Does the metadata comply with the Data Documentation Directive?**

**6.1.1 If metadata are non-existent or non-compliant, please explain:**

True

**6.2 Where will the metadata be hosted?**

Okeanos Explorer (EX1701): Kingman, Palmyra, Jarvis (Mapping)

**6. Data Documentation**

**5. Data Lineage and Quality**

**4. Resources**

**3. Point of Contact for Managing the Data**

**2. Point of Contact for this Data Producing Project**

06-Jan-17

Organization:

Page 3

An ISO format collection-level metadata record will be generated during pre-cruise planning

and published in an OER catalog and Web Accessible Folder (WAF) hosted at NCEI-MS for public discovery and access. The record will be harvested by data.gov.

<http://www.ncddc.noaa.gov/rdn/oer-waf/ISO/Resolved/>

ISO 19115-2 Geographic Information with Extensions for Imagery and Gridded Data will be the metadata standard employed; a NetCDF3 standard for oceanographic data will be employed for the SCS data; the Library of Congress standard, MAchine Readable Catalog (MARC), will be employed for NOAA Central Library records.

URL:

Meta Std:

**6.3 Process for producing and maintaining metadata:**

Metadata will be generated via xml editors or metadata generation tools.

* 1. **Do the data comply with the Data Access Directive?**
     1. **If the data will not be available to the public, or with limitations, provide a valid reason.**

Not Applicable

* + 1. **If there are limitations, describe how data are protected from unauthorized access.**

True

Account access to mission systems are maintained and controlled by the Program. Data access prior to public

accessibility is documented through the use of Data Request forms and standard operating procedures.

**7.2 Name and URL of organization or facility providing data access.**

National Centers for Environmental Information

www.ncei.noaa.gov; https://explore.noaa.gov/digitalatlas

Org:

URL:

* 1. **Approximate delay between data collection and dissemination. By what authority?**

Hold Time: data from Okeanos Explorer are immediately publicly accessible Authority:

* 1. **Prepare a Data Access Statement**

No data access constraints, unless data are protected under the National Historic Preservation Act of 1966.

* 1. **Actual or planned long-term data archive location:**

Data from this mission will be preserved and stewarded through the NOAA National Centers for Environmental Information. Refer to the Okeanos Explorer FY16 Data Management Plan at NOAA's EDMC DMP Repository (EX\_FY17\_DMP\_Final.pdf) for detailed descriptions of the processes, procedures, and partners involved in this collaborative effort.

* 1. **If no archive planned, why?**

**8.3 If any delay between data collection and submission to an archive facility, please explain.**

60-90 days

**8.4 How will data be protected from accidental or malicious modification or deletion?**

Okeanos Explorer (EX1701): Kingman, Palmyra, Jarvis (Mapping)

**8. Data Preservation and Protection**

**7. Data Access**

06-Jan-17

Page 4

Data management standard operating procedures minimizing accidental or malicious modification or deletion are in

place aboard the Okeanos Explorer and will be enforced.

**8.5 Prepare a Data Use Statement**

Data use shall be credited to NOAA Office of Ocean Exploration and Research.

Okeanos Explorer (EX1701): Kingman, Palmyra, Jarvis (Mapping)