{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2005,"n_cols":7,"rows_kept":2005,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1704","UTC to Local: ",-14,"UTC 2","UTC 3","UTC 4","Cruise Details: April 4th - 21st"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2017-04-03T18:29:12",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-04T08:29:12"},"AB",null,null,null,"turned on TRU"]
["2017-04-03T19:48:11.800",{"$f":"IF(ISBLANK(A6),\" \",((A6)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-04T09:48:11.800"},"DF","Sonar","Multibeam",null,"Ran BIST 01"]
["2017-04-03T19:59:21.490","2017-04-04T09:59:21.490","DF","Sonar","Multibeam",null,"BIST 01 all passed"]
["2017-04-03T20:15:12","2017-04-04T10:15:12","AB","Ship",null,null,"Underway"]
["2017-04-03T21:01:10.580","2017-04-04T11:01:10.580","DF","Sonar","Multibeam",null,"Started pinging in MMM, TSG on"]
["2017-04-03T21:01:37.460","2017-04-04T11:01:37.460","DF","Sonar",null,null,"Started pinging in MMM, TSG on"]
["2017-04-03T21:24:58.840","2017-04-04T11:24:58.840","CW","XBT",null,null,"Cast 001 collected and applied to line 0000"]
["2017-04-03T21:28:52.620","2017-04-04T11:28:52.620","DF","Sonar","Multibeam",null,"Begin survey line 0001"]
["2017-04-03T21:32:48.800","2017-04-04T11:32:48.800","AB","Sonar","Knudsen","Range","500"]
["2017-04-03T21:44:03.010","2017-04-04T11:44:03.010","CW","Issue",null,null,"Rollin' like cray cray"]
["2017-04-03T22:00:17.900","2017-04-04T12:00:17.900","AB","Sonar","Knudsen","Phase Range","Power 2, Pulse 2, Phase Range 1000-1500m, Range 500m, Gain 34db"]
["2017-04-03T22:05:59.060","2017-04-04T12:05:59.060","AB","Sonar","EK",null,"Range 5500m, Bottom Detect 8000m, 38khz passive"]
["2017-04-03T22:24:10.820","2017-04-04T12:24:10.820","AB","Sonar","Multibeam",null,"Min Depth 200, Maxs Depth 3500, Manual Deep Ping Mode, Max Angle 75/75, Along Direction 0, Spike Medium, Range Gate Normal, Phase Ramp Normal, Penetration Filter Off, All other filters off."]
["2017-04-03T22:26:46.150","2017-04-04T12:26:46.150","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2017-04-03T22:28:38","2017-04-04T12:28:38","Ab","Sonar","Multibeam","new line","0002"]
["2017-04-03T22:32:55.350","2017-04-04T12:32:55.350","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2017-04-03T22:38:44.370","2017-04-04T12:38:44.370","AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2017-04-03T22:44:25.710","2017-04-04T12:44:25.710","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2017-04-03T22:55:01.180","2017-04-04T12:55:01.180","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2017-04-03T23:14:43.670","2017-04-04T13:14:43.670","AB","Sonar","Multibeam","Ping Mode","Manual: Very Deep, blowing out in sector 2 (p/s)"]
["2017-04-03T23:18:16.170","2017-04-04T13:18:16.170","AB","Sonar","Multibeam","Ping Mode","Manual: Deep"]
["2017-04-03T23:18:17.690","2017-04-04T13:18:17.690","AB","Sonar","Multibeam","Max Angles","65/65"]
["2017-04-03T23:19:32.980","2017-04-04T13:19:32.980","AB","Sonar","Multibeam",null,"Aeration filter on"]
["2017-04-03T23:31:10.960","2017-04-04T13:31:10.960","AB","Sonar","Multibeam","Max Angles","60/75 (coverage 2600/2700)"]
["2017-04-03T23:34:25","2017-04-04T13:34:25","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2017-04-03T23:51:10.390","2017-04-04T13:51:10.390","AB","Sonar","Multibeam","Ping Mode","Manual very deep. Dropping out with heavy rolls. Reduced max angles to 52/52"]
["2017-04-03T23:52:27.970","2017-04-04T13:52:27.970","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2017-04-03T23:57:53.650","2017-04-04T13:57:53.650","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2017-04-04T00:05:07.580","2017-04-04T14:05:07.580","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2017-04-04T00:07:21.230","2017-04-04T14:07:21.230","CW","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-04-04T00:16:37.110","2017-04-04T14:16:37.110","CW","Sonar","Knudsen","Phase Range","2750-3250"]
["2017-04-04T00:29:13.140","2017-04-04T14:29:13.140","CW","Sonar","Multibeam","new line","Turn line 0005 (SIS Line cnt. Skipped 0004 for no apparent reason.)"]
["2017-04-04T00:49:19.220","2017-04-04T14:49:19.220","CW","Sonar","Multibeam","new line","Survey Line 0006"]
["2017-04-04T00:55:49.800","2017-04-04T14:55:49.800","CW","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-04-04T01:04:08.620","2017-04-04T15:04:08.620","CW","Sonar","Multibeam","Ping Mode","at 2000m, but Deep Mode just blows out to garbage. Keeping manual Very Deep."]
["2017-04-04T01:10:18.250",{"$f":"IF(ISBLANK(A40),\" \",((A40)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-04T15:10:18.250"},"CW","Sonar","Multibeam","Ping Mode","Tried again. Same thing at 1700m."]
["2017-04-04T01:05:35.690","2017-04-04T15:05:35.690","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2017-04-04T01:11:22.250","2017-04-04T15:11:22.250","CW","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-04-04T01:23:02.700","2017-04-04T15:23:02.700","CW","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-04-04T01:23:09.730","2017-04-04T15:23:09.730","CW","Weather","All",null,"Did we mention that there are heavy seas? Well there is."]
["2017-04-04T01:25:11.460","2017-04-04T15:25:11.460","CW","Sonar","Multibeam","Ping Mode","OMG, Deep is working!!!"]
["2017-04-04T01:26:06.170","2017-04-04T15:26:06.170","CW","Sonar","Knudsen","Phase Range","750-1250"]
["2017-04-04T01:26:06.170",{"$f":"IF(ISBLANK(A47),\" \",((A47)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-04T15:26:06.170"},"CW","Sonar","Multibeam","Ping Mode","Auto, going between Deep 1 and Deep 2"]
["2017-04-04T01:28:27.710","2017-04-04T15:28:27.710","CW","Sonar","Knudsen","Tx Power","1"]
["2017-04-04T01:28:47.390","2017-04-04T15:28:47.390","CW","Sonar","Knudsen","Tx Pulse","2"]
["2017-04-04T01:44:39.490","2017-04-04T15:44:39.490","CW","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-04-04T01:47:57.220","2017-04-04T15:47:57.220","CW","Issue",null,null,"POS Position Accuracy lamp red for about a minute."]
["2017-04-04T01:52:28.410","2017-04-04T15:52:28.410","CW","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-04-04T02:19:56.100","2017-04-04T16:19:56.100","CW","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-04-04T02:25:58.460","2017-04-04T16:25:58.460","CW","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-04-04T02:31:10.830","2017-04-04T16:31:10.830","CW","Sonar","Multibeam","new line","Turn at beginning of line 0008 (New Heading)"]
["2017-04-04T03:22:34.580","2017-04-04T17:22:34.580","CW","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-04-04T03:33:59.800","2017-04-04T17:33:59.800","CW","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-04-04T03:48:16.360","2017-04-04T17:48:16.360","AB","Sonar","Multibeam","new line","0010, turn"]
["2017-04-04T03:52:48.280","2017-04-04T17:52:48.280","AB","Sonar","Multibeam","new line","0011"]
["2017-04-04T03:59:31.520","2017-04-04T17:59:31.520","AB","ship",null,null,"shift 500m to starboard"]
["2017-04-04T04:10:14.760","2017-04-04T18:10:14.760","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2017-04-04T04:10:58.930","2017-04-04T18:10:58.930","CW","Sonar","Knudsen","Range","1000"]
["2017-04-04T04:11:17.170","2017-04-04T18:11:17.170","CW","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-04-04T04:22:50.560","2017-04-04T18:22:50.560","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-04T04:42:30.640","2017-04-04T18:42:30.640","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-04T03:59:31.520",{"$f":"IF(ISBLANK(A66),\" \",((A66)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-04T17:59:31.520"},"CW","ship",null,null,"Additional shift 500m to starboard"]
["2017-04-04T05:41:46.880","2017-04-04T19:41:46.880","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-04T05:41:48.610","2017-04-04T19:41:48.610","CW","XBT",null,null,"AXBT 002; applied to line 0014"]
["2017-04-04T05:58:28.600","2017-04-04T19:58:28.600","CW","Sonar","Multibeam","new line","Turn Line 0014"]
["2017-04-04T06:00:10.920","2017-04-04T20:00:10.920","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-04T06:17:55.560",{"$f":"IF(ISBLANK(A71),\" \",((A71)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-04T20:17:55.560"},"CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-04T06:31:51.940","2017-04-04T20:31:51.940","CW","Sonar","Multibeam","new line","New survey line 0016"]
["2017-04-04T06:41:43.240","2017-04-04T20:41:43.240","CW","Issue/Problem",null,null,"Ugh, data so bad. "]
["2017-04-04T06:42:31.230","2017-04-04T20:42:31.230","CW","Sonar","Multibeam","Ping Mode","at 4200m, switched to Extra Deep to abate horrible blowouts. "]
["2017-04-04T06:44:45.390","2017-04-04T20:44:45.390","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-04T07:06:58.040","2017-04-04T21:06:58.040","CW","Sonar","Multibeam","Ping Mode","Vewy Deep"]
["2017-04-04T07:08:05.480","2017-04-04T21:08:05.480","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-04T07:28:12.500","2017-04-04T21:28:12.500","CW","Sonar","Multibeam","Along Direction Pitch","-1"]
["2017-04-04T08:04:42.920","2017-04-04T22:04:42.920","DF","Sonar","Multibeam","Along Direction Pitch","-1.5"]
["2017-04-04T08:11:42.620","2017-04-04T22:11:42.620","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-04T08:30:17.480","2017-04-04T22:30:17.480","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-04T09:02:04.940","2017-04-04T23:02:04.940","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-04T09:20:00.940","2017-04-04T23:20:00.940","DF","Sonar","Multibeam","Along Direction Pitch",-2]
["2017-04-04T09:24:42.400","2017-04-04T23:24:42.400","DF","Sonar","Multibeam","Ping Mode","Extra Deep, to reduce drop outs ~3100 m"]
["2017-04-04T09:33:04.240","2017-04-04T23:33:04.240","DF","Sonar","Multibeam","New Line","begin turn line 0019"]
["2017-04-04T09:46:54.220","2017-04-04T23:46:54.220","DF","Sonar","Multibeam","Along Direction Pitch",-2.5]
["2017-04-04T09:51:41.910","2017-04-04T23:51:41.910","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-04T09:56:45.490","2017-04-04T23:56:45.490","DF","Sonar","Multibeam","new line","begin survey line 0020"]
["2017-04-04T09:59:42.660","2017-04-04T23:59:42.660","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-04T10:16:35.350","2017-04-05T00:16:35.350","DF","Sonar","EK",null,"tried using 1545 for EK80 sounds speed"]
["2017-04-04T10:25:28.840","2017-04-05T00:25:28.840","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-04-04T10:25:35.600","2017-04-05T00:25:35.600","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-04T10:57:15.100","2017-04-05T00:57:15.100","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-04T11:11:33.090","2017-04-05T01:11:33.090","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-04T11:40:41.510","2017-04-05T01:40:41.510","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-04-04T11:55:27.020","2017-04-05T01:55:27.020","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-04T12:06:13.950","2017-04-05T02:06:13.950","DF","XBT",null,null,"cast 003 collected and applied to line 0022"]
["2017-04-04T12:07:27.140","2017-04-05T02:07:27.140","DF","XBT",null,null,"cast 003 was unapplied to line 0022 due to large SV difference."]
["2017-04-04T12:13:47.350","2017-04-05T02:13:47.350","DF","Sonar","Multibeam",null,"begin turn line 0023"]
["2017-04-04T12:23:45.170","2017-04-05T02:23:45.170","DF","XBT",null,null,"cast 004 applied to line 0023"]
["2017-04-04T12:24:39.810","2017-04-05T02:24:39.810","DF","Sonar","Multibeam","Aeration Filter (On/Off)","On"]
["2017-04-04T12:38:45.200","2017-04-05T02:38:45.200","DF","Sonar","Multibeam","New Line","begin survey line 0024"]
["2017-04-04T13:03:33.330","2017-04-05T03:03:33.330","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-04T13:03:41.660","2017-04-05T03:03:41.660","DF","Sonar","Multibeam","Max Angles","40/40"]
["2017-04-04T13:12:54.860","2017-04-05T03:12:54.860","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-04-04T13:35:17.480","2017-04-05T03:35:17.480","DF","Sonar","Multibeam","Along Direction Pitch",-2.5]
["2017-04-04T13:53:05.970","2017-04-05T03:53:05.970","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-04-04T14:09:01.340","2017-04-05T04:09:01.340","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-04T14:11:34.630","2017-04-05T04:11:34.630","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-04T14:12:14.360","2017-04-05T04:12:14.360","DF","Sonar","Multibeam","Max Angles","36/36"]
["2017-04-04T14:36:15.390","2017-04-05T04:36:15.390","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-04T14:45:20.640","2017-04-05T04:45:20.640","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-04-04T14:56:58.040","2017-04-05T04:56:58.040","DF","Sonar","Multibeam","Along Direction Pitch",-1.5]
["2017-04-04T15:07:54.050","2017-04-05T05:07:54.050","DF","Sonar",null,null,"Started passive logging of ADCP"]
["2017-04-04T15:20:07.570","2017-04-05T05:20:07.570","DF","Sonar","Multibeam","New Line","begin turn line 0027"]
["2017-04-04T15:42:03.640","2017-04-05T05:42:03.640","DF","Sonar","Multibeam","New Line","begin survey line 0028"]
["2017-04-04T16:20:00.290","2017-04-05T06:20:00.290","DF","Sonar","Knudsen",null,"SBP was not receiving NAV data. Trouble shooting now to re connect NMEA. All previous files do not have NAV"]
["2017-04-04T16:30:44","2017-04-05T06:30:44","AB","Sonar","Knudsen",null,"GPS feed fixed with PC reboot. Started new line #20."]
["2017-04-04T16:43:35.430","2017-04-05T06:43:35.430","AB","Ship",null,null,"shift 500m to starboard"]
["2017-04-04T17:53:40.460","2017-04-05T07:53:40.460","AB","Sonar","Multibeam","new line","0031` turn"]
["2017-04-04T17:58:43.430","2017-04-05T07:58:43.430","AB","Sonar","Multibeam","new line","0032, transit speed 10 kts"]
["2017-04-04T19:29:49.570","2017-04-05T09:29:49.570","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-04T19:31:54.420","2017-04-05T09:31:54.420","AB","Sonar","Multibeam",null,"Range gates tight, lost bottom on stbd side"]
["2017-04-04T19:40:15.280","2017-04-05T09:40:15.280","AB","Sonar","Multibeam",null,"Ping mode very deep, max 55/55"]
["2017-04-04T20:22:15.640","2017-04-05T10:22:15.640","AB","XBT",null,null,"006 added to line 34"]
["2017-04-04T20:32:37.370","2017-04-05T10:32:37.370","AB","Sonar","Multibeam","Max Angles","60/60 Deep mode"]
["2017-04-04T20:37:21.630","2017-04-05T10:37:21.630","AB","Sonar","Knudsen",null,"Power 2, Pulse 2, Gain 34"]
["2017-04-04T20:37:41.510","2017-04-05T10:37:41.510","Ab","Sonar","Multibeam"]
["2017-04-04T20:40:23.170","2017-04-05T10:40:23.170","AB","Sonar","Multibeam","Ping Mode","Deep mode blowing out at 1500m, switching to very deep. 52/52"]
["2017-04-04T20:50:33.280","2017-04-05T10:50:33.280","AB","Sonar","Multibeam","New Line","0035"]
["2017-04-04T20:51:07.800","2017-04-05T10:51:07.800","AB","Sonar","Multibeam","Ping Mode","Deep 75/75"]
["2017-04-04T20:53:26.870","2017-04-05T10:53:26.870","AB","Sonar","Knudsen",null,"Power 1, pulse 2, range 500m"]
["2017-04-04T21:18:31.760","2017-04-05T11:18:31.760","CW","Sonar","Multibeam","Ping Mode","at 450m, set to Auto / Medium"]
["2017-04-04T21:23:41.960","2017-04-05T11:23:41.960","CW","Sonar","Knudsen","Phase Range","500-1000m"]
["2017-04-04T22:08:38.320",{"$f":"IF(ISBLANK(A135),\" \",((A135)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-05T12:08:38.320"},"AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2017-04-04T23:08:20.630","2017-04-05T13:08:20.630","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2017-04-04T23:24:40.520","2017-04-05T13:24:40.520","AB","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-04-04T23:24:53.710","2017-04-05T13:24:53.710","AB","Ship",null,null,"Drills"]
["2017-04-04T23:54:32.300","2017-04-05T13:54:32.300","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2017-04-05T01:23:51.910","2017-04-05T15:23:51.910","CW","Sonar","Knudsen","Phase Range","1000-2000m"]
["2017-04-05T01:27:45.140","2017-04-05T15:27:45.140","CW","Sonar","Multibeam","New Line","Turn Line 0040"]
["2017-04-05T01:38:49.700","2017-04-05T15:38:49.700","CW","Sonar","Multibeam","New Line","Survey Line 0041"]
["2017-04-05T02:40:30.930","2017-04-05T16:40:30.930","CW","Sonar","Knudsen","Range",500]
["2017-04-05T02:40:32.960","2017-04-05T16:40:32.960","CW","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-04-05T04:06:06.510","2017-04-05T18:06:06.510","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2017-04-05T04:44:36.410","2017-04-05T18:44:36.410","CW","Issue/Problem",null,null,"POS Heading accuray went up to 0.045, and GAMS went to Not Ready for a few minutes. S'all good now."]
["2017-04-05T05:03:02.980","2017-04-05T19:03:02.980","CW","Sonar","Knudsen","Range",1000]
["2017-04-05T05:03:04.780","2017-04-05T19:03:04.780","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-05T05:26:11.980","2017-04-05T19:26:11.980","CW","Sonar","Knudsen","Phase Range","500-1500"]
["2017-04-05T05:55:47.110","2017-04-05T19:55:47.110","CW","Sonar","Multibeam","New Line","Turn Line 0046"]
["2017-04-05T06:14:20.150","2017-04-05T20:14:20.150","CW","Issue/Problem","Knudsen",null,"Lost remote connection, then computer froze. Had to restart. "]
["2017-04-05T06:20:45.860","2017-04-05T20:20:45.860","CW","Sonar","Multibeam","New Line","Survey Line 0047"]
["2017-04-05T06:22:48.570","2017-04-05T20:22:48.570","CW","Sonar","Knudsen",null,"Restarted and recording. Pulse 2; Power 2; Gain 36"]
["2017-04-05T06:40:29","2017-04-05T20:40:29","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-05T07:40:45.760","2017-04-05T21:40:45.760","DF","XBT",null,null,"2 XBT casts spiked out at sruface, restarted AOML software. And tried again. 3 attempt spiked out"]
["2017-04-05T07:55:46.990",{"$f":"IF(ISBLANK(A156),\" \",((A156)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-05T21:55:46.990"},"CW","XBT",null,null,"Goin' old school. XBT 007 successful. 0047"]
["2017-04-05T07:42:08.500","2017-04-05T21:42:08.500","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-05T10:48:42.710","2017-04-06T00:48:42.710","DF","Sonar","Multibeam","New Line","begin turn line 0052"]
["2017-04-05T11:08:02.250","2017-04-06T01:08:02.250","DF","Sonar","Multibeam","New Line","begin survey line 0053"]
["2017-04-05T11:10:36.240","2017-04-06T01:10:36.240","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-05T11:13:01.290","2017-04-06T01:13:01.290","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-05T11:14:10.250","2017-04-06T01:14:10.250","DF","Ship",null,null,"requested 500 m move to STBD"]
["2017-04-05T11:40:48.180","2017-04-06T01:40:48.180","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-05T12:18:24.700","2017-04-06T02:18:24.700","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-05T12:25:38.450","2017-04-06T02:25:38.450","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-05T13:25:29.270","2017-04-06T03:25:29.270","DF","Ship",null,null,"Course change to avoid FAD, ~900-1000m to STBD then return to line"]
["2017-04-05T14:01:54.980","2017-04-06T04:01:54.980","DF","Ship",null,null,"Back on trackline"]
["2017-04-05T14:36:51.160","2017-04-06T04:36:51.160","AB","XBT",null,null,"XBT008 added to line 0056"]
["2017-04-05T15:06:52.700","2017-04-06T05:06:52.700","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-04-05T15:51:20.750","2017-04-06T05:51:20.750","DF","Sonar","Multibeam","New Line","turn and at end of survey line"]
["2017-04-05T16:18:13.470","2017-04-06T06:18:13.470","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-05T16:42:40.270","2017-04-06T06:42:40.270","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-05T16:44:17.620","2017-04-06T06:44:17.620","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-05T17:19:28.050","2017-04-06T07:19:28.050","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-05T17:19:42.180","2017-04-06T07:19:42.180","AB","Sonar","Multibeam","Ping Mode","Deep Max Angles 75/75"]
["2017-04-05T17:25:14.400","2017-04-06T07:25:14.400","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-05T17:31:34.110","2017-04-06T07:31:34.110","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-04-05T18:08:24.150","2017-04-06T08:08:24.150","DF","Sonar","Multibeam","New Line","turn at end of transit line 0062"]
["2017-04-05T18:10:20.850","2017-04-06T08:10:20.850","DF","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-05T18:24:33.840","2017-04-06T08:24:33.840","AB","Sonar","Knudsen","Phase Range","500-1000m"]
["2017-04-05T18:27:06.580","2017-04-06T08:27:06.580","AB","Sonar","Knudsen",null,"Power 1 Pulse 2"]
["2017-04-05T19:13:12.530","2017-04-06T09:13:12.530","AB","Sonar","Multibeam","New Line","0064, shallow turn; ping mode auto: medium"]
["2017-04-05T19:20:14.020","2017-04-06T09:20:14.020","AB","Sonar","Knudsen",null,"New line, 500m range, phase at 350-850. Shallow shelf. Gain 30."]
["2017-04-05T19:24:50.810","2017-04-06T09:24:50.810","AB","Sonar","Knudsen",null,"Multiple return  at ~675m depth."]
["2017-04-05T19:26:37.760","2017-04-06T09:26:37.760","AB","Sonar","Multibeam","New Line","0065, shallow turn"]
["2017-04-05T19:34:46.680","2017-04-06T09:34:46.680","AB","Sonar","Knudsen",null,"New line, 1000m range, power 2 pulse 2, now off the shelf."]
["2017-04-05T19:44:24.970","2017-04-06T09:44:24.970","AB","Sonar","Multibeam","New Line","0066"]
["2017-04-05T20:06:55.530","2017-04-06T10:06:55.530","AB","Sonar","Multibeam","New Line","0067 end of near shore line. Manuevering around traffic to come onto next line."]
["2017-04-05T20:09:13.200","2017-04-06T10:09:13.200","AB","Sonar","Knudsen",null,"New line"]
["2017-04-05T20:10:58.120","2017-04-06T10:10:58.120","AB","Sonar","Knudsen","Phase Range","1000-2000m"]
["2017-04-05T20:11:48.810","2017-04-06T10:11:48.810","AB","Sonar","Multibeam","Ping Mode","Deep Mode  "]
["2017-04-05T20:12:25.460","2017-04-06T10:12:25.460","AB","Sonar","Knudsen","Tx Pulse","4ms, gain 33 db"]
["2017-04-05T20:15:34.160","2017-04-06T10:15:34.160","AB","Sonar","Multibeam","New Line","0068"]
["2017-04-05T20:26:42.790","2017-04-06T10:26:42.790","AB","Sonar","Knudsen","Phase Range","500-1500m"]
["2017-04-05T20:52:34.610","2017-04-06T10:52:34.610","AB","XBT",null,null,"09 cut early, 10 bad probe, 11 good cast"]
["2017-04-05T21:17:47.480","2017-04-06T11:17:47.480","AB","XBT",null,null,"cast 11 has bad sound velocity values when added to SIS, 5 m/s off. Redoing cast."]
["2017-04-05T21:38:48.200","2017-04-06T11:38:48.200","AB","XBT",null,null,"Cast 12 is bad - wrong values on salinity in program."]
["2017-04-05T21:38:55.020","2017-04-06T11:38:55.020","AB","Sonar","Multibeam",null,"Immediate squall causing bad data quality, waiting until it passes to do another cast"]
["2017-04-05T22:13:23.120","2017-04-06T12:13:23.120","AB","Sonar","Multibeam","New Line","0069"]
["2017-04-05T22:14:02.610",{"$f":"IF(ISBLANK(A200),\" \",((A200)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-06T12:14:02.610"},"AB","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-04-05T22:25:08.960","2017-04-06T12:25:08.960","AB","XBT",null,null,"XBT 13 added to Line 0072"]
["2017-04-05T22:26:27.960","2017-04-06T12:26:27.960","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-05T22:37:04.610","2017-04-06T12:37:04.610","AB","Sonar","Multibeam","New Line","0073 turn"]
["2017-04-05T22:40:34.090","2017-04-06T12:40:34.090","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-05T22:41:18.170","2017-04-06T12:41:18.170","AB","Sonar","Multibeam","New Line","0074"]
["2017-04-05T23:04:12.630","2017-04-06T13:04:12.630","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-05T23:11:40.970","2017-04-06T13:11:40.970","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-05T23:20:30.760","2017-04-06T13:20:30.760","AB","Sonar","Knudsen","Phase Range","2000-3000m, power 3"]
["2017-04-05T23:46:15.520","2017-04-06T13:46:15.520","AB","Sonar","Multibeam","New Line","0076, turn"]
["2017-04-06T00:02:53.820","2017-04-06T14:02:53.820","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-06T00:03:30.610","2017-04-06T14:03:30.610","CW","Sonar","Multibeam","New Line","Survey Line 0077"]
["2017-04-06T00:18:26.930","2017-04-06T14:18:26.930","AB","Sonar","Multibeam","New Line","0078"]
["2017-04-06T00:28:56.090","2017-04-06T14:28:56.090","CW","Sonar","Multibeam",null,"Stopped logging for CTD test cast"]
["2017-04-06T00:35:53","2017-04-06T14:35:53","AB","CTD",null,null,"Test cast at surface for manual firing of water bottles."]
["2017-04-06T01:04:03.040","2017-04-06T15:04:03.040","AB","CTD",null,null,"Test cast complete. Manual firing successful. Water bottle holding test complete. Heading back to survey lines."]
["2017-04-06T01:05:47.070","2017-04-06T15:05:47.070","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-06T01:11:47.400","2017-04-06T15:11:47.400","AB","All",null,null,"Logging all sonars."]
["2017-04-06T02:51:59.660","2017-04-06T16:51:59.660","AB","Sonar","Multibeam","New Line","0081, turn"]
["2017-04-06T02:55:37.850","2017-04-06T16:55:37.850","AB","Sonar","Multibeam","New Line","0082"]
["2017-04-06T03:12:45.380","2017-04-06T17:12:45.380","AB","Sonar","Multibeam","New Line","0083  (>270 turn)"]
["2017-04-06T03:21:16.540","2017-04-06T17:21:16.540","AB","Sonar","All",null,"new lines started (MB line 0084)"]
["2017-04-06T03:21:39.930","2017-04-06T17:21:39.930","Ab","Sonar","Knudsen","Tx power",2]
["2017-04-06T03:36:57.460","2017-04-06T17:36:57.460","AB","Ship",null,null,"Shift 1000m to port"]
["2017-04-06T04:52:47.200","2017-04-06T18:52:47.200","CW","XBT",null,null,"XBT auto launcher had yet another failed cast, with spikes at the first 70m. Troubleshooting found that the control box on the fantail had accumulated water trapped inside. Fully dried it out and sprayed contact cleaner inside. Next launch was successful. YAY!!"]
["2017-04-06T04:54:48.720","2017-04-06T18:54:48.720","CW","XBT",null,null,"AXBT 014; applied to line 0085"]
["2017-04-06T05:04:12.640","2017-04-06T19:04:12.640","CW","Sonar","Multibeam","New Line","Turn line 0086"]
["2017-04-06T05:08:57.040","2017-04-06T19:08:57.040","CW","Sonar","Multibeam","New Line","Survey Line 0087"]
["2017-04-06T09:47:09.070","2017-04-06T23:47:09.070","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-06T09:47:42.710","2017-04-06T23:47:42.710","DF","Sonar","Multibeam","New Line","begin survey line 0092"]
["2017-04-06T09:58:29.120","2017-04-06T23:58:29.120","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-06T10:04:06.230","2017-04-07T00:04:06.230","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-06T10:37:40.840","2017-04-07T00:37:40.840","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-06T11:13:09.620","2017-04-07T01:13:09.620","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-04-06T11:20:28.040","2017-04-07T01:20:28.040","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-06T11:28:58.860","2017-04-07T01:28:58.860","DF","Sonar","Knudsen",null,"1500-2500, power 2"]
["2017-04-06T11:31:20.920","2017-04-07T01:31:20.920","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-06T11:37:03.930","2017-04-07T01:37:03.930","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-06T11:45:18.340","2017-04-07T01:45:18.340","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-06T11:46:53.620","2017-04-07T01:46:53.620","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-06T11:59:47.990","2017-04-07T01:59:47.990","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-06T11:59:58.830","2017-04-07T01:59:58.830","DF","XBT",null,null,"Cast 015 applied to line 0094"]
["2017-04-06T12:16:54.870","2017-04-07T02:16:54.870","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-06T12:27:55.060","2017-04-07T02:27:55.060","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-06T12:29:55.810","2017-04-07T02:29:55.810","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-06T12:38:56.140","2017-04-07T02:38:56.140","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-06T12:53:28.610","2017-04-07T02:53:28.610","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-06T16:24:28.480","2017-04-07T06:24:28.480","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-06T16:59:25.260","2017-04-07T06:59:25.260","DF","Sonar","Multibeam","New Line","begin turn line 0100"]
["2017-04-06T17:09:11.870","2017-04-07T07:09:11.870","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-06T17:20:37.590","2017-04-07T07:20:37.590","AB","Sonar","Multibeam","New Line","0101"]
["2017-04-06T18:03:36.700","2017-04-07T08:03:36.700","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-04-06T18:18:58.730","2017-04-07T08:18:58.730","DF","XBT",null,null,"cast 016 applied to line 0101"]
["2017-04-06T18:35:02.540","2017-04-07T08:35:02.540","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-06T21:39:26.550","2017-04-07T11:39:26.550","AB","Sonar","Multibeam","Max Angles","42/52, Auto: Very Deep Mode"]
["2017-04-06T22:06:50.510","2017-04-07T12:06:50.510","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-06T22:39:00.240","2017-04-07T12:39:00.240","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-06T23:25:41.650","2017-04-07T13:25:41.650","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-07T00:26:28.510","2017-04-07T14:26:28.510","AB","XBT",null,null,"XBT17 added to line 0108"]
["2017-04-07T00:28:10.330","2017-04-07T14:28:10.330","AB","Sonar","Multibeam","New Line","0109, new lines started on sbp and ek60"]
["2017-04-07T02:55:23.250",{"$f":"IF(ISBLANK(A260),\" \",((A260)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-07T16:55:23.250"},"CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-07T04:54:03.130","2017-04-07T18:54:03.130","CW","Sonar","Knudsen","Range",500]
["2017-04-07T04:54:05.340","2017-04-07T18:54:05.340","CW","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-07T07:48:31.990","2017-04-07T21:48:31.990","CW","Sonar","Multibeam","New Line","Turn Line 0117"]
["2017-04-07T07:49:17.440",{"$f":"IF(ISBLANK(A264),\" \",((A264)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-07T21:49:17.440"},"CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-07T08:10:21.940","2017-04-07T22:10:21.940","CW","Sonar","Multibeam","New Line","Survey Line 0118"]
["2017-04-07T08:34:44.020","2017-04-07T22:34:44.020","DF","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-07T08:36:36.240","2017-04-07T22:36:36.240","DF","XBT",null,null,"Cast 018 applied to line 0118"]
["2017-04-07T09:30:56.510","2017-04-07T23:30:56.510","DF","XBT",null,null,"XBT Cast 018 applied to line 0119, previous AXBT cast was slightly bad data "]
["2017-04-07T10:21:53.530","2017-04-08T00:21:53.530","DF","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-07T12:22:49.340","2017-04-08T02:22:49.340","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-04-07T14:36:36.560","2017-04-08T04:36:36.560","DF","Sonar","Knudsen","Phase Range","4000-4500"]
["2017-04-07T14:55:09","2017-04-08T04:55:09","DF","Sonar","Multibeam","New Line","begin turn line 0125"]
["2017-04-07T15:14:57.690","2017-04-08T05:14:57.690","DF","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-07T15:15:28.300","2017-04-08T05:15:28.300","DF","Sonar","Multibeam","New Line","begin survey line 0126"]
["2017-04-07T16:33:05.230","2017-04-08T06:33:05.230","AB","XBT",null,null,"XBT21 applied to line 0127"]
["2017-04-07T17:05:34.240","2017-04-08T07:05:34.240","DF","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-07T18:03:19.220","2017-04-08T08:03:19.220","DF","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-07T18:04:04.180","2017-04-08T08:04:04.180","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-07T18:04:44.160","2017-04-08T08:04:44.160","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-07T18:06:10.980","2017-04-08T08:06:10.980","DF","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-07T18:17:44.170","2017-04-08T08:17:44.170","DF","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-07T19:01:18.710","2017-04-08T09:01:18.710","AB","Ship",null,null,"shift 300m to port, auto: extra deep mode, getting 29/25 swath angles, 4500m coverage."]
["2017-04-07T19:23:13.180","2017-04-08T09:23:13.180","ab","Sonar","Multibeam","Ping Mode","auto: very deep, 40/40, doesn't improved coverage."]
["2017-04-07T19:45:39.750","2017-04-08T09:45:39.750","AB","Sonar","Knudsen","Gain Value",38]
["2017-04-07T19:47:18.910","2017-04-08T09:47:18.910","AB","Sonar","Multibeam",null,"Swath has increased to 42/39, 7000m coverage with no changes in the sonar settings"]
["2017-04-07T19:49:52.820","2017-04-08T09:49:52.820","AB","ship",null,null,"shift 300m to starboard to original line plan"]
["2017-04-07T21:47:19.060","2017-04-08T11:47:19.060","AB","Sonar","Multibeam","Ping Mode","Auto:extra deep; getting 33/32 and 5400m of coverage"]
["2017-04-07T21:57:02.340","2017-04-08T11:57:02.340","AB","Sonar","All",null,"New line (MB 0133)"]
["2017-04-07T21:58:16.470","2017-04-08T11:58:16.470","AB","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-07T22:19:13.300","2017-04-08T12:19:13.300","AB","Sonar","Multibeam","New Line","0134"]
["2017-04-07T23:40:50.470","2017-04-08T13:40:50.470","AB","Sonar","Knudsen","Phase Range","4500-5000m"]
["2017-04-08T00:10:32.060","2017-04-08T14:10:32.060","CW","XBT",null,null,"AXBT 022; applied to line 0135"]
["2017-04-08T00:37:12.070","2017-04-08T14:37:12.070","CW","Sonar","Multibeam","Ping Mode","Manual Very Deep for a little bit to get extra swath for overlap. Finger crossed."]
["2017-04-08T01:00:59.240","2017-04-08T15:00:59.240","CW","XBT",null,null,"AXBT 022 was found to be 3m/s off in SIS, causing yellow warning lights. Ditching that lame cast. "]
["2017-04-08T01:02:43.410","2017-04-08T15:02:43.410","CW","XBT",null,null,"XBT 023"]
["2017-04-08T01:03:40.910","2017-04-08T15:03:40.910","CW","Sonar","Multibeam","New Line","XBT 023 applied to new line 0137"]
["2017-04-08T03:21:47.890","2017-04-08T17:21:47.890","AB","Sonar","Multibeam","Max Angles","52/52"]
["2017-04-08T05:10:19.910","2017-04-08T19:10:19.910","CW","Sonar","Multibeam","New Line","Turn Line 0142"]
["2017-04-08T05:35:19.590","2017-04-08T19:35:19.590","CW","Sonar","Multibeam","New Line","Survey Line 0143"]
["2017-04-08T06:12:23.430","2017-04-08T20:12:23.430","CW","XBT",null,null,"XBT 024; applied to line 0143"]
["2017-04-08T07:30:00.380","2017-04-08T21:30:00.380","CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-08T08:11:27.730","2017-04-08T22:11:27.730","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-08T08:19:32.890","2017-04-08T22:19:32.890","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-04-08T09:22:29.580","2017-04-08T23:22:29.580","DF","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-08T10:47:53.570","2017-04-09T00:47:53.570","DF","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-08T12:08:02.650","2017-04-09T02:08:02.650","DF","Sonar","Multibeam","New Line","begin turn line 0150"]
["2017-04-08T12:36:31.120","2017-04-09T02:36:31.120","DF","Sonar","Multibeam","New Line","begin survey line 0151"]
["2017-04-08T16:43:14.480","2017-04-09T06:43:14.480","AB","Sonar","Multibeam","New Line",156]
["2017-04-08T16:43:37.280","2017-04-09T06:43:37.280","AB","XBT",null,null,"XBT26 applied to line 156"]
["2017-04-08T18:32:57.350","2017-04-09T08:32:57.350","AB","Sonar","Multibeam","New Line","0158 turn"]
["2017-04-08T18:36:59.430","2017-04-09T08:36:59.430","AB","Sonar","Multibeam","New Line","0159"]
["2017-04-08T19:00:58.190","2017-04-09T09:00:58.190","AB","Sonar","Multibeam","New Line","0160 turn"]
["2017-04-08T19:06:25.420","2017-04-09T09:06:25.420","AB","Sonar","Multibeam","New Line","0161"]
["2017-04-08T19:34:11.820","2017-04-09T09:34:11.820","AB","Ship",null,null,"Reducing speed to 5kts. Engineering maintenance."]
["2017-04-08T19:45:12.310","2017-04-09T09:45:12.310","AB","Ship",null,null,"Return to survey speed"]
["2017-04-08T19:45:27.350","2017-04-09T09:45:27.350","AB","Sonar","Knudsen","Phase Range","4750-5250m"]
["2017-04-09T00:13:18.760","2017-04-09T14:13:18.760","AB","Sonar","Multibeam","New Line","0167, turn"]
["2017-04-09T00:22:57.960","2017-04-09T14:22:57.960","AB","POS",null,null,"Lost Marinestar ~1min in Course Acquisition  mode. Height -4.42 in SIS"]
["2017-04-09T00:23:38.220","2017-04-09T14:23:38.220","AB","POS",null,null,"Marinestar in VBS, OK. Height still -4.42 in SIS"]
["2017-04-09T00:28:20.320","2017-04-09T14:28:20.320","AB","XBT",null,null,"XBT27 added to line 0168"]
["2017-04-09T00:33:07.010","2017-04-09T14:33:07.010","AB","Sonar","Multibeam",null,"Height back to normal at +12.51 and varying. "]
["2017-04-09T01:00:03.500","2017-04-09T15:00:03.500","CW","Sonar","Multibeam","New Line","Survey Line 0169"]
["2017-04-09T05:00:45.790","2017-04-09T19:00:45.790","AB","Sonar","Multibeam","New Line","0174 turn"]
["2017-04-09T05:07:10.540","2017-04-09T19:07:10.540","AB","Sonar","Multibeam","New Line","0175"]
["2017-04-09T05:46:33.460",{"$f":"IF(ISBLANK(A325),\" \",((A325)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-09T19:46:33.460"},"CW","Sonar","Multibeam","New Line","Turn at beginning of line 0176 "]
["2017-04-09T05:47:08.150","2017-04-09T19:47:08.150","CW","XBT",null,null,"XBT 028; applied to line 0176"]
["2017-04-09T08:20:58.140","2017-04-09T22:20:58.140","DF","Sonar","Multibeam","New Line","Begin turn line 0179"]
["2017-04-09T08:28:56.070","2017-04-09T22:28:56.070","DF","Sonar","Multibeam","New Line","begin survey line 0180"]
["2017-04-09T09:38:54.190",{"$f":"IF(ISBLANK(A329),\" \",((A329)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-09T23:38:54.190"},"DF","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-09T10:26:31.550","2017-04-10T00:26:31.550","DF","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-09T11:10:29.510","2017-04-10T01:10:29.510","DF","Sonar","Knudsen","Phase Range","4000-4500"]
["2017-04-09T11:42:47.980","2017-04-10T01:42:47.980","DF","XBT",null,null,"Cast 029 applied to line 0183"]
["2017-04-09T12:08:18.930","2017-04-10T02:08:18.930","DF","Sonar","Knudsen","Phase Range","3500-4000"]
["2017-04-09T12:08:44.500","2017-04-10T02:08:44.500","DF","Sonar","Multibeam","Max Angles","60/60"]
["2017-04-09T12:32:11.310","2017-04-10T02:32:11.310","DF","Sonar","Knudsen","Phase Range","3250-3750"]
["2017-04-09T12:32:41.910","2017-04-10T02:32:41.910","DF","Sonar","Multibeam","New Line","begin turn line 0185"]
["2017-04-09T12:42:12.920","2017-04-10T02:42:12.920","DF","Sonar","Multibeam","New Line","begin survey line 0186"]
["2017-04-09T13:00:35.740","2017-04-10T03:00:35.740","DF","Sonar","Knudsen","Phase Range","3500-4000"]
["2017-04-09T14:01:33.570","2017-04-10T04:01:33.570","DF","Sonar","Multibeam","New Line","begin turn line 0188"]
["2017-04-09T14:27:24.340","2017-04-10T04:27:24.340","DF","Sonar","Knudsen","Phase Range","3250-3750"]
["2017-04-09T14:49:19.590","2017-04-10T04:49:19.590","DF","Sonar","Knudsen","Phase Range","3000-3500"]
["2017-04-09T15:33:28.100","2017-04-10T05:33:28.100","DF","Sonar","Multibeam","New Line","begin survey line 0191"]
["2017-04-09T15:46:05.860","2017-04-10T05:46:05.860","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-09T15:46:15.260","2017-04-10T05:46:15.260","DF","Sonar","Knudsen","Phase Range","2750-3250"]
["2017-04-09T15:57:05.290","2017-04-10T05:57:05.290","DF","Sonar","Knudsen","Phase Range","2500--3000"]
["2017-04-09T16:12:19.900","2017-04-10T06:12:19.900","DF","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-04-09T16:18:32.620","2017-04-10T06:18:32.620","DF","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-04-09T16:21:52.630","2017-04-10T06:21:52.630","DF","Sonar","Multibeam","New Line","begin turn line 0192"]
["2017-04-09T16:29:37.500","2017-04-10T06:29:37.500","AB","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-04-09T16:36:22.770","2017-04-10T06:36:22.770","AB","XBT",null,null,"XBT30 added to new line 0193"]
["2017-04-09T16:42:12.060","2017-04-10T06:42:12.060","AB","All",null,null,"new line 0194"]
["2017-04-09T16:45:46.660","2017-04-10T06:45:46.660","AB","Sonar","Knudsen","Phase Range","2250-2750m"]
["2017-04-09T16:52:53.390","2017-04-10T06:52:53.390","DF","Sonar","Knudsen","Phase Range","2500-3000m"]
["2017-04-09T17:00:00.820","2017-04-10T07:00:00.820","AB","Sonar","Knudsen","Phase Range","2750-3250m"]
["2017-04-09T17:12:06.240","2017-04-10T07:12:06.240","AB","Sonar","Knudsen","Phase Range","3000-3500m"]
["2017-04-09T17:28:27.770","2017-04-10T07:28:27.770","DF","Sonar","Multibeam","New Line","begin turn line 0195"]
["2017-04-09T17:37:37.320","2017-04-10T07:37:37.320","DF","Sonar","Knudsen","Phase Range","3250-3750"]
["2017-04-09T17:47:16.750","2017-04-10T07:47:16.750","DF","Sonar","Multibeam","New Line","new line"]
["2017-04-09T17:59:09.120","2017-04-10T07:59:09.120","DF","Sonar","Knudsen","Phase Range","3000-3500"]
["2017-04-09T18:13:32.460","2017-04-10T08:13:32.460","DF","Sonar","Knudsen","Phase Range","2750-3250"]
["2017-04-09T18:27:44.400","2017-04-10T08:27:44.400","DF","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-04-09T18:36:58.280","2017-04-10T08:36:58.280","AB","Sonar","Multibeam","New Line","0197 turn"]
["2017-04-09T18:56:17.740","2017-04-10T08:56:17.740","AB","Sonar","Multibeam","New Line","0198 turn"]
["2017-04-09T18:58:57.950","2017-04-10T08:58:57.950","AB","Sonar","Multibeam","New Line","0199, new lines on ek and sbp"]
["2017-04-09T19:44:41.860","2017-04-10T09:44:41.860","AB","Sonar","Multibeam","New Line","0200, turn"]
["2017-04-09T19:47:32.800","2017-04-10T09:47:32.800","AB","Sonar","Multibeam","New Line","0201"]
["2017-04-09T21:10:26.910","2017-04-10T11:10:26.910","AB","Sonar","Multibeam","New Line","0203, turn"]
["2017-04-09T21:16:57.870","2017-04-10T11:16:57.870","AB","Sonar","Multibeam","New Line","0204"]
["2017-04-09T21:28:48.450","2017-04-10T11:28:48.450","CW","Sonar","Knudsen","Phase Range","2750-3250m"]
["2017-04-09T21:34:38.540","2017-04-10T11:34:38.540","CW","Sonar","Multibeam","Ping Mode","Shoaling past 3000m. Auto Ping Mode chose Deep, but of course cruddy returns came right away. Manually set back to Very Deep."]
["2017-04-09T21:45:56.580","2017-04-10T11:45:56.580","CW","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-04-09T21:58:08.350","2017-04-10T11:58:08.350","AB","Sonar","Multibeam","Ping Mode"," Deep 60/60"]
["2017-04-09T21:58:35.590","2017-04-10T11:58:35.590","AB","Sonar","Knudsen",null,"New line, phase range 1750-2250m"]
["2017-04-09T22:00:29.770","2017-04-10T12:00:29.770","AB","Sonar","Multibeam","Max Angles","75/60"]
["2017-04-09T22:26:03.990","2017-04-10T12:26:03.990","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2017-04-09T22:40:54.190","2017-04-10T12:40:54.190","AB","Sonar","Multibeam","New Line","0206"]
["2017-04-09T22:44:11.880","2017-04-10T12:44:11.880","AB","XBT",null,null,"XBT31 added to new line 0207"]
["2017-04-09T22:47:17.280","2017-04-10T12:47:17.280","AB","Sonar","Multibeam","Max Angles","65/65"]
["2017-04-09T22:48:06.970","2017-04-10T12:48:06.970","AB","Sonar","Knudsen","Phase Range","2500-3000m"]
["2017-04-09T22:56:12.840","2017-04-10T12:56:12.840","AB","Sonar","Multibeam","New Line","0208"]
["2017-04-09T23:04:23.280","2017-04-10T13:04:23.280","AB","Sonar","Knudsen","Phase Range","2250-2750m"]
["2017-04-09T23:07:20.800","2017-04-10T13:07:20.800","AB","POS",null,null,"Position accuracy dropped to ~1.0m lat, 0.9m long, 0.2m altitude."]
["2017-04-09T23:20:21.920","2017-04-10T13:20:21.920","AB","Sonar","Knudsen","Phase Range","2000-2500m"]
["2017-04-09T23:20:41.700","2017-04-10T13:20:41.700","AB","POS",null,null,"Pos accuracy still declined, but indicates GNSS mode"]
["2017-04-09T23:28:05.690","2017-04-10T13:28:05.690","AB","Sonar","Knudsen","Phase Range","1750-2250m"]
["2017-04-09T23:30:58","2017-04-10T13:30:58","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2017-04-09T23:34:00.490","2017-04-10T13:34:00.490","AB","Sonar","Knudsen","Phase Range","1250-1750m"]
["2017-04-09T23:35:57.280","2017-04-10T13:35:57.280","AB","Sonar","Multibeam","Max Angles","65/75"]
["2017-04-09T23:37:22.300","2017-04-10T13:37:22.300","AB","Sonar","Multibeam","New Line","0209, all sonars new line"]
["2017-04-09T23:43:09.830","2017-04-10T13:43:09.830","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2017-04-09T23:58:17.230","2017-04-10T13:58:17.230","AB","Sonar","Multibeam","New Line","0210 turn"]
["2017-04-10T00:01:02.470","2017-04-10T14:01:02.470","AB","Sonar","Multibeam","New Line","0211"]
["2017-04-10T00:15:24.260",{"$f":"IF(ISBLANK(A393),\" \",((A393)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-10T14:15:24.260"},"AB","Sonar","Multibeam",null,"secured for CTD cast, ADCP pinging, SBP Secured. EK60 on internal pinging"]
["2017-04-10T00:53:28","2017-04-10T14:53:28","AB","CTD",null,null,"CTD Test Cast at Malumalu"]
["2017-04-10T00:55:05.360","2017-04-10T14:55:05.360","AB","CTD",null,null,"In the water, on, to the surface and descending"]
["2017-04-10T00:55:23.800","2017-04-10T14:55:23.800","AB","CTD",null,null,"descending 30m/min"]
["2017-04-10T00:55:49.600","2017-04-10T14:55:49.600","AB","CTD",null,null,"descending 60m/min"]
["2017-04-10T00:56:34.410","2017-04-10T14:56:34.410","AB","CTD",null,null,"150m wire out 60m/min descending"]
["2017-04-10T00:57:28.310","2017-04-10T14:57:28.310","AB","CTD",null,null,"200m wire out 60m/min descending"]
["2017-04-10T00:58:18.120","2017-04-10T14:58:18.120","AB","CTD",null,null,"250m wire out 60m/min descending"]
["2017-04-10T01:02:54.030","2017-04-10T15:02:54.030","AB","CTD",null,null,"500m wire out 60m/min descending"]
["2017-04-10T01:04:31.070","2017-04-10T15:04:31.070","AB","CTD",null,null,"600m wire out 60m/min descending"]
["2017-04-10T01:07:45.740","2017-04-10T15:07:45.740","AB","CTD",null,null,"800m wire out 60m/min descending"]
["2017-04-10T01:11:34.850","2017-04-10T15:11:34.850","AB","CTD",null,null,"1000m descending 60m/min"]
["2017-04-10T01:12:47.110","2017-04-10T15:12:47.110","AB","CTD",null,null,"Altimeter working"]
["2017-04-10T01:13:00.440","2017-04-10T15:13:00.440","AB","CTD",null,null,"1100m descending 30m/min"]
["2017-04-10T01:14:46.550","2017-04-10T15:14:46.550","AB","CTD",null,null,"1150m, slowing to 15m/min"]
["2017-04-10T01:18:28.140","2017-04-10T15:18:28.140","AB","CTD",null,null,"All stop 1212m (Deck) Bottom depth on CTD 1207m, EK depth 1233m on 18khz. Altimeter 40m"]
[null," ",null,null,null,null,"Hypack is logging navigation. Target made for each depth of water sample. No nav on CTD."]
["2017-04-10T01:25:50.700","2017-04-10T15:25:50.700","AB","CTD",null,null,"Ascending 10m/min, 1100m, bottle 1, no lights for bottle fire on deck unit"]
["2017-04-10T01:31:32.040","2017-04-10T15:31:32.040","AB","CTD",null,null,"950m ascending 30m/min"]
["2017-04-10T01:34:20.880","2017-04-10T15:34:20.880","AB","CTD",null,null,"reduce to 10m/min, 900m bottles 2,3; no lights on CTD deck unit"]
["2017-04-10T01:34:22.950","2017-04-10T15:34:22.950","AB","CTD",null,null,"900m 10m/min"]
["2017-04-10T01:34:50.720","2017-04-10T15:34:50.720","AB","CTD",null,null,"increase to 30m/min"]
["2017-04-10T01:35:58.410","2017-04-10T15:35:58.410","AB","CTD",null,null,"bottle fire 4, 850m; no lights on deck unit"]
["2017-04-10T01:37:38.590","2017-04-10T15:37:38.590","AB","CTD"]
["2017-04-10T01:38:32.310","2017-04-10T15:38:32.310","AB","CTD",null,null,"bottle fire 6 800m"]
[null," ","AB","CTD",null,null,"bottle fire 7, 750m"]
[null," ","AB","CTD",null,null,"700m 10m, 7-8 bottles"]
["2017-04-10T01:48:49.480","2017-04-10T15:48:49.480","AB","CTD",null,null,"650m bottle fire"]
["2017-04-10T01:50:33.760","2017-04-10T15:50:33.760","AB","CTD",null,null,"600m, all stop,  2 bottles"]
["2017-04-10T01:53:53.410","2017-04-10T15:53:53.410","AB","CTD",null,null,"560m, all stop, 1 bottle"]
["2017-04-10T01:57:31.320","2017-04-10T15:57:31.320","AB","CTD",null,null,"460m, all stop, 2 bottles"]
["2017-04-10T02:00:20.920","2017-04-10T16:00:20.920","AB","CTD",null,null,"380m, all stop , 2 bottles"]
["2017-04-10T02:04:56.670","2017-04-10T16:04:56.670","AB","CTD",null,null,"260m, all stop, 1 bottle"]
["2017-04-10T02:09:18.970","2017-04-10T16:09:18.970","AB","CTD",null,null,"140m, all stop, 2 bottles"]
["2017-04-10T02:12:00.640","2017-04-10T16:12:00.640","AB","CTD",null,null,"80m, all stop, 2 bottles"]
["2017-04-10T02:14:00.040","2017-04-10T16:14:00.040","AB","CTD",null,null,"40m, all stop, 2 bottles"]
["2017-04-10T02:17:34.880","2017-04-10T16:17:34.880","AB","CTD",null,null,"CTD at surface, no bottles fired positive."]
["2017-04-10T02:53:06.660","2017-04-10T16:53:06.660","AB","CTD",null,null,"Testing firing mechanism on deck."]
["2017-04-10T03:11:16.780","2017-04-10T17:11:16.780","AB","CTD",null,null,"Test firing on deck unsucessful. Resuming mapping."]
["2017-04-10T03:12:19.110","2017-04-10T17:12:19.110","AB","CTD",null,null,"ADCP active pinging secured. In passive recording mode"]
["2017-04-10T03:14:53.870","2017-04-10T17:14:53.870","AB","Sonar",null,null,"All sonars pinging."]
["2017-04-10T03:21:21.810","2017-04-10T17:21:21.810","AB","Sonar","Multibeam","New Line","0212. Auto Deep. 75/75. Slope filter."]
["2017-04-10T03:26:25.080","2017-04-10T17:26:25.080","AB","Sonar","Knudsen",null,"Recording new line. Range 1000m, Phase Range 1000-2000m, Pulse 2, Power 2, Gain 36"]
["2017-04-10T03:31:38.390","2017-04-10T17:31:38.390","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-10T03:38:07.490","2017-04-10T17:38:07.490","CW","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-10T04:06:29.280","2017-04-10T18:06:29.280","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-10T04:07:10.010","2017-04-10T18:07:10.010","AB","Sonar","Multibeam",null,"Auto:Very Deep"]
["2017-04-10T04:07:42.730","2017-04-10T18:07:42.730","AB","Sonar","EK",null,"Range 5000, Bottom Detection 6000. "]
["2017-04-10T04:09:40.960","2017-04-10T18:09:40.960","AB","Sonar","Knudsen","Tx Pulse",4]
["2017-04-10T04:18:36.050","2017-04-10T18:18:36.050","AB","Sonar","Multibeam","New Line","0213 turn, POS position accuracy at 0.8m."]
["2017-04-10T04:21:26.310","2017-04-10T18:21:26.310","AB","Sonar","Multibeam","New Line","0214"]
["2017-04-10T05:01:18.540","2017-04-10T19:01:18.540","CW","XBT",null,null,"XBT 032 (thermal anomaly near 600 m; applied to line 0214)"]
["2017-04-10T05:21:35.410","2017-04-10T19:21:35.410","AB","Sonar","Knudsen","Tx power",3]
["2017-04-10T06:59:46.270","2017-04-10T20:59:46.270","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-10T08:02:53.030","2017-04-10T22:02:53.030","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-10T09:24:52.460","2017-04-10T23:24:52.460","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-10T09:53:05.430","2017-04-10T23:53:05.430","DF","Sonar","Multibeam","New Line","begin turn line 0220"]
["2017-04-10T09:55:55.200","2017-04-10T23:55:55.200","DF","Sonar","Multibeam","New Line","begin survey 0221"]
["2017-04-10T10:58:31.010","2017-04-11T00:58:31.010","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-10T11:14:30.930","2017-04-11T01:14:30.930","DF","Sonar","Multibeam","New Line","begin turn line 0223"]
["2017-04-10T11:22:20.140","2017-04-11T01:22:20.140","DF","Sonar","Multibeam","New Line","begin survey line 0224"]
["2017-04-10T11:39:58.310","2017-04-11T01:39:58.310","CW","XBT",null,null,"XBT 033; applied to line 0225"]
["2017-04-10T11:49:46.430","2017-04-11T01:49:46.430","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-10T11:58:37.930","2017-04-11T01:58:37.930","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-10T13:23:50.290","2017-04-11T03:23:50.290","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-10T13:25:18.630",{"$f":"IF(ISBLANK(A458),\" \",((A458)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-11T03:25:18.630"},"DF","Sonar","Multibeam","New Line","begin turn line 0228"]
["2017-04-10T13:46:31.100","2017-04-11T03:46:31.100","DF","Sonar","Multibeam","New Line","begin survey line 0229"]
["2017-04-10T13:52:24.110","2017-04-11T03:52:24.110","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-10T15:07:39.770","2017-04-11T05:07:39.770","DF","Sonar","Multibeam","Max Angles","60/60"]
["2017-04-10T15:52:35.290","2017-04-11T05:52:35.290","DF","Sonar","Multibeam","New Line","begin turn line 0232"]
["2017-04-10T16:09:10.340","2017-04-11T06:09:10.340","AB","Sonar","Multibeam","New Line","0233"]
["2017-04-10T16:12:10.450","2017-04-11T06:12:10.450","AB","Sonar","Multibeam","New Line","0233"]
["2017-04-10T16:17:36.770","2017-04-11T06:17:36.770","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-04-10T16:28:54.490","2017-04-11T06:28:54.490","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-10T16:36:59.110","2017-04-11T06:36:59.110","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-10T16:44:05.350","2017-04-11T06:44:05.350","AB","XBT",null,null,"XBT34 applied to line 235"]
["2017-04-10T17:06:35.900","2017-04-11T07:06:35.900","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-10T17:16:51.580","2017-04-11T07:16:51.580","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-10T17:55:59.140","2017-04-11T07:55:59.140","DF","Sonar","Multibeam","New Line","begin turn line 0237"]
["2017-04-10T18:13:47.370","2017-04-11T08:13:47.370","AB","Sonar","Multibeam","New Line","0238 turn"]
["2017-04-10T18:14:46.880","2017-04-11T08:14:46.880","AB","Sonar","Knudsen","Phase Range","3500-4500m, Power 2 Gain 37"]
["2017-04-10T18:16:08.110","2017-04-11T08:16:08.110","AB","Sonar","Multibeam","New Line","0239"]
["2017-04-10T19:25:22.720","2017-04-11T09:25:22.720","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-10T19:33:52.970","2017-04-11T09:33:52.970","AB","Sonar","Multibeam","New Line","0241 turn"]
["2017-04-10T19:38:49.370","2017-04-11T09:38:49.370","AB","Sonar","Multibeam","New Line","0242"]
["2017-04-10T19:41:54.980","2017-04-11T09:41:54.980","AB","Sonar","Multibeam","Max Angles","75/75"]
["2017-04-10T20:05:02.630","2017-04-11T10:05:02.630","AB","Sonar","Multibeam","New Line",243]
["2017-04-10T20:46:59","2017-04-11T10:46:59","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-10T21:03:35.410","2017-04-11T11:03:35.410","AB","Sonar","Multibeam","New Line","0244"]
["2017-04-10T21:06:25.740","2017-04-11T11:06:25.740","AB","Sonar","Multibeam","New Line","0245"]
["2017-04-10T21:27:23.080","2017-04-11T11:27:23.080","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-10T21:34:17.570","2017-04-11T11:34:17.570","AB","Sonar","Multibeam","New Line","0246 turn"]
["2017-04-10T21:38:08.180","2017-04-11T11:38:08.180","AB","Sonar","Multibeam","New Line","0247"]
["2017-04-10T22:14:51.160","2017-04-11T12:14:51.160","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-10T22:54:27.990","2017-04-11T12:54:27.990","AB","Sonar","Multibeam","New Line","0249 turn"]
["2017-04-10T23:04:44.840","2017-04-11T13:04:44.840","AB","Sonar","Multibeam","New Line","0250"]
["2017-04-10T23:07:15.370","2017-04-11T13:07:15.370","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-10T23:21:25.030","2017-04-11T13:21:25.030","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-10T23:41:59.090","2017-04-11T13:41:59.090","CW","XBT",null,null,"XBT 035; applied to line 0250"]
["2017-04-11T01:05:30.300","2017-04-11T15:05:30.300","CW","Ship",null,null,"TSG turned off per Engineering Dept. In SIS, Absorption Coefficient Salinity recorded at 34.86, and in Sound Speed set to Manual from Sensor, at 1545.61. TSG expected to be off for approx. 30 min."]
["2017-04-11T01:09:12.760","2017-04-11T15:09:12.760","CW","Sonar","Multibeam","New Line","New Line 0253 to accommodate secured TSG. "]
["2017-04-11T01:11:30.820","2017-04-11T15:11:30.820","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-11T01:47:17.880","2017-04-11T15:47:17.880","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-11T02:27:13.570","2017-04-11T16:27:13.570","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-11T02:36:12.620","2017-04-11T16:36:12.620","CW","Sonar","Knudsen","Phase Range","500-1500"]
["2017-04-11T02:44:18.310","2017-04-11T16:44:18.310","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-11T02:51:02.560","2017-04-11T16:51:02.560","CW","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-11T03:00:20.160","2017-04-11T17:00:20.160","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-11T04:14:04.950","2017-04-11T18:14:04.950","CW","Sonar","Multibeam","New Line","Turn Line 0257"]
["2017-04-11T04:17:00.680","2017-04-11T18:17:00.680","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-11T04:29:52.940","2017-04-11T18:29:52.940","CW","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-11T04:31:42.800","2017-04-11T18:31:42.800","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-11T04:36:25.630","2017-04-11T18:36:25.630","CW","Sonar","Multibeam","New Line","Survey Line 0258; new lines for EK & SBP"]
["2017-04-11T04:49:27.590","2017-04-11T18:49:27.590","CW","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-11T07:08:38.760","2017-04-11T21:08:38.760","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-11T08:12:16.100","2017-04-11T22:12:16.100","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-11T08:35:40.400","2017-04-11T22:35:40.400","DF","XBT",null,null,"cast 036 collected and applied to line 0262"]
["2017-04-11T08:41:15.480","2017-04-11T22:41:15.480","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-11T09:33:25.110","2017-04-11T23:33:25.110","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-11T10:44:27.710","2017-04-12T00:44:27.710","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-11T11:12:10.830","2017-04-12T01:12:10.830","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-11T11:30:36.370","2017-04-12T01:30:36.370","DF","Sonar",null,"New Line","New line for all sonars; begin turn line 0265"]
["2017-04-11T11:53:17.350","2017-04-12T01:53:17.350","DF","Sonar",null,"New Line","New line for all sonars; begin survey line 0266"]
["2017-04-11T12:42:54.600","2017-04-12T02:42:54.600","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-11T12:44:52.860","2017-04-12T02:44:52.860","DF","Sonar","Multibeam","Ping Mode","forced into Very Deep; AUTO was laggin' to switch"]
["2017-04-11T14:17:14.180","2017-04-12T04:17:14.180","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-04-11T14:56:35.120","2017-04-12T04:56:35.120","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-11T15:54:55.780","2017-04-12T05:54:55.780","DF","Sonar","Multibeam","Ping Mode","Auto"]
["2017-04-11T15:55:37.310","2017-04-12T05:55:37.310","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-11T16:01:42.010",{"$f":"IF(ISBLANK(A522),\" \",((A522)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-12T06:01:42.010"},"DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-04-11T17:00:19.290","2017-04-12T07:00:19.290","AB","XBT",null,null,"XBT38 added to line 0272"]
["2017-04-11T17:32:37.670","2017-04-12T07:32:37.670","DF","Sonar","Multibeam",null,"lost geographical display gridding in mid line 0272, data was still recording just display was out"]
["2017-04-11T18:12:39.450","2017-04-12T08:12:39.450","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-11T18:43:55.720","2017-04-12T08:43:55.720","AB","Sonar","Multibeam","New Line","0274 turn"]
["2017-04-11T18:47:55.810","2017-04-12T08:47:55.810","AB","Sonar","Multibeam","New Line","0275"]
["2017-04-11T19:06:02.590","2017-04-12T09:06:02.590","AB","Sonar","Multibeam","New Line","276 turn"]
["2017-04-11T19:10:50.080","2017-04-12T09:10:50.080","AB","Sonar","Multibeam","New Line","0277"]
["2017-04-11T23:11:17.520","2017-04-12T13:11:17.520",null,null,null,null,"drill"]
["2017-04-12T00:14:43.280","2017-04-12T14:14:43.280","AB","XBT",null,null,"XBT39 added to line 0283"]
["2017-04-12T00:45:04.800","2017-04-12T14:45:04.800","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-12T00:58:46.200","2017-04-12T14:58:46.200","AB","POS",null,null,"Gams not happy with long lines, going into \"Not ready.\""]
["2017-04-12T01:57:08.260","2017-04-12T15:57:08.260","CW","Sonar","Multibeam","New Line","Turn Line 0285"]
["2017-04-12T03:04:33.960","2017-04-12T17:04:33.960","CW","Sonar","Multibeam","New Line","Survey Line 0286; new EK & SBP lines"]
["2017-04-12T05:07:34.420","2017-04-12T19:07:34.420","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-12T06:18:44.530","2017-04-12T20:18:44.530","CW","Sonar","Knudsen",null,"SBP computer froze and lost remote connectionto EK screen. Tried trublshooting, but had to hard restart SBP computer. "]
["2017-04-12T06:26:11.330","2017-04-12T20:26:11.330","CW","Sonar","Knudsen","Start Pinging","All good now. Recording. "]
["2017-04-12T06:33:51.320","2017-04-12T20:33:51.320","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-12T09:19:52.020","2017-04-12T23:19:52.020","DF","XBT",null,null,"Cast 040 applied to line 0293"]
["2017-04-12T09:34:48.740","2017-04-12T23:34:48.740","DF","Sonar","Multibeam","New Line","Turn line 0294; new EK & SBP lines"]
["2017-04-12T09:59:45.850","2017-04-12T23:59:45.850","DF","Sonar","Multibeam","New Line","Survey Line 0295; new EK & SBP lines"]
["2017-04-12T13:02:09.010","2017-04-13T03:02:09.010","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-12T14:26:09.740","2017-04-13T04:26:09.740","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-12T14:37:15.740","2017-04-13T04:37:15.740","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-12T14:45:26.820","2017-04-13T04:45:26.820","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-12T15:20:01.550","2017-04-13T05:20:01.550","DF","Sonar","Multibeam","New Line","Turn Line 0301; new EK & SBP lines"]
["2017-04-12T15:41:07.150","2017-04-13T05:41:07.150","DF","Sonar","Multibeam","New Line","Survey line 0302; new EK & SBP lines"]
["2017-04-12T16:35:57.410","2017-04-13T06:35:57.410","DF","Issues",null,null,"high amount of interference across all sonars; possibly being caused my engineering work on sewage tanks."]
["2017-04-12T16:46:24.890","2017-04-13T06:46:24.890","AB","XBT",null,null,"XBT41 applied to line 0304"]
["2017-04-12T16:48:08.860","2017-04-13T06:48:08.860","AB","Sonar","Multibeam",null,"Interference filter on"]
["2017-04-12T16:58:37.730","2017-04-13T06:58:37.730","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-12T18:10:59.960","2017-04-13T08:10:59.960","DF","Ship",null,null,"Needle gunning has started"]
["2017-04-12T18:18:23.040","2017-04-13T08:18:23.040","DF","Ship",null,null,"requested 500 m to PORT for coverage"]
["2017-04-12T18:40:08.660","2017-04-13T08:40:08.660","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-12T19:23:24.320","2017-04-13T09:23:24.320","AB","Ship",null,null,"Shifting 500m to starboard"]
["2017-04-12T21:11:57.770","2017-04-13T11:11:57.770","AB","Sonar","Multibeam","New Line"," 0310 turn"]
["2017-04-12T21:16:57.700","2017-04-13T11:16:57.700","AB","Sonar","Multibeam","New Line","0311"]
["2017-04-13T00:30:00",{"$f":"IF(ISBLANK(A559),\" \",((A559)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-13T14:30:00"},"CW","Sonar","Knudsen","Tx Power",3]
["2017-04-13T00:31:59.700","2017-04-13T14:31:59.700","CW","XBT",null,null,"XBT 042; applied to line 0314"]
["2017-04-13T00:33:00",{"$f":"IF(ISBLANK(A561),\" \",((A561)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-13T14:33:00"},"CW","Sonar","Multibeam",null,"Trying to address big outer beam noise. Went out of Auto Ping Mode: Extra Deep to Manual Ping Mode: Very Deep for a few seconds, then Manual Extra Deep, and tightended the depth gates. Seems to have worked a bit, but I'm not sure if that is a valid solution. "]
["2017-04-13T00:46:18.670","2017-04-13T14:46:18.670","CW","Ship",null,null,"Shifting 500m to starboard to accommodate narrower than expected swath"]
["2017-04-13T01:06:38.750",{"$f":"IF(ISBLANK(A563),\" \",((A563)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-13T15:06:38.750"},"CW","POS",null,null,"POS position light out for a few minutes"]
["2017-04-13T01:08:09","2017-04-13T15:08:09","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-13T02:12:07.980","2017-04-13T16:12:07.980","CW","Sonar","Multibeam","New Line","Turn Line 0316"]
["2017-04-13T02:34:00.720","2017-04-13T16:34:00.720","CW","Sonar","Multibeam","New Line","Survey Line 0317; new EK & SBP lines"]
["2017-04-13T03:18:34.110","2017-04-13T17:18:34.110","CW","Sonar","Knudsen","Range",500]
["2017-04-13T03:18:36.320","2017-04-13T17:18:36.320","CW","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-13T05:39:32.880","2017-04-13T19:39:32.880","CW","Sonar","Multibeam","Ping Mode","Manual to Very Deep"]
["2017-04-13T06:08:14.820","2017-04-13T20:08:14.820","CW","Sonar","Multibeam","Ping Mode","At 4500m, and Very Deep sucks. Going to Extra Deep. Same coverage anyway."]
["2017-04-13T06:47:56.710","2017-04-13T20:47:56.710","CW","Sonar","Multibeam","Ping Mode","Very Deep again. Seems happier."]
["2017-04-13T07:24:00.790","2017-04-13T21:24:00.790","CW","Sonar","Multibeam","New Line","Turn Line 0322"]
["2017-04-13T07:50:02.320","2017-04-13T21:50:02.320","CW","Sonar","Multibeam","New Line","Survey Line 0323; new EK & SBP lines"]
["2017-04-13T08:33:20.920","2017-04-13T22:33:20.920","DF","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-13T08:45:16.880","2017-04-13T22:45:16.880","DF","XBT",null,null,"3 probes were wasted; each giving us an \"automatic launch\" situation where it wold skip the launch cycle and go directly into and collect data without actually launching probes. The computer lost nav and then coms with the deck unit so the system was restarted and an old gun was used. We were able to obtain a good cast after the restart and old gun were introduced. MK21 software would flah rapidly between \"Launch Probe\" and \"Collecting Data\" applied to line 0323"]
["2017-04-13T09:38:23.870","2017-04-13T23:38:23.870","DF","Sonar","Multibeam","Spike Filter Strength","Strong"]
["2017-04-13T09:40:30.270","2017-04-13T23:40:30.270","DF","Sonar","Multibeam","Spike Filter Strength","Medium"]
["2017-04-13T10:54:21.190","2017-04-14T00:54:21.190","DF","Ship",null,null,"significatn rolls have started and causing major roll artifacts in MB"]
["2017-04-13T11:29:16.410","2017-04-14T01:29:16.410","DF","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-13T12:05:13.950","2017-04-14T02:05:13.950","DF","Sonar","Multibeam","New Line","turn at beginning of line 0328; new EK & SBP lines"]
["2017-04-13T13:15:49.140","2017-04-14T03:15:49.140","DF","Sonar","Multibeam","New Line","turn line 0330; new EK & SBP lines"]
["2017-04-13T13:56:44.700","2017-04-14T03:56:44.700","DF","Sonar","Multibeam","New Line","turn line 0332; new EK & SBP Lines"]
["2017-04-13T14:17:43.160","2017-04-14T04:17:43.160","DF","Sonar","Multibeam","New Line","survey line 0333; new EK & SBP Lines"]
["2017-04-13T15:28:10.980","2017-04-14T05:28:10.980","DF","Sonar","Multibeam","New Line","Turn Line 0335; new EK & SBP Lines"]
["2017-04-13T15:47:16.690","2017-04-14T05:47:16.690","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-13T15:54:50.790","2017-04-14T05:54:50.790","DF","Sonar","Knudsen","Tx Power",3]
["2017-04-13T16:09:39.900","2017-04-14T06:09:39.900","DF","Sonar","Multibeam","New Line","Turn line 0336; new EK & SBP lines"]
["2017-04-13T16:16:49.790",{"$f":"IF(ISBLANK(A588),\" \",((A588)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-14T06:16:49.790"},"DF","Sonar","Multibeam","New Line","Survey line 0337; new EK & SBP Lines"]
["2017-04-13T16:36:26.030","2017-04-14T06:36:26.030","AB","XBT",null,null,"XBT 44 added to line 0338"]
["2017-04-13T19:00:39.560","2017-04-14T09:00:39.560","AB","Sonar","Knudsen","Phase Range","4250-4750m"]
["2017-04-13T19:13:14.180","2017-04-14T09:13:14.180","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-13T19:39:43.150","2017-04-14T09:39:43.150","AB","Sonar","Multibeam","New Line","0342 turn line"]
["2017-04-13T20:12:44.680","2017-04-14T10:12:44.680","AB","Sonar","Multibeam","New Line","0343"]
["2017-04-13T20:40:41.910","2017-04-14T10:40:41.910","AB","Sonar","Multibeam","New Line","0344 turn"]
["2017-04-13T20:37:28.560","2017-04-14T10:37:28.560","AB","Sonar","Multibeam","New Line","0345 returning 3nm west to pick up fill line"]
["2017-04-13T21:14:44.650","2017-04-14T11:14:44.650","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-13T21:20:27.010","2017-04-14T11:20:27.010","CW","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-04-13T21:29:42.030","2017-04-14T11:29:42.030","AB","Sonar","Multibeam","New Line","0346 turn"]
["2017-04-13T21:39:40.820","2017-04-14T11:39:40.820","AB","Sonar","Multibeam","New Line","0347"]
["2017-04-13T21:44:10.610","2017-04-14T11:44:10.610","AB","Sonar","Multibeam","New Line","0348"]
["2017-04-13T22:20:52.320","2017-04-14T12:20:52.320","AB","Sonar","Multibeam","Max Angles","65/65"]
["2017-04-13T22:27:01.250","2017-04-14T12:27:01.250","AB","Sonar","Multibeam","New Line","0350 "]
["2017-04-13T22:32:38.740","2017-04-14T12:32:38.740","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-13T22:46:08.860","2017-04-14T12:46:08.860","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-13T23:08:00.450","2017-04-14T13:08:00.450","AB","Sonar","Knudsen","Tx Pulse","8ms"]
["2017-04-13T23:12:36.250","2017-04-14T13:12:36.250","AB","Sonar","Multibeam","New Line","0351 turn"]
["2017-04-13T23:15:29.710","2017-04-14T13:15:29.710","AB","Sonar","Multibeam","New Line","0352"]
["2017-04-13T23:23:41.970","2017-04-14T13:23:41.970","AB","Sonar","Multibeam","Max Angles","45/48"]
["2017-04-13T23:39:22.960","2017-04-14T13:39:22.960","CW","Sonar","Multibeam","New Line","New Line 0353 (New Heading)"]
["2017-04-13T23:59:01.530","2017-04-14T13:59:01.530","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-04-14T00:24:08.150","2017-04-14T14:24:08.150","CW","XBT",null,null,"XBT 045; applied to line 0353"]
["2017-04-14T00:45:49.820","2017-04-14T14:45:49.820","AB","Sonar","Multibeam","New Line","0355 turn"]
["2017-04-14T00:49:52.490","2017-04-14T14:49:52.490","AB","Sonar","Multibeam","New Line","0356"]
["2017-04-14T00:51:41.540","2017-04-14T14:51:41.540","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-14T01:12:04.310","2017-04-14T15:12:04.310","AB","Sonar","Knudsen","Tx Pulse","16ms"]
["2017-04-14T01:44:08.660","2017-04-14T15:44:08.660","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-14T02:00:27.980","2017-04-14T16:00:27.980","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-14T03:04:21.210","2017-04-14T17:04:21.210","CW","Sonar","Multibeam","New Line","Turn Line 0359"]
["2017-04-14T03:28:57.250","2017-04-14T17:28:57.250","AB","Sonar","Multibeam","New Line","0360"]
["2017-04-14T04:22:48.410","2017-04-14T18:22:48.410","CW","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-14T04:32:34.360","2017-04-14T18:32:34.360","CW","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-14T05:39:52.400","2017-04-14T19:39:52.400","CW","Sonar","Multibeam","New Line","Turn Line 0363"]
["2017-04-14T06:03:02.870","2017-04-14T20:03:02.870","CW","Sonar","Multibeam","New Line","Survey Line 0354; new EK & SBP lines"]
["2017-04-14T06:04:11.650","2017-04-14T20:04:11.650","CW","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-14T06:53:05.630","2017-04-14T20:53:05.630","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-14T07:06:02.840","2017-04-14T21:06:02.840","CW","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-14T07:29:21.720","2017-04-14T21:29:21.720","CW","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-14T07:47:21.030","2017-04-14T21:47:21.030","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-04-14T08:15:54.660","2017-04-14T22:15:54.660","CW","Sonar","Multibeam","New Line","Turn at beginning of line 0367 (270 deg)"]
["2017-04-14T08:30:28.120","2017-04-14T22:30:28.120","DF","XBT",null,null,"Cast 046 applied to line 0367"]
["2017-04-14T09:02:58.360","2017-04-14T23:02:58.360","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-04-14T09:03:31.790","2017-04-14T23:03:31.790","DF","Sonar","Multibeam","New Line","turn at beginning of line 0368"]
["2017-04-14T09:05:56.980","2017-04-14T23:05:56.980","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-14T09:10:39.770","2017-04-14T23:10:39.770","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-14T09:10:53.270","2017-04-14T23:10:53.270","DF","Sonar","Multibeam",null,"Penetration filter: medium"]
["2017-04-14T09:29:00.300","2017-04-14T23:29:00.300","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-14T09:43:25.270","2017-04-14T23:43:25.270","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-14T09:44:56.900","2017-04-14T23:44:56.900","DF","Sonar","Multibeam",null,"Penetration filter: off"]
["2017-04-14T09:50:55.560","2017-04-14T23:50:55.560","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-14T10:25:30.210","2017-04-15T00:25:30.210","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-14T10:27:44.170","2017-04-15T00:27:44.170","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-14T10:58:26.490","2017-04-15T00:58:26.490","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-14T10:58:38.490","2017-04-15T00:58:38.490","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-04-14T11:07:32.010","2017-04-15T01:07:32.010","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-04-14T11:24:45.440","2017-04-15T01:24:45.440","DF","Sonar","Multibeam","New Line","Turn line 0371; new EK & SBP lines"]
["2017-04-14T11:27:23.240","2017-04-15T01:27:23.240","DF","Sonar","Multibeam","New Line","Survey line 0372; new EK & SBP lines"]
["2017-04-14T11:44:13.010","2017-04-15T01:44:13.010","DF","Sonar","Multibeam","New Line","Survey line 0373; new EK & SBP lines"]
["2017-04-14T12:47:33.220","2017-04-15T02:47:33.220","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-14T13:28:34.980","2017-04-15T03:28:34.980","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-14T13:28:50.320","2017-04-15T03:28:50.320","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-14T13:39:29.440","2017-04-15T03:39:29.440","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-14T13:43:59.690",{"$f":"IF(ISBLANK(A652),\" \",((A652)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-15T03:43:59.690"},"DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-14T14:12:08.390","2017-04-15T04:12:08.390","DF","Sonar","Multibeam","New Line","Turn at end of 0376"]
["2017-04-14T14:32:13.150","2017-04-15T04:32:13.150","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-04-14T14:44:02.550","2017-04-15T04:44:02.550","DF","Sonar","Multibeam","New Line","Turn line 0377; new EK & SBP lines"]
["2017-04-14T14:50:36.370","2017-04-15T04:50:36.370","DF","Sonar","Multibeam","New Line","Survey line 0378; new EK & SBP lines"]
["2017-04-14T15:36:13.010","2017-04-15T05:36:13.010","DF","Sonar","Multibeam",null,"Penetration filter: medium"]
["2017-04-14T15:37:16.740","2017-04-15T05:37:16.740","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-04-14T15:51:07.070","2017-04-15T05:51:07.070","DF","Sonar","Multibeam",null,"Pentration Filter: Off"]
["2017-04-14T16:37:47.040","2017-04-15T06:37:47.040","AB","XBT",null,null,"XBT48 applied to line 0380"]
["2017-04-14T17:20:19.050","2017-04-15T07:20:19.050","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-14T17:26:11.960","2017-04-15T07:26:11.960","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-14T17:55:10.860","2017-04-15T07:55:10.860","DF","Sonar","Multibeam","New Line","Turn line 0382; new EK & SBP lines"]
["2017-04-14T18:09:24.370","2017-04-15T08:09:24.370","AB","Sonar","Multibeam","New Line","0383 turn"]
["2017-04-14T18:12:22.990","2017-04-15T08:12:22.990","AB","Sonar","Multibeam","New Line","0384"]
["2017-04-14T19:13:45.410","2017-04-15T09:13:45.410","AB","Sonar","Knudsen","Phase Range","4000-5000m, Pulse 8ms"]
["2017-04-14T19:15:13.260","2017-04-15T09:15:13.260","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-14T21:28:18.440","2017-04-15T11:28:18.440","CW","Sonar","Multibeam","New Line","Turn Line 0388"]
["2017-04-14T21:51:05.630","2017-04-15T11:51:05.630","AB","Sonar","Multibeam","New Line","0389 "]
["2017-04-14T22:15:26.730","2017-04-15T12:15:26.730","AB","Ship",null,null,"Shift 500m to starboard"]
["2017-04-14T23:02:56.130","2017-04-15T13:02:56.130","AB","Sonar","Multibeam","New Line","0391"]
["2017-04-15T00:02:36.410","2017-04-15T14:02:36.410","AB","POS",null,null,"Course Acquistion ~1 min, vertical to 3m accuracy"]
["2017-04-15T00:04:01.830","2017-04-15T14:04:01.830","AB","Ship",null,null,"Shift 500m to starboard"]
["2017-04-15T01:13:46.920","2017-04-15T15:13:46.920","CW","XBT",null,null,"XBT 049; applied to line 0393"]
["2017-04-15T01:19:28.560","2017-04-15T15:19:28.560","AB","Sonar","Multibeam","New Line","0394"]
["2017-04-15T04:19:02.650","2017-04-15T18:19:02.650","CW","Sonar","Knudsen","Range",500]
["2017-04-15T04:19:33.590","2017-04-15T18:19:33.590","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-15T04:36:32.970","2017-04-15T18:36:32.970","CW","Sonar","Multibeam","Along Direction Pitch",-2]
["2017-04-15T04:39:07.570","2017-04-15T18:39:07.570","CW","Sonar","Multibeam","Max Angles","25/25"]
["2017-04-15T05:18:15.060","2017-04-15T19:18:15.060","CW","Sonar","Multibeam","New Line","Turn Line 0398"]
["2017-04-15T05:38:23","2017-04-15T19:38:23","CW","Sonar","Multibeam","New Line","Survey Line 0399; new EK & SBP lines"]
["2017-04-15T06:00:01.900","2017-04-15T20:00:01.900","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-04-15T07:04:41.680","2017-04-15T21:04:41.680","CW","Ship",null,null,"Heavier seas, and sonar lost a lot of swath earlier, so requested 500m move to port. Bridge tried riding coverage instead, and it wound up being quite liberal (1000m). Brought it back in to 600 from original line, and sea-state has improved more, so swath is better as well. Lessons learned. "]
["2017-04-15T07:16:34.340","2017-04-15T21:16:34.340","CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-15T08:08:36.100","2017-04-15T22:08:36.100","DF","Sonar","Multibeam","New Line","Turn line 0402; new EK & SBP lines"]
["2017-04-15T08:32:54.420","2017-04-15T22:32:54.420","DF","Sonar","Multibeam","Along Direction Pitch",-1.5]
["2017-04-15T08:34:04.310","2017-04-15T22:34:04.310","DF","Sonar","Multibeam","New Line","Survey Line 0403; new EK & SBP lines"]
["2017-04-15T08:37:51.950","2017-04-15T22:37:51.950","DF","Ship",null,null,"requested 800 m move to STBD"]
["2017-04-15T10:04:23.390","2017-04-16T00:04:23.390","DF","XBT",null,null,"cast 050 applied to line 0404"]
["2017-04-15T10:13:12.610","2017-04-16T00:13:12.610","DF","Sonar","Multibeam","Max Angles","34/34"]
["2017-04-15T11:06:11.390","2017-04-16T01:06:11.390","DF","Sonar","Multibeam","New Line","Turn line 0406; new EK & SBP lines"]
["2017-04-15T11:28:00.990","2017-04-16T01:28:00.990","DF","Sonar","Multibeam","New Line","Survey line 0407; new EK & SBP lines"]
["2017-04-15T13:56:51.860","2017-04-16T03:56:51.860","DF","Sonar","Multibeam","New Line","Turn line 0410; new EK & SBP lines"]
["2017-04-15T13:59:50.030","2017-04-16T03:59:50.030","DF","Sonar","Multibeam","New Line","Transit line 0411; new EK & SBP lines"]
["2017-04-15T15:55:41.610","2017-04-16T05:55:41.610","DF","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-15T16:39:32.400","2017-04-16T06:39:32.400","AB","XBT",null,null,"XBT51 added to line 0414"]
["2017-04-15T20:08:13.870","2017-04-16T10:08:13.870","AB","Sonar","Knudsen","Range","200m, Phase 5200-5400m Gain 36. Flat area"]
["2017-04-15T20:37:28.560","2017-04-16T10:37:28.560","AB","Sonar","Multibeam","New Line","0418 turn"]
["2017-04-15T20:39:54.530","2017-04-16T10:39:54.530","AB","Sonar","Multibeam","New Line","0419"]
["2017-04-15T20:44:24.460","2017-04-16T10:44:24.460","AB","Sonar","Knudsen","Range","500m, new line, phase range 4500-5000m"]
["2017-04-15T20:55:54.050","2017-04-16T10:55:54.050","AB","Sonar","Multibeam","Ping Mode","Very Deep, 40/40"]
["2017-04-15T20:58:16.430","2017-04-16T10:58:16.430","AB","POS",null,null,"Course Aquistion 1m accuracy"]
["2017-04-15T21:00:52.380","2017-04-16T11:00:52.380","AB","POS",null,null,"GNSS ok"]
["2017-04-15T21:01:16.670","2017-04-16T11:01:16.670","AB","POS",null,null,"CA mode again"]
["2017-04-15T21:01:27.660","2017-04-16T11:01:27.660","AB","Sonar","Knudsen","Phase Range","4000-4500m"]
["2017-04-15T21:04:08.340","2017-04-16T11:04:08.340","AB","POS",null,null,"Gams not ready, new line on MB 6.7 vertical and 1.5 x,y,"]
["2017-04-15T21:06:02.750","2017-04-16T11:06:02.750","AB","POS",null,null,"Corrections okay. Accuracy improving"]
["2017-04-15T21:13:01.690","2017-04-16T11:13:01.690","AB","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-15T21:42:33.800","2017-04-16T11:42:33.800","CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-15T22:17:39.760","2017-04-16T12:17:39.760","AB","Sonar","Knudsen","Phase Range","5000-5500m"]
["2017-04-15T22:54:18.130","2017-04-16T12:54:18.130","AB","Sonar","Multibeam","New Line","0422 turn"]
["2017-04-15T22:58:36.560","2017-04-16T12:58:36.560","AB","Sonar","Multibeam","New Line","0423"]
["2017-04-15T23:13:31.030","2017-04-16T13:13:31.030","AB","Sonar","Knudsen","Phase Range","5250-5750m"]
["2017-04-15T23:39:47.540","2017-04-16T13:39:47.540","AB","Sonar","EK","Change Range","6500m, Bottom Detectionh 6500m"]
["2017-04-15T23:46:42.450","2017-04-16T13:46:42.450","AB","Sonar","Knudsen","Phase Range","5000-5500m"]
["2017-04-16T00:00:54.770",{"$f":"IF(ISBLANK(A716),\" \",((A716)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-16T14:00:54.770"},"AB","Sonar","Multibeam","New Line","0424 turn"]
["2017-04-16T00:02:28.620","2017-04-16T14:02:28.620","AB","Sonar","Multibeam","New Line","0425"]
["2017-04-16T00:27:48.450","2017-04-16T14:27:48.450","CW","XBT",null,null,"XBT 052; applied to line 0425"]
["2017-04-16T00:30:07.440","2017-04-16T14:30:07.440","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-04-16T00:51:45.590","2017-04-16T14:51:45.590","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-16T02:11:20.530","2017-04-16T16:11:20.530","CW","Sonar","Multibeam","New Line","Turn Line 0428"]
["2017-04-16T02:26:22.490","2017-04-16T16:26:22.490","CW","Sonar","Multibeam","New Line","Survey Line 0429; new EK & SBP lines"]
["2017-04-16T02:35:22",{"$f":"IF(ISBLANK(A723),\" \",((A723)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-16T16:35:22"},"CW","Ship",null,null,"700m move to starboard"]
["2017-04-16T02:54:59.050","2017-04-16T16:54:59.050","CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-16T03:21:38",{"$f":"IF(ISBLANK(A725),\" \",((A725)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-16T17:21:38"},"CW","Ship",null,null,"200m move to starboard"]
["2017-04-16T04:09:00","2017-04-16T18:09:00","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-16T04:19:00.170","2017-04-16T18:19:00.170","CW","Sonar","Knudsen","Phase Range","5250-5750"]
["2017-04-16T04:25:09.160","2017-04-16T18:25:09.160","CW","POS",null,null,"GAMS popping in and out of Not Ready/Online"]
["2017-04-16T05:12:09.010","2017-04-16T19:12:09.010","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-16T05:46:53.350","2017-04-16T19:46:53.350","CW","Sonar","Knudsen","Phase Range","5250-5750"]
["2017-04-16T06:03:36.370","2017-04-16T20:03:36.370","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-16T06:13:15.320","2017-04-16T20:13:15.320","CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-16T06:24:40.410","2017-04-16T20:24:40.410","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-16T06:34:11.190","2017-04-16T20:34:11.190","CW","Sonar","Knudsen","Range",1000]
["2017-04-16T06:34:13.320","2017-04-16T20:34:13.320","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-16T07:00:59.630","2017-04-16T21:00:59.630","CW","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-04-16T07:14:18.200","2017-04-16T21:14:18.200","CW","Sonar","Multibeam","New Line","Turn at beginning of line 0434 (new heading). Bridge didn't call beforehand, so there's turn on previous line. New lines for EK & SBP"]
["2017-04-16T07:25:08.640","2017-04-16T21:25:08.640","CW","Ship",null,null,"Lost waypoint control after turn. Wonky trackline. "]
["2017-04-16T07:38:21.780","2017-04-16T21:38:21.780","CW","Ship",null,null,"Moving 700m back to port. "]
["2017-04-16T08:08:55.140","2017-04-16T22:08:55.140","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-16T08:17:47.350","2017-04-16T22:17:47.350","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-16T08:30:26.460","2017-04-16T22:30:26.460","CW","XBT",null,null,"XBT 053; applied to line 0435"]
["2017-04-16T09:19:45.810","2017-04-16T23:19:45.810","DF","Ship",null,null,"spped increased for transit line"]
["2017-04-16T11:35:01.410","2017-04-17T01:35:01.410","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-04-16T14:32:33.830","2017-04-17T04:32:33.830","DF","Sonar","Multibeam","New Line","Survey line 0442; new EK & SBP lines"]
["2017-04-16T15:40:51.600","2017-04-17T05:40:51.600","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-16T16:37:48.230","2017-04-17T06:37:48.230","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-16T16:56:09","2017-04-17T06:56:09","AB","XBT",null,null,"XBT54 added to line 0445"]
["2017-04-16T17:02:15.650","2017-04-17T07:02:15.650","AB","Sonar","Multibeam","New Line","0446 turn"]
["2017-04-16T17:21:21.090","2017-04-17T07:21:21.090","DF","Sonar","Multibeam","New Line","Survey line 0447; new EK & SBP lines"]
["2017-04-16T17:47:28.600","2017-04-17T07:47:28.600","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-16T18:03:41.070","2017-04-17T08:03:41.070","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-16T18:22:41.400","2017-04-17T08:22:41.400","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-16T19:06:02.240","2017-04-17T09:06:02.240","AB","Sonar","Multibeam","New Line","0449 turn line, shortening lines after 5000m of coverage on seamount."]
["2017-04-16T19:08:15.280","2017-04-17T09:08:15.280","AB","Sonar","Multibeam","New Line","0450"]
["2017-04-16T19:23:35.540","2017-04-17T09:23:35.540","AB","Sonar","Multibeam","New Line","0451 turn"]
["2017-04-16T19:24:50.730","2017-04-17T09:24:50.730","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-16T19:25:46.020","2017-04-17T09:25:46.020","AB","Sonar","Multibeam","New Line","0452"]
["2017-04-16T19:34:17.920","2017-04-17T09:34:17.920","AB","Sonar","Knudsen","Phase Range","3500m-4500m"]
["2017-04-16T19:36:11.580","2017-04-17T09:36:11.580","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-16T19:37:27.150","2017-04-17T09:37:27.150","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-16T21:02:52.170","2017-04-17T11:02:52.170","AB","Sonar","Multibeam","New Line","0454 turn line"]
["2017-04-16T21:04:30.080","2017-04-17T11:04:30.080","AB","Sonar","Multibeam","New Line","0455"]
["2017-04-16T21:24:29.540","2017-04-17T11:24:29.540","CW","Sonar","Multibeam","New Line","Survey Line 0456"]
["2017-04-16T21:50:09.110","2017-04-17T11:50:09.110","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-16T22:04:20.270","2017-04-17T12:04:20.270","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-16T22:12:09.900","2017-04-17T12:12:09.900","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-16T22:12:35.350","2017-04-17T12:12:35.350","AB","Sonar","Multibeam","Ping Mode","Deep, 70/50."]
["2017-04-16T22:15:16.930","2017-04-17T12:15:16.930","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-16T22:16:41.780","2017-04-17T12:16:41.780","AB","Sonar","Multibeam","Max Angles","75/45"]
["2017-04-16T22:39:47.510","2017-04-17T12:39:47.510","AB","Sonar","Multibeam","Ping Mode","Very Deep 52/52"]
["2017-04-16T22:40:22.260","2017-04-17T12:40:22.260","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-16T22:47:13.980","2017-04-17T12:47:13.980","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-16T23:04:31.640","2017-04-17T13:04:31.640","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-16T23:26:18.380","2017-04-17T13:26:18.380","AB","Sonar","Multibeam","New Line","0459 turn"]
["2017-04-16T23:29:13.990","2017-04-17T13:29:13.990","AB","Sonar","Multibeam","New Line","0460"]
["2017-04-16T23:43:24.110","2017-04-17T13:43:24.110","AB","Sonar","Multibeam","New Line","0461 turn"]
["2017-04-16T23:46:45.730","2017-04-17T13:46:45.730","AB","Sonar","Multibeam","New Line","0462"]
["2017-04-16T23:49:43.470","2017-04-17T13:49:43.470","AB","ship",null,null,"shift 1000m to port"]
["2017-04-16T23:51:11.500","2017-04-17T13:51:11.500","AB","POS",null,null,"Marinestar VBS, Gams in and out. Position at 1m accuracy"]
["2017-04-17T00:12:11.890","2017-04-17T14:12:11.890","CW","XBT",null,null,"XBT 055; applied to line 0463"]
["2017-04-17T00:14:28.330",{"$f":"IF(ISBLANK(A782),\" \",((A782)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-17T14:14:28.330"},"CW","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-17T00:17:41.370","2017-04-17T14:17:41.370","AB","Ship",null,null,"Shift 700m to port"]
["2017-04-17T01:01:27","2017-04-17T15:01:27","AB","Sonar","Multibeam","New Line","0464"]
["2017-04-17T01:32:59.850","2017-04-17T15:32:59.850","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-17T01:37:47.200","2017-04-17T15:37:47.200","AB","Sonar","Multibeam","Ping Mode","Auto, 52/52"]
["2017-04-17T01:42:31.340","2017-04-17T15:42:31.340","AB","Sonar","Multibeam","New Line","0465 turn, end of eastern seamount."]
["2017-04-17T01:43:37.320","2017-04-17T15:43:37.320","AB","Ship",null,null,"Increase to warp speed."]
["2017-04-17T01:46:59.310","2017-04-17T15:46:59.310","AB","Sonar","Multibeam","New Line","0466"]
["2017-04-17T03:56:59.410","2017-04-17T17:56:59.410","CW","Sonar","Multibeam","Max Angles","At 5575m and flat. Angles were at 30/30. Tried opening them up to 32/32, and the whole swath fell apart like a whiney baby. Went down to 28/28 and the baby is all happy and cooing again. Seems like they like to be swaddled right now. "]
["2017-04-17T05:04:57.110","2017-04-17T19:04:57.110","CW","Sonar","Knudsen","Range","500. Flat as Kansas."]
["2017-04-17T05:05:09.780","2017-04-17T19:05:09.780","CW","Sonar","Knudsen","Phase Range","5250-5750"]
["2017-04-17T05:23:02.370","2017-04-17T19:23:02.370","CW","POS",null,null,"Position light red for 20+ min"]
["2017-04-17T05:46:43.140","2017-04-17T19:46:43.140","CW","Sonar","Knudsen","Phase Range","5500-6000"]
["2017-04-17T06:20:57.790","2017-04-17T20:20:57.790","CW","Sonar","Knudsen","Phase Range","5250-5750"]
["2017-04-17T07:20:19.650","2017-04-17T21:20:19.650","CW","Sonar","Knudsen","Phase Range","5500-6000"]
["2017-04-17T08:18:17.060","2017-04-17T22:18:17.060","CW","XBT",null,null,"XBT 056; applied to line 0472"]
["2017-04-17T08:25:40.230","2017-04-17T22:25:40.230","DF","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-17T08:27:23.200","2017-04-17T22:27:23.200","DF","Sonar","Knudsen","Range",1000]
["2017-04-17T08:27:34.290","2017-04-17T22:27:34.290","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T08:39:34.780","2017-04-17T22:39:34.780","DF","Sonar","Multibeam","New Line","Turn line 0473; new EK & SBP lines"]
["2017-04-17T08:43:25","2017-04-17T22:43:25","DF","Sonar","Multibeam","New Line","Begin N Clipperton SM survey; Line 0476"]
["2017-04-17T08:53:23.560","2017-04-17T22:53:23.560","DF","Sonar","Multibeam","Max Angles","38/30"]
["2017-04-17T09:02:32.600","2017-04-17T23:02:32.600","DF","Sonar","Multibeam","Max Angles","40/40"]
["2017-04-17T09:47:26.900","2017-04-17T23:47:26.900","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-17T10:07:06.060","2017-04-18T00:07:06.060","DF","Sonar","Multibeam","New Line","Turn line 0476; new EK & SBP lines"]
["2017-04-17T10:27:17.640","2017-04-18T00:27:17.640","DF","Sonar","Multibeam","New Line","Survey Line 0477; new EK & SBP lines"]
["2017-04-17T10:47:10.550","2017-04-18T00:47:10.550","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T10:49:16.050","2017-04-18T00:49:16.050","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-17T10:55:06.590","2017-04-18T00:55:06.590","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-17T10:55:23.180","2017-04-18T00:55:23.180","DF","Sonar","Multibeam","Max Angles","75/75"]
["2017-04-17T11:07:51.180","2017-04-18T01:07:51.180","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-17T11:14:55.600","2017-04-18T01:14:55.600","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-17T11:22:49","2017-04-18T01:22:49","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-17T11:33:02.390","2017-04-18T01:33:02.390","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T11:34:37.110","2017-04-18T01:34:37.110","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-17T11:48:01.630","2017-04-18T01:48:01.630","DF","Sonar","Multibeam","New Line","Turn line 0479; new EK & SBP lines"]
["2017-04-17T12:08:45.190","2017-04-18T02:08:45.190","DF","Sonar","Multibeam","New Line","Survey Line 0480; new EK & SBP lines"]
["2017-04-17T12:18:50.210","2017-04-18T02:18:50.210","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T12:28:06.340","2017-04-18T02:28:06.340","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-17T12:32:20.350","2017-04-18T02:32:20.350","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-17T12:32:56.130","2017-04-18T02:32:56.130","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-17T12:36:46.040","2017-04-18T02:36:46.040","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-17T12:40:29.630","2017-04-18T02:40:29.630","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-17T12:52:22.790","2017-04-18T02:52:22.790","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-17T12:54:09.840","2017-04-18T02:54:09.840","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-17T12:58:28.850","2017-04-18T02:58:28.850","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-17T13:07:06.440","2017-04-18T03:07:06.440","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-17T13:09:55.650","2017-04-18T03:09:55.650","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T13:17:27.220","2017-04-18T03:17:27.220","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-17T13:28:08.970","2017-04-18T03:28:08.970","DF","Sonar","Multibeam",null,"MB Trackline error (spike way off into oblivion)"]
["2017-04-17T13:30:43.400","2017-04-18T03:30:43.400","DF","Sonar","Multibeam","New Line","Turn line 0482; new EK & SBP lines"]
["2017-04-17T13:50:55.190","2017-04-18T03:50:55.190","DF","Sonar","Multibeam","New Line","Survey Line 0483; new EK & SBP lines"]
["2017-04-17T14:15:37.370","2017-04-18T04:15:37.370","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T14:22:41.090","2017-04-18T04:22:41.090","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-17T14:27:31.480","2017-04-18T04:27:31.480","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-17T14:39:15.240","2017-04-18T04:39:15.240","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-17T15:01:11.970","2017-04-18T05:01:11.970","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-17T15:07:56.270","2017-04-18T05:07:56.270","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-17T15:15:26.820","2017-04-18T05:15:26.820","DF","Sonar","Multibeam","New Line","Turn line 0485; new EK & SBP lines"]
["2017-04-17T15:39:36.440","2017-04-18T05:39:36.440","DF","Sonar","Multibeam","New Line","Survey line 0486; new EK & SBP lines"]
["2017-04-17T16:42:50.370","2017-04-18T06:42:50.370","AB","XBT",null,null,"XBT57 added to line 0488"]
["2017-04-17T16:50:07.280","2017-04-18T06:50:07.280","AB","Ship",null,null,"Increase to warp speed."]
["2017-04-17T17:09:57.590","2017-04-18T07:09:57.590","AB","Sonar","Multibeam","New Line","0489 turn"]
["2017-04-17T18:11:10.650","2017-04-18T08:11:10.650","AB","Sonar","Multibeam","New Line","0490, 25/25"]
["2017-04-17T21:11:08.600","2017-04-18T11:11:08.600","AB","Sonar","Multibeam","New Line","0494, slight turn for new line, nadir artifacts reduced with new course"]
["2017-04-17T21:48:04",{"$f":"IF(ISBLANK(A847),\" \",((A847)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-18T11:48:04"},"AB","Sonar","Multibeam","Ping Mode","Switched to very deep for feature on port side. Max angles 50/38"]
["2017-04-17T22:11:07.730","2017-04-18T12:11:07.730","AB","Sonar","Multibeam","Max Angles","42/40"]
["2017-04-17T22:19:06.270","2017-04-18T12:19:06.270","AB","Sonar","Multibeam","Max Angles","40/40"]
["2017-04-17T22:55:33.030","2017-04-18T12:55:33.030","AB","Sonar","Multibeam","Ping Mode","Auto: extra deep; 40/40"]
["2017-04-17T23:58:20.020","2017-04-18T13:58:20.020","CW","XBT",null,null,"XBT 058; applied to line 0497"]
["2017-04-18T00:03:09.840","2017-04-18T14:03:09.840","AB","Sonar","Multibeam","New Line","0498"]
["2017-04-18T00:30:02.540","2017-04-18T14:30:02.540","AB","POS",null,null,"CA mode again"]
["2017-04-18T00:50:44.700","2017-04-18T14:50:44.700","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-18T01:41:01.480","2017-04-18T15:41:01.480","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-18T01:46:54.290","2017-04-18T15:46:54.290","AB","Sonar","Multibeam","Max Angles","50/45, very deep"]
["2017-04-18T01:54:40.610","2017-04-18T15:54:40.610","CW","Sonar","Multibeam","Ping Mode","Extra Deep 52/52"]
["2017-04-18T04:25:33.710","2017-04-18T18:25:33.710","CW","Sonar","Multibeam","New Line","Start S4a Survey Line Plan (New Heading); New Ek & SBP lines"]
["2017-04-18T04:44:41.330","2017-04-18T18:44:41.330","CW","POS",null,null,"Position light red; GAMS Not Ready/Standby; Nav Status CA"]
["2017-04-18T04:49:30.760","2017-04-18T18:49:30.760","CW","POS",null,null,"POS is happy now."]
["2017-04-18T04:50:08.140","2017-04-18T18:50:08.140","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-18T05:03:23.160","2017-04-18T19:03:23.160","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-18T06:09:03.070","2017-04-18T20:09:03.070","CW","Sonar","Multibeam","New Line","Turn Line 0505"]
["2017-04-18T06:30:22.890","2017-04-18T20:30:22.890","CW","Sonar","Multibeam","New Line","Survey Line 0506; new EK & SBP lines"]
["2017-04-18T06:38:38.020","2017-04-18T20:38:38.020","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-18T07:15:30.710","2017-04-18T21:15:30.710","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-18T07:23:32.950","2017-04-18T21:23:32.950","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-18T07:37:15.560","2017-04-18T21:37:15.560","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-18T07:57:14.480","2017-04-18T21:57:14.480","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-18T08:34:15.690","2017-04-18T22:34:15.690","DF","Sonar","Multibeam","New Line","Survey line 0510; new EK & SBP lines"]
["2017-04-18T08:47:22.340","2017-04-18T22:47:22.340","CW","XBT",null,null,"XBT 059; applied to line 0510"]
["2017-04-18T08:59:22.950","2017-04-18T22:59:22.950","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-04-18T09:04:42.850","2017-04-18T23:04:42.850","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-18T09:38:25.020","2017-04-18T23:38:25.020","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-18T10:24:21.120","2017-04-19T00:24:21.120","DF","Sonar","Multibeam","New Line","Turn line 0512; New EK & SBP lines"]
["2017-04-18T10:47:41.500","2017-04-19T00:47:41.500","DF","Sonar","Multibeam","New Line","Survey line 0513; New EK & SBP lines"]
["2017-04-18T12:29:23.230","2017-04-19T02:29:23.230","DF","Sonar","Multibeam","New Line","Turn line 0515; New EK & SBP lines"]
["2017-04-18T12:51:03.080","2017-04-19T02:51:03.080","DF","Sonar","Multibeam","New Line","Survey line 0516; New EK & SBP lines"]
["2017-04-18T13:22:31.750","2017-04-19T03:22:31.750","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-04-18T14:27:54.620","2017-04-19T04:27:54.620","DF","Sonar","Multibeam","New Line","Turn line 0518; New EK & SBP lines"]
["2017-04-18T14:47:47.130","2017-04-19T04:47:47.130","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-18T14:51:55.960","2017-04-19T04:51:55.960","DF","Sonar","Multibeam","New Line","Survey Line 0519; New EK & SBP lines"]
["2017-04-18T15:01:59.120","2017-04-19T05:01:59.120","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-18T15:38:51.850","2017-04-19T05:38:51.850","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-18T16:16:52.120","2017-04-19T06:16:52.120","DF","Sonar","Multibeam","New Line","Turn line 0521; New EK & SBP lines"]
["2017-04-18T16:32:45.870","2017-04-19T06:32:45.870","DF","XBT",null,null,"Cast 060 applied to line 0521"]
["2017-04-18T16:37:40.700","2017-04-19T06:37:40.700","DF","Sonar","Multibeam","New Line","Survey line 0522; new EK & SBP lines"]
["2017-04-18T18:14:36.110","2017-04-19T08:14:36.110","DF","Sonar","Multibeam","New Line","Survey line 0524; new EK & SBP lines"]
["2017-04-18T19:23:23.120","2017-04-19T09:23:23.120","AB","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-18T19:24:02.010","2017-04-19T09:24:02.010","AB","Sonar","Multibeam","New Line","0526 turn"]
["2017-04-18T19:26:11.790","2017-04-19T09:26:11.790","AB","Sonar","Multibeam","New Line","0527, new ek and sbp lines"]
["2017-04-18T19:42:00","2017-04-19T09:42:00","AB","Sonar","Multibeam","New Line","0528 turnline"]
["2017-04-18T19:43:42.860","2017-04-19T09:43:42.860","AB","Sonar","Multibeam","New Line","0529"]
["2017-04-18T20:13:55.500","2017-04-19T10:13:55.500","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-18T20:18:27.390","2017-04-19T10:18:27.390","AB","Sonar","Multibeam","Ping Mode","Very Deep 35/52"]
["2017-04-18T20:40:47.800","2017-04-19T10:40:47.800","AB","Sonar","Multibeam","Ping Mode","auto: extra deep; 50/50"]
["2017-04-18T20:51:21.690","2017-04-19T10:51:21.690","AB","Sonar","Multibeam","New Line","0531 turn, end of feature. New ek and spb lines"]
["2017-04-18T20:53:40.890","2017-04-19T10:53:40.890","AB","Sonar","Multibeam","New Line","0532"]
["2017-04-18T21:17:20.850","2017-04-19T11:17:20.850","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-18T21:27:15.310","2017-04-19T11:27:15.310","CW","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-18T22:34:23.270","2017-04-19T12:34:23.270","AB","Sonar","Multibeam",null,"outer beam noise stbd side"]
["2017-04-18T22:47:51.220","2017-04-19T12:47:51.220","AB","Sonar","Knudsen","Phase Range","5000-6000m"]
["2017-04-19T00:05:47.460","2017-04-19T14:05:47.460","AB","Sonar","Multibeam","New Line","0536"]
["2017-04-19T00:17:46.390","2017-04-19T14:17:46.390","AB","Sonar","Multibeam","New Line","0537 turn line. New ek and sbp line. Reduced to survey speed 8.5-9kts."]
["2017-04-19T00:18:23.240","2017-04-19T14:18:23.240","AB","Sonar","Multibeam","New Line","0538"]
["2017-04-19T00:22:49.350","2017-04-19T14:22:49.350","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-19T00:52:37.390","2017-04-19T14:52:37.390","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-04-19T01:20:35.740","2017-04-19T15:20:35.740","Ab","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-04-19T01:29:53.770","2017-04-19T15:29:53.770","CW","Sonar","Multibeam","Ping Mode","Auto: Extra Deep"]
["2017-04-19T01:41:24.620","2017-04-19T15:41:24.620","AB","Sonar","Multibeam","New Line","0540 turn line, new ek and sbp lines"]
["2017-04-19T01:44:34.100",{"$f":"IF(ISBLANK(A911),\" \",((A911)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-19T15:44:34.100"},"AB","Sonar","Multibeam","New Line","0541"]
["2017-04-19T01:53:26.330","2017-04-19T15:53:26.330","CW","XBT",null,null,"XBT 061; applied to line 0541"]
["2017-04-19T02:01:28.480","2017-04-19T16:01:28.480","CW","Issue",null,null,"SIS Red Border of Death twice in 10 min. Lost a few pings."]
["2017-04-19T02:10:53.350","2017-04-19T16:10:53.350","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-04-19T02:23:08.410","2017-04-19T16:23:08.410","CW","Sonar","Multibeam","New Line","Survey Line 0542; new EK & SBP lines"]
["2017-04-19T02:40:46.180","2017-04-19T16:40:46.180","CW","Ship",null,null,"Requested 1000m move to Port. Bridge decided to go Starboard at the beginning, so it looks pretty wonky on the trackline."]
["2017-04-19T03:49:04.860","2017-04-19T17:49:04.860","AB","Sonar","Multibeam","New Line","0544 turn, increasing to transit speed"]
["2017-04-19T03:56:16.190","2017-04-19T17:56:16.190","AB","Sonar","Multibeam","New Line","0545"]
["2017-04-19T05:39:17.870","2017-04-19T19:39:17.870","CW","Sonar","Multibeam",null,"Cross track window depth indicated 2.5m for a few seconds, followed by a few lost pings. Weird. "]
["2017-04-19T05:55:03.560","2017-04-19T19:55:03.560","CW","Sonar","Knudsen","Range",500]
["2017-04-19T05:55:19.550","2017-04-19T05:55:17.490","CW","Sonar","Knudsen","Phase Range","5000-5500"]
["2017-04-19T07:21:38.940","2017-04-19T21:21:38.940","CW","Sonar","Knudsen",null,"SBP computer froze. Lost remote connection on EK computer. Restarting."]
["2017-04-19T07:30:23.960","2017-04-19T21:30:23.960","CW","Sonar","Knudsen","Start Pinging","Restarted, pinging, recording, remoted."]
["2017-04-19T07:52:46.980","2017-04-19T21:52:46.980","CW","Sonar","Knudsen","Phase Range","4750-5250"]
["2017-04-19T08:04:03.260","2017-04-19T22:04:03.260","CW","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-04-19T08:10:04.130","2017-04-19T22:10:04.130","DF","Sonar","Knudsen","Phase Range","4250-4750"]
["2017-04-19T08:16:02.780","2017-04-19T22:16:02.780","DF","Sonar","Knudsen","Phase Range","4000-4500"]
["2017-04-19T08:32:50.940","2017-04-19T22:32:50.940","DF","XBT",null,null,"Cast 062 applied to line 0549"]
["2017-04-19T08:35:19.130","2017-04-19T22:35:19.130","DF","Sonar","Knudsen","Range",1000]
["2017-04-19T08:35:40.710","2017-04-19T22:35:40.710","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-19T08:52:59.820","2017-04-19T22:52:59.820","DF","Sonar","Multibeam","New Line","Turn line 0550; new EK & SBP lines"]
["2017-04-19T09:11:31.530","2017-04-19T23:11:31.530","DF","Sonar","Multibeam","New Line","Survey line 0551; new EK & SBP lines"]
["2017-04-19T09:16:16.010","2017-04-19T23:16:16.010","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-19T09:31:44.800","2017-04-19T23:31:44.800","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-19T09:49:33.400","2017-04-19T23:49:33.400","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-19T09:57:47.070","2017-04-19T23:57:47.070","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-19T10:09:14.350","2017-04-20T00:09:14.350","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-04-19T10:35:19.060","2017-04-20T00:35:19.060","DF","Sonar","Multibeam","New Line","Turn line 0553; New EK & SBP lines"]
["2017-04-19T10:53:16.640","2017-04-20T00:53:16.640","DF","Sonar","Multibeam","New Line","Survey line 0554; New EK & SBP lines"]
["2017-04-19T11:01:26.970","2017-04-20T01:01:26.970","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-04-19T12:17:20.070","2017-04-20T02:17:20.070","DF","Ship",null,null,"Transit line 0556; WARP SPEED!!!!!"]
["2017-04-19T12:18:07.860","2017-04-20T02:18:07.860","DF","Sonar","Multibeam","New Line","Transit line 0556, End S4a survey"]
["2017-04-19T16:15:37.540","2017-04-20T06:15:37.540","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-04-19T16:25:36.360","2017-04-20T06:25:36.360","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-19T16:36:40.330","2017-04-20T06:36:40.330","AB","XBT",null,null,"XBT63 added to line 0561"]
["2017-04-19T16:40:12.870","2017-04-20T06:40:12.870","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-19T16:45:33","2017-04-20T06:45:33","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-04-19T16:50:58.260","2017-04-20T06:50:58.260","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-19T17:22:19.100","2017-04-20T07:22:19.100","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-19T17:31:50.230","2017-04-20T07:31:50.230","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-19T17:41:19.010","2017-04-20T07:41:19.010","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-04-19T18:07:35.420","2017-04-20T08:07:35.420","DF","Sonar","Multibeam","Max Angles","75/75"]
["2017-04-19T19:19:12.720","2017-04-20T09:19:12.720","AB","Sonar","Multibeam","New Line","0565, new line ek and sbp"]
["2017-04-19T19:44:13.240","2017-04-20T09:44:13.240","AB","Sonar","Knudsen","Phase Range","1000-2000m"]
["2017-04-19T20:08:05.840","2017-04-20T10:08:05.840","AB","Sonar","Knudsen","Phase Range","1500-2500m, gain 35, power 2, pulse 4"]
["2017-04-19T20:26:01.150","2017-04-20T10:26:01.150","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-19T21:15:27.530","2017-04-20T11:15:27.530","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-19T21:50:09.860","2017-04-20T11:50:09.860","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-04-19T23:06:52.270","2017-04-20T13:06:52.270","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-04-19T23:14:45.510","2017-04-20T13:14:45.510","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-19T23:15:35.500","2017-04-20T13:15:35.500","AB","Sonar","Multibeam","New Line","0569 turn line south for food disposal, new ek and spb lines"]
["2017-04-19T23:17:11.620","2017-04-20T13:17:11.620","AB","Sonar","Multibeam","New Line","0570"]
["2017-04-19T23:41:20.790","2017-04-20T13:41:20.790","AB","Sonar","Knudsen","Phase Range","1000-2000m"]
["2017-04-19T23:42:54.530","2017-04-20T13:42:54.530","AB","Sonar","Multibeam","New Line","0571, new ek and sbp lines. Food disposal completed."]
["2017-04-19T23:47:32.990","2017-04-20T13:47:32.990","AB","Sonar","Knudsen","Tx Power","1, Tx Pulse 2, Gain 35dB"]
["2017-04-19T23:54:29.850","2017-04-20T13:54:29.850","AB","Sonar","Knudsen","Phase Range","500-1000m"]
["2017-04-19T23:56:41.670","2017-04-20T13:56:41.670","AB","Sonar","Multibeam","New Line","0572 turn line"]
["2017-04-20T00:00:08.840","2017-04-20T14:00:08.840","AB","Sonar","Multibeam","New Line","0573, new sbp and ek lines"]
["2017-04-20T00:01:18.270","2017-04-20T14:01:18.270","AB","Sonar","Knudsen",null,"Change range to 500m, phase 250-750, pulse 1"]
["2017-04-20T00:03:36.560","2017-04-20T14:03:36.560","AB","Sonar","Knudsen","Phase Range","500-1000m"]
["2017-04-20T00:08:32.890","2017-04-20T14:08:32.890","AB","Sonar","Knudsen","Phase Range","1000-1500m"]
["2017-04-20T00:09:13.360","2017-04-20T14:09:13.360","AB","Sonar","Knudsen",null,"Change range to 1000m, 1000-2000m phase range; power 2 pulse 2"]
["2017-04-20T00:15:37.670","2017-04-20T14:15:37.670","CW","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-04-20T00:24:41.820","2017-04-20T14:24:41.820","CW","Sonar","Multibeam","New Line","Turn at beginning of line 0574 (New Heading)"]
["2017-04-20T00:58:20.980",{"$f":"IF(ISBLANK(A975),\" \",((A975)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-20T14:58:20.980"},"Ab","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-20T00:59:04.850","2017-04-20T14:59:04.850","Ab","Sonar","Knudsen","Phase Range","2000-3000m, pulse 4"]
["2017-04-20T01:17:20.250","2017-04-20T15:17:20.250","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-20T01:18:29.580","2017-04-20T15:18:29.580","AB","Sonar","Multibeam","New Line","575, new ek and spb lines"]
["2017-04-20T01:25:30.400","2017-04-20T15:25:30.400","AB","Sonar","Knudsen","Phase Range","500-1000m"]
["2017-04-20T01:28:45.660","2017-04-20T15:28:45.660","AB","Sonar","Knudsen","Phase Range","1500-2500m"]
["2017-04-20T01:57:25.080","2017-04-20T15:57:25.080","CW","XBT",null,null,"XBT 064; applied to line 0575"]
["2017-04-20T02:14:09.770","2017-04-20T16:14:09.770","CW","Sonar","Multibeam","New Line","Turn at beginning of line 0576 (New Heading); new EK & SBP lines"]
["2017-04-20T02:34:44.240","2017-04-20T16:34:44.240","AB","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-20T02:50:40.310","2017-04-20T16:50:40.310","CW","Sonar","Multibeam","New Line","New Line for new heading"]
["2017-04-20T03:11:29.680","2017-04-20T17:11:29.680","CW","Sonar","Knudsen","Phase Range","2000-3000m"]
["2017-04-20T03:26:48.420","2017-04-20T17:26:48.420","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-20T03:41:01.390","2017-04-20T17:41:01.390","AB","Sonar","EK","Change Range","4500m"]
["2017-04-20T04:15:52.940","2017-04-20T18:15:52.940","CW","POS",null,null,"Position Accuracy Lamp Red for about 10-15 min./"]
["2017-04-20T04:41:21.170","2017-04-20T18:41:21.170","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-20T04:44:55.860","2017-04-20T18:44:55.860","CW","Sonar","Multibeam","New Line","Line 0579. New Heading. Beginning of Samoan Clipper Survey. New lines for EK & SBP"]
["2017-04-20T04:44:55.860",{"$f":"IF(ISBLANK(A991),\" \",((A991)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-04-20T18:44:55.860"},"CW","Ship",null,null,"6.5 kts for Clipper Survey"]
["2017-04-20T04:57:54.330","2017-04-20T18:57:54.330","CW","Sonar","Multibeam","Max Angles","At 3350m, 30/30 for 1820/1915 coverage"]
["2017-04-20T05:59:01.230","2017-04-20T19:59:01.230","CW","Sonar","Multibeam","New Line","Turn Line 0581"]
["2017-04-20T06:12:32.090","2017-04-20T20:12:32.090","CW","Sonar","Multibeam","New Line","Survey Line 0582; new EK & SBP lines"]
["2017-04-20T06:26:47.390","2017-04-20T20:26:47.390","CW","Sonar","Multibeam","Max Angles","25/25"]
["2017-04-20T07:23:08.030","2017-04-20T21:23:08.030","DF","Sonar","Multibeam","New Line","Turn line 0584"]
["2017-04-20T07:35:54.240","2017-04-20T21:35:54.240","DF","Sonar","Knudsen",null,"Pulse: 2, Power: 3, Gain: 38"]
["2017-04-20T07:38:48.270","2017-04-20T21:38:48.270","DF","Sonar","Multibeam","New Line","Survey line 0585; new EK & SBP lines"]
["2017-04-20T07:41:47.500","2017-04-20T21:41:47.500","DF","Sonar","Multibeam","Max Angles","30/30"]
["2017-04-20T07:54:15.820","2017-04-20T21:54:15.820","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-20T08:32:47.160","2017-04-20T22:32:47.160","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-04-20T08:49:39.310","2017-04-20T22:49:39.310","DF","Sonar","Multibeam","New Line","Turn line 0587; new EK & SBP lines"]
["2017-04-20T09:03:52.210","2017-04-20T23:03:52.210","CW","XBT",null,null,"XBT 065; applied to line 0587"]
["2017-04-20T09:08:18","2017-04-20T23:08:18","CW","Sonar","Multibeam","New Line","Survey Line 0588"]
["2017-04-20T09:21:18.430","2017-04-20T23:21:18.430","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-04-20T10:05:35.250","2017-04-21T00:05:35.250","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-20T10:18:46.390","2017-04-21T00:18:46.390","DF","Sonar","Multibeam","New Line","Turn line 0590; new EK & SBP lines"]
["2017-04-20T10:35:18.800","2017-04-21T00:35:18.800","DF","Sonar","Multibeam","New Line","Survey Line 0591; New EK & SBP lines"]
["2017-04-20T10:35:52.650","2017-04-21T00:35:52.650","DF","Sonar","Multibeam","Max Angles","32/32"]
["2017-04-20T11:31:44.920",{"$f":"IF(ISBLANK(A1010),\" \",((A1010)-DATE(1970,1,1))+25569+($C$1/24))","v":"2017-04-19T21:31:44.920"},"DF","Sonar","Multibeam",null,"Massive interference artifact occurred. Could not regain bottom, randomly stopped, forced into Very Deep mode to help, bridge verified nothing was turned on"]
["2017-04-20T11:32:20.940","2017-04-19T21:32:20.940","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-04-20T11:33:54.670","2017-04-19T21:33:54.670","DF","Sonar","Multibeam","Interference Filter (On/Off)","On"]
["2017-04-20T11:34:54.670","2017-04-19T21:34:54.670","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-04-20T11:42:58.830","2017-04-19T21:42:58.830","DF","Sonar","Multibeam","New Line","End Clipper Survey, Transit line 0593; new EK & SBP lines"]
["2017-04-20T11:54:21.100","2017-04-19T21:54:21.100","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-04-20T11:54:43.690","2017-04-19T21:54:43.690","DF","Sonar","Multibeam","Ping Mode","Auto"]
["2017-04-20T11:55:35.100","2017-04-19T21:55:35.100","DF","Sonar","Multibeam","Max Angles","75/75"]
["2017-04-20T12:07:23.750","2017-04-19T22:07:23.750","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-04-20T12:41:16.930","2017-04-19T22:41:16.930","DF","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-04-20T12:57:01.980","2017-04-19T22:57:01.980","DF","Sonar","Knudsen","Tx Power",1]
["2017-04-20T12:58:54.010","2017-04-19T22:58:54.010","DF","Sonar","Multibeam","New Line","Transit line 0595"]
["2017-04-20T14:50:09.340","2017-04-20T00:50:09.340","DF","Sonar","Knudsen","Tx Power",2]
["2017-04-20T16:14:27.790","2017-04-20T02:14:27.790","AB","Sonar","Multibeam","New Line","0599, new lines on ek and sbp"]
["2017-04-20T16:24:35.180","2017-04-20T02:24:35.180","DF","Sonar",null,null,"Secured all pinging for pre arrival manuevers"]
["2017-04-20T19:37:41.880","2017-04-20T05:37:41.880","AB","Ship",null,null,"Alongside fuel pier. Moving to main dock afterward. Powering down sonars after PU parameter export and BIST."]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1035),\" \",((A1035)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1099),\" \",((A1099)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1163),\" \",((A1163)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1227),\" \",((A1227)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1291),\" \",((A1291)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1355),\" \",((A1355)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1419),\" \",((A1419)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1483),\" \",((A1483)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1547),\" \",((A1547)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1611),\" \",((A1611)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1675),\" \",((A1675)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1739),\" \",((A1739)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1803),\" \",((A1803)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1867),\" \",((A1867)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1931),\" \",((A1931)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1995),\" \",((A1995)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["AB","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DF","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["CW","Weather","Knudsen","New Line","Secure","Gain Mode"]
["DS","Watch Change","All","Max Angles",null,"Gain Value"]
["CA","XBT",null,"Spike Filter Strength",null,"Process Shift"]
["MP","Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
[null,"Other",null,"Aeration Filter (On/Off)",null,"Range"]
[null,null,null,"Interference Filter (On/Off)",null,"Phase Mode"]
[null,null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]