{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2003,"n_cols":7,"rows_kept":2003,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1707","UTC to Local: ",10,"UTC 2","UTC 3","UTC 4","Cruise Details: Aug 8th - Aug 31st"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2017-08-07T19:57:58.260",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-07T09:57:58.260"},"DF","Sonar",null,null,"Remote start TRU"]
["2017-08-08T00:40:30.550",{"$f":"IF(ISBLANK(A6),\" \",((A6)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-07T14:40:30.550"},"DF","Sonar","Multibeam",null,"Running BIST 01"]
["2017-08-08T00:48:14.300","2017-08-07T14:48:14.300","DF","Sonar","Multibeam",null,"BIST 01 failed TX Channels"]
["2017-08-08T00:49:49.810","2017-08-07T14:49:49.810","DF","Sonar","Multibeam",null,"Running BIST 02"]
["2017-08-08T01:01:49.150","2017-08-07T15:01:49.150","DF","Sonar","Multibeam",null,"BIST 02 failed TX Channels, shutting down TRU to push boards"]
["2017-08-08T01:06:15.100","2017-08-07T15:06:15.100","DF","Sonar","Multibeam",null,"Restarted TRU remotely"]
["2017-08-08T01:19:43.630","2017-08-07T15:19:43.630","DF","Sonar","Multibeam",null,"Restarted SIS and began BIST 03"]
["2017-08-08T18:43:19.410","2017-08-08T08:43:19.410","DF","Sonar",null,null,"Brought up all software suites and folders"]
["2017-08-09T02:49:38.990","2017-08-08T16:49:38.990","AB","Ship",null,null,"Underway."]
["2017-08-09T04:18:05.250","2017-08-08T18:18:05.250","CW","XBT",null,null,"XBT 001. Not logging yet, so will be applied to SIS line 0000 when logging starts."]
["2017-08-09T04:19:07.920","2017-08-08T18:19:07.920","CW","Sonar","Multibeam","Start Logging","Line 0000"]
["2017-08-09T04:25:01.100","2017-08-08T18:25:01.100","CW","Sonar","EK","Start Pinging"]
["2017-08-09T04:25:39.170","2017-08-08T18:25:39.170","CW","Sonar","EK","Start Recording"]
["2017-08-09T04:46:22.710","2017-08-08T18:46:22.710","CW","Sonar","Multibeam","New Line","Start fancy survey line 0001 at 6kts"]
["2017-08-09T05:19:58.570","2017-08-08T19:19:58.570","AB","Sonar","Knudsen",null,"Pulse 2, Power 1, Gain 31dB, Range 500m, Phase 750-1250m"]
["2017-08-09T05:20:57.770","2017-08-08T19:20:57.770","AB","Sonar","EK",null,"18khz, Range 1500, Bottom Detection 7500"]
["2017-08-09T05:25:20.460","2017-08-08T19:25:20.460","AB","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-08-09T05:48:59.360","2017-08-08T19:48:59.360","CW","Sonar","Multibeam",null,"Multibeam got all cranky. Restarting. "]
["2017-08-09T05:50:54.010","2017-08-08T19:50:54.010","AB","Sonar",null,null,"EK and Knudsen on internal pinging until EM fixed"]
["2017-08-09T06:00:51.550","2017-08-08T20:00:51.550","CW","Sonar","Multibeam",null,"EM302 TRU restarted. New telnet. Starting SIS"]
["2017-08-09T07:28:52.050","2017-08-08T21:28:52.050","AB","Issue/Problem","Multibeam",null,"Still troubleshooting EM302"]
["2017-08-09T08:28:02.080","2017-08-08T22:28:02.080","CW","Issue/Problem","Multibeam",null,"Reseated all TX cards. BIST failed"]
["2017-08-09T08:28:31.120","2017-08-08T22:28:31.120","CW","Issue/Problem","Multibeam","BIST","Reseated TX cards 3 and 7. "]
["2017-08-09T08:29:52.890","2017-08-08T22:29:52.890","CW","Sonar","Multibeam","BIST","BIST all pass!!"]
["2017-08-09T08:30:11.810","2017-08-08T22:30:11.810","CW","Issue/Problem","Multibeam",null,"Even though BIST passed, telnet was still babbling about error, and pinging produced crap data"]
["2017-08-09T09:17:52.120","2017-08-08T23:17:52.120","CW","Issue/Problem","Multibeam",null,"Switched 0 slot TX card with new spare"]
["2017-08-09T10:52:45.300","2017-08-09T00:52:45.300","CW","XBT",null,null,"XBT 002. Not yet applied because the sonar is a whiney bastard."]
["2017-08-09T12:06:06.020","2017-08-09T02:06:06.020","DF","Issue/Problem","Multibeam",null,"Still troubleshooting EM302"]
["2017-08-09T12:27:22.640","2017-08-09T02:27:22.640","DF","Issue/Problem","Multibeam",null,"Noticed that the upper ethernet chord connection from lower power supply to upper unit has a light out. In the female ethernet connection only the top light is green while the lower light is out. "]
["2017-08-09T12:28:38.330","2017-08-09T02:28:38.330","DF","Issue/Problem","Multibeam",null,"BISTs are now indicating power issues, tc channel issues, and software update issues. I will keep attempting to troubleshoot."]
["2017-08-09T12:35:33.740","2017-08-09T02:35:33.740","DF","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-08-09T12:48:20.210","2017-08-09T02:48:20.210","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-09T13:13:45.960","2017-08-09T03:13:45.960","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-09T13:26:53.090","2017-08-09T03:26:53.090","DF","Issue/Problem","Multibeam",null,"TX Board in slot 19 has a bad connection with the ethernet cable. If the cable wiggles at all the connection is lost, have checked on it and it will randomly loose connection with the swell. Ran another BIST, status seems to be getting worse with RX Channels now failing as well. I am going to shut down the TRU and await further instruction. "]
["2017-08-09T13:39:45.010","2017-08-09T03:39:45.010","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-09T13:49:20.990","2017-08-09T03:49:20.990","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-09T13:59:52.260","2017-08-09T03:59:52.260","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-09T14:32:44.710","2017-08-09T04:32:44.710","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-09T16:26:27.060","2017-08-09T06:26:27.060","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-09T17:47:00.260","2017-08-09T07:47:00.260","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-09T18:55:26","2017-08-09T08:55:26","AB","Issue/Problem","Multibeam",null,"Problems with slot 18 and 19 connecting. Recorded in telnet session. CET reseated boards and checked connections. Restarted with no TX errors. But red light on SIS for sonar head connection failure when pinging."]
["2017-08-09T19:38:57.520","2017-08-09T09:38:57.520","AB","Issue/Problem","Multibeam",null,"Board in slot 4 was swapped to slot 0 because it is an older board version. Pinging. Red sonar head lighterror  is now green. Very Deep mode. 40/40. No filters. All sonars pinging from MBES trigger."]
["2017-08-09T19:40:50","2017-08-09T09:40:50","AB","XBT",null,null,"XBT 3 "]
["2017-08-09T19:47:52.270","2017-08-09T09:47:52.270","AB","Sonar","Multibeam",null,"XBT3 added to new line 0003."]
["2017-08-09T20:33:40.860","2017-08-09T10:33:40.860","AB","Sonar","Multibeam",null,"Very Deep, 37/37, no filters"]
["2017-08-09T20:43:58.940","2017-08-09T10:43:58.940","AB","Sonar","Knudsen","Range","500m"]
["2017-08-09T21:50:35","2017-08-09T11:50:35","AB","Sonar","Multibeam",null,"new line 0005"]
["2017-08-09T22:09:58.500","2017-08-09T12:09:58.500","AB","Sonar","Multibeam",null,"Slope filter"]
["2017-08-09T22:28:10.100","2017-08-09T12:28:10.100","AB","Sonar","Multibeam","Max Angle","35/35"]
["2017-08-09T22:45:05","2017-08-09T12:45:05","AB","Sonar","Multibeam","New Line","0006"]
["2017-08-09T23:30:54","2017-08-09T13:30:54","AB","ship",null,null,"Abandonship drill "]
["2017-08-09T23:49:50","2017-08-09T13:49:50","AB","Sonar","Multibeam","New Line","0007"]
["2017-08-09T23:57:08.400","2017-08-09T13:57:08.400","AB","Sonar","Multibeam","Max Angle","40/40"]
["2017-08-10T00:08:47.770","2017-08-09T14:08:47.770","AB","Sonar","Multibeam","Max Angle","45/45"]
["2017-08-10T00:31:26.500","2017-08-09T14:31:26.500","AB","Sonar","Multibeam","Max Angle","52/45"]
["2017-08-10T00:40:45","2017-08-09T14:40:45","AB","XBT",null,null,"0004"]
["2017-08-10T00:47:55.870","2017-08-09T14:47:55.870","AB","Sonar","Multibeam",null,"XBT4 added to new line 0008"]
["2017-08-10T00:50:55","2017-08-09T14:50:55","AB","Sonar","Multibeam","Max Angle","40/40, Manual:Very Deep. Slope filter, Med Spike filter"]
["2017-08-10T01:06:43.820","2017-08-09T15:06:43.820","AB","Sonar","Knudsen",null,"Pulse 4 Power 2, Gain 34, Range 500m, Phase 4500-5000"]
["2017-08-10T01:07:30.820","2017-08-09T15:07:30.820","AB","Sonar","EK",null,"Bottom Detection 7500, Range 5000"]
["2017-08-10T06:25:11.480","2017-08-09T20:25:11.480","CW","Sonar","Multibeam",null,"Slowing to 8.5 for sweet feature. SIS line 0014"]
["2017-08-10T06:50:09.790","2017-08-09T20:50:09.790","CW","Sonar","Knudsen","Range","1000 for feature. New line too. "]
["2017-08-10T06:50:45.100","2017-08-09T20:50:45.100","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-10T07:15:17","2017-08-09T21:15:17","CW","Ship",null,null,"back to transit speed"]
["2017-08-10T09:18:36.590","2017-08-09T23:18:36.590","CW","XBT",null,null,"XBT 005; applied to SIS line 0016"]
["2017-08-10T09:28:55.190","2017-08-09T23:28:55.190","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-10T09:32:50.270","2017-08-09T23:32:50.270","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-10T09:41:06.810",{"$f":"IF(ISBLANK(A72),\" \",((A72)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-09T23:41:06.810"},"DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-10T09:45:55.220","2017-08-09T23:45:55.220","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-10T09:51:53.210","2017-08-09T23:51:53.210","DF","Sonar","Multibeam","Max Angle","52/52"]
["2017-08-10T09:54:01.040","2017-08-09T23:54:01.040","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-10T10:04:51.760","2017-08-10T00:04:51.760","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-10T10:07:47.820","2017-08-10T00:07:47.820","DF","Sonar","Multibeam","Max Angle","31/31"]
["2017-08-10T10:10:09.180","2017-08-10T00:10:09.180","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-10T10:29:34.940","2017-08-10T00:29:34.940","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-10T10:29:42.250","2017-08-10T00:29:42.250","DF","Sonar","Multibeam","Max Angle","52/52"]
["2017-08-10T11:22:23.220","2017-08-10T01:22:23.220","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-10T11:22:35.660","2017-08-10T01:22:35.660","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-10T11:23:23.020","2017-08-10T01:23:23.020","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-10T11:23:36.900","2017-08-10T01:23:36.900","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-08-10T11:28:04.290","2017-08-10T01:28:04.290","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-10T11:28:29.020","2017-08-10T01:28:29.020","DF","Sonar","Multibeam","Max Angle","60/60"]
["2017-08-10T11:28:37.540","2017-08-10T01:28:37.540","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-10T11:37:51.390","2017-08-10T01:37:51.390","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-10T11:46:28.450","2017-08-10T01:46:28.450","DF","Sonar","Multibeam","New Line","begin turn line 0019"]
["2017-08-10T11:51:58.150","2017-08-10T01:51:58.150","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-10T11:52:33.790","2017-08-10T01:52:33.790","DF","Sonar","Multibeam","New Line","begin survey line 0020, Start Blackfin survey - survey speed"]
["2017-08-10T11:56:03.050","2017-08-10T01:56:03.050","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-10T12:12:33.320","2017-08-10T02:12:33.320","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-10T13:29:07.710","2017-08-10T03:29:07.710","DF","Sonar","Multibeam","Max Angle","65/65"]
["2017-08-10T13:29:46.330","2017-08-10T03:29:46.330","DF","Sonar","Multibeam","Max Angle","70/70"]
["2017-08-10T14:10:40.120","2017-08-10T04:10:40.120","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-10T14:35:52.350","2017-08-10T04:35:52.350","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-10T14:51:46.760","2017-08-10T04:51:46.760","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-10T15:20:57.070","2017-08-10T05:20:57.070","DF","Sonar","Multibeam","New Line","begin turn line 0024"]
["2017-08-10T15:33:58.150","2017-08-10T05:33:58.150","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-10T15:41:36.880","2017-08-10T05:41:36.880","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-10T15:47:15.650","2017-08-10T05:47:15.650","DF","Sonar","Multibeam","New Line","Begin survey line 0025"]
["2017-08-10T16:21:31.520","2017-08-10T06:21:31.520","DF","XBT",null,null,"Cast 006 applied to line 0025"]
["2017-08-10T16:22:19.910","2017-08-10T06:22:19.910","DF","Ship",null,null,"moved ship 1500 m to port for next line; then moved 500 m back for 1/3 coverage"]
["2017-08-10T16:27:36.020","2017-08-10T06:27:36.020","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-10T16:42:43.110","2017-08-10T06:42:43.110","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-10T17:13:55.070","2017-08-10T07:13:55.070","DF","Sonar","Knudsen","TX Pulse","2 ms"]
["2017-08-10T17:15:41.460","2017-08-10T07:15:41.460","DF","Sonar","Knudsen","TX Pulse","4 ms"]
["2017-08-10T17:19:13.040","2017-08-10T07:19:13.040","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-10T17:25:38.320","2017-08-10T07:25:38.320","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-10T18:03:40.580","2017-08-10T08:03:40.580","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-10T18:21:27","2017-08-10T08:21:27","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-10T18:39:34.080","2017-08-10T08:39:34.080","AB","Sonar","Knudsen",null,"needle gunning interference in SBP. Other data streams unaffected. Not on main feature. Approaching transit line."]
["2017-08-10T19:10:59.940","2017-08-10T09:10:59.940","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-10T19:14:19.950","2017-08-10T09:14:19.950","AB","Sonar","Multibeam",null,"New line 0030. Turn"]
["2017-08-10T19:16:30.380","2017-08-10T09:16:30.380","AB","Sonar",null,null,"New MB line 0031. New EK and SBP lines started. SBP interefence from deck work near sbp room."]
["2017-08-10T19:18:42","2017-08-10T09:18:42","AB","Ship",null,null,"Increase to transit speed"]
["2017-08-10T19:28:53.440","2017-08-10T09:28:53.440","AB","Sonar","Knudsen","Phase Range","1500-2500, new line"]
["2017-08-10T19:51:00.830","2017-08-10T09:51:00.830","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-10T19:56:20.680","2017-08-10T09:56:20.680","AB","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-10T19:56:44.090","2017-08-10T09:56:44.090","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-10T20:04:39.310","2017-08-10T10:04:39.310","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-10T20:08:27.240","2017-08-10T10:08:27.240","AB","Sonar","EK","Change Range","6000m"]
["2017-08-10T20:08:56.600","2017-08-10T10:08:56.600","AB","Sonar","Multibeam","Max Angle","35/35, auto: extra deep mode. Transit speed is 10-11 kts."]
["2017-08-10T22:20:14","2017-08-10T12:20:14","AB","XBT",null,null,7]
["2017-08-10T22:25:36.210","2017-08-10T12:25:36.210","AB","Sonar","Multibeam",null,"XBT007 added to new line 35"]
["2017-08-10T23:51:03.440","2017-08-10T13:51:03.440","AB","Sonar","Multibeam","Ping Mode","Very Deep, 52/52"]
["2017-08-10T23:51:42.740","2017-08-10T13:51:42.740","AB","Sonar","Knudsen","Phase Range","4000-5000 - noisy from engineering repairs"]
["2017-08-10T23:59:34.740","2017-08-10T13:59:34.740","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T00:05:55.010","2017-08-10T14:05:55.010","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-11T00:13:09.240","2017-08-10T14:13:09.240","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-11T00:14:00","2017-08-10T14:14:00","AB","Sonar","Multibeam","Ping Mode","Deep, 60/60, new line 0037"]
["2017-08-11T00:16:55.490","2017-08-10T14:16:55.490","AB","Sonar","Knudsen","Phase Range","2000-3000, Gain 34"]
["2017-08-11T00:39:25.200","2017-08-10T14:39:25.200","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-08-11T00:48:46.750","2017-08-10T14:48:46.750","AB","Sonar","Knudsen","Phase Range","3000-4000m, Gain 36"]
["2017-08-11T00:50:24.030",{"$f":"IF(ISBLANK(A136),\" \",((A136)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-10T14:50:24.030"},"AB","Sonar","Multibeam","Ping Mode","Very Deep, new line 0038, 52/52"]
["2017-08-11T00:51:59.070","2017-08-10T14:51:59.070","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-08-11T00:58:50.250","2017-08-10T14:58:50.250","AB","Sonar","Knudsen","Phase Range","4000-5000m, pulse 8ms"]
["2017-08-11T01:09:22.250","2017-08-10T15:09:22.250","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-08-11T01:14:57.250","2017-08-10T15:14:57.250","AB","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-11T01:43:30.840","2017-08-10T15:43:30.840","AB","Sonar","Multibeam","New Line","0039"]
["2017-08-11T02:56:40.420","2017-08-10T16:56:40.420","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-11T05:08:09.680","2017-08-10T19:08:09.680","CW","XBT",null,null,"XBT 008; applied to SIS line 0042"]
["2017-08-11T08:06:27.650","2017-08-10T22:06:27.650","CW","Sonar","All",null,"New lines for fancy survey. SIS line 0045"]
["2017-08-11T08:07:13.680","2017-08-10T22:07:13.680","CW","Ship",null,null,"Survey speed 8.5-9kts"]
["2017-08-11T08:39:05.880","2017-08-10T22:39:05.880","CW","Sonar","Knudsen","Tx Power",3]
["2017-08-11T09:24:01.150","2017-08-10T23:24:01.150","DF","Sonar","Knudsen",null,"2500-3500, TX power 2, TX pulse 2"]
["2017-08-11T09:51:07.360","2017-08-10T23:51:07.360","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-11T10:14:10.510","2017-08-11T00:14:10.510","CW","XBT",null,null,"XBT 009; applied to SIS line 0047"]
["2017-08-11T10:38:53.390","2017-08-11T00:38:53.390","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-11T10:59:13.440","2017-08-11T00:59:13.440","DF","Sonar","Multibeam","New Line","begin turn line 0049"]
["2017-08-11T11:05:34.700","2017-08-11T01:05:34.700","DF","Sonar","Multibeam","New Line","begin survey line 0050"]
["2017-08-11T11:35:06.010","2017-08-11T01:35:06.010","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-08-11T11:35:15.960","2017-08-11T01:35:15.960","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-11T11:53:06.260","2017-08-11T01:53:06.260","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T12:23:43.190","2017-08-11T02:23:43.190","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-11T12:35:02.780","2017-08-11T02:35:02.780","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T12:42:31.920","2017-08-11T02:42:31.920","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-11T13:52:00.930","2017-08-11T03:52:00.930","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T14:01:02.080","2017-08-11T04:01:02.080","DF","Sonar","Multibeam","New Line","begin turn line 0053"]
["2017-08-11T14:08:41.790","2017-08-11T04:08:41.790","DF","Sonar","Multibeam","New Line","begin survey line 0054"]
["2017-08-11T14:19:15.330","2017-08-11T04:19:15.330","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-11T14:55:30.180","2017-08-11T04:55:30.180","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-11T15:13:58.120","2017-08-11T05:13:58.120","DF","Sonar","Multibeam","New Line","begin turn line 0056"]
["2017-08-11T15:14:38.410","2017-08-11T05:14:38.410","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-11T15:15:04.570","2017-08-11T05:15:04.570","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-11T15:34:03.660","2017-08-11T05:34:03.660","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-11T15:34:11.790","2017-08-11T05:34:11.790","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-11T15:42:46.400","2017-08-11T05:42:46.400","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T16:08:34.580","2017-08-11T06:08:34.580","DF","XBT",null,null,"Cast 010 applied to line 0057"]
["2017-08-11T16:10:08.940","2017-08-11T06:10:08.940","DF","Sonar","Knudsen",null,"TX Power - 2, TX Pulse - 4"]
["2017-08-11T16:44:10.260","2017-08-11T06:44:10.260","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-11T17:16:38.310","2017-08-11T07:16:38.310","DF","Issue/Problem","Multibeam",null,"The 1 sensor light went red briefly then went green"]
["2017-08-11T17:33:06.770","2017-08-11T07:33:06.770","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T17:34:53.030","2017-08-11T07:34:53.030","AB","Sonar","Knudsen","Phase Range","4000-5000, Pulse 4"]
["2017-08-11T17:41:32.440","2017-08-11T07:41:32.440","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-11T17:56:28.290","2017-08-11T07:56:28.290","AB","Sonar","Knudsen","Tx Power","3, Tx Pulse 8"]
["2017-08-11T18:30:59.430","2017-08-11T08:30:59.430","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-11T18:48:40.430","2017-08-11T08:48:40.430","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-11T19:14:27.140","2017-08-11T09:14:27.140","AB","Sonar","Multibeam","New Line","0061, small degree turn toward fracture zone"]
["2017-08-11T19:17:17.420","2017-08-11T09:17:17.420","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-11T19:18:06.180","2017-08-11T09:18:06.180","AB","Ship",null,null,"Increase to warp speed"]
["2017-08-11T19:45:11.630","2017-08-11T09:45:11.630","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-11T20:42:31.820","2017-08-11T10:42:31.820","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-11T21:25:28.880","2017-08-11T11:25:28.880","BO","XBT",null,null,"011 added to line 63"]
["2017-08-11T22:21:47.810","2017-08-11T12:21:47.810","AB","Sonar","Multibeam","Ping Mode","Extra Deep, 35/35, New line 65"]
["2017-08-11T23:27:55.840","2017-08-11T13:27:55.840","AB","Other",null,null,"TSG turned off for welding leaky pipe. "]
["2017-08-12T00:18:02.620","2017-08-11T14:18:02.620","AB",null,null,null,"Sunphotometer Readings"]
["2017-08-12T00:25:18.270","2017-08-11T14:25:18.270","AB","Sonar","Multibeam","New Line","0067"]
["2017-08-12T00:31:31.950","2017-08-11T14:31:31.950","AB","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-12T00:35:08","2017-08-11T14:35:08","AB",null,null,null,"TSG back on"]
["2017-08-12T00:44:51.710","2017-08-11T14:44:51.710","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T01:20:24.790","2017-08-11T15:20:24.790","AB","Sonar",null,null,"All new lines started. Started Fracture Zone area. New line 68. Speed reduced to 8.5 to 9 knts"]
["2017-08-12T02:26:44.970","2017-08-11T16:26:44.970","CW","Sonar","Knudsen",null,"TVG Mode: 5logR"]
["2017-08-12T02:27:28.480","2017-08-11T16:27:28.480","CW","Sonar","Knudsen",null,"Pulse 4; Power 2; Gain 28"]
["2017-08-12T03:25:02.260","2017-08-11T17:25:02.260","CW","POS",null,null,"Dropouts like cray cray"]
["2017-08-12T04:30:58.760","2017-08-11T18:30:58.760","CT","XBT",null,null,"XBT 012, applies to SIS line 0071"]
["2017-08-12T09:38:25.490","2017-08-11T23:38:25.490","CW","XBT",null,null,"XBT 013; applied to SIS line 0076"]
["2017-08-12T10:39:58.590","2017-08-12T00:39:58.590","DF","Issue/Problem","Multibeam",null,"Position input missing error, went away within seconds"]
["2017-08-12T10:55:25.310","2017-08-12T00:55:25.310","DF","Issue/Problem","Multibeam",null,"Position input missing error, went away within seconds"]
["2017-08-12T11:08:02.810",{"$f":"IF(ISBLANK(A201),\" \",((A201)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-12T01:08:02.810"},"DF","Sonar","Multibeam","New Line","begin turn line 0078"]
["2017-08-12T11:31:32.260","2017-08-12T01:31:32.260","DF","Sonar","Multibeam","New Line","begin survey line 0079"]
["2017-08-12T11:39:55.250","2017-08-12T01:39:55.250","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T11:50:03.120","2017-08-12T01:50:03.120","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-12T11:59:15.160","2017-08-12T01:59:15.160","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-12T13:39:03.260","2017-08-12T03:39:03.260","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T13:57:37.180","2017-08-12T03:57:37.180","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-12T14:08:11.360","2017-08-12T04:08:11.360","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T14:43:11.350","2017-08-12T04:43:11.350","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-12T15:49:49.630","2017-08-12T05:49:49.630","DF","XBT",null,null,"Cast 014 applied to line 0083"]
["2017-08-12T16:29:57.380","2017-08-12T06:29:57.380","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T16:30:17.570","2017-08-12T06:30:17.570","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-12T16:45:01.010","2017-08-12T06:45:01.010","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T17:29:18.240","2017-08-12T07:29:18.240","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-12T17:55:46.340","2017-08-12T07:55:46.340","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-12T18:16:48.340","2017-08-12T08:16:48.340","BO","Other",null,null,"sun photometer"]
["2017-08-12T18:34:01","2017-08-12T08:34:01","AB","Sonar","Multibeam","New Line",86]
["2017-08-12T20:10:10.700","2017-08-12T10:10:10.700","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-12T20:18:02.600","2017-08-12T10:18:02.600","BO","Other",null,null,"sun photometer"]
["2017-08-12T21:07:29.030","2017-08-12T11:07:29.030","AB","Issue/Problem","Multibeam","Warning","Red position light error"]
["2017-08-12T21:09:05.080","2017-08-12T11:09:05.080","AB","Sonar","Multibeam",null,"Swath 6200m in 5700m of water"]
["2017-08-12T21:32:28.490","2017-08-12T11:32:28.490","AB","Sonar","Multibeam","New Line",89]
["2017-08-12T22:00:37","2017-08-12T12:00:37","CT","Other",null,null,"sun photometer"]
["2017-08-12T22:35:51","2017-08-12T12:35:51","AB","XBT",null,null,"14 - canceled at 321m"]
["2017-08-12T22:40:18","2017-08-12T12:40:18","AB","XBT",null,null,15]
["2017-08-12T22:47:34.440","2017-08-12T12:47:34.440","AB","Sonar","Multibeam",null,"XBT 15 added to new line 0091"]
["2017-08-12T23:07:35.790","2017-08-12T13:07:35.790","AB","Sonar","Knudsen","Gain Value","21 5logR"]
["2017-08-12T23:16:14.830","2017-08-12T13:16:14.830","AB","Sonar","Multibeam","New Line","92 turn line, new ek and sbp started"]
["2017-08-12T23:42:11.390","2017-08-12T13:42:11.390","AB","Sonar","All",null,"New lines started (MB line 93)"]
["2017-08-13T01:02:44.560","2017-08-12T15:02:44.560","CT","Other",null,null,"sun photometer"]
["2017-08-13T05:26:07.980","2017-08-12T19:26:07.980","CW","XBT",null,null,"XBT 017; applied to SIS line 0098"]
["2017-08-13T08:57:57.050","2017-08-12T22:57:57.050","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-08-13T09:53:06.570","2017-08-12T23:53:06.570","CW","XBT",null,null,"XBT 018; applied to SIS line 0103"]
["2017-08-13T12:21:37.160","2017-08-13T02:21:37.160","DF","Sonar","Multibeam","Aeration Filter (On/Off)","ON"]
["2017-08-13T12:24:44.150","2017-08-13T02:24:44.150","DF","Sonar","Multibeam","New Line","begin survey line 0107, new ek and SBP lines"]
["2017-08-13T12:25:13.400","2017-08-13T02:25:13.400","DF","Sonar","Multibeam","Along Direction Pitch",{"$f":"0-0.5","v":-0.5}]
["2017-08-13T12:31:28.030","2017-08-13T02:31:28.030","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-13T12:33:32.320","2017-08-13T02:33:32.320","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-13T12:45:17.790","2017-08-13T02:45:17.790","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-08-13T13:12:12.580","2017-08-13T03:12:12.580","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-13T16:26:25.060","2017-08-13T06:26:25.060","DF","XBT",null,null,"Cast 019 applied to line 0111"]
["2017-08-13T18:45:05.190","2017-08-13T08:45:05.190","AB","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-13T19:19:18.050","2017-08-13T09:19:18.050","AB","Sonar","Multibeam",null,"Slope filter off, range gate normal over features"]
["2017-08-13T19:25:02","2017-08-13T09:25:02","AB","Sonar","Multibeam","New Line",114]
["2017-08-13T20:04:28.680","2017-08-13T10:04:28.680","AB","Sonar","Multibeam",null,"Slope on, range small; Eric's horns in data over flat area"]
["2017-08-13T21:04:01.970","2017-08-13T11:04:01.970","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-13T21:25:02","2017-08-13T11:25:02","AB","Sonar","Multibeam","New Line",116]
["2017-08-13T22:16:26.610","2017-08-13T12:16:26.610","AB","XBT"]
["2017-08-13T22:21:21.800","2017-08-13T12:21:21.800","AB","Sonar","Multibeam",null,"XBT20 added to new line 117"]
["2017-08-13T22:28:53.180","2017-08-13T12:28:53.180","CT","Other",null,null,"Sun photometer"]
["2017-08-14T00:14:00.120","2017-08-13T14:14:00.120","AB","Sonar","All",null,"All new lines started (MB line 0119)"]
["2017-08-14T00:39:30.950","2017-08-13T14:39:30.950","CW","Sonar","All",null,"New Survey Lines. SIS line 0120"]
["2017-08-14T00:43:32.660","2017-08-13T14:43:32.660","CT","Other",null,null,"Sun photometer"]
["2017-08-14T02:41:06","2017-08-13T16:41:06","AB","Sonar","Multibeam","New Line",122]
["2017-08-14T03:39:20.490","2017-08-13T17:39:20.490","AB","Sonar","Multibeam","New Line",123]
["2017-08-14T03:47:07.680","2017-08-13T17:47:07.680","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-14T04:01:01.180","2017-08-13T18:01:01.180","AB","Sonar","Knudsen","Phase Range","5000-6000, Gain 21 5LogR"]
["2017-08-14T04:40:51.900","2017-08-13T18:40:51.900","CW","XBT",null,null,"XBT 021; applied to SIS line 0124"]
["2017-08-14T09:44:39.930","2017-08-13T23:44:39.930","DF","XBT",null,null,"Cast 022 applied to line 0129"]
["2017-08-14T10:03:17.070","2017-08-14T00:03:17.070","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-14T10:27:04.910","2017-08-14T00:27:04.910","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T12:16:18.540","2017-08-14T02:16:18.540","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-14T12:44:59.920","2017-08-14T02:44:59.920","DF","Sonar","Multibeam","New Line","begin turn line 0133, new ek and sbp line"]
["2017-08-14T13:09:44.730","2017-08-14T03:09:44.730","DF","Sonar","Multibeam","New Line","begin survey line 0134, new ek and sbp line"]
["2017-08-14T15:14:45.060","2017-08-14T05:14:45.060","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T15:42:11.650",{"$f":"IF(ISBLANK(A266),\" \",((A266)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-14T05:42:11.650"},"DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-14T15:58:18.360","2017-08-14T05:58:18.360","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T16:05:45.150","2017-08-14T06:05:45.150","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-14T16:27:49.660","2017-08-14T06:27:49.660","DF","XBT",null,null,"Cast 023 applied to line 0137"]
["2017-08-14T16:39:27.930","2017-08-14T06:39:27.930","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T17:36:15.120","2017-08-14T07:36:15.120","AB","Sonar","Multibeam",null,"Comm Error"]
["2017-08-14T18:38:12.870","2017-08-14T08:38:12.870","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-14T19:11:02.910","2017-08-14T09:11:02.910","AB","Sonar","Multibeam","New Line",140]
["2017-08-14T19:27:36.180","2017-08-14T09:27:36.180","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T19:33:10.350","2017-08-14T09:33:10.350","AB","Sonar","Knudsen","Phase Range","5500-6000"]
["2017-08-14T19:42:29.430","2017-08-14T09:42:29.430","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T19:47:02.750","2017-08-14T09:47:02.750","AB","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-14T20:38:27.440","2017-08-14T10:38:27.440","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-14T21:17:47.530","2017-08-14T11:17:47.530","AB","Sonar","Multibeam","New Line",142]
["2017-08-14T22:40:44.160","2017-08-14T12:40:44.160","AB","XBT",null,null,"2 failed casts (1 400m long, and one with bottom anomaly and no nav string)"]
["2017-08-14T22:40:56.870","2017-08-14T12:40:56.870","AB","Sonar","Multibeam",null,"XBT26 added to new mb line 0144"]
["2017-08-14T23:42:03.930","2017-08-14T13:42:03.930","AB","Sonar","Multibeam","New Line",145]
["2017-08-15T00:06:25.170","2017-08-14T14:06:25.170","AB","Ship",null,null,"Adjust speed to 8.5-9 knts. Slowing down because of current about 0.5 knts"]
["2017-08-15T00:46:51.390","2017-08-14T14:46:51.390","AB","Sonar","Multibeam","New Line",146]
["2017-08-15T01:07:19.170","2017-08-14T15:07:19.170","AB","All",null,null,"New lines started for turn (MB 147)"]
["2017-08-15T01:10:21.450","2017-08-14T15:10:21.450","AB","Sonar","Multibeam",null,"Yaw stabilization reset during the turn"]
["2017-08-15T01:31:34.310","2017-08-14T15:31:34.310","AB","All",null,"New Line","New lines started after turn (MB 148)"]
["2017-08-15T01:38:01","2017-08-14T15:38:01","AB","Sonar","Multibeam","Along Direction Pitch","-1;  motion and wind waves affecting the data going north"]
["2017-08-15T02:40:53.900","2017-08-14T16:40:53.900","AB","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-15T05:22:29.010","2017-08-14T19:22:29.010","CW","XBT",null,null,"XBT 027; applied to SIS line 0151"]
["2017-08-15T06:16:33","2017-08-14T20:16:33","CW","Ship",null,null,"Line plan changed to 4700 m spacing"]
["2017-08-15T09:48:00.530","2017-08-14T23:48:00.530","DF","XBT",null,null,"Cast 028 applied to line 0156"]
["2017-08-15T10:18:19.810","2017-08-15T00:18:19.810","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-15T11:37:25.550","2017-08-15T01:37:25.550","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-15T13:16:44.070","2017-08-15T03:16:44.070","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-15T13:21:20.130","2017-08-15T03:21:20.130","DF","Sonar","Multibeam","New Line","begin turn line 0160, new ek and sbp line"]
["2017-08-15T13:47:18.020","2017-08-15T03:47:18.020","DF","Sonar","Multibeam","New Line","begin survey line 0161, new ek and sbp line"]
["2017-08-15T14:45:52.800","2017-08-15T04:45:52.800","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-15T15:49:23.360","2017-08-15T05:49:23.360","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-15T15:59:15.710","2017-08-15T05:59:15.710","DF","XBT",null,null,"Cast 029 applied to line 0163"]
["2017-08-15T16:59:02.390","2017-08-15T06:59:02.390","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-15T19:47:19.780","2017-08-15T09:47:19.780","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-15T19:58:04.170","2017-08-15T09:58:04.170","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-15T20:00:28.530","2017-08-15T10:00:28.530","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-15T20:35:11.870","2017-08-15T10:35:11.870","BO","Sonar","Knudsen","Phase Range","6000-7000; also bumped gain up to 21"]
["2017-08-15T20:45:41.310","2017-08-15T10:45:41.310","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-15T20:48:36","2017-08-15T10:48:36","AB","Sonar","Multibeam","New Line","0168"]
["2017-08-15T21:44:18.210","2017-08-15T11:44:18.210","AB","XBT",null,null,30]
["2017-08-15T21:57:04.180","2017-08-15T11:57:04.180","BO","XBT",null,null,"applied cast 30 to line 0169"]
["2017-08-15T22:35:49","2017-08-15T12:35:49","CT","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-15T23:08:40.940","2017-08-15T13:08:40.940","AB","Sonar","Knudsen","Gain Value","20 5logR"]
["2017-08-16T00:48:01.580","2017-08-15T14:48:01.580","AB","Sonar","Multibeam","New Line",172]
["2017-08-16T01:08:42.140","2017-08-15T15:08:42.140","CT","Sun photometer",null,null,"Sun photometer"]
["2017-08-16T01:31:51.940","2017-08-15T15:31:51.940","AB","Sonar","All","New Line","All new lines started for turn (MB line 0173)"]
["2017-08-16T01:53:20.600","2017-08-15T15:53:20.600","AB","Ship",null,null,"reduce to 100RPMs for engineering tests"]
["2017-08-16T01:54:46.140","2017-08-15T15:54:46.140","AB","Sonar","All",null,"All new lines started after turn (MB0174)"]
["2017-08-16T04:50:44.330","2017-08-15T18:50:44.330","CT","XBT",null,null,"031 at line 0176"]
["2017-08-16T06:26:33.840","2017-08-15T20:26:33.840","CW","Sonar","Knudsen",null,"SBP computer crash. Lame-o"]
["2017-08-16T06:34:16.020","2017-08-15T20:34:16.020","CW","Sonar","Knudsen",null,"Okay, all good now. Restarted and recording with remote connection. Recording started with SBP line 132. "]
["2017-08-16T06:35:16.900","2017-08-15T20:35:16.900","CW","Sonar","Knudsen",null,"Pulse 8; Power 3; Gain 21 / 5logR"]
["2017-08-16T08:11:58.690","2017-08-15T22:11:58.690","CW","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-08-16T09:26:02.530","2017-08-15T23:26:02.530","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T10:06:21.580","2017-08-16T00:06:21.580","DF","XBT",null,null,"Cast 032 applied to line 0182"]
["2017-08-16T10:32:16.090","2017-08-16T00:32:16.090","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-16T10:43:20.910","2017-08-16T00:43:20.910","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T11:53:49.010","2017-08-16T01:53:49.010","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-16T13:10:26.250","2017-08-16T03:10:26.250","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T13:43:51.730","2017-08-16T03:43:51.730","DF","Sonar","Multibeam","New Line","begin turn line 0186, new ek and sbp lines"]
["2017-08-16T14:07:21.580","2017-08-16T04:07:21.580","DF","Sonar","Multibeam","New Line","begin survey 0187, new ek and sbp lines"]
["2017-08-16T15:20:40.010",{"$f":"IF(ISBLANK(A330),\" \",((A330)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-16T05:20:40.010"},"DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-16T15:57:14.840","2017-08-16T05:57:14.840","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T16:27:25.340","2017-08-16T06:27:25.340","BO","XBT",null,null,"XBT 033"]
["2017-08-16T16:31:07.710","2017-08-16T06:31:07.710","BO","XBT",null,null,"Cast 033 applied to line 0189"]
["2017-08-16T17:13:23.610","2017-08-16T07:13:23.610","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-16T19:10:27.110","2017-08-16T09:10:27.110","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T19:14:17.900","2017-08-16T09:14:17.900","BO","Ship",null,null,"Ship slowed down for five minutes to test thrusters, then came back up to survey speed"]
["2017-08-16T19:31:25.860","2017-08-16T09:31:25.860","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-16T20:09:48.710","2017-08-16T10:09:48.710","AB","Sonar","Multibeam","New Line","0193"]
["2017-08-16T20:21:22.570","2017-08-16T10:21:22.570","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T20:28:21.400","2017-08-16T10:28:21.400","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-16T20:42:35.860","2017-08-16T10:42:35.860","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T20:50:57.180","2017-08-16T10:50:57.180","BO","Sonar","Knudsen","Phase Range","6000-7000"]
["2017-08-16T21:07:45.450","2017-08-16T11:07:45.450","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-16T21:45:31.800","2017-08-16T11:45:31.800","BO","XBT",null,null,"Cast 034, applied to line 0194"]
["2017-08-16T22:37:41.690","2017-08-16T12:37:41.690","CT",null,null,null,"Changed the phase to 5000-6000"]
["2017-08-16T23:11:16.100","2017-08-16T13:11:16.100","AB",null,null,null,"Fire Drill"]
["2017-08-16T23:11:27.380","2017-08-16T13:11:27.380","AB","Sonar","Knudsen","Gain Value","20 5logR"]
["2017-08-16T23:32:45.160","2017-08-16T13:32:45.160","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T00:46:40.230","2017-08-16T14:46:40.230","CT","Other",null,null,"Sun photometer"]
["2017-08-17T01:05:28.650","2017-08-16T15:05:28.650","AB","Sonar","Multibeam","New Line","0198, along direction -1"]
["2017-08-17T01:57:30.380","2017-08-16T15:57:30.380","AB","all",null,"New Line","New lines started for turn (MBES 0199)"]
["2017-08-17T02:18:27.120","2017-08-16T16:18:27.120","AB","all",null,"New Line","New lines started after turn (MB 200)"]
["2017-08-17T04:31:52.010","2017-08-16T18:31:52.010","CT","XBT",null,null,"Cast 035, applied to line 0202"]
["2017-08-17T05:03:03.160","2017-08-16T19:03:03.160","CW","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-17T09:57:07.390","2017-08-16T23:57:07.390","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T09:57:15.990","2017-08-16T23:57:15.990","DF","XBT",null,null,"Cast 036 applied to line 207"]
["2017-08-17T11:21:02.360","2017-08-17T01:21:02.360","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-17T12:40:14.060","2017-08-17T02:40:14.060","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T14:12:48.340","2017-08-17T04:12:48.340","DF","Sonar","Multibeam","New Line","begin turn line 0212, new ek and sbp lines"]
["2017-08-17T14:31:09.540","2017-08-17T04:31:09.540","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-17T14:34:22.410","2017-08-17T04:34:22.410","DF","Sonar","Multibeam","New Line","begin survey line 0213, new ek and sbp lines"]
["2017-08-17T15:29:29.930","2017-08-17T05:29:29.930","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T16:25:25.470","2017-08-17T06:25:25.470","BO","XBT",null,null,"Cast 037, applied to line 0214"]
["2017-08-17T16:26:31.390","2017-08-17T06:26:31.390","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-17T17:34:05.200","2017-08-17T07:34:05.200","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T18:07:43.480","2017-08-17T08:07:43.480","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-17T18:25:50.910","2017-08-17T08:25:50.910","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T18:34:30.620","2017-08-17T08:34:30.620","AB","Sonar","Multibeam","New Line",217]
["2017-08-17T19:25:54.550","2017-08-17T09:25:54.550","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-17T19:37:40.640","2017-08-17T09:37:40.640","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T19:40:19","2017-08-17T09:40:19","AB","Sonar","Multibeam","New Line",218]
["2017-08-17T19:55:01.740","2017-08-17T09:55:01.740","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-17T20:18:29.970","2017-08-17T10:18:29.970","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-17T20:39:17.650","2017-08-17T10:39:17.650","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-17T20:41:32.300","2017-08-17T10:41:32.300","AB","Sonar","Multibeam","New Line",219]
["2017-08-17T20:48:04.010","2017-08-17T10:48:04.010","BO","Sonar","Knudsen","Phase Range","6000-7000"]
["2017-08-17T21:03:53.530","2017-08-17T11:03:53.530","AB","Ship",null,null,"way point control "]
["2017-08-17T21:05:16.210","2017-08-17T11:05:16.210","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-17T22:27:15.160","2017-08-17T12:27:15.160","CT","XBT",null,null,"Cast 038 canceled out, cast 039 at line 0220"]
["2017-08-18T00:36:18.850","2017-08-17T14:36:18.850","AB","Sonar","Multibeam","New Line","0223"]
["2017-08-18T02:01:22.480","2017-08-17T16:01:22.480","AB","Sonar","All",null,"New lines started on all sonars (MBES 225)"]
["2017-08-18T02:28:23.250","2017-08-17T16:28:23.250","CW","Sonar","All",null,"New lines started on all sonars (MBES 226)"]
["2017-08-18T04:48:16.090","2017-08-17T18:48:16.090","CT","XBT",null,null,"Cast 040 at line 0228"]
["2017-08-18T09:09:51.570","2017-08-17T23:09:51.570","CW","Sonar","Multibeam",null,"Never seen this before, but SIS went into Shallow Ping Mode and therefore couldn't find bottom. Wasn't even KVM'd into MB. Took a few moments to figure it out. Lost some data. Crapcrapcrap. "]
["2017-08-18T09:54:52.580","2017-08-17T23:54:52.580","CW","XBT",null,null,"XBT 041; applied to SIS line 0233"]
["2017-08-18T11:17:12.010","2017-08-18T01:17:12.010","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-18T12:55:36.790","2017-08-18T02:55:36.790","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-18T12:57:17.210","2017-08-18T02:57:17.210","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-08-18T14:11:00.970","2017-08-18T04:11:00.970","DF","Sonar","Multibeam","New Line","begin turn line 0238, new ek and sbp lines"]
["2017-08-18T14:33:18.670","2017-08-18T04:33:18.670","DF","Sonar","Multibeam","New Line","begin survey line 0239, new ek and sbp lines"]
["2017-08-18T15:59:49.380","2017-08-18T05:59:49.380","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-18T16:10:35.270","2017-08-18T06:10:35.270","DF","XBT",null,null,"Cast 042 applied to line 0240"]
["2017-08-18T16:19:30.550","2017-08-18T06:19:30.550","DF","Sonar","Knudsen","Phase Range","6000-7000"]
["2017-08-18T16:26:54.340",{"$f":"IF(ISBLANK(A394),\" \",((A394)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-18T06:26:54.340"},"DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-18T16:37:27.190","2017-08-18T06:37:27.190","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-18T17:07:04.450","2017-08-18T07:07:04.450","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-18T17:35:50.430","2017-08-18T07:35:50.430","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-18T18:20:25.380","2017-08-18T08:20:25.380","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-18T18:36:55.930","2017-08-18T08:36:55.930","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-18T19:17:29.230","2017-08-18T09:17:29.230","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-18T19:34:35.390","2017-08-18T09:34:35.390","AB","Sonar","Multibeam","New Line",244]
["2017-08-18T19:58:16.350","2017-08-18T09:58:16.350","AB","Sonar","Multibeam","New Line","245 turn to pick up holiday."]
["2017-08-18T20:18:29.720","2017-08-18T10:18:29.720","AB","Sonar","All",null,"New line 246, holdiay line in MBES. New lines started in EK and SBP."]
["2017-08-18T20:29:22.870","2017-08-18T10:29:22.870","AB","Sonar","Multibeam","New Line","turn after holiday, line 247"]
["2017-08-18T20:49:31.800","2017-08-18T10:49:31.800","AB","Sonar","All",null,"New lines started on all sonars. (MB 248). Holiday filled."]
["2017-08-18T22:29:08","2017-08-18T12:29:08","AB","XBT",null,null,"cast 43 on line 0249"]
["2017-08-19T00:51:06.270","2017-08-18T14:51:06.270","AB","Sonar","Multibeam","New Line",252]
["2017-08-19T00:51:20.940","2017-08-18T14:51:20.940","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T01:52:27.880","2017-08-18T15:52:27.880","AB","Sonar","Multibeam","New Line",253]
["2017-08-19T02:50:17.040","2017-08-18T16:50:17.040","AB","Sonar","Multibeam","New Line",254]
["2017-08-19T03:20:58.060","2017-08-18T17:20:58.060","CW","All",null,"New Line","New lines for turn. SIS line 0255"]
["2017-08-19T03:42:06.550","2017-08-18T17:42:06.550","AB","All",null,"New Line","New lines for end of turn. SIS line 256"]
["2017-08-19T04:43:33.450","2017-08-18T18:43:33.450","CW","XBT",null,null,"XBT 044; applied to SIS line 0257"]
["2017-08-19T09:22:17.330","2017-08-18T23:22:17.330","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-08-19T09:24:30.150","2017-08-18T23:24:30.150","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-19T09:29:35.460","2017-08-18T23:29:35.460","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T09:58:51.710","2017-08-18T23:58:51.710","CW","XBT",null,null,"XBT 45; applied to SIS line 0262"]
["2017-08-19T10:52:34.890","2017-08-19T00:52:34.890","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-19T11:42:29.820","2017-08-19T01:42:29.820","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T12:48:20.710","2017-08-19T02:48:20.710","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-19T13:24:17.750","2017-08-19T03:24:17.750","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T13:24:38.210","2017-08-19T03:24:38.210","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-19T13:31:55.520","2017-08-19T03:31:55.520","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T13:40:01.970","2017-08-19T03:40:01.970","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-19T13:44:19.360","2017-08-19T03:44:19.360","DF","Sonar","Knudsen","Phase Range","6000-7000"]
["2017-08-19T13:51:52.320","2017-08-19T03:51:52.320","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-19T14:02:55.620","2017-08-19T04:02:55.620","DF","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-19T14:06:58.220","2017-08-19T04:06:58.220","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T15:33:48.400","2017-08-19T05:33:48.400","DF","Sonar","Multibeam","New Line","begin turn line 0268"]
["2017-08-19T15:50:41.260","2017-08-19T05:50:41.260","DF","Sonar","Multibeam","New Line","begin transit line 0269, new ek and sbp lines"]
["2017-08-19T15:51:04.600","2017-08-19T05:51:04.600","DF","Ship",null,null,"transit speed; slowing down to survey speed over target seamounts"]
["2017-08-19T16:10:22.530","2017-08-19T06:10:22.530","DF","XBT",null,null,"Cast 046 applied to line 0269"]
["2017-08-19T17:00:59.340","2017-08-19T07:00:59.340","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-19T19:48:32.070","2017-08-19T09:48:32.070","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-19T20:01:17.100","2017-08-19T10:01:17.100","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T20:16:04.610","2017-08-19T10:16:04.610","AB","All",null,null,"New lines started for all sonars, crossline finished for MFZ. New SIS line 0274."]
["2017-08-19T21:45:49.730","2017-08-19T11:45:49.730","AB","Sonar","Knudsen","Phase Range","4500-5500m"]
["2017-08-19T21:56:33.420","2017-08-19T11:56:33.420","AB","Sonar","All",null,"All new lines created at turn. SIS 276"]
["2017-08-19T22:00:24.840","2017-08-19T12:00:24.840","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-19T22:44:07.750","2017-08-19T12:44:07.750","AB","XBT",null,null,"XBT48 added to new line 277."]
["2017-08-19T23:47:24.530","2017-08-19T13:47:24.530","AB","Sonar","Multibeam","New Line","0278"]
["2017-08-20T01:22:11.750","2017-08-19T15:22:11.750","AB","All",null,null,"New lines started on all sonars at turn. New MBES line 280."]
["2017-08-20T01:25:26.140","2017-08-19T15:25:26.140","AB","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-20T02:04:02.820","2017-08-19T16:04:02.820","AB","All",null,null,"New lines started on all sonars at turn. New MBES line 281."]
["2017-08-20T02:49:18.670","2017-08-19T16:49:18.670","CW","Ship",null,null,"Slowed to survey speed for feature. SIS line 0281"]
["2017-08-20T03:15:48.100","2017-08-19T17:15:48.100","CW","Sonar","Multibeam","Ping Mode","Very Deep for feature"]
["2017-08-20T03:16:09.880","2017-08-19T17:16:09.880","CW","Sonar","Multibeam","Max Angle","Incremented angles out for swath over feature, then brought them back in. 35/35 - 43/43"]
["2017-08-20T03:17:33.260","2017-08-19T17:17:33.260","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T03:17:56.480","2017-08-19T17:17:56.480","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T03:23:08.690",{"$f":"IF(ISBLANK(A450),\" \",((A450)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-19T17:23:08.690"},"CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T03:23:47.170","2017-08-19T17:23:47.170","CW","Sonar","Multibeam","Ping Mode","Back to Extra Deep"]
["2017-08-20T03:24:56.280","2017-08-19T17:24:56.280","CW","Ship",null,null,"Back to Transit Speed"]
["2017-08-20T03:26:08.210","2017-08-19T17:26:08.210","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-20T04:09:24.920","2017-08-19T18:09:24.920","CW","Ship",null,null,"Slowed to survey speed for feature. SIS line 0283"]
["2017-08-20T04:39:24.090","2017-08-19T18:39:24.090","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T04:41:31.880","2017-08-19T18:41:31.880","AB","Sonar","Multibeam","Ping Mode","Very Deep for feature"]
["2017-08-20T04:43:20.700","2017-08-19T18:43:20.700","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T04:54:55.800",{"$f":"IF(ISBLANK(A458),\" \",((A458)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-19T18:54:55.800"},"CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-20T04:59:39.780","2017-08-19T18:59:39.780","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-20T05:10:47.290","2017-08-19T19:10:47.290","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-20T05:10:49.160","2017-08-19T19:10:49.160","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T05:10:52.140","2017-08-19T19:10:52.140","CW","POS",null,null,"Several dropouts and lost pings. "]
["2017-08-20T05:14:31.850","2017-08-19T19:14:31.850","CW","XBT",null,null,"XBT 049; applied to SIS line 0284"]
["2017-08-20T05:17:10.700","2017-08-19T19:17:10.700","CW","Ship[",null,null,"Back to Transit Speed"]
["2017-08-20T05:17:37.030","2017-08-19T19:17:37.030","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-20T10:24:59.260","2017-08-20T00:24:59.260","CW","XBTq",null,null,"XBT 050; applied to SIS line 0289"]
["2017-08-20T11:45:02.740","2017-08-20T01:45:02.740","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T11:45:58.280","2017-08-20T01:45:58.280","DF","Ship",null,null,"Survey speed 8.5-9kts"]
["2017-08-20T12:09:59.990","2017-08-20T02:09:59.990","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-20T12:11:29.540","2017-08-20T02:11:29.540","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T12:22:22.700","2017-08-20T02:22:22.700","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-20T12:30:30.120","2017-08-20T02:30:30.120","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-20T12:41:53.150","2017-08-20T02:41:53.150","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-20T12:46:51.360","2017-08-20T02:46:51.360","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-20T12:47:09.750","2017-08-20T02:47:09.750","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-20T12:54:40.550","2017-08-20T02:54:40.550","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-20T13:04:39.690","2017-08-20T03:04:39.690","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-20T13:12:28.490","2017-08-20T03:12:28.490","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-20T13:18:42.420","2017-08-20T03:18:42.420","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-20T13:23:25.190","2017-08-20T03:23:25.190","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-20T13:28:31.060","2017-08-20T03:28:31.060","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-20T13:37:51.580","2017-08-20T03:37:51.580","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T13:52:07.120","2017-08-20T03:52:07.120","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T14:04:46.730","2017-08-20T04:04:46.730","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-08-20T14:36:09.920","2017-08-20T04:36:09.920","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-20T14:40:51.470","2017-08-20T04:40:51.470","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T15:10:53.820","2017-08-20T05:10:53.820","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-20T15:55:56.620","2017-08-20T05:55:56.620","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-20T16:46:36.860","2017-08-20T06:46:36.860","DF","XBT",null,null,"Cast 051 applied to line 0296"]
["2017-08-20T16:56:48.600","2017-08-20T06:56:48.600","DF","Ship",null,null,"Transit speed"]
["2017-08-20T17:02:51.450","2017-08-20T07:02:51.450","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-08-20T17:57:53.940","2017-08-20T07:57:53.940","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T18:07:41.200","2017-08-20T08:07:41.200","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-20T18:13:24.460","2017-08-20T08:13:24.460","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-20T18:20:50.610","2017-08-20T08:20:50.610","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-20T18:27:14.990","2017-08-20T08:27:14.990","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-20T18:36:36.310","2017-08-20T08:36:36.310","BO","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-20T18:36:58.380","2017-08-20T08:36:58.380","AB","Sonar","Multibeam","new Line",298]
["2017-08-20T18:41:22.670","2017-08-20T08:41:22.670","BO","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-20T18:52:16.520","2017-08-20T08:52:16.520","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-20T18:58:12.180","2017-08-20T08:58:12.180","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-20T18:59:59.550","2017-08-20T08:59:59.550","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-20T19:10:56.290","2017-08-20T09:10:56.290","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-20T19:14:34.420","2017-08-20T09:14:34.420","AB","Sonar","Knudsen","Gain Value","20 5logR, Pulse 8, Phase Range 4000-5000"]
["2017-08-20T19:15:56.620","2017-08-20T09:15:56.620","AB","Ship",null,null,"Resume warp"]
["2017-08-20T19:21:52.340","2017-08-20T09:21:52.340","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T19:35:03.950","2017-08-20T09:35:03.950","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-20T19:44:08.970","2017-08-20T09:44:08.970","AB","Sonar","All",null,"New lines started for turn. MB line 300."]
["2017-08-20T21:00:45.050","2017-08-20T11:00:45.050","AB","Sonar","Multibeam",null,"COM2 error"]
["2017-08-20T22:22:15.440","2017-08-20T12:22:15.440","AB","XBT",null,null,"XBT 53 added to new SIS line 303."]
["2017-08-20T23:34:24.130","2017-08-20T13:34:24.130","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-20T23:47:50.750","2017-08-20T13:47:50.750","CT","Sonar","All",null,"New lines started for turn. MB line 305. Reduced to survey speed."]
["2017-08-20T23:50:00.270","2017-08-20T13:50:00.270","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T00:05:23.690","2017-08-20T14:05:23.690","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T00:23:33.530","2017-08-20T14:23:33.530","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T00:27:55.810","2017-08-20T14:27:55.810","CT","Other",null,null,"Sun photometer"]
["2017-08-21T00:31:19.930","2017-08-20T14:31:19.930","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T00:48:39.790","2017-08-20T14:48:39.790","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T01:25:13.310","2017-08-20T15:25:13.310","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T01:56:31.130","2017-08-20T15:56:31.130","CW","Sonar","All",null,"New lines for turn. SIS line 0308"]
["2017-08-22T01:56:31.125","2017-08-21T15:56:31.125","AB","Ship",null,null,"Continue 1000m past turn for more coverage. Line plan is shifted 1000m to the west."]
["2017-08-21T02:18:47.810","2017-08-20T16:18:47.810","CW","Sonar","All",null,"New survey lines. SIS line 0309"]
["2017-08-21T02:28:10.510",{"$f":"IF(ISBLANK(A523),\" \",((A523)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-20T16:28:10.510"},"CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T02:30:19.380","2017-08-20T16:30:19.380","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T02:33:40.650","2017-08-20T16:33:40.650","CW","Sonar","Multibeam","Ping Mode","Deeepp."]
["2017-08-21T02:37:53.880","2017-08-20T16:37:53.880","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-21T03:05:11.340","2017-08-20T17:05:11.340","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T03:05:52.860","2017-08-20T17:05:52.860","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T03:07:04.190","2017-08-20T17:07:04.190","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-21T03:19:04.410","2017-08-20T17:19:04.410","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T03:19:52.550","2017-08-20T17:19:52.550","CW","Sonar","Multibeam","Ping Mode","Deep "]
["2017-08-21T03:32:34.810","2017-08-20T17:32:34.810","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-21T03:37:00.320","2017-08-20T17:37:00.320","AB","Ship",null,null,"Shift lineplan 500m east"]
["2017-08-21T03:39:15.990","2017-08-20T17:39:15.990","AB","Sonar","Knudsen","Phase Range","1500-2000, Power 2, Pulse 4"]
["2017-08-21T03:41:58.450","2017-08-20T17:41:58.450","AB","Sonar","Knudsen","Tx Power","1, Pulse 2"]
["2017-08-21T03:47:29.260","2017-08-20T17:47:29.260","AB","Ship",null,null,"Turning to port to investigate small row boat off the port bow to make sure it isn't in distress. New lines started on all sonars. (MB 311)"]
["2017-08-21T03:52:10.910","2017-08-20T17:52:10.910","AB","Sonar","Knudsen","Gain Value","18 5logR"]
["2017-08-22T03:58:11","2017-08-21T17:58:11","AB","Ship",null,null,"No people in boat adrift. "]
["2017-08-21T04:03:40.800","2017-08-20T18:03:40.800","AB","Sonar","All",null,"All new lines started for all sonars (MB Line 312)"]
["2017-08-21T04:24:00.790","2017-08-20T18:24:00.790","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-21T04:32:27.520","2017-08-20T18:32:27.520","AB","Sonar","Knudsen","Phase Range","2500-3500, Power 2, Pulse 8"]
["2017-08-21T04:33:20.510","2017-08-20T18:33:20.510","CW","All",null,null,"New line for turn. SIS line 0314"]
["2017-08-21T04:55:18.520","2017-08-20T18:55:18.520","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-21T04:56:32.760","2017-08-20T18:56:32.760","CW","All",null,null,"New survey lines. SIS line 0316"]
["2017-08-21T04:57:14.320","2017-08-20T18:57:14.320","CW","Ship",null,null,"500m added to line spacing"]
["2017-08-21T04:58:05.170","2017-08-20T18:58:05.170","CW","Sonar","Knudsen","Tx Power",3]
["2017-08-21T05:06:21.470","2017-08-20T19:06:21.470","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T05:07:20.710","2017-08-20T19:07:20.710","CW","Sonar","Multibeam","Ping Mode","Deep "]
["2017-08-21T05:13:07.820","2017-08-20T19:13:07.820","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T05:28:24.880","2017-08-20T19:28:24.880","AB","Ship",null,null,"Shift line plan an additional 1000m to port."]
["2017-08-21T05:28:43.720","2017-08-20T19:28:43.720","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T05:34:37.170","2017-08-20T19:34:37.170","CW","XBT",null,null,"XBT54 added to line 315"]
["2017-08-21T05:37:32.850","2017-08-20T19:37:32.850","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T05:43:06.170","2017-08-20T19:43:06.170","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T05:46:50.240","2017-08-20T19:46:50.240","AB","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-21T06:15:44.140","2017-08-20T20:15:44.140","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T06:15:47.440","2017-08-20T20:15:47.440","CW","Ship",null,null,"Nudging 500m to stbd for coverage"]
["2017-08-21T06:17:31.950","2017-08-20T20:17:31.950","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T06:28:13.990","2017-08-20T20:28:13.990","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T06:30:46.560","2017-08-20T20:30:46.560","CW","Sonar","Multibeam","Ping Mode","Deep "]
["2017-08-21T06:31:46.970","2017-08-20T20:31:46.970","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T06:34:33.800","2017-08-20T20:34:33.800","CW","Sonar","Knudsen","Tx Power",2]
["2017-08-21T06:43:57.800",{"$f":"IF(ISBLANK(A563),\" \",((A563)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-20T20:43:57.800"},"CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-21T06:43:57.800","2017-08-20T20:43:57.800","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T06:51:04.760","2017-08-20T20:51:04.760","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T06:51:08.750","2017-08-20T20:51:08.750","CW","Sonar","Knudsen","Tx Power",3]
["2017-08-21T07:02:08.290","2017-08-20T21:02:08.290","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T07:08:13.580","2017-08-20T21:08:13.580","CW","All",null,null,"Turn lines to transit. SIS line 0318"]
["2017-08-21T07:15:25.670","2017-08-20T21:15:25.670","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-21T07:25:45.790","2017-08-20T21:25:45.790","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-21T07:39:07.400","2017-08-20T21:39:07.400","CW","All",null,null,"Transit lines. SIS line 0319. "]
["2017-08-21T07:39:29.050","2017-08-20T21:39:29.050","CW","Ship",null,null,"Transit Speed"]
["2017-08-21T07:46:34.920","2017-08-20T21:46:34.920","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T07:51:31.680","2017-08-20T21:51:31.680","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-21T07:52:55.020","2017-08-20T21:52:55.020","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-21T09:53:44.570","2017-08-20T23:53:44.570","CW","XBT",null,null,"XBT 055; applied to SIS line 0321"]
["2017-08-21T10:37:31.520","2017-08-21T00:37:31.520","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-21T14:32:44.810","2017-08-21T04:32:44.810","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-21T14:40:44.030","2017-08-21T04:40:44.030","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-21T15:50:10.480","2017-08-21T05:50:10.480","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-21T16:07:55.440","2017-08-21T06:07:55.440","DF","XBT",null,null,"Cast 056 applied to line 0327"]
["2017-08-21T16:08:55.680","2017-08-21T06:08:55.680","DF","Ship",null,null,"Survey speed 8.5-9kts"]
["2017-08-21T16:15:43.690","2017-08-21T06:15:43.690","DF","Sonar","Multibeam","new Line","begin survey line 0328; starting new seamount survey"]
["2017-08-21T16:19:22.330","2017-08-21T06:19:22.330","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-21T16:24:51.570","2017-08-21T06:24:51.570","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-21T16:26:20.410","2017-08-21T06:26:20.410","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T16:31:56.240","2017-08-21T06:31:56.240","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T16:39:40.200","2017-08-21T06:39:40.200","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T16:50:16.030",{"$f":"IF(ISBLANK(A589),\" \",((A589)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-21T06:50:16.030"},"DF","Sonar","Multibeam","Ping Mode","Deep "]
["2017-08-21T16:53:20.410","2017-08-21T06:53:20.410","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T17:08:57.190","2017-08-21T07:08:57.190","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T17:15:37.150","2017-08-21T07:15:37.150","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-21T17:15:52.660","2017-08-21T07:15:52.660","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T17:28:44.210","2017-08-21T07:28:44.210","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T17:41:07.300","2017-08-21T07:41:07.300","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T17:42:11.680","2017-08-21T07:42:11.680","AB","Sonar","All",null,"New lines started for all sonars, MB line 330"]
["2017-08-21T17:52:07.570","2017-08-21T07:52:07.570","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T17:56:12.720","2017-08-21T07:56:12.720","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T18:03:38.820","2017-08-21T08:03:38.820","BO","Sonar","all",null,"New lines started for all sonars, MB line 331"]
["2017-08-21T18:08:37.620","2017-08-21T08:08:37.620","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T18:11:58.780","2017-08-21T08:11:58.780","BO","Sonar ","Knudsen","Phase Range","3500-4500"]
["2017-08-21T18:36:31.060","2017-08-21T08:36:31.060","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T19:08:20.860","2017-08-21T09:08:20.860","BO","sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T19:15:50.360","2017-08-21T09:15:50.360","BO","sonar","All",null,"New Lines started for all sonars, MB line 333"]
["2017-08-21T19:16:23.850","2017-08-21T09:16:23.850","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T19:31:17.190","2017-08-21T09:31:17.190","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-21T19:34:17.650","2017-08-21T09:34:17.650","AB","Sonar","All",null,"New lines started for all sonars, MB line 334"]
["2017-08-21T19:45:46.280","2017-08-21T09:45:46.280","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T20:42:42.970","2017-08-21T10:42:42.970","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-21T20:49:06.940","2017-08-21T10:49:06.940","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T20:49:52.810","2017-08-21T10:49:52.810","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-22T21:00:53","2017-08-22T11:00:53","AB","Issue/Problem","Multibeam","Warning","SIS program crashed without help."]
["2017-08-21T21:04:34.720","2017-08-21T11:04:34.720","BO","sonar","All",null,"New lines started on Knudsen and EK60. "]
["2017-08-21T21:06:40.990","2017-08-21T11:06:40.990","BO","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-21T21:13:05.350","2017-08-21T11:13:05.350","BO","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-21T21:26:12.470","2017-08-21T11:26:12.470","AB","Issue/Problem","Multibeam",null,"SIS program restarted with Telnet and Data distribution. No new survey started. Used EX1707B. Took about 5 minutes to update the video feed for the grid and backscatter, but was still recording data. Checked in Qimera."]
["2017-08-21T21:17:34.240","2017-08-21T11:17:34.240","AB","Sonar","Multibeam",null,"New line 335. "]
["2017-08-21T21:36:03.330","2017-08-21T11:36:03.330","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-21T21:36:39.060","2017-08-21T11:36:39.060","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-21T21:45:13.780","2017-08-21T11:45:13.780","AB","Sonar","Multibeam","Ping Mode","M:Very Deep"]
["2017-08-21T21:46:18.580","2017-08-21T11:46:18.580","Ab","Ship",null,null,"Increase to warp speed"]
["2017-08-21T21:48:34.260","2017-08-21T11:48:34.260","AB","Sonar","Knudsen","Phase Range","3500-4500, Power 3"]
["2017-08-21T21:50:25.750","2017-08-21T11:50:25.750","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-21T21:59:18.640","2017-08-21T11:59:18.640","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-21T22:01:40.160","2017-08-21T12:01:40.160","AB","Sonar","Multibeam"]
["2017-08-21T22:21:17.780","2017-08-21T12:21:17.780","CT",null,null,null,"Slowed down due to the dolphins in the jacuzzi "]
["2017-08-21T22:22:07.320","2017-08-21T12:22:07.320","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-21T22:26:24.400","2017-08-21T12:26:24.400","AB","Sonar","Multibeam","Ping Mode","Extra Deep, Max 35/35"]
["2017-08-21T22:41:02.260","2017-08-21T12:41:02.260","AB","XBT",null,null,"Had to restarted CTD computer. Loss of Nav. XBT 57 completed."]
["2017-08-21T22:48:12.940","2017-08-21T12:48:12.940","AB","Sonar","Multibeam",null,"XBT57 applied to new line 339"]
["2017-08-21T22:49:59.450","2017-08-21T12:49:59.450","AB","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-21T23:36:55.300","2017-08-21T13:36:55.300","AB","Sonar","Multibeam",null,"Small range gate"]
["2017-08-22T00:52:26.570","2017-08-21T14:52:26.570","AB","Ship",null,null,"Diverting from course due to life ring seen floating in the water"]
["2017-08-22T00:53:43.920","2017-08-21T14:53:43.920","AB","Sonar","All",null,"All new lines started.  MB line 342"]
["2017-08-22T01:05:18.880","2017-08-21T15:05:18.880","AB","Sonar","All",null,"All new lines started.  MB line 343"]
["2017-08-22T03:20:35.440",{"$f":"IF(ISBLANK(A636),\" \",((A636)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-21T17:20:35.440"},"CW","Sonar","Multibeam","Ping Mode","Very Deep "]
["2017-08-22T03:20:35.440","2017-08-21T17:20:35.440","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-22T03:42:17.760","2017-08-21T17:42:17.760","CT","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T05:28:14.790","2017-08-21T19:28:14.790","CT","XBT",null,null,"Cast 058 at line 0347"]
["2017-08-22T05:48:56.960","2017-08-21T19:48:56.960","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-22T06:08:05.040","2017-08-21T20:08:05.040","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T06:19:58.920","2017-08-21T20:19:58.920","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T06:26:15.410","2017-08-21T20:26:15.410","CW","All",null,null,"New Survey lines for turn onto NorthRidge_West. SIS line 0349"]
["2017-08-22T06:30:33.090","2017-08-21T20:30:33.090","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-22T06:35:54.130","2017-08-21T20:35:54.130","CW","Sonar","Multibeam","Ping Mode","Deep "]
["2017-08-22T06:36:14.450","2017-08-21T20:36:14.450","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-22T06:38:03.940","2017-08-21T20:38:03.940","CW","Sonar","Multibeam","Max Angle","incrementing up to 70/70"]
["2017-08-22T06:39:30.860","2017-08-21T20:39:30.860","CW","Ship",null,null,"Lost Waypoint Control, but Bri is maintaining XTE very well. "]
["2017-08-22T06:48:56.170","2017-08-21T20:48:56.170","CW","Ship",null,null,"Waypoint Control is back. Yay!"]
["2017-08-22T06:51:13.080","2017-08-21T20:51:13.080","CW","Sonar","Knudsen","Tx Power",2]
["2017-08-22T07:36:58.730","2017-08-21T21:36:58.730","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-22T07:50:30.290","2017-08-21T21:50:30.290","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T08:08:51.670",{"$f":"IF(ISBLANK(A653),\" \",((A653)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-21T22:08:51.670"},"CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T10:03:06.860","2017-08-22T00:03:06.860","CW","XBT",null,null,"XBT 059; applied to SIS line 0352"]
["2017-08-22T10:32:39.310","2017-08-22T00:32:39.310","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T10:37:44.920","2017-08-22T00:37:44.920","DF","Sonar","Multibeam","new Line","begin survey line 0354; new survey area"]
["2017-08-22T11:30:12.960","2017-08-22T01:30:12.960","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T12:44:16.230","2017-08-22T02:44:16.230","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T12:44:29.930","2017-08-22T02:44:29.930","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-22T13:24:20.670","2017-08-22T03:24:20.670","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-22T13:33:54.250","2017-08-22T03:33:54.250","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T13:55:09.470","2017-08-22T03:55:09.470","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T14:00:21.270","2017-08-22T04:00:21.270","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T15:02:27.250","2017-08-22T05:02:27.250","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T16:23:28.710","2017-08-22T06:23:28.710","DF","Sonar","Multibeam","new Line","begin turn line 0360; new ek and sbp lines"]
["2017-08-22T16:48:50.170","2017-08-22T06:48:50.170","BO","XBT",null,null,"Cast 060 applied to line 360"]
["2017-08-22T16:49:41.780","2017-08-22T06:49:41.780","DF","Sonar","Multibeam","New Line","begin survey line 0361; new ek and sbp lines"]
["2017-08-22T16:53:55.140","2017-08-22T06:53:55.140","DF","Ship",null,null,"Requested 1200 m move to STBD for reduce overlap"]
["2017-08-22T16:55:46.630","2017-08-22T06:55:46.630","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T17:18:41.410","2017-08-22T07:18:41.410","DF","Ship",null,null,"Had to make slight course adjustment to avoid bouy"]
["2017-08-22T17:38:08.440","2017-08-22T07:38:08.440","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-22T17:56:25.990","2017-08-22T07:56:25.990","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T18:23:07.920","2017-08-22T08:23:07.920","AB","Sonar","Knudsen","Tx Power",2]
["2017-08-22T18:40:09.620","2017-08-22T08:40:09.620","AB","Sonar","Knudsen","Gain Value","15 5logR"]
["2017-08-22T18:51:09","2017-08-22T08:51:09","AB","Sonar","Multibeam","new Line",363]
["2017-08-22T19:10:22.700","2017-08-22T09:10:22.700","AB","Sonar","Knudsen","Gain Value","16 5logR"]
["2017-08-22T19:17:45.090","2017-08-22T09:17:45.090","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-22T19:50:37.520","2017-08-22T09:50:37.520","AB","Sonar","Multibeam","new Line","364, Ping mode Deep, Max Angle 60/60, Range Gate Normal"]
["2017-08-22T19:53:32.400","2017-08-22T09:53:32.400","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-22T20:46:24.640","2017-08-22T10:46:24.640","BO","Sun photometer",null,null,"Sun photometer reading!"]
["2017-08-22T20:49:12.090","2017-08-22T10:49:12.090","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-22T21:02:41.520","2017-08-22T11:02:41.520","AB","Sonar","Multibeam","new Line","Line 366, ping mode changed to very deep"]
["2017-08-22T21:09:28.500","2017-08-22T11:09:28.500","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-22T21:35:54.230","2017-08-22T11:35:54.230","AB","Sonar","Knudsen","Tx Pulse","8ms, Tx Power 3"]
["2017-08-22T21:43:40.170","2017-08-22T11:43:40.170","AB","Sonar","All",null,"New lines started on all sonars for turn. MB line 367. Line plan shifted an additional 1000m south. "]
["2017-08-22T22:10:54.820","2017-08-22T12:10:54.820","AB","Sonar","All",null,"New lines started on all sonars after turn. MB line 368."]
["2017-08-22T22:34:27.720","2017-08-22T12:34:27.720","AB","XBT",null,null,"XBT 61 added to new line 369. "]
["2017-08-22T22:39:03.490","2017-08-22T12:39:03.490","AB","Sonar","Knudsen","Tx Power",2]
["2017-08-22T22:53:29.570","2017-08-22T12:53:29.570","AB","Sonar","Knudsen","Tx Power","3, Gain 17 5logR"]
["2017-08-22T23:40:03.360","2017-08-22T13:40:03.360","AB","Sonar","Knudsen","Tx Power",2]
["2017-08-23T00:35:45","2017-08-22T14:35:45","AB","Sonar","Multibeam","new Line",371]
["2017-08-23T00:51:01.480","2017-08-22T14:51:01.480","AB","Sonar","Knudsen","Tx Power",3]
["2017-08-23T01:25:23.670","2017-08-22T15:25:23.670","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T01:55:10.090","2017-08-22T15:55:10.090","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T02:22:31.310","2017-08-22T16:22:31.310","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-23T02:53:22.150","2017-08-22T16:53:22.150","CW","All",null,"new Line","Turn yo. SIS line 0373"]
["2017-08-23T04:01:42.310","2017-08-22T18:01:42.310","CW","All",null,"new Line","New Survey LInes. SIS line 0376"]
["2017-08-23T04:26:32.510","2017-08-22T18:26:32.510","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-23T04:37:20.270","2017-08-22T18:37:20.270","CW","POS",null,null,"GAMS Not Ready for several minutes"]
["2017-08-23T04:40:22.080","2017-08-22T18:40:22.080","CW","POS",null,null,"Okay GAMS are back!"]
["2017-08-23T04:41:16.390","2017-08-22T18:41:16.390","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-23T05:15:43.750","2017-08-22T19:15:43.750","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T05:29:09.620","2017-08-22T19:29:09.620","CW","XBT",null,null,"XBT 062; applied to SIS line 0377"]
["2017-08-23T05:41:36.030","2017-08-22T19:41:36.030","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T05:57:31.240","2017-08-22T19:57:31.240","CW","Ship",null,null,"500m line shift to stbd"]
["2017-08-23T06:23:00.010","2017-08-22T20:23:00.010","CW","Sonar","Knudsen",null,"SBP crash. Nice. Line 255 .sgy; line 254.kea/keb"]
["2017-08-23T06:24:27.280","2017-08-22T20:24:27.280","CW","Ship",null,null,"500m line shift to stbd"]
["2017-08-23T06:30:17.130","2017-08-22T20:30:17.130","CW","Sonar","Knudsen","Start Recording","SBP restarted. Line 256 on all files"]
["2017-08-23T06:33:04.690","2017-08-22T20:33:04.690","CW","Sonar","Knudsen","Start Recording","Pulse 8; Power 3; Gain 18 / 5logR"]
["2017-08-23T07:23:19.550","2017-08-22T21:23:19.550","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T07:41:58.060","2017-08-22T21:41:58.060","CW","All",null,null,"New lines for turn and jumping lines. SIS line 0380"]
["2017-08-23T07:45:55.440","2017-08-22T21:45:55.440","CW","Sonar","Multibeam",null,"Red Screen of Death. Gummy Bears sacrificed."]
["2017-08-23T07:47:38.380","2017-08-22T21:47:38.380","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T08:00:44.830","2017-08-22T22:00:44.830","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T08:24:33.730","2017-08-22T22:24:33.730","CW","All",null,null,"New Survey lines. SIS line 0381"]
["2017-08-23T08:46:47.950","2017-08-22T22:46:47.950","CW","All",null,null,"New lines for turn. SIS line 0382"]
["2017-08-23T08:53:35.100",{"$f":"IF(ISBLANK(A717),\" \",((A717)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-22T22:53:35.100"},"CW","Ship",null,null,"Started turn without realizing line shifts from earlier, so it's 1000m south. But it's over previous coverage, so it's not to much of a biggie. But yeah, my bad!"]
["2017-08-23T08:56:09.290","2017-08-22T22:56:09.290","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T09:07:46.180","2017-08-22T23:07:46.180","CW","All",null,null,"New lines for turn onto North Ridge Center line plan. SIS line 0383"]
["2017-08-23T09:25:23.790","2017-08-22T23:25:23.790","CW","Sonar","Multibeam","Ping Mode","Deep "]
["2017-08-23T10:01:28.580","2017-08-23T00:01:28.580","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-23T10:32:48.530","2017-08-23T00:32:48.530","CW","XBT",null,null,"XBT 063; applied to SIS line 0384"]
["2017-08-23T11:14:30.130","2017-08-23T01:14:30.130","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-23T11:14:42.200","2017-08-23T01:14:42.200","DF","Sonar","Multibeam","Max Angle","75/75"]
["2017-08-23T11:48:52.350","2017-08-23T01:48:52.350","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T12:12:12.250","2017-08-23T02:12:12.250","DF","Sonar","Multibeam","New Line","begin turn line 0387, new ek and sbp lines"]
["2017-08-23T12:34:45.430","2017-08-23T02:34:45.430","DF","Sonar","Multibeam","New Line","begin survey line 0388, new ek and sbp lines"]
["2017-08-23T12:42:21.930","2017-08-23T02:42:21.930","DF","Ship",null,null,"requested 1000 m move to PORT for coverage"]
["2017-08-23T13:18:06.780","2017-08-23T03:18:06.780","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-23T14:43:15.460","2017-08-23T04:43:15.460","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-23T14:44:35.750","2017-08-23T04:44:35.750","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-23T14:47:11.860","2017-08-23T04:47:11.860","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-23T15:34:14.110","2017-08-23T05:34:14.110","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-23T15:34:38.480","2017-08-23T05:34:38.480","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T15:41:24.910","2017-08-23T05:41:24.910","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T16:35:18.550","2017-08-23T06:35:18.550","DF","XBT",null,null,"Cast 064 applied to line 0392"]
["2017-08-23T17:22:21.870","2017-08-23T07:22:21.870","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T17:49:55.660","2017-08-23T07:49:55.660","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-23T18:14:07.620","2017-08-23T08:14:07.620","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-23T18:14:37.320","2017-08-23T08:14:37.320","AB","Sonar","Multibeam","Ping Mode","Deep, New line 394. Max angle 60/60"]
["2017-08-23T18:32:24.130","2017-08-23T08:32:24.130","BO","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-23T18:42:37.670","2017-08-23T08:42:37.670","AB","Sonar","Multibeam","Max Angle","70/70"]
["2017-08-23T18:43:31.120","2017-08-23T08:43:31.120","AB","Sonar","Knudsen","Tx Power","2, new line"]
["2017-08-23T19:07:56.230","2017-08-23T09:07:56.230","BO","Sonar","Knudsen","Phase Range","2500-2500"]
["2017-08-23T19:35:08.860","2017-08-23T09:35:08.860","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-23T19:45:20.800","2017-08-23T09:45:20.800","BO","Sonar","Multibeam","Ping Mode","Very deep"]
["2017-08-23T19:47:30.660","2017-08-23T09:47:30.660","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T19:57:44.390","2017-08-23T09:57:44.390","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-23T20:08:00.150","2017-08-23T10:08:00.150","BO","sonar","all",null,"new line on all sonar. MB line 0396"]
["2017-08-23T20:10:47.350","2017-08-23T10:10:47.350","AB","Sonar","Knudsen","Tx Power","3, Gain 18 5logR"]
["2017-08-23T20:45:26.780","2017-08-23T10:45:26.780","BO","Sonar","All",null,"new lines on all sonar, MB line 0398"]
["2017-08-23T20:47:52.710","2017-08-23T10:47:52.710","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-23T21:11:32.070","2017-08-23T11:11:32.070","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-23T21:15:25.190","2017-08-23T11:15:25.190","BO","Sonar","Multibeam","Ping Mode","Deep, new line 0400, max angle 70/70"]
["2017-08-23T21:19:34.310","2017-08-23T11:19:34.310","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-23T21:35:51.180","2017-08-23T11:35:51.180","AB","Sonar","Knudsen","Phase Range","2000-3000-, power 2, pulse 4, 16 5logR"]
["2017-08-23T21:36:54.310","2017-08-23T11:36:54.310","CT","Other",null,null,"Sun photometer reading!"]
["2017-08-23T22:25:01.770","2017-08-23T12:25:01.770","CT","XBT",null,null,"Cast 065 at line0401"]
["2017-08-23T22:55:55.250","2017-08-23T12:55:55.250","AB","Ship",null,null,"Fire Drill."]
["2017-08-23T23:34:06.190","2017-08-23T13:34:06.190","AB","Sonar","Multibeam","New Line",404]
["2017-08-23T23:34:50.680","2017-08-23T13:34:50.680","AB","Sonar","Knudsen","Phase Range","4000-5000, Power 3, Pulse 8, Gain 20 5logR"]
["2017-08-23T23:49:58.540","2017-08-23T13:49:58.540","AB","Sonar","Knudsen","Gain Value","14 5logR"]
["2017-08-24T00:47:07.800","2017-08-23T14:47:07.800","CT","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T01:01:35.420","2017-08-23T15:01:35.420","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T01:10:11.520","2017-08-23T15:10:11.520","AB","Sonar","Multibeam","Ping Mode","Deep, new line 406"]
["2017-08-24T01:22:28.300","2017-08-23T15:22:28.300","CT","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-24T02:06:22.770","2017-08-23T16:06:22.770","AB","Sonar","Knudsen","Phase Range","3000-4000, Gain 16 5logR"]
["2017-08-24T02:12:01.200","2017-08-23T16:12:01.200","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T02:20:35.480","2017-08-23T16:20:35.480","AB","Sonar","Multibeam","Ping Mode","Very Deep, New MB line 408"]
["2017-08-24T04:08:59.600","2017-08-23T18:08:59.600","CW","All",null,null,"New lines for turn. SIS line0 411"]
["2017-08-24T04:28:48.170","2017-08-23T18:28:48.170","CW","All",null,null,"New Survey lines. SIS line 0412"]
["2017-08-24T04:40:47.590","2017-08-23T18:40:47.590","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-24T04:50:55.010","2017-08-23T18:50:55.010","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T05:03:04.480","2017-08-23T19:03:04.480","CT","XBT",null,null,"Cast 066 at line 0412"]
["2017-08-24T05:03:04.480","2017-08-23T19:03:04.480","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-24T06:26:45.420","2017-08-23T20:26:45.420","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T06:42:24.950","2017-08-23T20:42:24.950","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T07:06:29.990","2017-08-23T21:06:29.990","CW","Sonar","Knudsen","Phase Range","25600-3500"]
["2017-08-24T08:12:46.130",{"$f":"IF(ISBLANK(A779),\" \",((A779)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-23T22:12:46.130"},"CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T08:22:45.930","2017-08-23T22:22:45.930","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T08:52:36.240","2017-08-23T22:52:36.240","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-24T09:09:35.950","2017-08-23T23:09:35.950","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T10:03:41.760","2017-08-24T00:03:41.760","CW","XBT",null,null,"XBT 067; applied to SIS line 0417"]
["2017-08-24T11:54:21.230","2017-08-24T01:54:21.230","DF","Sonar","Multibeam","New Line","begin turn line 0420; new ek and sbp lines"]
["2017-08-24T12:19:48.800","2017-08-24T02:19:48.800","DF","Sonar","Multibeam","New Line","begin survey line 0421; new ek and sbp lines"]
["2017-08-24T15:33:30.150","2017-08-24T05:33:30.150","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T15:42:55.820","2017-08-24T05:42:55.820","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T15:53:21.670","2017-08-24T05:53:21.670","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-24T15:55:17.390","2017-08-24T05:55:17.390","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-24T16:05:52.510","2017-08-24T06:05:52.510","DF","XBT",null,null,"Cast 068 applied to line 0424"]
["2017-08-24T16:11:24.050","2017-08-24T06:11:24.050","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-24T16:36:24.890","2017-08-24T06:36:24.890","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T16:52:21.480","2017-08-24T06:52:21.480","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T17:02:46.390","2017-08-24T07:02:46.390","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-24T17:29:12.610","2017-08-24T07:29:12.610","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-24T17:46:53.530","2017-08-24T07:46:53.530","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-24T17:58:31.120","2017-08-24T07:58:31.120","AB","Sonar","Multibeam","New Line","427 turn line. New lines started for all sonars."]
["2017-08-24T18:11:15.450","2017-08-24T08:11:15.450","AB","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-24T18:24:29.340","2017-08-24T08:24:29.340","AB","sonar","All",null,"All new sonars lines started. MB line 428"]
["2017-08-24T19:00:23.580","2017-08-24T09:00:23.580","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-24T19:25:21","2017-08-24T09:25:21","AB","Sonar","Multibeam","New Line",429]
["2017-08-24T19:57:01.290","2017-08-24T09:57:01.290","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T20:04:02.640","2017-08-24T10:04:02.640","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T20:18:29.950","2017-08-24T10:18:29.950","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-24T20:38:45.530","2017-08-24T10:38:45.530","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T20:44:11.490","2017-08-24T10:44:11.490","AB","Sonar","Multibeam","New Line",431]
["2017-08-24T20:55:41.040","2017-08-24T10:55:41.040","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T21:01:53.840","2017-08-24T11:01:53.840","AB","Sonar","Knudsen","Phase Range","4000-4500"]
["2017-08-24T21:06:52.030","2017-08-24T11:06:52.030","AB","Sonar","Knudsen","Phase Range","4000-4500"]
["2017-08-24T21:08:34.830","2017-08-24T11:08:34.830","AB","Sonar","All",null,"All new lines started for turn (MB line 0423)"]
["2017-08-24T21:31:04.060","2017-08-24T11:31:04.060","AB","Sonar","All",null,"All new lines started for turn (MB line 433)"]
["2017-08-24T21:52:40.890","2017-08-24T11:52:40.890","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-24T22:14:24.750","2017-08-24T12:14:24.750","CT","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-24T22:27:35.890","2017-08-24T12:27:35.890","CT","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-24T22:49:52.940","2017-08-24T12:49:52.940","AB","XBT",null,null,"XBT 69 added to New SIS line 435."]
["2017-08-24T22:59:26.370","2017-08-24T12:59:26.370","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-24T23:03:03.680","2017-08-24T13:03:03.680","AB","All",null,null,"All new lines started for turn (MB line 436)"]
["2017-08-24T23:28:32.610","2017-08-24T13:28:32.610","AB","All",null,null,"All new lines started for turn (MB line 437)"]
["2017-08-24T23:52:06.180","2017-08-24T13:52:06.180","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-24T23:54:37.670","2017-08-24T13:54:37.670","CT","Other",null,null,"Sun photometer reading!"]
["2017-08-25T00:06:41.740","2017-08-24T14:06:41.740","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T00:22:14.490","2017-08-24T14:22:14.490","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-25T00:48:08.540","2017-08-24T14:48:08.540","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T00:48:41.660","2017-08-24T14:48:41.660","AB","Sonar","Knudsen","Phase Range","4500-5500; Power 3"]
["2017-08-25T00:54:32.580","2017-08-24T14:54:32.580","AB","All",null,null,"All new lines started for turn (MB line 439)"]
["2017-08-25T01:16:17","2017-08-24T15:16:17","AB","All",null,null,"All new lines started for turn (MB line 440)"]
["2017-08-25T01:16:42.850","2017-08-24T15:16:42.850","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T01:35:36.950","2017-08-24T15:35:36.950","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T01:41:53.170","2017-08-24T15:41:53.170","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T02:17:56.240","2017-08-24T16:17:56.240","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T02:22:14.510","2017-08-24T16:22:14.510","CW","All",null,null,"New lines for turn. SIS 0442"]
["2017-08-25T02:24:14.120","2017-08-24T16:24:14.120","AB","Sonar","Multibeam","New Line",443]
["2017-08-25T03:14:26.870","2017-08-24T17:14:26.870","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T03:44:10.020","2017-08-24T17:44:10.020","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T03:58:24.620","2017-08-24T17:58:24.620","AB","Sonar","Knudsen",null,"Gain 18 5logR, Power 2"]
["2017-08-25T04:26:57.650","2017-08-24T18:26:57.650","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T05:05:18.930","2017-08-24T19:05:18.930","CT","XBT",null,null,"Cast 070 at line 0445"]
["2017-08-25T05:09:51.770","2017-08-24T19:09:51.770","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-25T05:10:09.940","2017-08-24T19:10:09.940","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS."]
["2017-08-25T05:11:28.130","2017-08-24T19:11:28.130","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T05:18:09.400","2017-08-24T19:18:09.400","CW","Sonar","Knudsen","Tx Power",3]
["2017-08-25T07:01:48.480","2017-08-24T21:01:48.480","CW","All",null,null,"New lines for turn. SIS line 0448"]
["2017-08-25T07:09:54.650",{"$f":"IF(ISBLANK(A843),\" \",((A843)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-24T21:09:54.650"},"CW","All",null,null,"New survey lines. SIS line 0449"]
["2017-08-25T07:09:58.190","2017-08-24T21:09:58.190","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T07:11:09.190","2017-08-24T21:11:09.190","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-25T08:45:40.860","2017-08-24T22:45:40.860","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T09:10:21.420","2017-08-24T23:10:21.420","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T09:35:10.430","2017-08-24T23:35:10.430","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T09:54:32.470","2017-08-24T23:54:32.470","CW","XBT",null,null,"XBT 071, applied to SIS line 0451"]
["2017-08-25T11:18:11.030","2017-08-25T01:18:11.030","DF","Sonar","Multibeam","New Line","begin turn line 0454; new ek and sbp lines"]
["2017-08-25T11:39:55.950","2017-08-25T01:39:55.950","DF","Sonar","Multibeam","New Line","begin survey line 0455; new ek and sbp lines"]
["2017-08-25T12:06:27.820","2017-08-25T02:06:27.820","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T13:00:10.120","2017-08-25T03:00:10.120","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T13:10:31.390","2017-08-25T03:10:31.390","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T14:00:36.540","2017-08-25T04:00:36.540","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-25T14:20:20.600","2017-08-25T04:20:20.600","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-25T14:24:24.790","2017-08-25T04:24:24.790","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T14:28:13.710","2017-08-25T04:28:13.710","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T14:46:50.750","2017-08-25T04:46:50.750","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T15:15:35.020","2017-08-25T05:15:35.020","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T15:32:04.950","2017-08-25T05:32:04.950","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T15:48:47.430","2017-08-25T05:48:47.430","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T16:11:40.720","2017-08-25T06:11:40.720","BO","XBT",null,null,"Cast 072 applied to line 0459"]
["2017-08-25T16:24:13.230","2017-08-25T06:24:13.230","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T16:29:57.410","2017-08-25T06:29:57.410","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T17:01:45.810","2017-08-25T07:01:45.810","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T17:05:10.600","2017-08-25T07:05:10.600","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T18:30:38.120","2017-08-25T08:30:38.120","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T18:47:08.400","2017-08-25T08:47:08.400","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T19:39:57.930","2017-08-25T09:39:57.930","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T20:04:50.230","2017-08-25T10:04:50.230","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T20:33:00.910","2017-08-25T10:33:00.910","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-25T20:54:11.480","2017-08-25T10:54:11.480","AB","All",null,null,"New lines started on all sonars (MB 465)"]
["2017-08-25T21:00:11.890","2017-08-25T11:00:11.890","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-25T21:20:48.540","2017-08-25T11:20:48.540","AB","All ",null,null,"New lines started for all sonars (MB 466)"]
["2017-08-25T21:47:24.210","2017-08-25T11:47:24.210","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T21:47:56.540","2017-08-25T11:47:56.540","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T22:15:09.920","2017-08-25T12:15:09.920","CT",null,null,null,"3000-4000"]
["2017-08-25T22:21:22","2017-08-25T12:21:22","AB","Sonar","Multibeam","New Line",467]
["2017-08-25T22:30:09.080","2017-08-25T12:30:09.080","CT","XBT",null,null,"XBT74 added to line 467"]
["2017-08-25T22:55:01.250","2017-08-25T12:55:01.250","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-25T22:56:22.610","2017-08-25T12:56:22.610","AB","Sonar","Multibeam","New Line",468]
["2017-08-25T22:56:38.230","2017-08-25T12:56:38.230","AB","Ship",null,null,"Steering Causalty Drill, new lines started 468. Dropping speed."]
["2017-08-25T23:07:19.270","2017-08-25T13:07:19.270","AB","Ship",null,null,"Drill complete. Coming back around to the line."]
["2017-08-25T23:12:12.130","2017-08-25T13:12:12.130","AB","All",null,null,"All new lines started when back online after the drill. MB line 469. Increasing to survey speed"]
["2017-08-25T23:23:57.710","2017-08-25T13:23:57.710","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-25T23:54:15.660","2017-08-25T13:54:15.660","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T00:41:32.770","2017-08-25T14:41:32.770","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T01:16:27.830","2017-08-25T15:16:27.830","CT","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T01:42:07.590","2017-08-25T15:42:07.590","CT","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T01:57:01.630","2017-08-25T15:57:01.630","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-26T02:02:47.180","2017-08-25T16:02:47.180","AB","All",null,null,"New lines started for \"270 turn\" (MB 472)"]
["2017-08-26T02:08:27.760","2017-08-25T16:08:27.760","AB","All",null,null,"New lines started after turn (MB 473)"]
["2017-08-26T02:45:42.940","2017-08-25T16:45:42.940","CT","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T02:51:33.400","2017-08-25T16:51:33.400","CW","All",null,null,"New survey lines. SIS line 0474"]
["2017-08-26T02:59:54.110","2017-08-25T16:59:54.110","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-26T03:12:03.390","2017-08-25T17:12:03.390","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-26T03:12:21.760","2017-08-25T17:12:21.760","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS."]
["2017-08-26T03:16:28.820","2017-08-25T17:16:28.820","CW","Ship",null,null,"300m move to port for coverage in Extra Deep"]
["2017-08-26T03:18:41.370","2017-08-25T17:18:41.370","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-26T04:02:46.620","2017-08-25T18:02:46.620","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-26T04:34:49.990","2017-08-25T18:34:49.990","CW","XBT",null,null,"XBT 075; applied to SIS line 0476"]
["2017-08-26T04:58:30.750","2017-08-25T18:58:30.750","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-26T04:58:32.840","2017-08-25T18:58:32.840","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS. SIS line 0477"]
["2017-08-26T04:59:55.200","2017-08-25T18:59:55.200","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T05:07:45.560","2017-08-25T19:07:45.560","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T05:35:23.350","2017-08-25T19:35:23.350","CW","All",null,null,"New lines for 270 turn. SIS line 0478"]
["2017-08-26T05:36:28.880",{"$f":"IF(ISBLANK(A908),\" \",((A908)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-25T19:36:28.880"},"CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T05:49:07.950","2017-08-25T19:49:07.950","CW","All",null,null,"New survey lines. SIS line 0479"]
["2017-08-26T05:53:05.620","2017-08-25T19:53:05.620","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T06:39:07.900","2017-08-25T20:39:07.900","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T07:45:29.140","2017-08-25T21:45:29.140","CW","All",null,null,"New survey lines. SIS line 0481"]
["2017-08-26T07:46:09.760","2017-08-25T21:46:09.760","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-26T09:30:05.340","2017-08-25T23:30:05.340","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-26T09:34:25.510","2017-08-25T23:34:25.510","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-08-26T09:53:52.040","2017-08-25T23:53:52.040","CW","XBT",null,null,"XBT 076; applied to SIS line 0483"]
["2017-08-26T10:21:34.950","2017-08-26T00:21:34.950","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-26T10:21:49.020","2017-08-26T00:21:49.020","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-26T10:26:25.480","2017-08-26T00:26:25.480","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-26T10:26:45.010","2017-08-26T00:26:45.010","DF","Sonar","Multibeam","Max Angle","75/75"]
["2017-08-26T10:59:38.940","2017-08-26T00:59:38.940","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-26T12:09:25.860","2017-08-26T02:09:25.860","DF","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-26T12:13:59.530","2017-08-26T02:13:59.530","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-26T12:16:42.640","2017-08-26T02:16:42.640","DF","Sonar","Multibeam","New Line","begin turn line 0486; new ek and sbp lines"]
["2017-08-26T12:24:16.620","2017-08-26T02:24:16.620","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-26T12:43:54.490","2017-08-26T02:43:54.490","DF","Sonar","Multibeam","New Line","begin survey line 0487; new ek and sbp lines"]
["2017-08-26T12:52:44.610","2017-08-26T02:52:44.610","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T14:23:22","2017-08-26T04:23:22","DF","Sonar","Multibeam","New Line","begin turn line 0489; new ek and sbp lines"]
["2017-08-26T14:36:35.840","2017-08-26T04:36:35.840","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-26T14:49:33.710","2017-08-26T04:49:33.710","DF","Sonar","Multibeam","New Line","begin survey line 0490; new ek and sbp lines"]
["2017-08-26T15:05:40.290","2017-08-26T05:05:40.290","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-26T15:06:01.150","2017-08-26T05:06:01.150","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-26T15:14:48.970","2017-08-26T05:14:48.970","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-26T15:15:14.630","2017-08-26T05:15:14.630","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-26T15:15:21.140","2017-08-26T05:15:21.140","DF","Sonar","Multibeam","Max Angle","52/50"]
["2017-08-26T15:21:26.520","2017-08-26T05:21:26.520","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-26T15:21:35.220","2017-08-26T05:21:35.220","DF","Sonar","Multibeam","Max Angle","62/52"]
["2017-08-26T15:23:51.810","2017-08-26T05:23:51.810","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-26T15:46:09.810","2017-08-26T05:46:09.810","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-08-26T15:48:28.480","2017-08-26T05:48:28.480","DF","Sonar","Multibeam","Max Angle","62/50"]
["2017-08-26T16:09:56.600","2017-08-26T06:09:56.600","DF","XBT",null,null,"Cast 077 applied to line 0491"]
["2017-08-26T16:10:43.930","2017-08-26T06:10:43.930","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-26T16:10:50.410","2017-08-26T06:10:50.410","DF","Sonar","Multibeam","Max Angle","60/60"]
["2017-08-26T16:14:11.960","2017-08-26T06:14:11.960","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-26T16:14:28.830","2017-08-26T06:14:28.830","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-26T16:23:09.950","2017-08-26T06:23:09.950","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T16:39:40","2017-08-26T06:39:40","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T16:58:58.540","2017-08-26T06:58:58.540","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-26T17:47:58.660","2017-08-26T07:47:58.660","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-26T17:53:06.230","2017-08-26T07:53:06.230","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T18:21:22.700","2017-08-26T08:21:22.700","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T18:48:05.720","2017-08-26T08:48:05.720","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-26T18:55:02.150","2017-08-26T08:55:02.150","BO","Sonar","Knudsen","phase Range","3500-4500"]
["2017-08-26T18:57:39.410","2017-08-26T08:57:39.410","BO","Sonar","All",null,"New turn line 0495, new lines on ek60 and sbp"]
["2017-08-26T19:18:41.550","2017-08-26T09:18:41.550","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T19:20:40.770","2017-08-26T09:20:40.770","AB","Sonar","Knudsen","phase Range","4500-5500"]
["2017-08-26T19:25:25.510","2017-08-26T09:25:25.510","BO","Sonar","All",null,"new survey line 0496, new lines on ek60 and sbp"]
["2017-08-26T19:26:43.500","2017-08-26T09:26:43.500","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T19:27:33.800","2017-08-26T09:27:33.800","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T20:18:29.200","2017-08-26T10:18:29.200","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-26T21:26:49.760","2017-08-26T11:26:49.760","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-26T22:01:47.300","2017-08-26T12:01:47.300","CT","Other",null,null,"Sun photometer reading!"]
["2017-08-26T22:15:41.120","2017-08-26T12:15:41.120","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-26T22:30:35.520","2017-08-26T12:30:35.520","AB","Sonar","Multibeam","Ping Mode","Deep, 75/75, New line 500"]
["2017-08-26T22:31:54.870","2017-08-26T12:31:54.870","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-26T22:40:08.400","2017-08-26T12:40:08.400","AB","XBT",null,null,"XBT78 added to new line 501"]
["2017-08-26T22:43:14.290","2017-08-26T12:43:14.290","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-26T22:50:05.020","2017-08-26T12:50:05.020","AB","Sonar","Multibeam","Ping Mode","Very Deep, new line 502"]
["2017-08-26T23:04:09.660","2017-08-26T13:04:09.660","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-26T23:18:11.400","2017-08-26T13:18:11.400",null,null,null,null,"MOB Drills."]
["2017-08-26T23:47:00.590","2017-08-26T13:47:00.590","AB","Sonar","Multibeam",null,"Testing line 505 during MOB drills, has copy of cast 78 added with an \"_B\" to test Qimera data processing."]
["2017-08-26T23:47:58.120",{"$f":"IF(ISBLANK(A972),\" \",((A972)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-26T13:47:58.120"},"CT","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-26T23:56:50.060","2017-08-26T13:56:50.060","CT","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T00:12:46.700","2017-08-26T14:12:46.700","AB","All",null,null,"Drill complete. All new lines started (MB507). Moving gradually back to the survey line."]
["2017-08-27T00:38:35.820","2017-08-26T14:38:35.820","AB","Sonar","Knudsen","Phase Range","4000-5000, 3500-4500"]
["2017-08-27T00:59:40.640","2017-08-26T14:59:40.640","AB","Sonar","Multibeam","New Line","0508. Back online from drills."]
["2017-08-27T01:23:45.470","2017-08-26T15:23:45.470","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T01:55:56.200","2017-08-26T15:55:56.200","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T01:56:49.620","2017-08-26T15:56:49.620","CT","Other",null,null,"Sun photometer reading!"]
["2017-08-27T02:08:42.350","2017-08-26T16:08:42.350","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T02:19:04.100","2017-08-26T16:19:04.100","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T02:28:24.180","2017-08-26T16:28:24.180","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T02:42:11.660","2017-08-26T16:42:11.660","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T03:25:49.070","2017-08-26T17:25:49.070","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T03:30:37","2017-08-26T17:30:37","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T03:51:51.140","2017-08-26T17:51:51.140","CT","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T04:01:55.460","2017-08-26T18:01:55.460","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T04:01:55.460","2017-08-26T18:01:55.460","CW","All",null,null,"Turning early. New lines. SIS line 0512"]
["2017-08-27T04:22:01.560","2017-08-26T18:22:01.560","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T04:35:41.550","2017-08-26T18:35:41.550","CW","All ",null,null,"New survey lines. SIS line 0513"]
["2017-08-27T04:48:26.970","2017-08-26T18:48:26.970","CW","XBT",null,null,"XBT 079; applied to SIS line 0513"]
["2017-08-27T06:04:12.150","2017-08-26T20:04:12.150","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T06:04:30.280","2017-08-26T20:04:30.280","CW","Sonar","Knudsen","Tx Power",3]
["2017-08-27T06:08:55.740","2017-08-26T20:08:55.740","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T07:20:33.010","2017-08-26T21:20:33.010","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T07:28:16","2017-08-26T21:28:16","CW","Ship",null,null,"Slow 300m shift to stbd for coverage. Returning to line afterward."]
["2017-08-27T09:35:44.390","2017-08-26T23:35:44.390","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T10:10:23.500","2017-08-27T00:10:23.500","CW","XBT",null,null,"XBT 080; applied to SIS line 0518"]
["2017-08-27T10:13:23.310","2017-08-27T00:13:23.310","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T10:41:35.060","2017-08-27T00:41:35.060","DF","Sonar","Multibeam","New Line","begin turn line 0520; new ek and sbp lines"]
["2017-08-27T10:49:27.560","2017-08-27T00:49:27.560","DF","Sonar","Multibeam",null,"navigation teleportation"]
["2017-08-27T11:09:08.550","2017-08-27T01:09:08.550","DF","Sonar","Multibeam","New Line","begin survey line 0521; newq ek and sbp lines"]
["2017-08-27T11:36:42.460","2017-08-27T01:36:42.460","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T11:47:18.590","2017-08-27T01:47:18.590","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T12:06:39.350","2017-08-27T02:06:39.350","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T12:27:44.440","2017-08-27T02:27:44.440","DF","Sonar","Multibeam","New Line","begin turn line 0523; new ek and sbp lines"]
["2017-08-27T12:53:29.940","2017-08-27T02:53:29.940","DF","Sonar","Multibeam","New Line","begin survey line 0524; new ek and sbp lines"]
["2017-08-27T13:06:57.930","2017-08-27T03:06:57.930","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T13:23:42.770","2017-08-27T03:23:42.770","DF","Sonar","Multibeam",null,"The SV profile and used have become yellow; personnel not availble to conduct and XBT so I will try to monitor the data quality"]
["2017-08-27T13:25:13.870","2017-08-27T03:25:13.870","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-27T13:25:59.760","2017-08-27T03:25:59.760","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-27T13:26:08.670","2017-08-27T03:26:08.670","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-27T13:29:10.650","2017-08-27T03:29:10.650","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-27T13:34:14.570","2017-08-27T03:34:14.570","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-27T13:44:01.070","2017-08-27T03:44:01.070","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-27T13:45:55.630","2017-08-27T03:45:55.630","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T13:52:50.170","2017-08-27T03:52:50.170","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T14:03:00.170","2017-08-27T04:03:00.170","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T14:06:46.590","2017-08-27T04:06:46.590","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T14:17:40.130","2017-08-27T04:17:40.130","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-08-27T14:18:28.530","2017-08-27T04:18:28.530","DF","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-27T14:26:06.980","2017-08-27T04:26:06.980","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-08-27T15:17:13.650","2017-08-27T05:17:13.650","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T15:24:33.250","2017-08-27T05:24:33.250","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-27T15:27:49.290","2017-08-27T05:27:49.290","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-27T15:30:16.280","2017-08-27T05:30:16.280","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T15:38:53.170","2017-08-27T05:38:53.170","DF","Sonar","Multibeam","New Line","begin turn line 0527; new ek and sbp lines"]
["2017-08-27T16:03:14.180","2017-08-27T06:03:14.180","DF","Sonar","Multibeam","New Line","begin turn line 0528; new ek and sbp lines"]
["2017-08-27T16:05:30.120","2017-08-27T06:05:30.120","DF","Sonar","Multibeam","New Line","begin survey line 0529"]
["2017-08-27T16:06:12.660","2017-08-27T06:06:12.660","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T16:16:20.630","2017-08-27T06:16:20.630","DF","XBT",null,null,"Cast 081 applied to line 0529"]
["2017-08-27T16:43:18.030","2017-08-27T06:43:18.030","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-27T16:51:32.820","2017-08-27T06:51:32.820","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T17:15:35.780","2017-08-27T07:15:35.780","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-27T17:15:50.410","2017-08-27T07:15:50.410","DF","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T17:32:41.650",{"$f":"IF(ISBLANK(A1036),\" \",((A1036)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-27T07:32:41.650"},"AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T17:42:18.270","2017-08-27T07:42:18.270","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T17:53:25.660","2017-08-27T07:53:25.660","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T18:00:05.230","2017-08-27T08:00:05.230","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T18:24:48.280","2017-08-27T08:24:48.280","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T18:32:13.940","2017-08-27T08:32:13.940","BO","Sonar","All",null,"New turn line 0532, new lines on Ek60 and SBP"]
["2017-08-27T18:40:33.110","2017-08-27T08:40:33.110","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T18:51:23.600","2017-08-27T08:51:23.600","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-27T19:41:29.830","2017-08-27T09:41:29.830","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-27T20:03:52.730","2017-08-27T10:03:52.730","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-27T20:29:12.500","2017-08-27T10:29:12.500","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-27T20:45:56.140","2017-08-27T10:45:56.140","AB","Sonar",null,null,"All new lines started on all sonars. Transit south begins! MB line 535."]
["2017-08-27T20:49:12.270","2017-08-27T10:49:12.270","AB","Sonar","Multibeam","New Line","New line 536. Increase to warp speed."]
["2017-08-27T20:55:21.660","2017-08-27T10:55:21.660","BO","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-27T21:03:28.390","2017-08-27T11:03:28.390","BO","Sonar","Knudsen","Phase Range","5500-6500"]
["2017-08-27T21:23:38.890","2017-08-27T11:23:38.890","AB","Sonar","Multibeam","Ping Mode","Extra Deep; New line 537"]
["2017-08-27T22:03:58.610","2017-08-27T12:03:58.610","AB","All ",null,null,"All new lines started for turn (MB 538)"]
["2017-08-27T22:11:00.140","2017-08-27T12:11:00.140","CT","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-27T22:33:05.850","2017-08-27T12:33:05.850","AB","Ship",null,null,"Reduced speed to 3 knots for small boat drills."]
["2017-08-27T23:12:22.830","2017-08-27T13:12:22.830","CT","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-27T23:42:25.250","2017-08-27T13:42:25.250","CT","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-27T23:49:44.820","2017-08-27T13:49:44.820","ab","Sonar","Knudsen",null,"Pulse 4, Power 2"]
["2017-08-28T00:15:32.220","2017-08-27T14:15:32.220","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-28T00:15:48.360","2017-08-27T14:15:48.360","AB","Sonar","Multibeam","Ping Mode","Deep, New line 541"]
["2017-08-28T00:38:18.320","2017-08-27T14:38:18.320","AB","Sonar","Knudsen","Gain Value","15 5logR"]
["2017-08-28T01:01:47.230","2017-08-27T15:01:47.230","AB","Ship",null,null,"increasing to transit speed."]
["2017-08-28T01:09:10.950","2017-08-27T15:09:10.950","AB","XBT",null,null,"XBT82 added to new line 542"]
["2017-08-28T01:18:43.530","2017-08-27T15:18:43.530","AB","Sonar","Multibeam","New Line","543, Ping mode Very Deep."]
["2017-08-28T01:20:12.210","2017-08-27T15:20:12.210","AB","Sonar","Knudsen","Phase Range","2500-3500, 18 5logR"]
["2017-08-28T01:40:50.010","2017-08-27T15:40:50.010","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T01:55:52.510","2017-08-27T15:55:52.510","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-28T02:01:25.150","2017-08-27T16:01:25.150","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-28T02:05:27.340","2017-08-27T16:05:27.340","AB","Sonar","Knudsen",null,"Pulse 8, Power 3"]
["2017-08-28T02:18:33.770","2017-08-27T16:18:33.770","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-28T02:18:47.150","2017-08-27T16:18:47.150","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS. SIS line 0544"]
["2017-08-28T09:56:32.920","2017-08-27T23:56:32.920","CW","XBT",null,null,"XBT 083; applied to SIS line 0551"]
["2017-08-28T10:10:14.220","2017-08-28T00:10:14.220","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-08-28T14:07:18.160","2017-08-28T04:07:18.160","DF","Ship",null,null,"Slowed to survey speed for Paganini seamount"]
["2017-08-28T14:08:03.660","2017-08-28T04:08:03.660","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-08-28T14:08:22.400","2017-08-28T04:08:22.400","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-28T14:08:29.870","2017-08-28T04:08:29.870","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-08-28T14:12:07.940","2017-08-28T04:12:07.940","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-28T14:28:17.350","2017-08-28T04:28:17.350","DF","Sonar","Multibeam","New Line","Begin survey line 0557; new ek and sbp lines; Begin Paganini Seamount Survey"]
["2017-08-28T14:35:12.320","2017-08-28T04:35:12.320","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T14:49:31.330","2017-08-28T04:49:31.330","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-28T15:25:58.810","2017-08-28T05:25:58.810","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T15:34:43.170","2017-08-28T05:34:43.170","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-28T15:42:19.630","2017-08-28T05:42:19.630","DF","Sonar","Multibeam","New Line","begin turn line 0559; new ek and sbp lines"]
["2017-08-28T16:03:58.460","2017-08-28T06:03:58.460","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T16:04:57.760","2017-08-28T06:04:57.760","DF","Sonar","Multibeam","New Line","begin survey line 0560; new ek and sbp lines"]
["2017-08-28T16:09:56.980","2017-08-28T06:09:56.980","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-28T16:21:58.050","2017-08-28T06:21:58.050","DF","XBT",null,null,"Cast 084 applied to line 0560"]
["2017-08-28T16:26:26.510","2017-08-28T06:26:26.510","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-28T16:56:01.340","2017-08-28T06:56:01.340","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-28T16:56:15.270","2017-08-28T06:56:15.270","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-28T17:01:11.240","2017-08-28T07:01:11.240","DF","Sonar","Knudsen","Gain Value",19]
["2017-08-28T17:02:03.750","2017-08-28T07:02:03.750","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-28T17:03:00.180","2017-08-28T07:03:00.180","DF","Sonar","Multibeam","Along Direction Pitch",0]
["2017-08-28T17:08:37.140","2017-08-28T07:08:37.140","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T17:13:13.870","2017-08-28T07:13:13.870","DF","Sonar","Multibeam",null,"Geographical display stopped grdding but data was still coming in; tried starting new line and changing gridding settings but no avail"]
["2017-08-28T17:16:17.480","2017-08-28T07:16:17.480","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-28T17:17:12.360","2017-08-28T07:17:12.360","DF","Sonar","Multibeam",null,"Gridding in Geographic indow came back after I started a Waterfall tear off"]
["2017-08-28T17:18:34.460","2017-08-28T07:18:34.460","DF","Sonar","Multibeam","New Line","begin turn line 0563"]
["2017-08-28T17:41:13.510","2017-08-28T07:41:13.510","AB","Sonar","All",null,"All new lines started for turn (SIS line 564)"]
["2017-08-28T17:49:31.740",{"$f":"IF(ISBLANK(A1100),\" \",((A1100)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-28T07:49:31.740"},"BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-28T17:55:36.480","2017-08-28T07:55:36.480","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T18:02:24.170","2017-08-28T08:02:24.170","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-28T18:10:55.960","2017-08-28T08:10:55.960","AB","Ship",null,null,"Shift line plan 500m to NE."]
["2017-08-28T18:12:06.060","2017-08-28T08:12:06.060","BO","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-28T18:13:09.480","2017-08-28T08:13:09.480","AB","Sonar","Multibeam","Ping Mode","Deep, New line 565, Max angle 60/65"]
["2017-08-28T18:16:37.740","2017-08-28T08:16:37.740","AB","Sonar","Multibeam","Max Angle","75/75"]
["2017-08-28T18:25:23.950","2017-08-28T08:25:23.950","AB","Sonar",null,null,"New line 566"]
["2017-08-28T18:33:05.840","2017-08-28T08:33:05.840","BO","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-28T18:47:36.880","2017-08-28T08:47:36.880","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-28T18:59:00.240","2017-08-28T08:59:00.240","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T19:03:00.430","2017-08-28T09:03:00.430","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-28T19:04:53.450","2017-08-28T09:04:53.450","AB","Sonar","All",null,"All new lines started for turn. MB line 567"]
["2017-08-28T19:05:49.460","2017-08-28T09:05:49.460","AB","Sonar","Multibeam","New Line",568]
["2017-08-28T19:06:16.920","2017-08-28T09:06:16.920","AB","Ship",null,null,"increasing to transit speed. (About 9.5 in the 075 direction)"]
["2017-08-28T19:08:09.200","2017-08-28T09:08:09.200","AB","Other",null,null,"POS in VBS."]
["2017-08-28T19:17:49.430","2017-08-28T09:17:49.430","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-28T19:39:59.330","2017-08-28T09:39:59.330","AB","Sonar","Multibeam","Ping Mode","Extra Deep. 35/35"]
["2017-08-28T19:50:13.190","2017-08-28T09:50:13.190","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-28T20:37:07.950","2017-08-28T10:37:07.950","BO","Other",null,null,"Sun photometer reading!"]
["2017-08-28T22:23:15.600","2017-08-28T12:23:15.600","AB","XBT",null,null,"XBT85 added to new line 572"]
["2017-08-28T22:25:21.730","2017-08-28T12:25:21.730","AB","Other",null,null,"POS in VBS. Seems in VBS more frequently today."]
["2017-08-28T22:31:49.650","2017-08-28T12:31:49.650","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-28T22:39:00.110","2017-08-28T12:39:00.110","AB","Sonar","Multibeam","Ping Mode","Very Deep, New line 573, Max angle 52/52"]
["2017-08-28T22:45:46.120","2017-08-28T12:45:46.120","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-28T22:50:14.380","2017-08-28T12:50:14.380","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T22:57:34.600","2017-08-28T12:57:34.600","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-28T23:01:30.290","2017-08-28T13:01:30.290","AB","Sonar","All",null,"All new lines started for turn (MB line 574)"]
["2017-08-28T23:04:19.160","2017-08-28T13:04:19.160","AB",null,"Multibeam","New Line","575, line over Mozart Seamount for EX1708"]
["2017-08-28T23:05:38.120","2017-08-28T13:05:38.120","CT","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-28T23:27:19.900","2017-08-28T13:27:19.900","ab","Sonar","Multibeam","New Line","576, deep"]
["2017-08-28T23:33:52.700","2017-08-28T13:33:52.700","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-28T23:37:42.560","2017-08-28T13:37:42.560","AB","Sonar","Multibeam","Ping Mode","Very Deep, new line 577"]
["2017-08-28T23:42:13.760","2017-08-28T13:42:13.760","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-28T23:46:40.910","2017-08-28T13:46:40.910","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T00:00:50.810","2017-08-28T14:00:50.810","AB","Sonar","Knudsen","Phase Range","4500-5000"]
["2017-08-29T00:22:27.950","2017-08-28T14:22:27.950","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-08-29T01:01:59.290","2017-08-28T15:01:59.290","AB","Sonar","Multibeam","Max Angle","52/52"]
["2017-08-29T01:59:44.130","2017-08-28T15:59:44.130","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-29T03:48:05.120","2017-08-28T17:48:05.120","CT","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-29T03:54:37.720","2017-08-28T17:54:37.720","CT","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T04:00:13.210","2017-08-28T18:00:13.210","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-29T04:21:26.780","2017-08-28T18:21:26.780","CW","Sonar","Multibeam","Ping Mode","Deep."]
["2017-08-29T04:21:52.790","2017-08-28T18:21:52.790","CW","Sonar","Multibeam","New Line","New line for sweet BS. SIS line 0582"]
["2017-08-29T04:24:11.430","2017-08-28T18:24:11.430","CW","Sonar","Knudsen","Phase Range","3500-3500"]
["2017-08-29T04:27:48.370","2017-08-28T18:27:48.370","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-29T04:38:00.330","2017-08-28T18:38:00.330","CW","POS",null,null,"Bouncing around in Marinestar VBS and GAMS - Not Ready for several minutes."]
["2017-08-29T04:39:22.920","2017-08-28T18:39:22.920","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T04:49:20.620","2017-08-28T18:49:20.620","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T04:52:32.490","2017-08-28T18:52:32.490","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-29T04:52:34.660","2017-08-28T18:52:34.660","CW","Sonar","Multibeam","New Line","New line for sweet BS. SIS line 0583"]
["2017-08-29T05:01:48.900","2017-08-28T19:01:48.900","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T05:03:28.350","2017-08-28T19:03:28.350","CT","XBT",null,null,"Cast 086 at line 0583"]
["2017-08-29T05:21:53.080","2017-08-28T19:21:53.080","CT","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-29T05:36:47.490","2017-08-28T19:36:47.490","CW","All ",null,null,"New lines for turn. SIS line 0584"]
["2017-08-29T05:37:11.060","2017-08-28T19:37:11.060","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-29T07:24:32.320","2017-08-28T21:24:32.320","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-29T07:24:33.590","2017-08-28T21:24:33.590","CW","Sonar","Multibeam","New Line","New line for sweet BS. SIS line 0586"]
["2017-08-29T07:25:44.220","2017-08-28T21:25:44.220","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T07:34:36.930","2017-08-28T21:34:36.930","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-29T07:52:28.210","2017-08-28T21:52:28.210","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T08:07:22.590","2017-08-28T22:07:22.590","CW","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-29T08:08:55.330","2017-08-28T22:08:55.330","CW","Sonar","Multibeam","New Line","New line for sweet BS. SIS line 0587"]
["2017-08-29T08:09:07.230","2017-08-28T22:09:07.230","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T08:23:46.530",{"$f":"IF(ISBLANK(A1164),\" \",((A1164)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-28T22:23:46.530"},"CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-29T08:23:48.280","2017-08-28T22:23:48.280","CW","Sonar","Multibeam","New Line","New line for sweet BS. SIS line 0588"]
["2017-08-29T08:24:15.770","2017-08-28T22:24:15.770","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-29T08:34:41.650","2017-08-28T22:34:41.650","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T08:43:03.020","2017-08-28T22:43:03.020","CW","All",null,null,"New lines for turn to Sibelius Seamount line plan. SIS line 0589"]
["2017-08-29T09:26:58.990","2017-08-28T23:26:58.990","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-29T09:53:56.240","2017-08-28T23:53:56.240","CW","XBT",null,null,"XBT 087; applied to SIS line 0590"]
["2017-08-29T10:10:03.170","2017-08-29T00:10:03.170","DF","Sonar","Multibeam","New Line","begin turn line 0591; new ek and sbp lines"]
["2017-08-29T10:10:30.490","2017-08-29T00:10:30.490","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-29T10:20:26.340","2017-08-29T00:20:26.340","DF","Sonar","Multibeam","New Line","begin survey line 0592; new ek and sbp lines; Start Sibelius Seamount Survey."]
["2017-08-29T10:32:02.240","2017-08-29T00:32:02.240","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T10:37:57.960","2017-08-29T00:37:57.960","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-29T10:38:03.910","2017-08-29T00:38:03.910","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-29T10:45:31.650","2017-08-29T00:45:31.650","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T10:54:35.030","2017-08-29T00:54:35.030","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-29T11:03:53.750","2017-08-29T01:03:53.750","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T11:28:19.670","2017-08-29T01:28:19.670","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T11:30:18.830","2017-08-29T01:30:18.830","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-29T12:06:17.370","2017-08-29T02:06:17.370","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-29T12:43:43.140","2017-08-29T02:43:43.140","DF","Sonar","Multibeam","New Line","begin turn line 0595; new ek and sbp lines"]
["2017-08-29T13:06:40.190","2017-08-29T03:06:40.190","DF","Sonar","Multibeam","New Line","begin survey line 0596; new ek and abp lines"]
["2017-08-29T13:12:27.470","2017-08-29T03:12:27.470","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T13:18:15.870","2017-08-29T03:18:15.870","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-29T13:42:22.050","2017-08-29T03:42:22.050","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T13:59:48.370","2017-08-29T03:59:48.370","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T14:07:47.690","2017-08-29T04:07:47.690","DF","Sonar","Multibeam",null,"Geographic display stopped gridding AGAIN!!! Not sure why it keeps doing this but it seems to be around the same distance/duration before coming back. Charlie noticed this over time."]
["2017-08-29T14:12:04.160","2017-08-29T04:12:04.160","DF","Sonar","Multibeam",null,"Switched to Very Deep from Deep ping mode and the geographical display came back immediately. Im not 100% sure that’s what corrected it or coincidence."]
["2017-08-29T14:32:03.640","2017-08-29T04:32:03.640","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-29T14:32:52.990","2017-08-29T04:32:52.990","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T14:43:00.600","2017-08-29T04:43:00.600","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-29T15:11:01.960","2017-08-29T05:11:01.960","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T15:26:16.120","2017-08-29T05:26:16.120","DF","Sonar","Multibeam","New Line","Begin turn line 0599; new ek and sbp lines"]
["2017-08-29T15:47:15.210","2017-08-29T05:47:15.210","DF","Sonar","Multibeam","New Line","begin survey line 0600; new ek and sbp lines"]
["2017-08-29T15:48:05.670","2017-08-29T05:48:05.670","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T15:53:28.770","2017-08-29T05:53:28.770","DF","Ship",null,null,"requested 1000 m move to PORT for coverage"]
["2017-08-29T15:58:56.670","2017-08-29T05:58:56.670","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-29T16:18:40.740","2017-08-29T06:18:40.740","BO","XBT",null,null,"csat 88, applied to line 0600"]
["2017-08-29T16:30:27.100","2017-08-29T06:30:27.100","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T16:48:16.050","2017-08-29T06:48:16.050","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T16:53:53.410","2017-08-29T06:53:53.410","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-29T17:28:41.090","2017-08-29T07:28:41.090","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-29T17:35:58.530","2017-08-29T07:35:58.530","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-29T17:40:26.130","2017-08-29T07:40:26.130","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-29T18:09:09.540","2017-08-29T08:09:09.540","BO","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-29T18:13:41.390","2017-08-29T08:13:41.390","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-29T18:17:44.530","2017-08-29T08:17:44.530","BO","Sonar","All",null,"new line 0603, new lines on ek60 and sbp, end of Sibelius seamount survey, speed increased to maximum"]
["2017-08-29T18:21:16.310","2017-08-29T08:21:16.310","AB","Sonar","Multibeam","Ping Mode","Very Deep, new line 604"]
["2017-08-29T18:22:22.920","2017-08-29T08:22:22.920","BO","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T18:29:23.290","2017-08-29T08:29:23.290","BO","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-29T18:53:46.450","2017-08-29T08:53:46.450","AB","Sonar","Multibeam","Ping Mode","Extra Deep. 35/35. new line 605"]
["2017-08-29T18:57:42.310","2017-08-29T08:57:42.310","AB","Ship",null,null,"Shift back to original line plan"]
["2017-08-29T19:42:39.950","2017-08-29T09:42:39.950","BO","Other",null,null,"Sun Photometer reading!!"]
["2017-08-29T20:02:08.970","2017-08-29T10:02:08.970","AB","Sonar","Multibeam","Ping Mode","Very Deep, New line 607, pre-turn"]
["2017-08-29T20:03:38.810","2017-08-29T10:03:38.810","AB","Sonar",null,null,"New lines started on EK60 and Knudsen, turn"]
["2017-08-29T20:05:36.770","2017-08-29T10:05:36.770","AB","Sonar","Multibeam","New Line","new line for turn. MB line 608"]
["2017-08-29T20:10:38.760","2017-08-29T10:10:38.760","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T20:14:57.230","2017-08-29T10:14:57.230","AB","Sonar","Knudsen",null,"Gain 18, Pulse 8, Power 3"]
["2017-08-29T20:32:53.930","2017-08-29T10:32:53.930","BO","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-29T20:40:31.190","2017-08-29T10:40:31.190","AB","Sonar","Knudsen",null,"Power 2"]
["2017-08-29T21:07:36.040","2017-08-29T11:07:36.040","AB","Sonar","Multibeam","New Line",609]
["2017-08-29T21:09:23.450","2017-08-29T11:09:23.450","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-29T21:15:05.560","2017-08-29T11:15:05.560","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-29T21:26:25.380","2017-08-29T11:26:25.380","AB","Sonar","Multibeam","New Line",609]
["2017-08-29T21:57:51.400","2017-08-29T11:57:51.400","AB","Ship",null,null,"Track shifted 500m to port."]
["2017-08-29T22:08:42.760",{"$f":"IF(ISBLANK(A1228),\" \",((A1228)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-29T12:08:42.760"},"AB","XBT",null,null,"XBT89 added to new line 611, extra deep ping mode, 35/35"]
["2017-08-29T22:56:39.390","2017-08-29T12:56:39.390","CT","Other",null,null,"Sun photometer reading"]
["2017-08-30T00:49:14.820","2017-08-29T14:49:14.820","CT","Other",null,null,"Sun photometer reading"]
["2017-08-30T01:34:57.200","2017-08-29T15:34:57.200","AB","Sonar","Multibeam","Ping Mode","Very Deep, 52/52. New line started 615."]
["2017-08-30T01:43:29.840","2017-08-29T15:43:29.840","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-30T01:44:09.730","2017-08-29T15:44:09.730","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-30T01:54:45.220","2017-08-29T15:54:45.220","AB","All",null,null,"All new lines started for turn (MB line 616)."]
["2017-08-30T02:09:31.400","2017-08-29T16:09:31.400","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-30T02:23:11","2017-08-29T16:23:11","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-30T03:00:35","2017-08-29T17:00:35","CW","All",null,null,"New lines for turn. SIS line 0618"]
["2017-08-30T03:08:38.240","2017-08-29T17:08:38.240","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-30T03:09:11.310","2017-08-29T17:09:11.310","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-30T03:12:48.730","2017-08-29T17:12:48.730","CW","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-30T03:12:58.050","2017-08-29T17:12:58.050","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS. SIS line 0619"]
["2017-08-30T03:13:23.940","2017-08-29T17:13:23.940","CW","Sonar","Multibeam","Max Angle","Incrementing angles to 75/75"]
["2017-08-30T03:14:15.370","2017-08-29T17:14:15.370","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-30T03:57:54.070","2017-08-29T17:57:54.070","CT","All",null,null,"New lines for turn. SIS line 0620"]
["2017-08-30T04:08:41.990","2017-08-29T18:08:41.990","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-30T05:03:30.090","2017-08-29T19:03:30.090","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-30T05:12:35.480","2017-08-29T19:12:35.480","CW","All",null,null,"New lines for turn. SIS line 0622"]
["2017-08-30T05:12:42.620","2017-08-29T19:12:42.620","CW","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-08-30T05:25:24.490","2017-08-29T19:25:24.490","CW","Sonar","Multibeam","Ping Mode","Extra Deep"]
["2017-08-30T05:25:26.390","2017-08-29T19:25:26.390","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS. SIS line 0623"]
["2017-08-30T05:46:10.390","2017-08-29T19:46:10.390","CW","XBT",null,null,"XBT 090; applied to SIS line 0623"]
["2017-08-30T06:26:06.980","2017-08-29T20:26:06.980","CW","Ship",null,null,"Moving stbd for coverage"]
["2017-08-30T06:39:17.520","2017-08-29T20:39:17.520","CW","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-30T06:39:20.210","2017-08-29T20:39:20.210","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS. SIS line 0625"]
["2017-08-30T07:39:11.620","2017-08-29T21:39:11.620","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-30T09:04:28.260","2017-08-29T23:04:28.260","CW","Ship",null,null,"500m move to port for holiday pickup near Char-Cheko Crater"]
["2017-08-30T09:54:47.940","2017-08-29T23:54:47.940","CW","XBT",null,null,"XBT 091; applied to SIS line 0628"]
["2017-08-30T13:56:52.990","2017-08-30T03:56:52.990","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-30T14:53:19.050","2017-08-30T04:53:19.050","DF","Ship",null,null,"Requested 3000 m move to STBD for coverage"]
["2017-08-30T16:09:05.800","2017-08-30T06:09:05.800","DF","XBT",null,null,"Cast 092 applied to line 0634"]
["2017-08-30T16:11:38.360","2017-08-30T06:11:38.360","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-30T16:35:35.270","2017-08-30T06:35:35.270","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-30T17:53:33.620","2017-08-30T07:53:33.620","AB","Sonar","Multibeam",null,"Turned off scanning function. It was not turned on by any person."]
["2017-08-30T19:53:11.670","2017-08-30T09:53:11.670","BO","Other",null,null,"sun photometer reading "]
["2017-08-30T21:04:13.950","2017-08-30T11:04:13.950","AB","Ship",null,null,"Shifting slowing back to original Transit south trackline from 3000m offset."]
["2017-08-30T22:48:06.960","2017-08-30T12:48:06.960","AB","XBT",null,null,"XBT93 added to line 642"]
["2017-08-30T23:00:12.360","2017-08-30T13:00:12.360","CT","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-31T00:58:04.750","2017-08-30T14:58:04.750","CT","Other",null,null,"Sun photometer reading"]
["2017-08-31T01:44:51.200","2017-08-30T15:44:51.200","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-08-31T02:39:22.860","2017-08-30T16:39:22.860","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-08-31T02:53:28.940","2017-08-30T16:53:28.940","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-08-31T03:06:41.290","2017-08-30T17:06:41.290","CW","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-31T03:06:42.870","2017-08-30T17:06:42.870","CW","Sonar","Multibeam","New Line","New line for new Ping Mode and sweet BS. SIS line 0647"]
["2017-08-31T03:06:44.770","2017-08-30T17:06:44.770","CW","Sonar","Multibeam","Max Angle","Incrementing angles to 75/75"]
["2017-08-31T03:10:08.120","2017-08-30T17:10:08.120","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-31T03:11:22.290","2017-08-30T17:11:22.290","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-31T03:49:43.760","2017-08-30T17:49:43.760","CT","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-31T04:10:12.420","2017-08-30T18:10:12.420","CT","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-08-31T04:53:35.650","2017-08-30T18:53:35.650","CW","XBT",null,null,"XBT 094; applied to SIS line 0648"]
["2017-08-31T04:56:02.140","2017-08-30T18:56:02.140","CW","Sonar","Knudsen","Tx Power",1]
["2017-08-31T04:56:18.930","2017-08-30T18:56:18.930","CW","Sonar","Knudsen","Tx Pulse",4]
["2017-08-31T04:57:09.690","2017-08-30T18:57:09.690","CW","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-31T05:25:58.270","2017-08-30T19:25:58.270","CW","Sonar","Knudsen","Phase Range","500-1500"]
["2017-08-31T05:28:05.980","2017-08-30T19:28:05.980","CW","Sonar","Multibeam","Ping Mode","Auto for Deep 1 & 2 switch"]
["2017-08-31T06:39:54.530","2017-08-30T20:39:54.530","CW","Sonar","Multibeam","Ping Mode","Big ol slope. Back to Manual Deep"]
["2017-08-31T06:40:45.920","2017-08-30T20:40:45.920","CW","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-08-31T06:41:15.870","2017-08-30T20:41:15.870","CW","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-31T06:41:40.260","2017-08-30T20:41:40.260","CW","Sonar","Knudsen","Tx Power",2]
["2017-08-31T06:46:55.450","2017-08-30T20:46:55.450","CW","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-31T07:18:57.630","2017-08-30T21:18:57.630","CW","Sonar","Multibeam",null,"Sector dropout crap. Forrced it into VD, then back to D"]
["2017-08-31T07:21:33.600","2017-08-30T21:21:33.600","CW","All",null,null,"New lines for turn. SIS line 0652"]
["2017-08-31T09:11:23.070",{"$f":"IF(ISBLANK(A1292),\" \",((A1292)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-08-30T23:11:23.070"},"DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-08-31T09:37:36.850","2017-08-30T23:37:36.850","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-31T09:50:00.140","2017-08-30T23:50:00.140","CW","XBT",null,null,"XBT 095; applied to SIS line 0654"]
["2017-08-31T11:21:12.010","2017-08-31T01:21:12.010","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-08-31T11:30:30.710","2017-08-31T01:30:30.710","DF","Sonar","Multibeam","Ping Mode","Very Deep"]
["2017-08-31T11:31:03.370","2017-08-31T01:31:03.370","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-08-31T11:39:34.200","2017-08-31T01:39:34.200","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-31T11:41:52.600","2017-08-31T01:41:52.600","DF","Sonar","Multibeam","Ping Mode","Very Deep; kept losing bottom in Deep"]
["2017-08-31T11:42:30.300","2017-08-31T01:42:30.300","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-08-31T12:06:26.460","2017-08-31T02:06:26.460","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-31T12:07:44.910","2017-08-31T02:07:44.910","DF","Sonar","Multibeam","Ping Mode","Very Deep; still lossing bottom in Deep (~3100 m)"]
["2017-08-31T12:09:36.750","2017-08-31T02:09:36.750","DF","Sonar","Multibeam","New Line","begin turn line 0657; new ek and sbp lines"]
["2017-08-31T12:19:00.760","2017-08-31T02:19:00.760","DF","Sonar","Multibeam","New Line","begin survey line 0658; new ek and sbp lines; 6 knots"]
["2017-08-31T12:21:12.740","2017-08-31T02:21:12.740","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-08-31T12:21:18.690","2017-08-31T02:21:18.690","DF","Sonar","Multibeam","Ping Mode","Deep"]
["2017-08-31T12:55:07.560","2017-08-31T02:55:07.560","DF","Sonar","Multibeam",null,"Complete white out of the water column window for about 5-8 seconds. 2x's"]
["2017-08-31T12:58:46.250","2017-08-31T02:58:46.250","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-08-31T13:03:45.840","2017-08-31T03:03:45.840","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-08-31T13:03:56.250","2017-08-31T03:03:56.250","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-08-31T13:10:32.020","2017-08-31T03:10:32.020","DF","Sonar","Multibeam","Ping Mode","AUTO"]
["2017-08-31T13:10:40.500","2017-08-31T03:10:40.500","DF","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-08-31T13:11:04.330","2017-08-31T03:11:04.330","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-08-31T13:20:25.620","2017-08-31T03:20:25.620","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-08-31T13:21:20.020","2017-08-31T03:21:20.020","DF","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-08-31T13:24:26.480","2017-08-31T03:24:26.480","DF","Sonar","Multibeam",null,"Getting holes in the out sector boundaries"]
["2017-08-31T13:31:28.310","2017-08-31T03:31:28.310","DF","Sonar","Knudsen","Phase Range","500-1500"]
["2017-08-31T13:37:04.140","2017-08-31T03:37:04.140","DF","Sonar","Multibeam","Max Angle","62/70"]
["2017-08-31T13:39:25.360","2017-08-31T03:39:25.360","DF","Sonar","Multibeam","Max Angle","60/73; brought angles in the reduce holes"]
["2017-08-31T13:40:32.770","2017-08-31T03:40:32.770","DF","Sonar","Multibeam","Max Angle","70/75"]
["2017-08-31T13:47:32.650","2017-08-31T03:47:32.650","DF","Sonar","Multibeam","Max Angle","75/75"]
["2017-08-31T14:10:17.530","2017-08-31T04:10:17.530","DF","Sonar","Multibeam","New Line","begin transit line 0660; end target survey. New ek and sbp lines"]
["2017-08-31T14:12:00.890","2017-08-31T04:12:00.890","DF","Ship",null,null,"Will make necessary speed to arrive at PH by 0615"]
["2017-08-31T14:30:01.250","2017-08-31T04:30:01.250","DF","Sonar","Knudsen",null,"Secured recording and pinging <500 m"]
["2017-08-31T15:52:22.030","2017-08-31T05:52:22.030","DF","Sonar",null,null,"Secured MB and EK for PH approach"]
["2017-08-31T16:06:43.300","2017-08-31T06:06:43.300","DF","Sonar","Multibeam",null,"SIS crashed while closing out the Helmsman display; reopened to run final BIST and export PU param."]
["2017-08-31T18:35:34.830","2017-08-31T08:35:34.830","AB",null,null,null,"Topside units powered down. Dock at Pier F9 Ford Island."]
[null,{"$f":"IF(ISBLANK(A1328),\" \",((A1328)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1353),\" \",((A1353)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1417),\" \",((A1417)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1481),\" \",((A1481)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1545),\" \",((A1545)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1609),\" \",((A1609)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1673),\" \",((A1673)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1737),\" \",((A1737)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1801),\" \",((A1801)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1865),\" \",((A1865)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1929),\" \",((A1929)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1993),\" \",((A1993)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":14,"n_cols":7,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["AB","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DF","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["CW","Weather","Knudsen","New Line","Secure","Gain Mode","New Lines"]
["BO","Watch Change","All","Max Angle","Start Recording","Gain Value"]
["CT","XBT",null,"Spike Filter Strength","Bottom Detection","Process Shift"]
[null,"Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
[null,"Other",null,"Aeration Filter (On/Off)",null,"Range"]
[null,"Sun photometer",null,"Interference Filter (On/Off)",null,"Phase Mode"]
[null,null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]
[null,null,null,"BIST",null,"Start Recording"]
[null,null,null,"Warning"]