{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":8,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":836,"n_cols":7,"rows_kept":836,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1710","UTC to Local Ratio: ",5,"UTM17N","UTM16N",null,"Cruise Details: Nov 15th - Nov 22nd"]
[]
["UTC Time","Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2017-11-16T05:20:24",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569-(C1/24))","v":"2017-11-16T00:20:24"},"CW","Sonar","Multibeam","BIST","BIST 01 All Pass. Yeeeeahhhhh!!!"]
["2017-11-16T10:39:00.280",{"$f":"IF(ISBLANK(A6),\" \",((A6)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-11-16T05:39:00.280"},"DF","Sonar","EK",null,"Started pinging."]
["2017-11-16T10:43:30.560",{"$f":"IF(ISBLANK(A7),\" \",((A7)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-11-16T05:43:30.560"},"DF","Sonar","Multibeam","BIST","Running BIST 02"]
["2017-11-16T10:46:55.520","2017-11-16T05:46:55.520","DF","Ship",null,null,"Manuvering for traffic"]
["2017-11-16T10:53:02.060","2017-11-16T05:53:02.060","DF","Sonar","Multibeam","BIST","BIST 02 All Pass"]
["2017-11-16T10:55:01.160","2017-11-16T05:55:01.160","DF","Sonar","Multibeam",null,"Started TSG. Started pinging. Marine mammal mode"]
["2017-11-16T11:12:39.280","2017-11-16T06:12:39.280","DF","XBT",null,null,"Cast 001 applied to line 0000, cast was only to 55 m, will do another when we are in deeper waters"]
["2017-11-16T11:25:07.290","2017-11-16T06:25:07.290","DF","Sonar","Multibeam",null,"Began logging"]
["2017-11-16T11:34:28.960","2017-11-16T06:34:28.960","DF","Sonar","EK",null,"Started logging"]
["2017-11-16T12:36:58.300","2017-11-16T07:36:58.300","DF","XBT",null,null,"Cast 002 applied to line 0001"]
["2017-11-16T12:57:04.130","2017-11-16T07:57:04.130","KL","Sonar","All","New line","New lines for turn, MB line 0002"]
["2017-11-16T13:26:17.550","2017-11-16T08:26:17.550","KL","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-16T13:38:29.470","2017-11-16T08:38:29.470","DF","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-16T13:56:16.330","2017-11-16T08:56:16.330","DF","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-11-16T14:06:27.300","2017-11-16T09:06:27.300","KL","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-16T14:44:34.770","2017-11-16T09:44:34.770","KL","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-11-16T14:51:32.550","2017-11-16T09:51:32.550","KL","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-16T15:12:44.110","2017-11-16T10:12:44.110","CW","Sonar","Knudsen","Tx Power",3]
["2017-11-16T15:26:43.120","2017-11-16T10:26:43.120","KL","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-11-16T15:32:39.210","2017-11-16T10:32:39.210","KL","Sonar","Knudsen","Phase Range","2750-3250"]
["2017-11-16T16:26:43.980","2017-11-16T11:26:43.980","KL","Sonar","Knudsen","Phase Range","3000-3500"]
["2017-11-16T16:38:36.530","2017-11-16T11:38:36.530","CW","Sonar","Knudsen","Phase Range","2750-3250"]
["2017-11-16T16:58:39.940","2017-11-16T11:58:39.940","KL","Sonar","Knudsen","Phase Range","3000-3500"]
["2017-11-16T17:06:24.060","2017-11-16T12:06:24.060","AB","Sonar","Knudsen",null,"Tx Power 2, Tx Pulse 8"]
["2017-11-16T17:37:54.810","2017-11-16T12:37:54.810","CW","XBT",null,null,"XBT 003; applied to line 0006"]
["2017-11-16T19:59:13.660","2017-11-16T14:59:13.660","CW","Sonar","All","New line","New lines for turn, MB line 0010"]
["2017-11-16T21:12:33.060","2017-11-16T16:12:33.060","AB","ADCP",null,null,"passive logging"]
["2017-11-16T21:56:09.030","2017-11-16T16:56:09.030","AB","Sonar","Knudsen","Phase Range","3000-3500m"]
["2017-11-16T22:31:03.520","2017-11-16T17:31:03.520","AB","Sonar","Knudsen","Phase Range","2750-3250"]
["2017-11-16T23:25:24","2017-11-16T18:25:24","AB","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-11-17T00:11:44.300","2017-11-16T19:11:44.300","AB","Sonar","Multibeam",null,"Interference on sonar."]
["2017-11-17T00:24:40.220","2017-11-16T19:24:40.220","AB","XBT",null,null,"XBT004 added to MB line 0014"]
["2017-11-17T00:27:36.460","2017-11-16T19:27:36.460","AB","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-17T00:33:56.690","2017-11-16T19:33:56.690","AB","Sonar","Multibeam",null,"Sonar interference, nothing from the bridge, no contacts"]
["2017-11-17T00:49:55.160","2017-11-16T19:49:55.160","AB","Sonar","Multibeam","Along Direction Pitch","-1"]
["2017-11-17T00:59:32.540","2017-11-16T19:59:32.540","AB","Sonar","Multibeam","Ping mode","Very Deep"]
["2017-11-17T01:38:38.910","2017-11-16T20:38:38.910","AB","Sonar",null,null,"All sonars secured. ADCP secured."]
["2017-11-17T01:44:53.510","2017-11-16T20:44:53.510","AB",null,null,null,"SCS data secured and restarted with position data only."]
["2017-11-17T18:12:59.240","2017-11-17T13:12:59.240","DS","Sonar","Multibeam","Start Pinging","soft start multibeam in Nicaraguan waters"]
["2017-11-17T18:19:18.940","2017-11-17T13:19:18.940","DS","Sonar","Multibeam","Start Logging","full power"]
["2017-11-17T18:22:26.490","2017-11-17T13:22:26.490","AB","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-17T18:57:55.510","2017-11-17T13:57:55.510","AB","Sonar",null,null,"New lines started on all sonars for turn. MB line 0017."]
["2017-11-17T19:02:34.770","2017-11-17T14:02:34.770","AB","XBT",null,null,"XBT5 added to line 0017"]
["2017-11-17T19:10:25.360","2017-11-17T14:10:25.360","AB","Sonar","Multibeam",null,"Display gap"]
["2017-11-17T19:58:14.660","2017-11-17T14:58:14.660","AB","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-17T20:55:21.440","2017-11-17T15:55:21.440","DS","Sonar","Multibeam","Along Direction Pitch","set tilt to -1 to get rid of \"horns\" near nadir"]
["2017-11-17T21:23:15.230","2017-11-17T16:23:15.230","CW","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-17T21:27:10.850","2017-11-17T16:27:10.850","CW","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-11-17T23:16:09.420","2017-11-17T18:16:09.420","AB","Sonar","Multibeam","New line","0022"]
["2017-11-18T00:14:01","2017-11-17T19:14:01","AB","Sonar","Multibeam","New line","0023"]
["2017-11-18T01:06:30.280","2017-11-17T20:06:30.280","VD","XBT",null,null,"XBT 006 added to line 0023"]
["2017-11-18T01:17:59.830","2017-11-17T20:17:59.830","AB","Sonar","Multibeam","New line","0024"]
["2017-11-18T01:20:10.430","2017-11-17T20:20:10.430","AB","Sonar","Multibeam",null,"Video display gap"]
["2017-11-18T03:14:32","2017-11-17T22:14:32","AB","Sonar","Multibeam","New line","0026"]
["2017-11-18T03:27:01.370","2017-11-17T22:27:01.370","AB","Sonar",null,null,"New lines started on all sonars for turn. MB line 0027."]
["2017-11-18T03:30:04.110","2017-11-17T22:30:04.110","AB","Sonar","Multibeam","New line","0028 after turn."]
["2017-11-18T03:50:14.990","2017-11-17T22:50:14.990","AB","Sonar","Knudsen","Phase Range","750-1250m"]
["2017-11-18T04:50:45.840","2017-11-17T23:50:45.840","DF","Sonar","Knudsen","Phase Range","500-1000"]
["2017-11-18T05:03:26.720","2017-11-18T00:03:26.720","DF","Sonar","Multibeam",null,"Some kind of interference caused an almost total los of the PORT side of the swath. "]
["2017-11-18T05:21:30.980","2017-11-18T00:21:30.980","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-11-18T05:31:45.840","2017-11-18T00:31:45.840","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-11-18T05:47:53.550","2017-11-18T00:47:53.550","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-11-18T05:50:02.690","2017-11-18T00:50:02.690","DF","Sonar","Knudsen","Phase Range","250-750"]
["2017-11-18T05:53:57.510","2017-11-18T00:53:57.510","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-11-18T07:09:34.850","2017-11-18T02:09:34.850","VD","XBT",null,null,"cast 007 applied to line 0031"]
["2017-11-18T07:55:36.070","2017-11-18T02:55:36.070","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-11-18T08:58:46",{"$f":"IF(ISBLANK(A71),\" \",((A71)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-11-18T03:58:46"},"DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-11-18T11:10:33.480","2017-11-18T06:10:33.480","DF","Sonar","Multibeam","New line","Manuvering for traffic"]
["2017-11-18T13:28:55.610","2017-11-18T08:28:55.610","KL","Sonar","Knudsen","Phase Range","Phase shift to 750-1250"]
["2017-11-18T13:38:32.190","2017-11-18T08:38:32.190","CW","Sonar","Knudsen","Tx Power","power increased to 2"]
["2017-11-18T13:53:44.130","2017-11-18T08:53:44.130","CW","Sonar","Knudsen","Tx Pulse","2 ms"]
["2017-11-18T13:53:45.920","2017-11-18T08:53:45.920","CW","XBT",null,null,"XBT 008; applied to line 0038"]
["2017-11-18T14:23:51.120","2017-11-18T09:23:51.120","KL","Sonar","Knudsen","Phase Range","1000-1500m"]
["2017-11-18T15:12:56.230","2017-11-18T10:12:56.230","KL","Sonar","Knudsen","Phase Range","1250-1750m"]
["2017-11-18T16:19:46.020","2017-11-18T11:19:46.020","CW","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-18T16:22:46","2017-11-18T11:22:46","CW","Sonar","Knudsen","Tx Power",3]
["2017-11-18T16:28:24.930","2017-11-18T11:28:24.930","CW","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-18T16:36:39.910","2017-11-18T11:36:39.910","CW","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-18T16:47:17.310","2017-11-18T11:47:17.310","KL","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-18T17:05:22.190","2017-11-18T12:05:22.190","KL","All",null,null,"Got off course briefly"]
["2017-11-18T17:17:47.870","2017-11-18T12:17:47.870","CW","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-18T17:27:14.220","2017-11-18T12:27:14.220","CW","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-18T17:28:43.630","2017-11-18T12:28:43.630","CW","Sonar","Knudsen","Range","1000. New Line"]
["2017-11-18T17:29:04.340","2017-11-18T12:29:04.340","CW","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-11-18T17:48:40.800","2017-11-18T12:48:40.800","KL","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-11-18T18:19:42.320","2017-11-18T13:19:42.320","KL","Sonar","All",null,"New lines for turn. MB line 0044"]
["2017-11-18T18:23:40.780","2017-11-18T13:23:40.780","CW","Sonar","Multibeam","Ping mode","Very Deep. Deep was being an ass with blowouts"]
["2017-11-18T18:25:29.890","2017-11-18T13:25:29.890","CW","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-11-18T18:38:08.190","2017-11-18T13:38:08.190","CW","Sonar","Multibeam","Along Direction Pitch",-1.5]
["2017-11-18T18:58:15.560","2017-11-18T13:58:15.560","CW","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-11-18T19:08:50","2017-11-18T14:08:50","CW","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-11-18T19:10:50.130","2017-11-18T14:10:50.130","CW","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-11-18T19:24:38.690","2017-11-18T14:24:38.690","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-11-18T19:33:19.090","2017-11-18T14:33:19.090","KL","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-11-18T19:41:28.210","2017-11-18T14:41:28.210","DS","Sonar","Multibeam","New Line","geographical display is not showing bathy grid with new pings, but data still coming in. broke line to test. "]
["2017-11-18T19:49:25.970","2017-11-18T14:49:25.970","DS","Sonar","Multibeam","Along Direction Pitch","changed from -1 to 0"]
["2017-11-18T19:52:44.930","2017-11-18T14:52:44.930","CW","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-11-18T20:12:06.620","2017-11-18T15:12:06.620","CW","XBT",null,null,"XBT009; applied to line 0046"]
["2017-11-18T20:27:40.160","2017-11-18T15:27:40.160","CW","Sonar","Multibeam",null,"Data still not appearing in Geographical display past 5000m, but it's still coming in other displays. Hopefully once we shoal up from 5000m it will come back in. Gummy Bears have been sacrificed, btw. "]
["2017-11-18T20:33:22.330","2017-11-18T15:33:22.330","AB","Sonar","Knudsen","Tx Pulse","8ms, Gain: 18 5logR"]
["2017-11-18T21:17:19.920","2017-11-18T16:17:19.920","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-11-18T22:14:47.630","2017-11-18T17:14:47.630","DS","Sonar","Multibeam",null,"geographical disply returned to normal around 4700 meters. Problem appears to be depth related since display returned to normal at roughly the same depth it was lost on other side of Cayman Trench."]
["2017-11-18T23:13:35.460","2017-11-18T18:13:35.460","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-11-18T23:43:11.730","2017-11-18T18:43:11.730","AB","Sonar","Knudsen","Phase Range","3500-4500, Gain 18 5logR"]
["2017-11-18T23:45:56.700","2017-11-18T18:45:56.700","AB","Sonar","EK",null,"Range 5500m, Bottom Detection 6000m"]
["2017-11-18T23:47:47.420","2017-11-18T18:47:47.420","AB","Sonar","Multibeam","New line","0050"]
["2017-11-18T23:48:44.190","2017-11-18T18:48:44.190","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-11-18T23:54:13.810","2017-11-18T18:54:13.810","AB","Sonar","Knudsen","Phase Range","2500-3500m"]
["2017-11-18T23:58:36.250","2017-11-18T18:58:36.250","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-11-19T00:47:56.500","2017-11-18T19:47:56.500","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-11-19T01:02:03.570","2017-11-18T20:02:03.570","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-11-19T01:15:10.440","2017-11-18T20:15:10.440","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-11-19T01:20:04.260","2017-11-18T20:20:04.260","AB","Sonar","Knudsen","Phase Range","3000-4000m"]
["2017-11-19T01:24:48.650","2017-11-18T20:24:48.650","AB","Sonar","Knudsen","Phase Range","3500-4500m"]
["2017-11-19T01:43:08.900","2017-11-18T20:43:08.900","AB","Sonar","Knudsen","Phase Range","4000-5000m"]
["2017-11-19T01:52:48.430","2017-11-18T20:52:48.430","AB","Sonar","Knudsen","Phase Range","4500-5500"]
["2017-11-19T02:01:03.220","2017-11-18T21:01:03.220","AB","Sonar","EK",null,"Range 6000, Bottom Detection 7000"]
["2017-11-19T02:05:00.680","2017-11-18T21:05:00.680","AB","Sonar","EK",null,"Range 6500"]
["2017-11-19T02:05:13.400","2017-11-18T21:05:13.400","AB","Sonar","Knudsen","Phase Range","5000-6000"]
["2017-11-19T02:32:56.900","2017-11-18T21:32:56.900","RH","XBT",null,null,"XBT 10 added to line 52"]
["2017-11-19T02:44:01.900","2017-11-18T21:44:01.900","AB","Sonar","Multibeam","Along Direction Pitch",-1]
["2017-11-19T02:45:10.890","2017-11-18T21:45:10.890","AB","Sonar","Multibeam","New Line","0053"]
["2017-11-19T03:05:32.660","2017-11-18T22:05:32.660","AB","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-11-19T03:06:01.860","2017-11-18T22:06:01.860","AB","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-11-19T03:18:42.360","2017-11-18T22:18:42.360","AB","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-11-19T03:28:40.530","2017-11-18T22:28:40.530","AB","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-11-19T03:30:45.990","2017-11-18T22:30:45.990","AB","Sonar","Multibeam","Ping mode","Auto: Deep. Max angles 75/75"]
["2017-11-19T03:32:46.740","2017-11-18T22:32:46.740","AB","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-11-19T03:33:11.390","2017-11-18T22:33:11.390","AB","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-11-19T03:38:40.440","2017-11-18T22:38:40.440","AB","Sonar","Knudsen",null,"Tx Power 1, Tx Pulse 4"]
["2017-11-19T03:42:02.950","2017-11-18T22:42:02.950","AB","Ship",null,null,"Reducing speed to 8.5-9.0 knts"]
["2017-11-19T03:48:52.440",{"$f":"IF(ISBLANK(A136),\" \",((A136)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-11-18T22:48:52.440"},"AB","Sonar","Knudsen","Tx Pulse","4, Gain 15 5log R"]
["2017-11-19T03:51:15.960","2017-11-18T22:51:15.960","AB","Sonar","EK",null,"Range 3000"]
["2017-11-19T04:17:10.380","2017-11-18T23:17:10.380","AB","Sonar","Knudsen","Phase Range","1000-2000"]
["2017-11-19T05:10:50.470","2017-11-19T00:10:50.470","DF","Sonar","Knudsen","Phase Range","1500-2500"]
["2017-11-19T05:12:20.680","2017-11-19T00:12:20.680","DF","Sonar","Multibeam","Ping mode","AUTO"]
["2017-11-19T05:52:43.260","2017-11-19T00:52:43.260","DF","Sonar","EK",null,"Bottom detection 5000 m"]
["2017-11-19T05:57:35.950","2017-11-19T00:57:35.950","DF","Sonar","Knudsen","Phase Range","2000-3000"]
["2017-11-19T06:15:04.320","2017-11-19T01:15:04.320","DF","Sonar","Knudsen","Phase Range","2500-3500"]
["2017-11-19T06:15:15.860","2017-11-19T01:15:15.860","DF","Sonar","EK","Change Range",3500]
["2017-11-19T07:13:17.970","2017-11-19T02:13:17.970","DF","Sonar","Multibeam","New Line","new line at turn; new EK and SBP lines"]
["2017-11-19T07:25:34.940","2017-11-19T02:25:34.940","DF","Sonar","EK","Change Range",3800]
["2017-11-19T07:29:21.190","2017-11-19T02:29:21.190","DF","Sonar","Multibeam","Ping mode","Very Deep; Deep kept penetrating through bottom. @3000 m"]
["2017-11-19T08:29:30.540","2017-11-19T03:29:30.540","DF","XBT",null,null,"Cast 011 applied to line 0059"]
["2017-11-19T08:45:18.340","2017-11-19T03:45:18.340","DF","Sonar","Multibeam","Ping mode","AUTO"]
["2017-11-19T08:48:07.400","2017-11-19T03:48:07.400","DF","Sonar","Multibeam","Ping mode","Very Deep; Deep kept penetrating through bottom. @2850 m"]
["2017-11-19T09:08:57.050","2017-11-19T04:08:57.050","DF","Sonar","Multibeam","New Line","new line for turn, 0060; new ek and sbp lines"]
["2017-11-19T09:37:35.570","2017-11-19T04:37:35.570","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-11-19T10:43:46.970","2017-11-19T05:43:46.970","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-11-19T10:44:04.820","2017-11-19T05:44:04.820","DF","Sonar","Knudsen","TX Power",3]
["2017-11-19T11:06:46.160","2017-11-19T06:06:46.160","DF","Sonar","Multibeam","Slope Filter (On/Off)","Off"]
["2017-11-19T11:07:05.020","2017-11-19T06:07:05.020","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-11-19T11:07:15.140","2017-11-19T06:07:15.140","DF","Sonar","Multibeam","Along Direction Pitch",-0.5]
["2017-11-19T11:08:44.260","2017-11-19T06:08:44.260","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-11-19T11:09:33.730","2017-11-19T06:09:33.730","DF","Sonar","Knudsen","Phase Range","3000-4000"]
["2017-11-19T11:11:09","2017-11-19T06:11:09","DF","Ship",null,null,"Entering Cuban waters"]
["2017-11-19T12:30:47","2017-11-19T07:30:47","DF","Sonar","Knudsen","Phase Range","3500-4500"]
["2017-11-19T12:00:59.610","2017-11-19T07:00:59.610","DF","Sonar","Knudsen","Phase Range","4000-5000"]
["2017-11-19T12:16:03.670","2017-11-19T07:16:03.670","DF","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-11-19T12:16:13.800","2017-11-19T07:16:13.800","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-11-19T12:56:34.460","2017-11-19T07:56:34.460","CW","Sonar","Knudsen","Range","500. New Line. Flat and bo-ring!!"]
["2017-11-19T12:57:19.970","2017-11-19T07:57:19.970","CW","Sonar","Knudsen","Phase Range","4250-5250"]
["2017-11-19T14:42:12.160","2017-11-19T09:42:12.160","CW","XBT",null,null,"XBT 012; applied to line 0065"]
["2017-11-19T15:13:15.740","2017-11-19T10:13:15.740","KL","Ship",null,null,"Entering UTM 16N"]
["2017-11-19T16:50:38.360","2017-11-19T11:50:38.360","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-11-19T17:34:45.510","2017-11-19T12:34:45.510","DS","Sonar","Multibeam","Along Direction Pitch","changed from 0.5 to 1"]
["2017-11-19T18:03:21.820","2017-11-19T13:03:21.820","CW","All",null,"New Line","New lines for turn. MB line 0069"]
["2017-11-19T20:52:46","2017-11-19T15:52:46","KL","XBT",null,null,"XBT 013; applied to line 0071"]
["2017-11-20T00:22:28","2017-11-19T19:22:28","AB","Sonar","Knudsen","Phase Range","4000-4500"]
["2017-11-20T01:05:31","2017-11-19T20:05:31","AB","Sonar","Knudsen","Phase Range","3750-4250"]
["2017-11-20T01:31:32.460","2017-11-19T20:31:32.460","AB","Sonar","Knudsen","Phase Range","3500-4000"]
["2017-11-20T02:32:58.060","2017-11-19T21:32:58.060","AB","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-11-20T02:38:48.850","2017-11-19T21:38:48.850","AB","Sonar","Knudsen",null,"Tx Power 2, Tx Pulse 4"]
["2017-11-20T02:39:38.930","2017-11-19T21:39:38.930","AB","Sonar","Multibeam","Ping mode","Deep. 75/75. Heading up the shelf"]
["2017-11-20T02:40:49.800","2017-11-19T21:40:49.800","AB","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-11-20T02:41:07.120","2017-11-19T21:41:07.120","AB","Ship",null,null,"Increasing speed to 9.5 knots"]
["2017-11-20T02:45:20.960","2017-11-19T21:45:20.960","AB","Sonar","EK","Change Range","3500m"]
["2017-11-20T02:58:26.510","2017-11-19T21:58:26.510","AB","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-20T03:02:27.910","2017-11-19T22:02:27.910","AB","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-11-20T03:08:04.110","2017-11-19T22:08:04.110","RH","XBT",null,null,"XBT 14 applied to line 0078 "]
["2017-11-20T03:11:11.750","2017-11-19T22:11:11.750","AB","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-20T03:30:34.770","2017-11-19T22:30:34.770","AB","Sonar","Multibeam",null,"New line 0079 at turn"]
["2017-11-20T03:40:01.590","2017-11-19T22:40:01.590","AB","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-20T04:19:43.290","2017-11-19T23:19:43.290","DF","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-20T04:26:11.530","2017-11-19T23:26:11.530","AB","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-20T04:30:05.040","2017-11-19T23:30:05.040","DF","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-11-20T04:35:14.930","2017-11-19T23:35:14.930","AB","Sonar","Knudsen","Phase Range","750-1250, Tx Power 1 Px Pulse 2"]
["2017-11-20T04:39:30.430","2017-11-19T23:39:30.430","DF","Sonar","Knudsen","Phase Range","500-1000"]
["2017-11-20T04:43:21.920","2017-11-19T23:43:21.920","DF","Sonar","Multibeam","Along Direction Pitch",0.5]
["2017-11-20T04:46:32.470","2017-11-19T23:46:32.470","DF","Sonar","Knudsen","Phase Range","750-1250"]
["2017-11-20T04:47:28.980","2017-11-19T23:47:28.980","DF","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-11-20T04:50:49.700","2017-11-19T23:50:49.700","DF","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-20T05:09:14.450","2017-11-20T00:09:14.450","DF","Sonar","Knudsen","TX Power",2]
["2017-11-20T05:34:15.980","2017-11-20T00:34:15.980","DF","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-20T06:41:15.490","2017-11-20T01:41:15.490","DF","Sonar","Multibeam",null,"Have seen some interference randomly for a very brief period, causes loss of bottom"]
["2017-11-20T07:12:46.720","2017-11-20T02:12:46.720","DF","Sonar","Multibeam","Slope Filter (On/Off)","On"]
["2017-11-20T07:14:15.550",{"$f":"IF(ISBLANK(A201),\" \",((A201)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-11-20T02:14:15.550"},"DF","Sonar","Multibeam","New Line","New line 0083 at turn; new ek and sbp lines"]
["2017-11-20T07:20:37.410","2017-11-20T02:20:37.410","DF","Sonar","Multibeam",null,"Geographical display is not showing bathy grid with new pings, but data still coming in. Opened waterfall tearoff to confirm "]
["2017-11-20T09:28:14.510","2017-11-20T04:28:14.510","DF","XBT",null,null,"Cast 015 applied to line 0086"]
["2017-11-20T11:10:14.070","2017-11-20T06:10:14.070","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-11-20T13:15:02.060","2017-11-20T08:15:02.060","CW","Sonar","Multibeam",null,"Lost griddin for a bit. Came back!"]
["2017-11-20T13:35:29.120","2017-11-20T08:35:29.120","CW","POS",null,null,"Several dropouts, including naughty red screen of death. "]
["2017-11-20T13:54:32.870","2017-11-20T08:54:32.870","KL","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-20T14:11:52.580","2017-11-20T09:11:52.580","KL","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-11-20T15:02:16.630","2017-11-20T10:02:16.630","KL","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-20T15:08:47.500","2017-11-20T10:08:47.500","KL","Sonar","All","New Line","New line; MB 0091 ship altering course for traffic"]
["2017-11-20T15:45:04.690","2017-11-20T10:45:04.690","CW","XBT",null,null,"XBT 016; applied to line 0092"]
["2017-11-20T17:15:13","2017-11-20T12:15:13","KL","Sonar","Multibeam",null,"Lost griddin for a bit. Came back!"]
["2017-11-20T17:36:58.600","2017-11-20T12:36:58.600","KL","Sonar","Multibeam",null,"Range Gate: Normal"]
["2017-11-20T18:51:03.670","2017-11-20T13:51:03.670","CW","Sonar","Knudsen","Phase Range","2500-3000"]
["2017-11-20T19:30:36.050","2017-11-20T14:30:36.050","CW","Sonar","Knudsen","Phase Range","2250-2750"]
["2017-11-20T19:37:52","2017-11-20T14:37:52","KL","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-11-20T19:39:58.850","2017-11-20T14:39:58.850","KL","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-20T19:58:21.470","2017-11-20T14:58:21.470","CW","Sonar","Knudsen","Phase Range","1500-2000"]
["2017-11-20T20:20:14.520","2017-11-20T15:20:14.520","CW","Sonar","Knudsen","Tx Power",3]
["2017-11-20T20:20:28.850","2017-11-20T15:20:28.850","CW","Sonar","Knudsen","Phase Range","2000-2500"]
["2017-11-20T21:30:59.850","2017-11-20T16:30:59.850","AB","Ship ",null,null,"Reduced speed to 8 knots"]
["2017-11-20T21:40:00","2017-11-20T16:40:00","AB","Other",null,null,"UCTD testing"]
["2017-11-20T21:46:28.460","2017-11-20T16:46:28.460","AB","Sonar",null,null,"New lines started at turn for all sonars. MB line 99."]
["2017-11-20T21:48:31.600","2017-11-20T16:48:31.600","AB","Sonar","Multibeam","New Line",100]
["2017-11-20T22:08:13.950","2017-11-20T17:08:13.950","AB","Sonar","Knudsen","Tx Power","2, Gain 16 5 log R"]
["2017-11-20T22:37:29.680","2017-11-20T17:37:29.680","AB","Sonar","Knudsen","Phase Range","1750-2250"]
["2017-11-20T23:13:29.450","2017-11-20T18:13:29.450","AB","Sonar","Multibeam",null,"Over 3 m/s difference for SVP. Still reeling in UCTD."]
["2017-11-20T23:17:41.380","2017-11-20T18:17:41.380","AB","Other",null,null,"UCTD on deck."]
["2017-11-20T23:34:26.400","2017-11-20T18:34:26.400","AB","Sonar","Knudsen","Phase Range","1500-2000m"]
["2017-11-20T23:46:06.010","2017-11-20T18:46:06.010","RH","XBT",null,null,"XBT applied to line 101"]
["2017-11-20T23:52:30.730","2017-11-20T18:52:30.730","AB","Sonar","Multibeam","New Line","0102"]
["2017-11-21T00:11:46.990","2017-11-20T19:11:46.990","AB","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-21T00:40:34.320","2017-11-20T19:40:34.320","AB","Sonar","Multibeam",null,"Display gap"]
["2017-11-21T00:54:40","2017-11-20T19:54:40","AB","Sonar","Multibeam","New Line","0103"]
["2017-11-21T02:12:36.190","2017-11-20T21:12:36.190","AB","Sonar","Multibeam",null,"Display gap"]
["2017-11-21T02:28:01.320","2017-11-20T21:28:01.320","AB","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-11-21T02:48:56.050","2017-11-20T21:48:56.050","AB","Sonar","Multibeam","New Line","0104"]
["2017-11-21T02:59:28.690","2017-11-20T21:59:28.690","AB","sonar","Knudsen","TX Power","2, Tx Pulse 2, Gain 14 5logR"]
["2017-11-21T03:24:03.950","2017-11-20T22:24:03.950","AB","Sonar","Multibeam","New Line","0106, turn. In the USA. Swaths from following few lins may overlap with Cuban EEZ."]
["2017-11-21T03:39:48.390","2017-11-20T22:39:48.390","AB","Sonar","Multibeam","New Line","0107. All new lines started on all sonars."]
["2017-11-21T04:03:07.100","2017-11-20T23:03:07.100","AB","Sonar","Multibeam","New Line","0108"]
["2017-11-21T05:11:07.060","2017-11-21T00:11:07.060","DF","Sonar","Multibeam","New Line","Begin turn line 0110"]
["2017-11-21T05:16:12.660","2017-11-21T00:16:12.660","DF","Ship",null,null,"Requested to shift the next survey line 1500 m North (PORT) for less overlap"]
["2017-11-21T05:30:12.540","2017-11-21T00:30:12.540","DF","Sonar","Multibeam","New Line","Begin survey line 0111; new ek and sbp lines"]
["2017-11-21T05:34:57","2017-11-21T00:34:57","DF","Sonar","Knudsen","Phase Range","750-1250"]
["2017-11-21T05:50:20","2017-11-21T00:50:20","DF","XBT",null,null,"Cast 018 applied to line 0111"]
["2017-11-21T06:32:44.750","2017-11-21T01:32:44.750","DF","Sonar","Multibeam",null,"COM 1 error"]
["2017-11-21T07:56:00","2017-11-21T02:56:00","MPM","Sonar","Knudsen","Phase Range","750-1250"]
["2017-11-21T09:07:53.610","2017-11-21T04:07:53.610","DF","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-11-21T10:05:46.200","2017-11-21T05:05:46.200","DF","Sonar","Knudsen","Phase Range","1250-1750"]
["2017-11-21T11:33:35.020","2017-11-21T06:33:35.020","DF","XBT",null,null,"Cast 019 applied to line 0117"]
["2017-11-21T11:44:15.590","2017-11-21T06:44:15.590","DF","Sonar","Multibeam","New Line","begin turn line 0118; new EK and SBP lines"]
["2017-11-21T11:50:10.740","2017-11-21T06:50:10.740","DF","Ship",null,null,"Requested to shift the next survey line 1500 m North (STBD) for less overlap"]
["2017-11-21T12:03:07.370","2017-11-21T07:03:07.370","DF","Sonar","Multibeam","New Line","Begin survey line 0119; new EK and SBP lines"]
["2017-11-21T12:11:41.210","2017-11-21T07:11:41.210","DF","Ship",null,null,"Traffic situation arising in about 1 hr; ship may have to make a drastic turn to STBD or slow down to 4/5 knots"]
["2017-11-21T12:12:56.950","2017-11-21T07:12:56.950","DF","Ship",null,null,"Requested 1000 m move to STBD for less overlap in coverage."]
["2017-11-21T12:39:59","2017-11-21T07:39:59","KL","Ship",null,null,"Traffic situation continues, adjusting course 10 degrees to Stbd. May cause overlap issues. "]
["2017-11-21T12:41:39.710","2017-11-21T07:41:39.710","KL","Sonar","Knudsen","Phase Range","1000-1500"]
["2017-11-21T13:35:15","2017-11-21T08:35:15","CW","Sonar","Multibeam",null,"Small data gap, but over previous data. So we got that going for us, which is nice. "]
["2017-11-21T13:34:47","2017-11-21T08:34:47","CW","Ship",null,null,"Traffic drama is over. Back on trackline that was adjuisted earlier."]
["2017-11-21T14:06:36.510","2017-11-21T09:06:36.510","CW","Ship",null,null,"500m shift to port"]
["2017-11-21T14:15:22.570","2017-11-21T09:15:22.570","CW","Sonar","Knudsen","Phase Range","750-1250"]
["2017-11-21T14:42:47.610","2017-11-21T09:42:47.610","DS","Sonar","Multibeam",null,"requested bridge shift 500m to port (south) to increase line overlap. "]
["2017-11-21T15:14:37.250","2017-11-21T10:14:37.250","KL","XBT",null,null,"Cast 020 applied to line 122"]
["2017-11-21T15:22:55.250","2017-11-21T10:22:55.250","KL","Sonar","Knudsen","Tx Power","Reduced to 1"]
["2017-11-21T15:28:13.290","2017-11-21T10:28:13.290","KL","Sonar","Knudsen","Gain Value","Increased to 15"]
["2017-11-21T15:37:11.530","2017-11-21T10:37:11.530","KL","Sonar","Knudsen","Tx Pulse","Increased to 4 ms"]
["2017-11-21T16:16:04.090",{"$f":"IF(ISBLANK(A268),\" \",((A268)-DATE(1970,1,1))+25569-($C$1/24))","v":"2017-11-21T11:16:04.090"},"CW","Sonar","Knudsen","Tx Power","Up to 2"]
["2017-11-21T16:16:13.930","2017-11-21T11:16:13.930","CW","Sonar","Knudsen","Tx Pulse","Down to 1ms"]
["2017-11-21T18:41:17.490","2017-11-21T13:41:17.490","DS","XBT",null,null,"two XBT casts canceled part way through, troubleshooting software."]
["2017-11-21T18:43:39.520","2017-11-21T13:43:39.520","DS","Sonar","Multibeam","New Line","end survey line 125, start turn line 126"]
["2017-11-21T18:46:44.080","2017-11-21T13:46:44.080","DS","Sonar","Knudsen",null,"new turn line"]
["2017-11-21T19:00:50.120","2017-11-21T14:00:50.120","DS","Sonar","Multibeam","New Line","new survey line 127"]
["2017-11-21T19:30:55.440","2017-11-21T14:30:55.440","CW","XBT`",null,null,"XBT 0-21; applied to line 0127"]
["2017-11-21T21:01:07","2017-11-21T16:01:07","AB","Sonar","Multibeam","New Line","0129"]
["2017-11-21T21:47:08.380","2017-11-21T16:47:08.380","AB","ship",null,null,"Increased speed to 10-10.5 knots for traffic avoidance. "]
["2017-11-21T22:10:27","2017-11-21T17:10:27","AB","Sonar","Multibeam","New Line","0130"]
["2017-11-21T22:40:48.810","2017-11-21T17:40:48.810","AB","Ship",null,null,"Reducing speed to 9.0-9.5 knots. Shifting 1000m to port (north)."]
["2017-11-21T22:54:43.090","2017-11-21T17:54:43.090","AB","XBT",null,null,"XBT22 added to line 0130"]
["2017-11-21T23:14:02.560","2017-11-21T18:14:02.560","AB","Ship",null,null,"Shifting additional 700m port (north). Total 1700m."]
["2017-11-22T00:02:11.970","2017-11-21T19:02:11.970","AB","Sonar","Multibeam","Along Direction Pitch",0]
["2017-11-22T00:02:34.020","2017-11-21T19:02:34.020","AB","Sonar","Multibeam","New Line","0132"]
["2017-11-22T00:15:04.830","2017-11-21T19:15:04.830","AB","Sonar",null,null,"New lines on all sonars for turns, MB line 0133."]
["2017-11-22T00:32:57.730","2017-11-21T19:32:57.730","AB","Sonar","Multibeam","New Line","0133"]
["2017-11-22T01:35:12.740","2017-11-21T20:35:12.740","AB","Ship",null,null,"Shifting 1000m to port (south)."]
["2017-11-22T01:55:53.460","2017-11-21T20:55:53.460","AB","Ship ",null,null,"shifting additional 500m to port. Total 1500m. "]
["2017-11-22T02:01:31.990","2017-11-21T21:01:31.990","AB","Sonar",null,"New line","New lines on all sonars after shift. Mb line 0136"]
["2017-11-22T02:05:11.730","2017-11-21T21:05:11.730","AB","XBT",null,null,"XBT23 added to line 0136"]
["2017-11-22T02:54:13.910","2017-11-21T21:54:13.910","DS","Sonar","Multibeam",null,"asked bridge to move 500 m to port gradually for more overlap"]
["2017-11-22T03:02:00.350","2017-11-21T22:02:00.350","AB","Sonar","Multibeam","New Line","0137"]
["2017-11-22T03:38:54.510","2017-11-21T22:38:54.510","AB","Sonar","EK",null,"Range 1200m"]
["2017-11-22T04:03:23.890","2017-11-21T23:03:23.890","AB","Sonar",null,null,"All new sonar files started at turn. MB line 0139."]
["2017-11-22T04:18:17.040","2017-11-21T23:18:17.040","AB","Sonar",null,null,"All new lines started after turn. MB line 0140."]
["2017-11-22T05:07:26.050","2017-11-22T00:07:26.050","DF","XBT",null,null,"Cast 024 applied to line 0140"]
["2017-11-22T05:17:16.790","2017-11-22T00:17:16.790","DF","Ship",null,null,"Fishing gear in our path, will depart trackline to avoid"]
["2017-11-22T07:07:53.870","2017-11-22T02:07:53.870","DF","XBT",null,null,"Cast 025 applied to line 0142"]
["2017-11-22T08:55:14.650","2017-11-22T03:55:14.650","DF","Sonar","Multibeam","New Line","begin final transit line to sea buoy 0145; new EK and SBP lines"]
["2017-11-22T08:59:31.530","2017-11-22T03:59:31.530","DF","Ship",null,null,"Increase to warp speed for sea buoy arrival, may slow down briefly for wreck site if we have the spare time"]
["2017-11-22T09:05:09.190","2017-11-22T04:05:09.190","DF","Ship",null,null,"Correction… ship will maintain 9.5 knots until we arrive at potential wreck site then slow down"]
["2017-11-22T09:06:00.910","2017-11-22T04:06:00.910","DF","Sonar","Knudsen","Phase Range","500-1000"]
["2017-11-22T09:39:52.670","2017-11-22T04:39:52.670","DF","XBT",null,null,"Cast 026 applied to line 0145"]
["2017-11-22T10:05:47.230","2017-11-22T05:05:47.230","DF","Sonar","Knudsen",null,"250-750; TX Power to 1"]
["2017-11-22T10:11:34.480","2017-11-22T05:11:34.480","DF","Sonar","Multibeam",null,"Range Gate: Small"]
["2017-11-22T10:13:39.940","2017-11-22T05:13:39.940","DF","Sonar","Knudsen",null,"Secured for cruise @ 280 m; started getting shadow artifact in screen"]
["2017-11-22T10:15:00.290","2017-11-22T05:15:00.290","DF","Ship",null,null,"Slowing to 8-8.5 for potential wreck site"]
["2017-11-22T10:23:51.280","2017-11-22T05:23:51.280","DF","Ship",null,null,"Resuming ludacris speed to sea buoy"]
["2017-11-22T10:44:55.610","2017-11-22T05:44:55.610","DF",null,null,null,"TSG Secured"]
["2017-11-22T10:54:05.300","2017-11-22T05:54:05.300","DF","Ship",null,null,"Ship is manuevering for traffic"]
["2017-11-22T10:56:58.800","2017-11-22T05:56:58.800","DF",null,null,null,"Had a network dropout last night, caused gap in mozaik backscatter. Unsure of exact time"]
["2017-11-22T11:11:51.610","2017-11-22T06:11:51.610","DF","Sonar",null,null,"MB and EK sonars secured"]
["2017-11-22T12:06:07.700","2017-11-22T07:06:07.700","DS","Sonar",null,null,"Turned on bottom track ADCP 300 kHz going in to Key West"]
["2017-11-22T13:24:09.970","2017-11-22T08:24:09.970","DS","Sonar",null,null,"Reached port in Key West at Navy Pier. ADCP secured. "]
["2017-11-22T13:25:20.310","2017-11-22T08:25:20.310","DS","Sonar","All",null,"End of cruise. Turning off EK60 and ADCP deck units. TRU will be left on for next cruise. "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A332),\" \",((A332)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A396),\" \",((A396)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A460),\" \",((A460)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A524),\" \",((A524)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A588),\" \",((A588)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A652),\" \",((A652)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A716),\" \",((A716)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A780),\" \",((A780)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":14,"n_cols":7,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["AB","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DF","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["CW","Weather","Knudsen","New Line","Secure","Gain Mode","New Line"]
["DS","Watch Change","All","Max Angle","Start Recording","Gain Value"]
["KL","XBT",null,"Spike Filter Strength",null,"Process Shift"]
["VD","Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
["MPM","Other",null,"Aeration Filter (On/Off)",null,"Range"]
["RH","CTD",null,"Interference Filter (On/Off)",null,"Phase Mode"]
[null,null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]
[null,null,null,"BIST",null,"Start Pinging"]
[null,null,null,null,null,"Start Recording"]