{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":903,"n_cols":7,"rows_kept":903,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1802","UTC to Local: ",-5,"UTC 2","UTC 3","UTC 4","Cruise Details: March 23th - April 5th"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2018-04-11T16:12:51.340",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-11T11:12:51.340"},"CW","Sonar","Multibeam","Start Pinging","BIST 01. All pass. Yeahuh"]
["2018-04-11T23:05:39.330","2018-04-11T18:05:39.330","CW","Sonar","EK","Start Pinging"]
[null," ","CW","Sonar","Knudsen","Start Pinging"]
["2018-04-11T23:05:30.040","2018-04-11T18:05:30.040","CW","Sonar","Multibeam","Start Logging","Begin EX1803!!! Line 0000, SSM Server Mode on"]
["2018-04-12T00:31:27.060","2018-04-11T19:31:27.060","CW","XBT",null,null,"Cast 01"]
["2018-04-12T00:50:21.690","2018-04-11T19:50:21.690","JM","Watch Change"]
["2018-04-12T00:50:39.230","2018-04-11T19:50:39.230","JM","Sonar","Knudsen","Start Pinging","Start logging. Tx Pulse 1, Power 1, Gain 16dB"]
["2018-04-12T01:46:52.940","2018-04-11T20:46:52.940","JM","Sonar","Multibeam","New Line","Start turn, line 6"]
["2018-04-12T01:51:10.660","2018-04-11T20:51:10.660","JM","Sonar","Knudsen","Tx Pulse","Pulse 2"]
["2018-04-12T01:56:36.380","2018-04-11T20:56:36.380","JM","Sonar","All","New Line","End turn, line 7"]
["2018-04-12T02:56:06.900","2018-04-11T21:56:06.900","CW",null,null,null,"Securing SCS for UCH protocol. Did it a few hours earlier due to loggin in with CAC card issues; i.e. CAC cards suuuuukk."]
["2018-04-12T05:16:50.590","2018-04-12T00:16:50.590","JM","XBT",null,null,"Cast 02"]
["2018-04-12T05:31:55.770","2018-04-12T00:31:55.770","JM","XBT",null,null,"XBT applied to line 0010"]
["2018-04-12T10:21:01.100","2018-04-12T05:21:01.100","JM","Sonar","All","Secure","Arriving at Dive site #1"]
["2018-04-12T22:10:15.700","2018-04-12T17:10:15.700","CW","Sonar","Multibeam","BIST","BIST 02 All Pass"]
["2018-04-12T22:49:36.920","2018-04-12T17:49:36.920","CW","Sonar","Multibeam","Start Pinging","Changed Raw file directory for data management "]
["2018-04-12T22:50:24.180","2018-04-12T17:50:24.180","CW","Sonar",null,null,"ADCP Passive Mode. Not logging position due to UCH"]
["2018-04-12T22:50:43.700","2018-04-12T17:50:43.700","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-12T22:50:55.820","2018-04-12T17:50:55.820","CW","Sonar","EK","Start Pinging"]
["2018-04-12T22:51:21.780","2018-04-12T17:51:21.780","CW","Sonar","Knudsen","Start Pinging","Pulse1; Power 1; Gain 21dB 5logR; Range 500; Phase Mode: Auto"]
["2018-04-12T22:53:09.640","2018-04-12T17:53:09.640","CW","Sonar","Multibeam","Start Logging","Full Power; MB Line 0018"]
["2018-04-12T23:29:56.240","2018-04-12T18:29:56.240","CW","XBT",null,null,"XBT 003; applied to MB line 0017"]
["2018-04-12T23:45:26.160","2018-04-12T18:45:26.160","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0018"]
["2018-04-12T23:55:07.530","2018-04-12T18:55:07.530","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0019"]
["2018-04-13T00:16:11.620","2018-04-12T19:16:11.620","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0020"]
["2018-04-13T00:16:13.760","2018-04-12T19:16:13.760","CW","Sonar","Knudsen","New Line"]
["2018-04-13T00:20:24.920","2018-04-12T19:20:24.920","CW","Sonar","Knudsen","Gain Mode","Was 5logR, now it's None"]
["2018-04-13T00:23:52.530","2018-04-12T19:23:52.530","CW","Sonar","Knudsen","Tx Power",2]
["2018-04-13T00:53:44.590","2018-04-12T19:53:44.590","CW","Sonar","Knudsen","Gain Value",25]
["2018-04-13T00:54:06.840","2018-04-12T19:54:06.840","CW","Sonar","Knudsen","Tx Pulse",2]
["2018-04-13T00:58:07.870","2018-04-12T19:58:07.870","CW","Sonar","Knudsen","Phase Range","Phase Mode: Auto seems to be working well, but keeping an eye on it!"]
["2018-04-13T01:07:01.100","2018-04-12T20:07:01.100","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2018-04-13T01:07:26.070","2018-04-12T20:07:26.070","CW",null,null,null,"SEEPS!!! Line 0020"]
["2018-04-13T01:45:54.100","2018-04-12T20:45:54.100","JM","XBT",null,null,"Cast #5"]
["2018-04-13T01:49:47.080","2018-04-12T20:49:47.080","JM","XBT",null,null,"Cast #5 applied to Line 0020"]
["2018-04-13T02:40:56.730","2018-04-12T21:40:56.730","CW","Issue",null,null,"SV out of range. Waiting a lil be before doing anorther AXBT. MB line 0021"]
["2018-04-13T02:49:34.870","2018-04-12T21:49:34.870","CW","XBT",null,null,"We cheated. Reprocessed AXBT005 with new Salinity, TSS, Extended. Overwrote previous cast due to naming convention restraints. Applied to new MB line 0022. SV is happy now!"]
["2018-04-13T02:51:36.750","2018-04-12T21:51:36.750","CW","Sonar","Multibeam","New Line","New MB line 0022. See SV/XBT note above. "]
["2018-04-13T02:56:33.460","2018-04-12T21:56:33.460","CW","Sonar","Knudsen","Tx Pulse",4]
["2018-04-13T02:56:54.940","2018-04-12T21:56:54.940","CW","Sonar","Knudsen","Gain Value","30dB"]
["2018-04-13T03:27:36.600","2018-04-12T22:27:36.600","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0023"]
["2018-04-13T03:27:38.120","2018-04-12T22:27:38.120","CW","Sonar","Knudsen","New Line"]
["2018-04-13T03:27:40.710","2018-04-12T22:27:40.710","CW","Sonar","EK","New Line"]
["2018-04-13T03:27:47.530","2018-04-12T22:27:47.530","CW","Ship",null,null,"Heavy traffic. Need to adjust course to stbd to accommodate. Also going 7kts instead of planned 9.5"]
["2018-04-13T04:26:10.590","2018-04-12T23:26:10.590","CW","Ship",null,null,"Traffic situations have finished. Moving back to original trackline. "]
["2018-04-13T04:28:02.140","2018-04-12T23:28:02.140","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0024"]
["2018-04-13T04:28:28","2018-04-12T23:28:28","CW","Sonar","Knudsen","New Line"]
["2018-04-13T04:28:30.550","2018-04-12T23:28:30.550","CW","Sonar","EK","New Line"]
["2018-04-13T04:28:38.910","2018-04-12T23:28:38.910","CW","Issue",null,null,"SV not happy again. "]
["2018-04-13T04:56:30.200","2018-04-12T23:56:30.200","CW","XBT",null,null,"AXBT006 applied to MB line 0024"]
["2018-04-13T05:06:27.210","2018-04-13T00:06:27.210","CW","Issue",null,null,"SV not happy only 15 min later"]
["2018-04-13T05:50:06.970","2018-04-13T00:50:06.970","CW","Issue",null,null,"Reprocessed AXBT006; smoothed TSS a little better. Changed name to AXBT007, and applied to new MB line 0026. Yellow warning SV cells went to normal at 1532.4"]
["2018-04-13T07:19:51.550","2018-04-13T02:19:51.550","JM","Sonar","All","New Line","Begin Turn. MB line 0028"]
["2018-04-13T07:20:18.880","2018-04-13T02:20:18.880","JM","Sonar","Multibeam","Along Direction Pitch",0]
["2018-04-13T07:20:45.180","2018-04-13T02:20:45.180","JM","Sonar","Multibeam",null,"Penetration filter too weak"]
["2018-04-13T07:33:04.400","2018-04-13T02:33:04.400","JM","Sonar","All","New Line","End Turn. MB line 0029"]
["2018-04-13T07:57:16.360","2018-04-13T02:57:16.360","JM","Sonar","Multibeam",null,"Penetration filter to off"]
["2018-04-13T09:20:01.810","2018-04-13T04:20:01.810","JM","Sonar","All","New Line","Begin Turn. MB line 0031"]
["2018-04-13T09:27:58.800","2018-04-13T04:27:58.800","JM","Sonar","All","New Line","End Turn. MB line 0032"]
["2018-04-13T10:12:35.070","2018-04-13T05:12:35.070","JM","Sonar","All","New Line","Begin Turn. MB line 0033"]
["2018-04-13T10:19:55.400","2018-04-13T05:19:55.400","JM","Sonar","All","New Line","End Turn. MB line 0034"]
["2018-04-13T10:46:05.030","2018-04-13T05:46:05.030","JM","Sonar","All","Secure","Arrive at dive site #2"]
["2018-04-13T22:00:12","2018-04-13T17:00:12","CW","Sonar","Multibeam","BIST","BIST 03 All Pass"]
["2018-04-13T22:03:47.480","2018-04-13T17:03:47.480","CW","Sonar",null,null,"ADCP Passive Mode. Not logging position due to UCH protocols"]
["2018-04-13T22:03:49.360",{"$f":"IF(ISBLANK(A69),\" \",((A69)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-13T17:03:49.360"},"CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-13T22:20:03.860","2018-04-13T17:20:03.860","CW","Sonar","EK","Start Pinging"]
["2018-04-13T22:20:07.150","2018-04-13T17:20:07.150","CW","Sonar","Knudsen","Start Pinging","Recording. Pulse 2; Power 2; Gain 33 dB; Range 500; Phase Mode: Auto."]
["2018-04-13T22:20:07.150","2018-04-13T17:20:07.150","CW","Sonar","Multibeam","Start Logging","Full Power; MB Line 0035"]
["2018-04-13T22:25:07","2018-04-13T17:25:07","CW","XBT",null,null,"AXBT 007; applied to MB line 0035"]
["2018-04-13T23:40:03","2018-04-13T18:40:03","CW","Ship",null,null,"UCH operations completed. SCS restarted with normal protocals, milers, and messages. "]
["2018-04-14T00:01:51.700","2018-04-13T19:01:51.700","CW",null,null,null,"ADCP passive but logging position"]
["2018-04-14T00:19:56.230","2018-04-13T19:19:56.230","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0039"]
["2018-04-14T00:19:58.060","2018-04-13T19:19:58.060","CW","Sonar","Knudsen","New Line"]
["2018-04-14T00:19:59.920","2018-04-13T19:19:59.920","CW","Sonar","EK","New Line"]
["2018-04-14T00:40:50.610","2018-04-13T19:40:50.610","CW","Ship",null,null,"700m move to stbd for less overlap"]
["2018-04-14T00:41:31.160","2018-04-13T19:41:31.160","CW","Issue",null,null,"SIS gridding was going in and out, but seems to be better now. "]
["2018-04-14T01:04:20.950","2018-04-13T20:04:20.950","CW","Issue",null,null,"SIS gridding still struggling."]
["2018-04-14T01:34:30.280","2018-04-13T20:34:30.280","JM","Sonar","Multibeam",null,"Max depth 4000m"]
["2018-04-14T02:47:48.890","2018-04-13T21:47:48.890","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0044"]
["2018-04-14T02:47:50.620","2018-04-13T21:47:50.620","CW","Sonar","Knudsen","New Line"]
["2018-04-14T02:47:52.690","2018-04-13T21:47:52.690","CW","Sonar","EK","New Line"]
["2018-04-14T03:02:59.740","2018-04-13T22:02:59.740","CW","Ship",null,null,"Traffic situations ahead. May have some deviations from trackline on MB line 0044."]
["2018-04-14T03:34:40.940","2018-04-13T22:34:40.940","CW","Ship",null,null,"Begin deviation to port for traffic. "]
["2018-04-14T03:35:01.230","2018-04-13T22:35:01.230","CW","POS",null,null,"POS Position light out. Not known for how long."]
["2018-04-14T03:36:17.730","2018-04-13T22:36:17.730","CW","POS",null,null,"Position light's back on. "]
["2018-04-14T03:47:49.770","2018-04-13T22:47:49.770","CW","XBT",null,null,"AXBT 008; applied to MB line 0045"]
["2018-04-14T04:04:32.800","2018-04-13T23:04:32.800","CW","Ship",null,null,"Back on original trackline…. For now."]
["2018-04-14T04:04:34.700","2018-04-13T23:04:34.700","CW","Sonar","Multibeam","New Line","New line for returing to trackline. MB line 0046"]
["2018-04-14T04:34:17.700","2018-04-13T23:34:17.700","CW","Sonar","Multibeam","New Line","New line after turn. MB line 0046"]
["2018-04-14T04:37:02.370","2018-04-13T23:37:02.370","CW","Sonar","Knudsen","New Line"]
["2018-04-14T04:37:04.340","2018-04-13T23:37:04.340","CW","Sonar","EK","New Line"]
["2018-04-14T05:23:21.950","2018-04-14T00:23:21.950","CW","Sonar","Multibeam",null,"Penetration Filter: Medium"]
["2018-04-14T05:36:02.800","2018-04-14T00:36:02.800","CW","Sonar","Knudsen","Tx Pulse",2]
["2018-04-14T05:36:55.230","2018-04-14T00:36:55.230","CW","Sonar","Knudsen","Tx Power",2]
["2018-04-14T06:20:08.250","2018-04-14T01:20:08.250","JM",null,null,null,"Seep! Line 0047"]
["2018-04-14T07:39:29.850","2018-04-14T02:39:29.850","JM","Sonar","Knudsen","tx power",1]
["2018-04-14T07:59:47.640","2018-04-14T02:59:47.640","JM","XBT",null,null,"Cast #9"]
["2018-04-14T08:08:19.700","2018-04-14T03:08:19.700","JM","XBT",null,null,"Cast #9 applied to line 0049"]
["2018-04-14T08:29:34.440","2018-04-14T03:29:34.440","JM","Sonar","All","New Line","End turn, MB line 0050"]
["2018-04-14T09:43:52.020","2018-04-14T04:43:52.020","JM","Sonar","Knudsen","tx power",2]
["2018-04-14T09:44:46.460","2018-04-14T04:44:46.460","JM","Sonar","All","New Line","End turn, MB line 0052"]
["2018-04-14T10:03:56.040","2018-04-14T05:03:56.040","JM","Sonar","Knudsen","tx power",1]
["2018-04-14T10:28:58.090","2018-04-14T05:28:58.090","JM","Sonar","All","New Line","Begin turn, MB line 0053"]
["2018-04-14T10:49:45.120","2018-04-14T05:49:45.120","JM","Sonar","All","Secure","Arrive at dive site #3"]
["2018-04-14T13:12:39.840","2018-04-14T08:12:39.840","MW",null,null,null,"Dive Aborted"]
["2018-04-14T13:12:52.320","2018-04-14T08:12:52.320","MW","Sonar","Multibeam",null,"Pinging and Recording"]
["2018-04-14T13:13:11.820","2018-04-14T08:13:11.820","MW","Sonar","Knudsen",null,"Pinging"]
["2018-04-14T13:13:37.130","2018-04-14T08:13:37.130","MW","Sonar","EK",null,"Pinging"]
["2018-04-14T13:15:47.790","2018-04-14T08:15:47.790","MW","Sonar","Knudsen",null,"Recording"]
["2018-04-14T13:16:04.560","2018-04-14T08:16:04.560","MW","Sonar","Ek",null,"Recording"]
["2018-04-14T13:30:27.510","2018-04-14T08:30:27.510","MW","XBT",null,null,"AXBT Cast 010"]
["2018-04-14T13:31:22.340","2018-04-14T08:31:22.340","MW","Sonar","Multibeam",null,"Cast 010 Applioed to line0054"]
["2018-04-14T13:35:33.710","2018-04-14T08:35:33.710","MW","Sonar","All",null,"New Lines"]
["2018-04-14T13:39:27","2018-04-14T08:39:27","MW","Sonar","All",null,"New Survey Line 0056"]
["2018-04-14T13:44:13.640","2018-04-14T08:44:13.640","MW","Sonar","Multibeam",null,"SSM Server Mode On"]
["2018-04-14T14:04:56.470","2018-04-14T09:04:56.470","MW","Sonar","All",null,"Turn Line 057"]
["2018-04-14T14:31:49.500","2018-04-14T09:31:49.500","MW","Sonar","All",null,"Turn Line 0058"]
["2018-04-14T14:36:23.170","2018-04-14T09:36:23.170","MW","Sonar","All",null,"Survey Line 0059"]
["2018-04-14T14:54:48.560","2018-04-14T09:54:48.560","MW","Sonar","All",null,"Turn Line 0060"]
["2018-04-14T14:56:32.970","2018-04-14T09:56:32.970","MW","Sonar","All",null,"Survey Line 060"]
["2018-04-14T15:27:19.060","2018-04-14T10:27:19.060","MW","Sonar","All",null,"Turn Line 0062"]
["2018-04-14T15:31:55.610","2018-04-14T10:31:55.610","MW","Sonar","All",null,"Survey Line 0063"]
["2018-04-14T16:15:56.750","2018-04-14T11:15:56.750","MW",null,null,null,"500m Shift to Starboard"]
["2018-04-14T16:16:18.120","2018-04-14T11:16:18.120","MW","XBT",null,null,"Cast 011"]
["2018-04-14T16:16:42.810","2018-04-14T11:16:42.810","MW","Sonar","Multibeam",null,"Cast 11 Applied to Line 0063"]
["2018-04-14T17:46:35.410","2018-04-14T12:46:35.410","MW","All",null,null,"Turn Line 006"]
["2018-04-14T18:06:19.490","2018-04-14T13:06:19.490","MW","All",null,null,"Turn Line 0067"]
["2018-04-14T18:38:29.860","2018-04-14T13:38:29.860","MW","XBT",null,null,"Cast 012; applied to MB line 0068"]
["2018-04-14T19:11:33.730",{"$f":"IF(ISBLANK(A133),\" \",((A133)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-14T14:11:33.730"},"CW","Sonar","Multibeam",null,"SSM Server Mode On"]
["2018-04-14T19:25:40.120","2018-04-14T14:25:40.120","CW","Sonar","Multibeam","Along Direction Pitch",-1]
["2018-04-14T19:26:06.310","2018-04-14T14:26:06.310","CW","Sonar","Multibeam",null,"Gridding is not working again."]
["2018-04-14T20:45:18.190","2018-04-14T15:45:18.190","CW","Sonar","Knudsen","Phase Range","Auto Phase not happy with sea state. Keeps shooting all over the place. Back to Manual 100-300. Range 200 since it's pretty flat. "]
["2018-04-14T21:17:17","2018-04-14T16:17:17","CW","Sonar","Knudsen","Range",500]
["2018-04-14T21:28:51.670","2018-04-14T16:28:51.670","CW","Sonar","Knudsen","Gain Mode","35dB"]
["2018-04-14T21:30:59.750","2018-04-14T16:30:59.750","CW","Sonar","Knudsen","Tx Pulse",2]
["2018-04-15T02:43:12.600","2018-04-14T21:43:12.600","CW","XBT",null,null,"AXBT 013"]
["2018-04-15T02:43:30.870","2018-04-14T21:43:30.870","CW","XBT",null,null,"AXBT 013; applied to MB line 0076"]
["2018-04-15T04:56:02.980","2018-04-14T23:56:02.980","JM","Issue/Problem",null,null,"Lost Marinestar RTK. Alt. error >1m. Started new MB line 0079. "]
["2018-04-15T05:03:42.950","2018-04-15T00:03:42.950","JM","Sonar","Multibeam",null,"Marinestar back. New MB line 0080. *Going in and out. Alt. <1m"]
["2018-04-15T05:40:05.470","2018-04-15T00:40:05.470","JM","Issue/Problem",null,null,"Marinestar continues to go in and out although we have only been going about 3 knots due to swells"]
["2018-04-15T06:53:11.630","2018-04-15T01:53:11.630","JM","Sonar","All","Secure","Securing because bad seas and we are going less than 2 knots"]
["2018-04-15T14:07:43.550","2018-04-15T09:07:43.550","MW","Sonar",null,null,"Pinging and Recording, Knudsen still off"]
["2018-04-15T17:13:56.650","2018-04-15T12:13:56.650","CW","Sonar","Multibeam","Along Direction Pitch",0]
["2018-04-16T00:30:15.810","2018-04-15T19:30:15.810","CW","Issue",null,null,"POS Nav Status not happy. "]
["2018-04-16T00:40:19.690","2018-04-15T19:40:19.690","CW","Sonar","Multibeam","New Line","Turning due south now I guess. "]
["2018-04-16T01:18:12.790","2018-04-15T20:18:12.790","CW","Sonar","EK",null,"Cool stuff happening around 0100 UTC. Seep?"]
["2018-04-16T01:44:37.160","2018-04-15T20:44:37.160","CW","Sonar","EK",null,"Again at 1:43 UTC"]
["2018-04-16T02:30:59.920","2018-04-15T21:30:59.920","CW","Sonar","Knudsen","Start Pinging","Recording. Pulse 2; Power 2; Gain 33 dB; Range 500; Phase Mode: Auto."]
["2018-04-16T02:59:32.930","2018-04-15T21:59:32.930","CW","XBT",null,null,"AXBT014; applied to MB line 0096"]
["2018-04-16T03:26:04.240","2018-04-15T22:26:04.240","JM",null,null,null,"Seep line 96"]
["2018-04-16T04:53:00.050","2018-04-15T23:53:00.050","JM","Sonar","Multibeam","New Line","Position out, altitude accurace at 10m. Started new line 0098"]
["2018-04-16T04:56:59.830","2018-04-15T23:56:59.830","JM",null,null,null,"Position came back"]
["2018-04-16T05:37:41.260","2018-04-16T00:37:41.260","CW","Sonar","Multibeam",null,"Gates 500-3000"]
["2018-04-16T07:28:30.300","2018-04-16T02:28:30.300","JM","XBT",null,null,"Cast #15"]
["2018-04-16T07:38:52.930","2018-04-16T02:38:52.930","JM","XBT",null,null,"Cast #15 applied to line 0100"]
["2018-04-16T08:47:22.850","2018-04-16T03:47:22.850","JM","Sonar","Knudsen","Phase Range","1000. New line"]
["2018-04-16T10:46:43.350","2018-04-16T05:46:43.350","JM","Sonar","All","Secure","arrive at dive site #4. Start adcp"]
["2018-04-16T21:32:20.220","2018-04-16T16:32:20.220","CW","Sonar","Multibeam","BIST","All Pass"]
["2018-04-16T21:59:14.020","2018-04-16T16:59:14.020","CW","Sonar",null,null,"ADCP passive"]
["2018-04-16T21:52:52.920","2018-04-16T16:52:52.920","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-16T21:47:07.390","2018-04-16T16:47:07.390","CW","Sonar","EK","Start Pinging"]
["2018-04-16T21:47:09.770","2018-04-16T16:47:09.770","CW","Sonar","Knudsen","Start Pinging"]
["2018-04-16T22:15:35.580","2018-04-16T17:15:35.580","CW","Sonar","Multibeam","Start Logging","MB line 0105"]
["2018-04-16T22:15:32.370","2018-04-16T17:15:32.370","CW","XBT",null,null,"AXBT 016; applied to MB line 0105"]
["2018-04-17T01:51:04.150","2018-04-16T20:51:04.150","JM","Sonar","Multibeam",null,"Penetration filter weak, aeration off"]
["2018-04-17T02:57:37.480","2018-04-16T21:57:37.480","JM","XBT",null,null,"AXBT 017 Cast"]
["2018-04-17T03:04:52.360","2018-04-16T22:04:52.360","JM","XBT",null,null,"AXBT 017 Cast applied to the end of line 0109"]
["2018-04-17T03:33:00.200","2018-04-16T22:33:00.200","CW","Sonar","Knudsen","Range","500. New Line"]
["2018-04-17T07:16:57.210","2018-04-17T02:16:57.210","JM","XBT",null,null,"AXBT 018 Cast"]
["2018-04-17T07:23:14.260","2018-04-17T02:23:14.260","JM","XBT",null,null,"AXBT 018 Cast applied to line 0114"]
["2018-04-17T10:22:04.110","2018-04-17T05:22:04.110","JM","Sonar","Multibeam","New Line","start turn, line 0118"]
["2018-04-17T10:33:23.530","2018-04-17T05:33:23.530","JM","Sonar","Multibeam","New Line","end turn, line 0119"]
["2018-04-17T10:50:20.220","2018-04-17T05:50:20.220","JM","Sonar","All","Secure","Arrive dive site, start ADCP"]
["2018-04-17T21:56:38.500","2018-04-17T16:56:38.500","CW","Sonar","Multibeam","BIST","BIST 05 All Pass"]
["2018-04-17T21:56:35.880","2018-04-17T16:56:35.880","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-17T21:56:33.870","2018-04-17T16:56:33.870","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-17T21:56:50.280","2018-04-17T16:56:50.280","CW","Sonar","EK","Start Pinging"]
["2018-04-17T21:56:52.780","2018-04-17T16:56:52.780","CW","Sonar","Knudsen","Start Pinging"]
["2018-04-17T22:07:42.550","2018-04-17T17:07:42.550","CW","Sonar","Multibeam","Start Logging","MB line 0105"]
["2018-04-17T22:31:15.610","2018-04-17T17:31:15.610","CW","XBT",null,null,"AXBT 019; applied to MB line 0120"]
["2018-04-18T03:10:04.430","2018-04-17T22:10:04.430","CW","XBT",null,null,"AXBT020; applied to MB line 0125"]
["2018-04-18T03:48:08.540","2018-04-17T22:48:08.540","CW","Sonar","Multibeam",null,"SIS crashed!! I guess from trying to zoom out."]
["2018-04-18T03:51:23.190","2018-04-17T22:51:23.190","CW","Sonar","Multibeam",null,"SIS restarted."]
["2018-04-18T03:55:37.800","2018-04-17T22:55:37.800","CW","Sonar","Multibeam","New Line","0125. Not gridding though. "]
["2018-04-18T05:27:24.210","2018-04-18T00:27:24.210","CW","POS",null,null,"Nav Status: Pri. DGPS"]
["2018-04-18T06:50:14.490","2018-04-18T01:50:14.490","CW","Sonar","Multibeam","New Line","Turn line 0131"]
["2018-04-18T07:08:22.460","2018-04-18T02:08:22.460","CW","Sonar","Multibeam","New Line","Survey Line 0132"]
["2018-04-18T07:08:26.330","2018-04-18T02:08:26.330","CW","Sonar","EK","New Line"]
["2018-04-18T07:08:28.440","2018-04-18T02:08:28.440","CW","Sonar","Knudsen","New Line"]
["2018-04-18T07:18:54.310","2018-04-18T02:18:54.310","JM","XBT",null,null,"Cast #21 applied to line 0132"]
["2018-04-18T08:05:52.610","2018-04-18T03:05:52.610","JM","Sonar","Multibeam","New Line","Turn line 0133"]
["2018-04-18T08:20:23.070","2018-04-18T03:20:23.070","JM","Sonar","All","New Line","End Turn, MB line 0134"]
["2018-04-18T09:31:32.290",{"$f":"IF(ISBLANK(A197),\" \",((A197)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-18T04:31:32.290"},"MW","Sonar","All","New Line","Turn Line 0136"]
["2018-04-18T10:02:02.520","2018-04-18T05:02:02.520","MW","Sonar","All","New Line","Survey Line 0137"]
["2018-04-18T10:22:57.100","2018-04-18T05:22:57.100","JM","Sonar","All","New Line","MB line 0138"]
["2018-04-18T10:45:34.460","2018-04-18T05:45:34.460","JM","Sonar","All","Secure","Arrive at dive site. Start ADCP"]
["2018-04-18T21:43:57.750","2018-04-18T16:43:57.750","CW","Sonar","Multibeam","BIST","BIST 06 All Pass"]
["2018-04-18T21:53:43.270","2018-04-18T16:53:43.270","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-18T21:52:44.960","2018-04-18T16:52:44.960","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-18T22:51:45.050","2018-04-18T17:51:45.050","CW","Sonar","EK","Start Pinging"]
["2018-04-18T22:51:46.840","2018-04-18T17:51:46.840","CW","Sonar","Knudsen","Start Pinging"]
["2018-04-18T22:54:51.980","2018-04-18T17:54:51.980","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0139"]
["2018-04-18T23:23:45.860","2018-04-18T18:23:45.860","CW","XBT",null,null,"AXBT 022; applied to MB line 0139"]
["2018-04-19T01:59:25.740","2018-04-18T20:59:25.740","JM","XBT",null,null,"AXBT023 cast"]
["2018-04-19T02:06:43.330","2018-04-18T21:06:43.330","JM","XBT",null,null,"AXBT023 cast applied to MB line 0143"]
["2018-04-19T06:28:18.970","2018-04-19T01:28:18.970","JM","Sonar","Knudsen","Gain Value",35]
["2018-04-19T07:33:22.340","2018-04-19T02:33:22.340","JM","XBT",null,null,"AXBT024 cast"]
["2018-04-19T07:40:10.140","2018-04-19T02:40:10.140","JM","XBT",null,null,"AXBT024 cast applied to MB line 0148"]
["2018-04-19T08:50:04.430","2018-04-19T03:50:04.430","JM","Sonar","Knudsen","Tx Pulse","1ms"]
["2018-04-19T11:34:05.870","2018-04-19T06:34:05.870","JM","Sonar","Multibeam",null,"Stop logging while we aren't moving for engine repair"]
["2018-04-19T11:38:40.060","2018-04-19T06:38:40.060","MW","Sonar","Multibeam",null,"Pinging and Loggin"]
["2018-04-19T12:33:25.330","2018-04-19T07:33:25.330","JM","Sonar","All","Secure","Arrive at dive site. Start ADCP"]
["2018-04-19T21:30:58.980","2018-04-19T16:30:58.980","CW","Sonar","Multibeam",null,"NEW SURVEY!!! EX1803_B"]
["2018-04-19T21:37:26.770","2018-04-19T16:37:26.770","CW","Sonar","Multibeam","BIST","BIST 07 All Pass"]
["2018-04-19T22:07:27.730","2018-04-19T17:07:27.730","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-19T22:07:30.040","2018-04-19T17:07:30.040","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-19T22:21:45.540","2018-04-19T17:21:45.540","CW","Sonar","EK","Start Pinging"]
["2018-04-19T22:21:48.240","2018-04-19T17:21:48.240","CW","Sonar","Knudsen","Start Pinging"]
["2018-04-19T22:22:00.130","2018-04-19T17:22:00.130","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0002"]
["2018-04-19T22:58:50.710","2018-04-19T17:58:50.710","CW","XBT",null,null,"AXBT 025; applied to MB line 0002"]
["2018-04-19T23:57:43.430","2018-04-19T18:57:43.430","CW","Sonar","Knudsen",null,"TVG Mode 5logR off. Pulse 2, Power 2 Gain Val 30dB, Range 500"]
["2018-04-20T03:18:20.770","2018-04-19T22:18:20.770","JM","XBT",null,null,"AXBT 026; applied to MB line 0007"]
["2018-04-20T04:13:37.850","2018-04-19T23:13:37.850","JM","Sonar","Knudsen","Range","1000m. New line"]
["2018-04-20T05:32:54.940","2018-04-20T00:32:54.940","JM","Sonar","Multibeam","New Line","Begin turn, MB line 0010"]
["2018-04-20T05:46:04.150","2018-04-20T00:46:04.150","JM","Sonar","All","New Line","End turn, MB line 0011"]
["2018-04-20T07:11:03.600","2018-04-20T02:11:03.600","JM","Sonar","Multibeam","New Line","Begin turn, MB line 0013"]
["2018-04-20T07:25:43.320","2018-04-20T02:25:43.320","JM","Sonar","All","New Line","End turn, MB line 0014"]
["2018-04-20T07:25:46.860","2018-04-20T02:25:46.860","JM","Sonar","Knudsen","Range","500m. "]
["2018-04-20T07:42:45.770","2018-04-20T02:42:45.770","JM","XBT",null,null,"AXBT 027 cast"]
["2018-04-20T07:49:00.410","2018-04-20T02:49:00.410","JM","XBT",null,null,"AXBT 027 cast applied to MB line 0014"]
["2018-04-20T08:24:34.400","2018-04-20T03:24:34.400","JM","Sonar","Multibeam","New Line","Begin turn early due to traffic, MB line 0015. "]
["2018-04-20T08:36:59.480","2018-04-20T03:36:59.480","JM","Sonar","All","New Line","End turn, MB line 0016"]
["2018-04-20T09:37:02.090","2018-04-20T04:37:02.090","JM","Sonar","Multibeam","New Line","Begin turn, MB line 0017"]
["2018-04-20T09:44:40.380","2018-04-20T04:44:40.380","JM","Sonar","All","New Line","End turn, MB line 0018"]
["2018-04-20T10:46:22.580","2018-04-20T05:46:22.580","JM","Sonar","All","Secure","Arrive dive site. ADCP"]
["2018-04-20T21:29:35.780","2018-04-20T16:29:35.780","CW","Sonar","Multibeam","BIST","BIST 08 RX Noise Fail - ROV still in water, ship moving 1.26knts"]
["2018-04-20T21:57:59.800","2018-04-20T16:57:59.800","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-20T21:29:49.810","2018-04-20T16:29:49.810","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-20T21:58:04.440","2018-04-20T16:58:04.440","CW","Sonar","EK","Start Pinging"]
["2018-04-20T21:58:06.810","2018-04-20T16:58:06.810","CW","Sonar","Knudsen","Start Pinging"]
["2018-04-20T22:18:28.180","2018-04-20T17:18:28.180","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0019"]
["2018-04-20T22:24:17.810","2018-04-20T17:24:17.810","CW","XBT",null,null,"AXBT 028; applied to MB line 0019"]
["2018-04-20T22:48:59.670","2018-04-20T17:48:59.670","CW","Sonar","Knudsen",null,"Auto Phase Range off. "]
["2018-04-20T23:25:01.170","2018-04-20T18:25:01.170","CW","Sonar","Knudsen",null,"Range 1000. New line"]
["2018-04-21T02:35:31.070","2018-04-20T21:35:31.070","JM","Sonar","Knudsen",null,"Range 500. New line"]
["2018-04-21T02:47:57.120","2018-04-20T21:47:57.120","JM","XBT",null,null,"AXBT 029 cast"]
["2018-04-21T02:55:38.580","2018-04-20T21:55:38.580","JM","XBT",null,null,"AXBT 029 cast, applied to MB  line 0023"]
["2018-04-21T02:51:40.730","2018-04-20T21:51:40.730","JM","Sonar","Knudsen",null,"Range 1000. New line"]
["2018-04-21T02:56:44.120","2018-04-20T21:56:44.120","JM",null,null,null,"SEEP line 0023"]
["2018-04-21T07:38:42.370","2018-04-21T02:38:42.370","JM","XBT",null,null,"AXBT 030 cast"]
["2018-04-21T07:45:05.570","2018-04-21T02:45:05.570","JM","XBT",null,null,"AXBT 030 cast, applied to MB  line 0029"]
["2018-04-21T08:57:24.640","2018-04-21T03:57:24.640","JM","Sonar","Multibeam",null,"Penetration filter to weak"]
["2018-04-21T11:33:51.710","2018-04-21T06:33:51.710","JM","XBT",null,null,"AXBT 031 cast"]
["2018-04-21T11:40:16.360","2018-04-21T06:40:16.360","JM","XBT",null,null,"AXBT 031 cast, applied to MB  line 0033"]
["2018-04-21T11:42:51.730","2018-04-21T06:42:51.730","JM","Sonar","Knudsen",null,"Range 500m. New line"]
["2018-04-21T13:52:44.280","2018-04-21T08:52:44.280","MW","XBT",null,null,"Cast 032"]
["2018-04-21T13:53:00.500",{"$f":"IF(ISBLANK(A261),\" \",((A261)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-21T08:53:00.500"},"MW","Sonar","Multibeam",null,"Cast 32 Applied to Line 036"]
["2018-04-21T14:19:15.840","2018-04-21T09:19:15.840","MW","Sonar","Multibeam",null,"SSM Server Mode on - we are transiting infront of the MS delta"]
["2018-04-22T02:35:28.630","2018-04-21T21:35:28.630","CW","Sonar","Knudsen",null,"Secured for return to port. "]
["2018-04-22T03:28:03.930","2018-04-21T22:28:03.930","CW","Ship",null,null,"TSG Secured for return to port. "]
["2018-04-22T03:38:39.400","2018-04-21T22:38:39.400","JM","Sonar","Multibeam","Secure","MB and EK secured @100m"]
["2018-04-23T15:59:47","2018-04-23T10:59:47","CW","All",null,"Secure","Shutting down sonars for hull dive"]
["2018-04-23T20:00:54.120","2018-04-23T15:00:54.120","CW","All",null,null,"Dive complete. Restarting systems"]
["2018-04-24T19:47:04.080","2018-04-24T14:47:04.080","MW","Sonar",null,"Pinging"]
["2018-04-24T22:19:40.390","2018-04-24T17:19:40.390","MW",null,null,null,"SSM Server Mode on for shallow water transit, Line 050"]
["2018-04-24T22:20:38.100","2018-04-24T17:20:38.100","MW","Sonar","Multibeam","Start Logging","MB Line 0050"]
["2018-04-25T03:09:41.920","2018-04-24T22:09:41.920","CW","Sonar","Knudsen","Start Pinging","Logging. Pulse 2; Power 1; Gain 26; Range 200; Phase Range 100-300"]
["2018-04-25T03:34:23.250","2018-04-24T22:34:23.250","CW","Sonar","EK",null,"Output to SCS lost feed again. Must be after a EK restart? Something to note whenver software or GPT's are secured. Not too hard to set up again though. Kevin did good on the SOP"]
["2018-04-25T03:43:38.590","2018-04-24T22:43:38.590","CW","POS",null,null,"Positioning going in and out. "]
["2018-04-25T03:45:21.990",{"$f":"IF(ISBLANK(A274),\" \",((A274)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-24T22:45:21.990"},"CW","Sonar","Knudsen","Range","500. New line"]
["2018-04-25T04:07:56.870","2018-04-24T23:07:56.870","CW",null,null,null,"SSM Synthetic Profile Server OFF"]
["2018-04-25T04:08:02.640","2018-04-24T23:08:02.640","CW","XBT",null,null,"AXBT 033; applied to MB line 0055"]
["2018-04-25T06:09:25.280","2018-04-25T01:09:25.280","CW","XBT",null,null,"AXBT 034; applied to MB line 0057"]
["2018-04-25T06:15:16.970","2018-04-25T01:15:16.970","CW","Sonar","Knudsen","Gain Value",30]
["2018-04-25T08:14:55.010","2018-04-25T03:14:55.010","JM","XBT",null,null,"AXBT 035 cast"]
["2018-04-25T08:21:50.640",{"$f":"IF(ISBLANK(A280),\" \",((A280)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-25T03:21:50.640"},"JM","XBT",null,null,"AXBT 035 cast applied to MB line 0060"]
["2018-04-25T09:26:06.320",{"$f":"IF(ISBLANK(A281),\" \",((A281)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-25T04:26:06.320"},"JM","Sonar","All","New Line","Turn. MB line 0062"]
["2018-04-25T09:54:20.720","2018-04-25T04:54:20.720","JM","Sonar","Multibeam","New Line","Begin turn MB line 0063"]
["2018-04-25T10:01:17.430","2018-04-25T05:01:17.430","JM","Sonar","All","New Line","End turn MB line 0064. Knudsen range 1000m"]
["2018-04-25T10:38:26.230","2018-04-25T05:38:26.230","JM","Sonar","Multibeam","New Line","Begin turn MB line 0067. *0066 was skipped"]
["2018-04-25T10:38:57.730","2018-04-25T05:38:57.730","JM","Sonar","All","New Line","End turn MB line 0068"]
["2018-04-25T10:51:03.110","2018-04-25T05:51:03.110","JM","Sonar","All","Secure","Arrive at Desoto Canyon dive site. Start ADCP"]
["2018-04-25T21:22:21.440","2018-04-25T16:22:21.440","CW","Sonar","Multibeam","BIST","BIST 09. All Pass"]
["2018-04-25T21:53:13.580","2018-04-25T16:53:13.580","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-25T21:55:28.390","2018-04-25T16:55:28.390","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-25T21:55:30.520","2018-04-25T16:55:30.520","CW","Sonar","EK","Start Pinging","Recording"]
["2018-04-25T21:55:37.660","2018-04-25T16:55:37.660","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-04-25T22:13:09.180","2018-04-25T17:13:09.180","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0069"]
["2018-04-25T22:27:15.170","2018-04-25T17:27:15.170","CW","XBT",null,null,"AXBT 036; applied to MB line 00"]
["2018-04-25T23:01:25.290","2018-04-25T18:01:25.290","CW","Sonar","Multibeam","New Line","270 Turn; new MB line 0069"]
["2018-04-25T23:08:37.920","2018-04-25T18:08:37.920","CW","Ship",null,null,"Mistake on a turn. 0069 is now just a turn line. New line will start when we are back on the line plan."]
["2018-04-25T23:13:21.160","2018-04-25T18:13:21.160","CW","Sonar","Multibeam","New Line","Back on line after that lame turn. MB line 0071"]
["2018-04-25T23:14:00.250","2018-04-25T18:14:00.250","CW","Sonar","Knudsen","New Line"]
["2018-04-25T23:14:14.530","2018-04-25T18:14:14.530","CW","Sonar","EK","New Line"]
["2018-04-25T23:29:06.560","2018-04-25T18:29:06.560","MW","Sonar","All","New Line"]
["2018-04-25T23:41:16.910","2018-04-25T18:41:16.910","MW","XBT",null,null,"Cast 037 Applied tyo Line 0073"]
["2018-04-25T23:52:41.430","2018-04-25T18:52:41.430","CW","Sonar","Knudsen","Range","500. New line"]
["2018-04-26T02:32:00.550","2018-04-25T21:32:00.550","JM","XBT",null,null,"Cast 038"]
["2018-04-26T02:37:49.860","2018-04-25T21:37:49.860","JM","XBT",null,null,"Cast 038. Applied to line 0076"]
["2018-04-26T04:00:33.580","2018-04-25T23:00:33.580","JM","Sonar","Multibeam","New Line","Begin turn line 0078"]
["2018-04-26T04:18:32.430","2018-04-25T23:18:32.430","JM","Sonar","All","New Line","End turn. MB line 0079"]
["2018-04-26T04:51:25.430","2018-04-25T23:51:25.430","JM","XBT",null,null,"Cast 039"]
["2018-04-26T04:56:57.640","2018-04-25T23:56:57.640","JM","XBT",null,null,"Cast 039. Applied to line 0080"]
["2018-04-26T04:59:44.470","2018-04-25T23:59:44.470","JM","Sonar","Multibeam","New Line","Turn line 0081"]
["2018-04-26T05:23:54.590","2018-04-26T00:23:54.590","CW","Sonar","Knudsen","Range","200. New Line"]
["2018-04-26T06:45:34.830","2018-04-26T01:45:34.830","JM","Sonar","Multibeam","New Line","Begin 270 turn line 0083"]
["2018-04-26T06:54:03.020","2018-04-26T01:54:03.020","JM","Sonar","All","New Line","End turn. MB line 0084"]
["2018-04-26T06:57:46.120","2018-04-26T01:57:46.120","JM","XBT",null,null,"Cast 040"]
["2018-04-26T07:02:47.880","2018-04-26T02:02:47.880","JM","XBT",null,null,"Cast 040. Applied to line 0084"]
["2018-04-26T07:36:20.040","2018-04-26T02:36:20.040","JM","Sonar","Knudsen","Phase Range","1000m. New line"]
["2018-04-26T08:45:05.390","2018-04-26T03:45:05.390","JM","Sonar","Multibeam","New Line","Begin turn line 0086"]
["2018-04-26T08:52:22.710","2018-04-26T03:52:22.710","JM","Sonar","All","New Line","End turn. MB line 0087"]
["2018-04-26T08:54:46.080","2018-04-26T03:54:46.080","JM","XBT",null,null,"Cast 041"]
["2018-04-26T08:59:57.120","2018-04-26T03:59:57.120","JM","XBT",null,null,"Cast 041. Applied to line 0087"]
["2018-04-26T09:23:04.400","2018-04-26T04:23:04.400","JM","Sonar","Multibeam","New Line","Begin turn line 0088"]
["2018-04-26T09:31:57.110","2018-04-26T04:31:57.110","JM","Sonar","All","New Line","End turn. MB line 0089"]
["2018-04-26T10:06:28.760","2018-04-26T05:06:28.760","JM","Sonar","Multibeam","New Line","Begin 270 turn line 0090"]
["2018-04-26T10:19:00.310","2018-04-26T05:19:00.310","JM","Sonar","All","New Line","End turn. MB line 0091"]
["2018-04-26T10:39:09.140","2018-04-26T05:39:09.140","JM","Sonar","All","Secure","Arrive at dive site. Start ADCP"]
["2018-04-26T21:18:10.860","2018-04-26T16:18:10.860","CW","Sonar","Multibeam","BIST","BIST 10. All Pass"]
["2018-04-26T22:01:43.340","2018-04-26T17:01:43.340","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-26T22:01:43.340",{"$f":"IF(ISBLANK(A326),\" \",((A326)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-26T17:01:43.340"},"CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-26T22:32:17.030","2018-04-26T17:32:17.030","CW","Sonar","EK","Start Pinging","Recording"]
["2018-04-26T22:32:20.360","2018-04-26T17:32:20.360","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-04-26T22:35:56.110","2018-04-26T17:35:56.110","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0092"]
["2018-04-26T22:47:40.430","2018-04-26T17:47:40.430","CW","XBT",null,null,"AXBT 042; applied to MB line 0092"]
["2018-04-26T23:45:58.010","2018-04-26T18:45:58.010","CW","Sonar","All",null,"Turn Line 0095"]
["2018-04-27T00:03:39.170","2018-04-26T19:03:39.170","CW","Sonar","Knudsen","Range","500. New line"]
["2018-04-27T00:56:39.960","2018-04-26T19:56:39.960","JM","Watch Change",null,null,"Hi there"]
["2018-04-27T01:01:56.330","2018-04-26T20:01:56.330","JM","XBT",null,null,"AXBT Cast 043"]
["2018-04-27T01:07:15.140","2018-04-26T20:07:15.140","JM","XBT",null,null,"AXBT Cast 043 applied to MB line 0096"]
["2018-04-27T01:59:26.300","2018-04-26T20:59:26.300","JM","Sonar","Multibeam","New Line","Turn line 0098"]
["2018-04-27T03:31:28.950",{"$f":"IF(ISBLANK(A337),\" \",((A337)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-26T22:31:28.950"},"JM","XBT",null,null,"AXBT Cast 044"]
["2018-04-27T03:36:42.150","2018-04-26T22:36:42.150","JM","XBT",null,null,"AXBT Cast 044 applied to MB line 0099"]
["2018-04-27T03:55:01.540","2018-04-26T22:55:01.540","CW","Sonar","Multibeam","New Line","Turn line 0100"]
["2018-04-27T04:15:46.140","2018-04-26T23:15:46.140","CW","Sonar","Knudsen","New Line"]
["2018-04-27T04:15:47.950","2018-04-26T23:15:47.950","CW","Sonar","EK","New Line"]
["2018-04-27T04:15:49.520","2018-04-26T23:15:49.520","CW","Sonar","Multibeam","New Line","Survey line 0101"]
["2018-04-27T23:59:39.330","2018-04-27T18:59:39.330","CW","Sonar","Multibeam","BIST","BIST 12. All Pass"]
["2018-04-28T00:03:21.790","2018-04-27T19:03:21.790","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-28T00:02:32.930","2018-04-27T19:02:32.930","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-28T00:03:39.270","2018-04-27T19:03:39.270","CW","Sonar","EK","Start Pinging","Recording"]
["2018-04-28T00:03:40.990","2018-04-27T19:03:40.990","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-04-28T01:01:58.200","2018-04-27T20:01:58.200","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0113"]
["2018-04-28T01:15:39.220","2018-04-27T20:15:39.220","CW","XBT",null,null,"AXBT 047; applied to MB line 0113"]
["2018-04-28T03:59:24.420","2018-04-27T22:59:24.420","JM","XBT",null,null,"AXBT cast 048"]
["2018-04-28T04:05:42.570","2018-04-27T23:05:42.570","JM","XBT",null,null,"AXBT cast 048 applied to MB line 0116"]
["2018-04-28T05:10:29.080","2018-04-28T00:10:29.080","CW","Sonar","Multibeam","Ping Mode","Auto Off, Manual Deep. "]
["2018-04-28T06:28:27.660","2018-04-28T01:28:27.660","JM","XBT",null,null,"AXBT cast 049"]
["2018-04-28T06:33:38.910","2018-04-28T01:33:38.910","JM","XBT",null,null,"AXBT cast 049 applied to MB line 0118"]
["2018-04-28T09:15:02.400","2018-04-28T04:15:02.400","JM","XBT",null,null,"AXBT cast 050"]
["2018-04-28T09:20:18.120","2018-04-28T04:20:18.120","JM","XBT",null,null,"AXBT cast 050 applied to MB line 0121"]
["2018-04-28T09:40:55.970","2018-04-28T04:40:55.970","JM","Sonar","Knudsen","Range","200m. New line"]
["2018-04-28T10:33:51.600","2018-04-28T05:33:51.600","JM","Sonar","Multibeam","New Line","Turn line 0123"]
["2018-04-28T10:41:18.670","2018-04-28T05:41:18.670","JM","Sonar","All","New Line","End Turn. MB line 124"]
["2018-04-28T10:59:20","2018-04-28T05:59:20","JM","Sonar","All","Secure","Arrive at dive site. Start ADCP"]
["2018-04-29T00:03:52.910","2018-04-28T19:03:52.910","CW","Sonar","Multibeam","BIST","BIST 13. Rx Noise Fail"]
["2018-04-29T00:03:54.520","2018-04-28T19:03:54.520","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-29T00:04:07.720","2018-04-28T19:04:07.720","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-29T00:05:38.590","2018-04-28T19:05:38.590","CW","Sonar","EK","Start Pinging","Recording"]
["2018-04-29T00:05:40.490","2018-04-28T19:05:40.490","CW","Sonar","Knudsen","Start Pinging","Recording"]
[null," ","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0125"]
["2018-04-29T00:16:59.650","2018-04-28T19:16:59.650","CW","XBT",null,null,"No XBT, running SSP SPS for shoal waters"]
["2018-04-29T00:32:59.210","2018-04-28T19:32:59.210","MW",null,null,null,"SIS restarted.  Would not bring in Background Images"]
["2018-04-29T01:50:10.460","2018-04-28T20:50:10.460","JM","Sonar","Multibeam","New Line","Turn line 0128"]
["2018-04-29T01:55:22.740","2018-04-28T20:55:22.740","JM","Sonar","All","New Line","End Turn. MB line 129"]
["2018-04-29T02:17:35.650","2018-04-28T21:17:35.650","JM","XBT",null,null,"AXBT cast 051"]
["2018-04-29T02:21:53.090","2018-04-28T21:21:53.090","JM","XBT",null,null,"AXBT cast 051 applied to MB line 0130"]
["2018-04-29T04:41:24.360","2018-04-28T23:41:24.360","CW","XBT",null,null,"AXBT 052; applied to MB line 0132"]
["2018-04-29T04:46:07.020","2018-04-28T23:46:07.020","CW","Sonar","Multibeam","New Line","New line for turn. MB 0133"]
["2018-04-29T04:46:09.480","2018-04-28T23:46:09.480","CW","Sonar","EK","New Line"]
["2018-04-29T04:46:11.450","2018-04-28T23:46:11.450","CW","Sonar","Knudsen","New Line"]
["2018-04-29T04:58:24.960","2018-04-28T23:58:24.960","CW","Sonar","Multibeam","New Line","New line for turn. MB 0134"]
["2018-04-29T04:58:27.090","2018-04-28T23:58:27.090","CW","Sonar","EK","New Line"]
["2018-04-29T04:58:30.260","2018-04-28T23:58:30.260","CW","Sonar","Knudsen","New Line"]
["2018-04-29T05:31:20.650","2018-04-29T00:31:20.650","CW","Sonar","Multibeam","New Line","New line for turn. MB 0135"]
["2018-04-29T05:31:22.630","2018-04-29T00:31:22.630","CW","Sonar","EK","New Line"]
["2018-04-29T05:31:24.500","2018-04-29T00:31:24.500","CW","Sonar","Knudsen","New Line"]
["2018-04-29T06:32:05.700","2018-04-29T01:32:05.700","JM","XBT",null,null,"AXBT cast 053"]
["2018-04-29T06:35:56.360","2018-04-29T01:35:56.360","JM","XBT",null,null,"AXBT cast 053 applied to MB line 0136"]
["2018-04-29T08:28:18.180","2018-04-29T03:28:18.180","JM","XBT",null,null,"AXBT cast 054"]
["2018-04-29T08:31:46.020","2018-04-29T03:31:46.020","JM","Sonar","All","New Line","Turn"]
["2018-04-29T08:31:49.430","2018-04-29T03:31:49.430","JM","XBT",null,null,"AXBT cast 054 applied to MB line 0139"]
["2018-04-29T09:15:03.250","2018-04-29T04:15:03.250","JM","Sonar","Multibeam",null,"Noisey. Slowing down ship speed"]
["2018-04-29T10:40:11.600","2018-04-29T05:40:11.600","JM","Sonar","All","Secure","Arrive at dive site. Start ADCP"]
["2018-04-29T22:42:44.400","2018-04-29T17:42:44.400","CW","Sonar","Multibeam","BIST","BIST 14. Rx Noise Fail"]
["2018-04-29T22:48:34.770","2018-04-29T17:48:34.770","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-29T22:48:41.730","2018-04-29T17:48:41.730","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-04-29T23:02:11.100","2018-04-29T18:02:11.100","CW","Sonar","EK","Start Pinging","Recording"]
["2018-04-29T23:02:13.520","2018-04-29T18:02:13.520","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-04-29T23:02:15.940","2018-04-29T18:02:15.940","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0143"]
["2018-04-29T23:02:56.600","2018-04-29T18:02:56.600","CW","XBT",null,null,"Cast 055 Applied to Line 0143"]
["2018-04-30T00:55:35.960","2018-04-29T19:55:35.960","JM","Watch Change",null,null,"Hey there"]
["2018-04-30T02:18:39.960","2018-04-29T21:18:39.960","CW","Sonar","Multibeam","New Line","Turn on MB 147"]
["2018-04-30T02:23:11.030",{"$f":"IF(ISBLANK(A399),\" \",((A399)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-29T21:23:11.030"},"CW","Sonar","All","New Line","Survey Line 148"]
["2018-04-30T02:26:06.120","2018-04-29T21:26:06.120","JM","XBT",null,null,"AXBT cast 056"]
["2018-04-30T02:31:52.670","2018-04-29T21:31:52.670","JM","XBT",null,null,"AXBT cast 056 applied to MB line 0148"]
["2018-04-30T03:48:09.590","2018-04-29T22:48:09.590","CW","Sonar","Multibeam","New Line","Turn on MB line 0150"]
["2018-04-30T03:48:50.040","2018-04-29T22:48:50.040","CW","Sonar","EK","New Line"]
["2018-04-30T03:48:50.040",{"$f":"IF(ISBLANK(A404),\" \",((A404)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-29T22:48:50.040"},"CW","Sonar","Knudsen","New Line"]
["2018-04-30T03:56:29.220",{"$f":"IF(ISBLANK(A405),\" \",((A405)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-29T22:56:29.220"},"CW","Sonar","Multibeam","New Line","New survey line 0151"]
["2018-04-30T04:28:08.990","2018-04-29T23:28:08.990","JM","XBT",null,null,"AXBT cast 057"]
["2018-04-30T04:32:22.460","2018-04-29T23:32:22.460","JM","XBT",null,null,"AXBT cast 057 applied to MB line 0151"]
["2018-04-30T04:35:50.990","2018-04-29T23:35:50.990","CW","Sonar","Multibeam","New Line","Turn at beginning of MB line 0153"]
["2018-04-30T04:36:33.380","2018-04-29T23:36:33.380","CW","Sonar","EK","New Line"]
["2018-04-30T04:36:35.760","2018-04-29T23:36:35.760","CW","Sonar","Knudsen","New Line"]
["2018-04-30T05:10:58.100","2018-04-30T00:10:58.100","JM","Sonar","Multibeam","New Line","Begin turn, MB line 154"]
["2018-04-30T05:20:42.960","2018-04-30T00:20:42.960","JM","Sonar","All","New Line","End turn, MB Line 155"]
["2018-04-30T06:38:16.870","2018-04-30T01:38:16.870","CW","Sonar","All","New Line","MB line 0157"]
["2018-04-30T06:55:03.510","2018-04-30T01:55:03.510","JM","XBT",null,null,"AXBT cast 058"]
["2018-04-30T07:00:59.430","2018-04-30T02:00:59.430","JM","XBT",null,null,"AXBT cast 058 applied to MB line 0157"]
["2018-04-30T07:28:03.640","2018-04-30T02:28:03.640","JM","Sonar","Multibeam","New Line","Begin turn, MB line 158"]
["2018-04-30T07:46:03.550","2018-04-30T02:46:03.550","JM","Sonar","All","New Line","End turn, MB Line 159"]
["2018-04-30T08:23:08.060","2018-04-30T03:23:08.060","JM","Sonar","Multibeam","New Line","Begin turn, MB line 160"]
["2018-04-30T08:41:22.300","2018-04-30T03:41:22.300","JM","Sonar","All","New Line","End turn, MB Line 161"]
["2018-04-30T09:25:25.740","2018-04-30T04:25:25.740","JM","Sonar","Multibeam","New Line","Begin turn, MB line 162"]
["2018-04-30T09:44:25.100","2018-04-30T04:44:25.100","JM","Sonar","All","New Line","End turn, MB Line 163"]
["2018-04-30T10:17:54.450","2018-04-30T05:17:54.450","JM","Sonar","All","New Line","End turn, MB Line 164"]
["2018-04-30T10:50:03.850","2018-04-30T05:50:03.850","JM","Sonar","All","Secure","Arrive at dive site. Start ADCP"]
["2018-04-30T23:28:59.070","2018-04-30T18:28:59.070","CW","Sonar","Multibeam","BIST","BIST 15 All Pass"]
["2018-04-30T23:52:04.120","2018-04-30T18:52:04.120","CW","Sonar",null,null,"ADCP Secured"]
["2018-04-30T23:53:04.110","2018-04-30T18:53:04.110","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-05-01T00:17:40.070","2018-04-30T19:17:40.070","CW","Sonar","EK","Start Pinging","Recording"]
["2018-05-01T00:17:41.810","2018-04-30T19:17:41.810","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-05-01T00:17:44.440","2018-04-30T19:17:44.440","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0165"]
["2018-05-01T00:34:37.180",{"$f":"IF(ISBLANK(A430),\" \",((A430)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-04-30T19:34:37.180"},"CW","XBT",null,null,"Cast 059 Applied to Line 0165"]
["2018-05-01T01:21:00.970","2018-04-30T20:21:00.970","JM","Sonar",null," start logging","EK and Knudsen"]
["2018-05-01T01:56:02.550","2018-04-30T20:56:02.550","CW","Sonar","Multibeam","New Line","270 turn on new line 0167"]
["2018-05-01T02:11:06.930","2018-04-30T21:11:06.930","CW","Sonar","All","New Line","New Survey Lines. MB 0168"]
["2018-05-01T03:23:53.710","2018-04-30T22:23:53.710","JM","Sonar","Multibeam","New Line","Begin turn, MB line 170"]
["2018-05-01T03:49:43.310","2018-04-30T22:49:43.310","JM","Sonar","All","New Line","End turn, MB Line 171"]
["2018-05-01T04:42:19.050","2018-04-30T23:42:19.050","JM","XBT",null,null,"AXBT cast 060"]
["2018-05-01T04:47:09.640","2018-04-30T23:47:09.640","JM","XBT",null,null,"AXBT cast 060 applied to MB line 0172"]
["2018-05-01T05:09:20.280","2018-05-01T00:09:20.280","JM","Sonar","Multibeam","New Line","Begin turn, MB line 173"]
["2018-05-01T05:27:39.040","2018-05-01T00:27:39.040","JM","Sonar","All","New Line","End turn, MB Line 174"]
["2018-05-01T08:05:56.420","2018-05-01T03:05:56.420","JM","XBT",null,null,"AXBT cast 061"]
["2018-05-01T08:10:59.760","2018-05-01T03:10:59.760","JM","XBT",null,null,"AXBT cast 061 applied to MB line 0176"]
["2018-05-01T08:52:20.780","2018-05-01T03:52:20.780","JM","Ship",null,null,"Altering coarse to avoid fishing gear. New line 0178"]
["2018-05-01T09:30:18.010","2018-05-01T04:30:18.010","JM","Sonar","Multibeam","New Line","Begin turn, MB line 179"]
["2018-05-01T09:48:00.370","2018-05-01T04:48:00.370","JM","Sonar","All","New Line","End turn, MB Line 180"]
["2018-05-01T10:20:07.270","2018-05-01T05:20:07.270","JM","Sonar","Multibeam","New Line","Begin turn, MB line 181"]
["2018-05-01T10:25:41.260","2018-05-01T05:25:41.260","JM","Sonar","All","New Line","End turn, MB Line 182"]
["2018-05-01T10:43:04.950","2018-05-01T05:43:04.950","JM","Sonar","All","Secure","Start ADCP"]
["2018-05-01T21:24:50.700","2018-05-01T16:24:50.700","CW","Sonar","Multibeam","BIST","BIST 16 All Pass"]
["2018-05-01T21:59:46.150","2018-05-01T16:59:46.150","CW","Sonar",null,null,"ADCP Secured"]
["2018-05-01T21:26:20.900","2018-05-01T16:26:20.900","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-05-01T22:22:12.600","2018-05-01T17:22:12.600","CW","Sonar","EK","Start Pinging","Recording"]
["2018-05-01T22:22:14.200","2018-05-01T17:22:14.200","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-05-01T22:21:56.790","2018-05-01T17:21:56.790","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 0183"]
["2018-05-01T22:35:57.940","2018-05-01T17:35:57.940","CW","XBT",null,null,"Cast 062Applied to Line 0183"]
["2018-05-02T01:00:13.610","2018-05-01T20:00:13.610","JM","Sonar","Knudsen","Range","500m"]
["2018-05-02T01:37:41.340","2018-05-01T20:37:41.340","JM","Sonar","Knudsen","Range","200m"]
["2018-05-02T02:17:42.700","2018-05-01T21:17:42.700","CW","XBT",null,null,"AXBT 063; applied to MB line 0186"]
["2018-05-02T05:35:08.260","2018-05-02T00:35:08.260","JM","XBT",null,null,"AXBT cast 064"]
["2018-05-02T05:39:02.050","2018-05-02T00:39:02.050","JM","XBT",null,null,"AXBT cast 064 applied to MB line 0191"]
["2018-05-02T08:27:37.490","2018-05-02T03:27:37.490","JM","XBT",null,null,"AXBT cast 065"]
["2018-05-02T08:32:34.340","2018-05-02T03:32:34.340","JM","XBT",null,null,"AXBT cast 065 applied to MB line 0193"]
["2018-05-02T09:50:38.170","2018-05-02T04:50:38.170","JM","Sonar","Multibeam","New Line","Begin turn, MB line 196"]
["2018-05-02T09:56:40.990","2018-05-02T04:56:40.990","JM","Sonar","All","New Line","End turn, MB Line 197"]
["2018-05-02T10:24:29.170","2018-05-02T05:24:29.170","JM","Sonar","Multibeam","New Line","Begin turn, MB line 199"]
["2018-05-02T10:30:10.170","2018-05-02T05:30:10.170","JM","XBT",null,null,"AXBT cast 066 apploieds to line 199"]
["2018-05-02T10:33:52.970","2018-05-02T05:33:52.970","JM","Sonar","All","New Line","End turn, MB Line 200"]
["2018-05-02T10:50:33.820",{"$f":"IF(ISBLANK(A467),\" \",((A467)-DATE(1970,1,1))+25569+($C$1/24))","v":"2018-05-02T05:50:33.820"},"JM","Sonar","All","Secure","Arrive dive site. ADCP on"]
["2018-05-02T21:29:28.970","2018-05-02T16:29:28.970","CW","Sonar","Multibeam","BIST","BIST 17 All Pass"]
["2018-05-02T22:00:59.110","2018-05-02T17:00:59.110","CW","Sonar",null,null,"ADCP Secured"]
["2018-05-02T22:01:01.290","2018-05-02T17:01:01.290","CW","Sonar","Multibeam","Start Pinging","Mammal Mode -20"]
["2018-05-02T22:25:18.150","2018-05-02T17:25:18.150","CW","Sonar","EK","Start Pinging","Recording"]
["2018-05-02T22:25:15.670","2018-05-02T17:25:15.670","CW","Sonar","Knudsen","Start Pinging","Recording"]
["2018-05-02T22:25:20.990","2018-05-02T17:25:20.990","CW","Sonar","Multibeam","Start Logging","Max Power. MB line 202"]
["2018-05-02T22:59:52.560","2018-05-02T17:59:52.560","CW","XBT",null,null,"Cast 067Applied to Line 0204"]
["2018-05-02T22:33:29.400","2018-05-02T17:33:29.400","CW","Sonar","Multibeam","New Line","Turn line 0203"]
["2018-05-02T22:43:04.760","2018-05-02T17:43:04.760","CW","Sonar","All","New Line","New Survey Lines. MB 0204"]
["2018-05-03T01:02:37.670","2018-05-02T20:02:37.670","CW","Sonar","Multibeam","New Line","Turn line 0207"]
["2018-05-03T01:12:34.550","2018-05-02T20:12:34.550","CW","Sonar","All","New Line","New Survey Lines. MB 0208"]
["2018-05-03T02:22:48.250","2018-05-02T21:22:48.250","JM","XBT",null,null,"AXBT cast 068"]
["2018-05-03T02:27:09.080","2018-05-02T21:27:09.080","JM","XBT",null,null,"AXBT cast 068 applied to MB line 0211"]
["2018-05-03T04:22:26.790","2018-05-02T23:22:26.790","CW","XBT",null,null,"AXBT 069; applied to MB line 0212"]
["2018-05-03T06:01:21.350","2018-05-03T01:01:21.350","JM","Sonar","Multibeam","New Line","Begin turn, MB line 215"]
["2018-05-03T06:09:44.680","2018-05-03T01:09:44.680","JM","Sonar","All","New Line","End turn, MB Line 216"]
["2018-05-03T06:26:49.990","2018-05-03T01:26:49.990","JM","XBT",null,null,"AXBT cast 070"]
["2018-05-03T06:31:05.310","2018-05-03T01:31:05.310","JM","XBT",null,null,"AXBT cast 070 applied to MB line 0216"]
["2018-05-03T07:51:15.340","2018-05-03T02:51:15.340","JM","XBT",null,null,"AXBT cast 071"]
["2018-05-03T07:55:23.120","2018-05-03T02:55:23.120","JM","XBT",null,null,"AXBT cast 071 applied to MB line 0218"]
["2018-05-03T09:56:41.620","2018-05-03T04:56:41.620","JM","Sonar","All","New Line","Turn, MB Line 221"]
["2018-05-03T09:59:41.570","2018-05-03T04:59:41.570","JM","XBT",null,null,"AXBT cast 072"]
["2018-05-03T10:04:33.810","2018-05-03T05:04:33.810","JM","XBT",null,null,"AXBT cast 072 applied to MB line 0221"]
["2018-05-03T10:47:17.600","2018-05-03T05:47:17.600","JM","Sonar","All",null,"Arrival in Key West"]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A530),\" \",((A530)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A594),\" \",((A594)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A658),\" \",((A658)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A722),\" \",((A722)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A786),\" \",((A786)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A850),\" \",((A850)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":13,"n_cols":8,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","ADCP","EK60","Knudsen","All"]
["MW","Sonar","Multibeam","Ping Mode","Start Pinging","Change Range","Tx Power","Start up"]
["JM","Ship","EK","Along Direction Pitch","Secure","Start Pinging","Tx Pulse","Secure"]
["CW","Weather","Knudsen","New Line","Passive","Secure","Gain Mode","New Line"]
[null,"Watch Change","All","Max Angle",null,"New Line","Gain Value"]
[null,"XBT",null,"Spike Filter Strength",null,null,"Process Shift"]
[null,"Issue/Problem",null,"Slope Filter (On/Off)",null,null,"Tx Blanking"]
[null,"Other",null,"Aeration Filter (On/Off)",null,null,"Range"]
[null,null,null,"Interference Filter (On/Off)",null,null,"Phase Mode"]
[null,null,null,"Start Pinging",null,null,"Start Pinging"]
[null,null,null,"Secure",null,null,"Secure"]
[null,null,null,"Start Logging",null,null,"Phase Range"]
[null,null,null,"BIST"]