{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":1993,"n_cols":7,"rows_kept":1993,"cut":false,"hidden":false,"merged":[]}
["EX-18-04 VIIRS"]
["May 9, 2018 - May 18, 2018"]
["Key West, Florida to Mayport, Florida"]
["Cruise ID: EX1804","UTC to Local: ",-4,"UTC 2","UTC 3","UTC 4","Cruise Details: May 9 to May 18"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2018-05-09T22:13:37.620",{"$f":"IF(ISBLANK(A8),\" \",((A8)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-09T18:13:37.620"},"AB","Sonar","Multibeam","Ping Mode","Pinging, not logging. Settings: Max Angles 75/75, Auto Ping Mode:Shallow, Along Direction 0 degrees, Filters: Med Spike, Normal Range Gate, Normal Phase Ramp, Penetration Off."]
["2018-05-09T22:20:34.720",{"$f":"IF(ISBLANK(A9),\" \",((A9)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-09T18:20:34.720"},"MW","Sonar","EK","Start Pinging"]
["2018-05-09T22:53:29.640","2018-05-09T18:53:29.640","MW","AXBT",null,null,"AXBT001 added to SIS"]
["2018-05-09T22:54:22.180","2018-05-09T18:54:22.180","AB","Sonar","Multibeam","Start Logging","Line 0000. Survey Speed 9 knots."]
["2018-05-09T22:54:54.320","2018-05-09T18:54:54.320","AB","Sonar","EK",null,"Start logging 200, 120, 70 an 18 kHz. Ranges at 250m."]
["2018-05-09T23:19:22.420","2018-05-09T19:19:22.420","AB","Sonar","Multibeam","New Line","0001."]
["2018-05-09T23:24:38.070","2018-05-09T19:24:38.070","AB","Sonar","EK","Change Range","All sonars change range to 300m."]
["2018-05-10T01:01:35.360","2018-05-09T21:01:35.360","NB","Sonar","Multibeam","Interference Filter (On/Off)","Interference filter on, experiencing very short periodic blowouts"]
["2018-05-10T01:07:19.730","2018-05-09T21:07:19.730","NB","Sonar","Multibeam","Ping Mode","Ping mode very shallow"]
["2018-05-10T01:10:30.800","2018-05-09T21:10:30.800","NB","Sonar","Multibeam","Ping Mode","Ping mode shallow"]
["2018-05-10T01:32:16.990","2018-05-09T21:32:16.990","NB","Sonar","Multibeam","Ping Mode","Ping Mode medium"]
["2018-05-10T01:35:22.650","2018-05-09T21:35:22.650","NB","Sonar","Multibeam","Ping Mode","Ping mode shallow"]
["2018-05-10T01:41:36.590","2018-05-09T21:41:36.590","NB","Sonar","Multibeam","Interference Filter (On/Off)","Interference filter off, still seeing blow out issue."]
["2018-05-10T01:44:12.770","2018-05-09T21:44:12.770","NB","Sonar","Multibeam","New Line","SOL 0003"]
["2018-05-10T01:46:56.700","2018-05-09T21:46:56.700","NB","Sonar","Multibeam","Aeration Filter (On/Off)"]
["2018-05-10T01:48:23.660","2018-05-09T21:48:23.660","NB","Sonar","Multibeam","Ping Mode","Ping mode medium"]
["2018-05-10T01:51:27.550","2018-05-09T21:51:27.550","NB","Sonar","Knudsen","Start Pinging","TX Pulse 0.5 m/s, Gain 20dB, Range 200"]
["2018-05-10T04:27:49.240","2018-05-10T00:27:49.240","NB","Sonar","Multibeam","New Line","SOL 006"]
["2018-05-10T05:06:07.710","2018-05-10T01:06:07.710","NB","AXBT",null,null,"0002."]
["2018-05-10T05:53:53.680","2018-05-10T01:53:53.680","AB","Sonar","Multibeam",null,"Added AXBT002 to line 0007"]
["2018-05-10T05:54:53.850","2018-05-10T01:54:53.850","AB","Sonar","Knudsen","Phase Mode","300-500."]
["2018-05-10T06:19:23.550","2018-05-10T02:19:23.550","AB","Sonar","Knudsen",null,"Tested, auto gain. Return to previous settings. Gain 30. Tx Pulse 1.0"]
["2018-05-10T06:43:01.510","2018-05-10T02:43:01.510","AB","Sonar","Knudsen","Phase Mode","400-600. "]
["2018-05-10T06:54:30.410","2018-05-10T02:54:30.410","AB","Sonar","EK","Change Range","750m"]
["2018-05-10T09:07:37.250","2018-05-10T05:07:37.250","AB","Sonar","Multibeam","New Line","0013."]
["2018-05-10T09:13:19.740","2018-05-10T05:13:19.740","AB","Sonar","Knudsen","Phase Mode","400-600"]
["2018-05-10T09:18:43.840","2018-05-10T05:18:43.840","AB","Sonar","Knudsen","Phase Mode","300-500"]
["2018-05-10T09:26:13.850","2018-05-10T05:26:13.850","AB","Sonar","Knudsen","Phase Mode","200-400"]
["2018-05-10T09:50:49.040","2018-05-10T05:50:49.040","NB","Sonar","Multibeam","Ping Mode","Shallow"]
["2018-05-10T09:51:54.340","2018-05-10T05:51:54.340","NB","Sonar","Knudsen","Secure","Depth below 150m"]
["2018-05-10T09:59:05.750","2018-05-10T05:59:05.750","NB","Sonar","Multibeam","Ping Mode","Very Shallow"]
["2018-05-10T10:10:29.100","2018-05-10T06:10:29.100","NB","Sonar","Multibeam","New Line","0014"]
["2018-05-10T11:05:37.430","2018-05-10T07:05:37.430","NB","AXBT",null,null,"002-20180210 NOT APPLIED, switched to WOA due to shallow water"]
["2018-05-10T11:16:28.490","2018-05-10T07:16:28.490","NB","Sonar","Multibeam",null,"PU Sensor error- Frequency of received Attitude datagrams on port COM2 less than 90% or expected"]
["2018-05-10T11:18:00.620","2018-05-10T07:18:00.620","NB","Sonar","Multibeam","New Line","0015"]
["2018-05-10T21:46:45.960","2018-05-10T17:46:45.960","AB","Sonar","Multibeam",null,"Settings: Manual:Very Shallow, 0 degrees alongtrack, no filters'; Line 0026, simulated SVP profile from World Atlas."]
["2018-05-10T22:01:35.520","2018-05-10T18:01:35.520","AB","Sonar","Knudsen",null,"Previously secured."]
["2018-05-10T22:01:50.490","2018-05-10T18:01:50.490","AB","Sonar","EK",null,"Range 100m, Bottom Detection 1000m, Logging 18,70,120,200 kHz. "]
["2018-05-11T00:01:05.070","2018-05-10T20:01:05.070","NB","Sonar","Multibeam","New Line","0029"]
["2018-05-11T00:57:49.550","2018-05-10T20:57:49.550","NB","Sonar","Multibeam","New Line","0031"]
["2018-05-11T01:27:54.860","2018-05-10T21:27:54.860","NB","Sonar","Multibeam","New Line","0032"]
["2018-05-11T02:05:19.690","2018-05-10T22:05:19.690","NB","Sonar","Multibeam","New Line","0033"]
["2018-05-11T02:37:51.450","2018-05-10T22:37:51.450","NB","Sonar","Multibeam","New Line","0034"]
["2018-05-11T04:45:25.110","2018-05-11T00:45:25.110","AB","Sonar","Multibeam","New Line","0037"]
["2018-05-11T06:00:48.310","2018-05-11T02:00:48.310","AB","Sonar","Multibeam","New Line","0040"]
["2018-05-11T07:03:33.650","2018-05-11T03:03:33.650","AB","Sonar","Multibeam","New Line","0041"]
["2018-05-11T07:04:24.180","2018-05-11T03:04:24.180","AB","Sonar","Multibeam",null,"PPS, flashed red OFF on SIS"]
["2018-05-11T07:35:00.250","2018-05-11T03:35:00.250","AB","Sonar","Multibeam","New Line","0042"]
["2018-05-11T08:09:32","2018-05-11T04:09:32","AB","Sonar","Multibeam","New Line","0043"]
["2018-05-11T08:46:10.040","2018-05-11T04:46:10.040","AB","Sonar","Multibeam","New Line","0044"]
["2018-05-11T09:26:52.450","2018-05-11T05:26:52.450","NB","Sonar","Multibeam","New Line","0045"]
["2018-05-11T09:56:54.080","2018-05-11T05:56:54.080","NB","Sonar","Multibeam","New Line","0046"]
["2018-05-11T10:27:42.920","2018-05-11T06:27:42.920","NB","Sonar","Multibeam","New Line","0047"]
["2018-05-11T10:58:12.250","2018-05-11T06:58:12.250","NB","Sonar","Multibeam","New Line","0048"]
["2018-05-11T11:26:32.570","2018-05-11T07:26:32.570","NB","Sonar","Multibeam","Secure","Stopped Pinging and Logging to run BIST, troubleshoot data drop outs. BIST pass with full colors"]
["2018-05-11T13:12:07.400","2018-05-11T09:12:07.400","MW","Sonar","EK","Secure"]
["2018-05-11T17:58:42.790","2018-05-11T13:58:42.790","CW","Sonar","Multibeam","Start Logging","MB line 0049"]
["2018-05-11T17:59:09.230","2018-05-11T13:59:09.230","CW","Sonar","Knudsen","Start Logging"]
["2018-05-11T21:50:47.310","2018-05-11T17:50:47.310","AB","Sonar","EK","Start Pinging"]
["2018-05-11T22:03:05.450","2018-05-11T18:03:05.450","AB","Sonar",null,null,"Logging EM302 and EK60"]
["2018-05-11T22:04:30.810","2018-05-11T18:04:30.810","AB","Sonar","EK","Change Range","150m all sonars"]
["2018-05-11T22:50:50.250","2018-05-11T18:50:50.250","MW","Sonar","Multibeam","Secure","Secure for Troubleshoointgf Timout Error on Board One"]
["2018-05-11T23:15:57.880","2018-05-11T19:15:57.880","AB","Sonar","Multibeam",null,"TRU restarted. Several board reset errors in telnet."]
["2018-05-11T23:37:02.460","2018-05-11T19:37:02.460","NB","Sonar","Multibeam",null,"Telnet error timeout on board 22. Running BIST"]
["2018-05-11T23:43:27.300","2018-05-11T19:43:27.300","NB","Sonar","Multibeam",null,"BIST TX board failure on 22, power failures 22 and 23. Restarting TRU and re-seeding board 22. "]
["2018-05-11T23:57:07.470",{"$f":"IF(ISBLANK(A73),\" \",((A73)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-11T19:57:07.470"},"NB","Sonar","Multibeam",null,"Telenet receive board error. BIST failed RX32 Test. Reseeded all receive boards. Restarted again"]
["2018-05-12T00:10:58.220","2018-05-11T20:10:58.220","NB","Sonar","Multibeam",null,"Blank telenet, re-entering cmd. Telenet response, running BIST. BIST all pass, sequence timeout on board one in Telnet. "]
["2018-05-12T00:21:50.680","2018-05-11T20:21:50.680","NB","Sonar","Multibeam","Start Pinging","Still seeing Telenet timeout message board 11. Still seeing data dropouts. Telenet timeout board 8. Far left red meatball, com 1 in Attitude? "]
["2018-05-12T00:28:24.570","2018-05-11T20:28:24.570","NB","Sonar","Multibeam","Secure","Reseeding all TRU ethernet cables. All meatballs green in SIS. All pass BIST. "]
["2018-05-12T00:48:33.790","2018-05-11T20:48:33.790","NB","Sonar","Multibeam","Start Pinging","All systems appear to be a go. "]
["2018-05-12T00:52:45.520","2018-05-11T20:52:45.520","NB","Sonar","EK",null,"logging as slave wth multibeam"]
["2018-05-12T00:53:17.750","2018-05-11T20:53:17.750","NB","Sonar","Multibeam","Start Logging","line 0052"]
["2018-05-12T01:12:23.980","2018-05-11T21:12:23.980","NB","Sonar","Knudsen","Start Pinging","TX Pulse 1, TX power, 1, Gain mode: Manual 26db, Rang: 200, Phase Range 100-300. "]
["2018-05-12T01:38:29.460","2018-05-11T21:38:29.460","NB","Sonar","Multibeam","New Line","0053"]
["2018-05-12T01:46:18.080","2018-05-11T21:46:18.080","NB","Sonar","Multibeam",null,"Telenet TSP sequence timeout board 13. No visible issue with data. Message rerpeats as Telenet cycles through"]
["2018-05-12T02:14:33.870","2018-05-11T22:14:33.870","NB","Sonar","Multibeam","New Line","line 0054"]
["2018-05-12T02:44:57.490","2018-05-11T22:44:57.490","NB","Sonar","Multibeam","New Line","line 0055"]
["2018-05-12T03:18:29.110","2018-05-11T23:18:29.110","NB","Sonar","Multibeam","New Line","line 0056"]
["2018-05-12T03:18:59.550","2018-05-11T23:18:59.550","NB","AXBT",null,null,"depth has exceeded 200m, switching from WOA server to XBT. "]
["2018-05-12T03:33:47.120","2018-05-11T23:33:47.120","NB","Sonar","Multibeam","Ping Mode","applied EX1804_0003_20180512 to line 0056"]
["2018-05-12T03:51:13.420","2018-05-11T23:51:13.420","NB","Sonar","Multibeam","New Line","Line 0057"]
["2018-05-12T04:08:55.650","2018-05-12T00:08:55.650","NB","Sonar","Multibeam",null,"Telenet TSP Sequence timeout board 13 error increase in frequency"]
["2018-05-12T06:16:54.650","2018-05-12T02:16:54.650","AB","Sonar","EK","Change Range","500m "]
["2018-05-12T07:35:40.290","2018-05-12T03:35:40.290","NB","Sonar","Multibeam","New Line","Line 0061"]
["2018-05-12T07:59:32.620","2018-05-12T03:59:32.620","AB","Sonar","Knudsen","Phase Mode","350-450, Range 100m"]
["2018-05-12T08:06:29.090","2018-05-12T04:06:29.090","NB","Sonar","Multibeam","New Line","Line 0062"]
["2018-05-12T08:43:49.690","2018-05-12T04:43:49.690","NB","Sonar","Multibeam","New Line","Line 0063"]
["2018-05-12T08:48:38.700","2018-05-12T04:48:38.700","AB","Sonar","Knudsen","Phase Mode","400-500m, Gain 33"]
["2018-05-12T09:12:52.400","2018-05-12T05:12:52.400","AB","Sonar","Knudsen","Phase Mode","450-550m"]
["2018-05-12T09:25:38.860","2018-05-12T05:25:38.860","NB","AXBT",null,null,"EX1804_0004_180512 applied to line 0063"]
["2018-05-12T09:39:35.650","2018-05-12T05:39:35.650","AB","Sonar","Knudsen","Phase Mode","500-600"]
["2018-05-12T09:55:38.920","2018-05-12T05:55:38.920","NB","Sonar","Knudsen","Phase Mode","550-650"]
["2018-05-12T09:55:46.910","2018-05-12T05:55:46.910","NB","Sonar","Multibeam","New Line","Line 0065. Deveated significantly from original course to avoid large cluster of fishing vessels, broke line for turn. "]
["2018-05-12T10:01:05.280","2018-05-12T06:01:05.280","NB","AXBT",null,null,"launching AXBT over Desoto Canyon. EX1804_0005_180512 applied to line 0065"]
["2018-05-12T10:15:59.020","2018-05-12T06:15:59.020","NB","Sonar","Multibeam",null,"PU Sensor error- Frequency of received Attitude datagrams on port COM2 less than 90% or expected"]
["2018-05-12T10:17:31.680","2018-05-12T06:17:31.680","NB","Sonar","Multibeam","New Line","Start line 0066 for turn back onto course after fishing vessel detour."]
["2018-05-12T10:18:16.570","2018-05-12T06:18:16.570","NB","Sonar","Multibeam","Ping Mode","Medium"]
["2018-05-12T10:18:56.730","2018-05-12T06:18:56.730","NB","Sonar","Knudsen","Gain Value","31 dB"]
["2018-05-12T10:20:38.330","2018-05-12T06:20:38.330","NB","Sonar","Knudsen","Phase Mode","400-500"]
["2018-05-12T10:24:24.650","2018-05-12T06:24:24.650","NB","Sonar","Knudsen","Phase Mode","350-450"]
["2018-05-12T10:55:36.730","2018-05-12T06:55:36.730","NB","Sonar","Knudsen","Phase Mode","300-400"]
["2018-05-12T10:55:50.860","2018-05-12T06:55:50.860","NB","Sonar","Multibeam","New Line","line 0067"]
["2018-05-12T11:26:52.880","2018-05-12T07:26:52.880","NB","Sonar","Multibeam","New Line","line 0068"]
["2018-05-12T11:27:03.370","2018-05-12T07:27:03.370","NB","Sonar","Knudsen","Phase Mode","250-350"]
["2018-05-12T11:34:16.410","2018-05-12T07:34:16.410","NB","AXBT",null,null,"EX1804_AXBT0006_180512"]
["2018-05-12T12:30:45.080","2018-05-12T08:30:45.080","MW","Sonar","Knudsen","Secure","100m"]
["2018-05-12T12:39:47.140","2018-05-12T08:39:47.140","MW","Sonar","Multibeam","Ping Mode","Auto -> Shallow"]
["2018-05-12T12:46:58.030","2018-05-12T08:46:58.030","MW","Sonar","Multibeam","Secure","Pinging not Logging"]
["2018-05-12T14:44:09.900","2018-05-12T10:44:09.900","MW","Sonar","Multibeam",null,"Logging"]
["2018-05-12T15:36:45.210","2018-05-12T11:36:45.210","CW","Sonar","Multibeam","Secure","VIIRS Station 7"]
["2018-05-12T19:44:27.410","2018-05-12T15:44:27.410","CW","Sonar","Multibeam","Secure","VIIRS Station 8; still secured"]
["2018-05-12T22:05:23.780","2018-05-12T18:05:23.780","AB","Ship",null,null,"Sampling station complete. Approaching survey line."]
["2018-05-12T22:05:54.060","2018-05-12T18:05:54.060","AB","Sonar","EK",null,"New line."]
["2018-05-12T22:06:09.280","2018-05-12T18:06:09.280","AB","Sonar","Multibeam","New Line","WOA online. Line 0071. Max angle 68/68."]
["2018-05-12T22:12:58.330","2018-05-12T18:12:58.330","AB","Ship",null,null,"Reducing speed for traffic."]
["2018-05-12T23:53:13.280","2018-05-12T19:53:13.280","NB","Ship",null,null,"Breaking off of planned line by about a mile for pipe obstruction. "]
["2018-05-13T01:06:13.960","2018-05-12T21:06:13.960","NB","Sonar","Multibeam","New Line","SOL 0074. back onplanned line."]
["2018-05-13T01:41:29.110","2018-05-12T21:41:29.110","NB","AXBT",null,null,"Below 200m. EX1804_AXBT0007_180513 applied to SIS line 0074. Terrible Sound speed agreement in SIS, switched WOA server back on. "]
["2018-05-13T01:51:46.290","2018-05-12T21:51:46.290","NB","Sonar","Multibeam","Ping Mode","Auto -> Medium"]
["2018-05-14T01:51:46.290","2018-05-13T21:51:46.290","NB","Sonar","Multibeam","New Line",75]
["2018-05-13T01:53:54.810","2018-05-12T21:53:54.810","NB","Sonar","Knudsen","Start Pinging","TX Pulse: 1, TX Pwer: 1, Gain value: 30dB, Range: 200, Phase: 200-400"]
["2018-05-13T02:00:35.070","2018-05-12T22:00:35.070","AB","Sonar","Knudsen","Phase Mode","300-500."]
["2018-05-13T02:13:36.130","2018-05-12T22:13:36.130","NB","Sonar","Knudsen","Phase Mode","400-600"]
["2018-05-13T02:18:42.200","2018-05-12T22:18:42.200","NB","AXBT",null,null,"EX1804_AXBT0008_180513 applied to SIS line 0075"]
["2018-05-13T02:26:25.670","2018-05-12T22:26:25.670","NB","Sonar","Multibeam","New Line","Line 0075"]
["2018-05-13T02:28:17.220","2018-05-12T22:28:17.220","NB","Sonar","Knudsen","Phase Mode","500-700"]
["2018-05-13T02:29:50.850","2018-05-12T22:29:50.850","NB","Sonar","Multibeam","Ping Mode","Auto -> Deep"]
["2018-05-13T02:32:50.880","2018-05-12T22:32:50.880","NB","Sonar","Knudsen","Gain Value","35 dB"]
["2018-05-13T02:37:04.050","2018-05-12T22:37:04.050","NB","Sonar","Knudsen","Phase Mode","700-900"]
["2018-05-13T02:44:23.750",{"$f":"IF(ISBLANK(A137),\" \",((A137)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-12T22:44:23.750"},"NB","Sonar","Knudsen","Phase Mode","800-1000"]
["2018-05-13T02:52:03.190","2018-05-12T22:52:03.190","NB","Sonar","Knudsen","Phase Mode","900-1100"]
["2018-05-13T02:58:23.420","2018-05-12T22:58:23.420","NB","Sonar","Multibeam","New Line","line 0076"]
["2018-05-13T03:00:58.730","2018-05-12T23:00:58.730","NB","AXBT",null,null,"EX1804_AXBT009_180513 applied to SIS line 0077"]
["2018-05-13T03:15:23.430","2018-05-12T23:15:23.430","NB","Sonar","Knudsen","Gain Mode","New lline, switched gain mode to manual for beter quality "]
["2018-05-13T03:29:06.050","2018-05-12T23:29:06.050","NB","Sonar","Knudsen","Phase Mode","1200-1400"]
["2018-05-13T03:29:50.370","2018-05-12T23:29:50.370","NB","Sonar","Multibeam","New Line","Line 0078"]
["2018-05-13T03:48:04.610","2018-05-12T23:48:04.610","AB","Sonar","Knudsen","Range","500m. New line"]
["2018-05-13T04:14:20.600","2018-05-13T00:14:20.600","NB","Sonar","Multibeam","Max Angle","65/65"]
["2018-05-13T04:57:11.880","2018-05-13T00:57:11.880","AB","Sonar","Knudsen",null,"Power 2, Pulse 2, Gain 38. New line. Phase 1750-2250."]
["2018-05-13T05:23:58.930","2018-05-13T01:23:58.930","AB","Sonar","Knudsen","Phase Mode","2000-2500"]
["2018-05-13T05:39:18.380","2018-05-13T01:39:18.380","AB","Sonar","EK",null,"Range 3000"]
["2018-05-13T06:11:12.910","2018-05-13T02:11:12.910","AB","AXBT",null,null,"AXBT10 added to line 0080."]
["2018-05-13T06:11:35.970","2018-05-13T02:11:35.970","AB","Sonar","Knudsen","Phase Mode","2250-2750"]
["2018-05-13T06:29:07.880","2018-05-13T02:29:07.880","NB","Sonar","Multibeam","New Line",81]
["2018-05-13T07:11:11.190","2018-05-13T03:11:11.190","AB","Sonar","Multibeam","New Line","0082"]
["2018-05-13T07:25:48.830","2018-05-13T03:25:48.830","AB","Sonar","Knudsen",null,"Tx Pulse 4, Gain 35, New line"]
["2018-05-13T08:07:56.130","2018-05-13T04:07:56.130","AB","Sonar","Multibeam","New Line","0083, turn"]
["2018-05-13T08:26:49.340","2018-05-13T04:26:49.340","AB","Sonar","Multibeam","New Line","0084, new line on all sonars."]
["2018-05-13T08:40:17.610","2018-05-13T04:40:17.610","AB","AXBT",null,null,11]
["2018-05-13T08:48:17.720","2018-05-13T04:48:17.720","AB","Sonar","Multibeam",null,"AXBT 11 added to new SIS line 86"]
["2018-05-13T08:51:09.360","2018-05-13T04:51:09.360","AB","Sonar","Knudsen",null,"Pulse 2, Gain 34."]
["2018-05-13T09:52:33.200","2018-05-13T05:52:33.200","NB","Sonar","Multibeam","New Line","New line all sonars into turn. SIS SOL 0088"]
["2018-05-13T09:54:15.440","2018-05-13T05:54:15.440","NB","Sonar","Knudsen","Gain Value",40]
["2018-05-13T10:13:34.760","2018-05-13T06:13:34.760","NB","Sonar","Multibeam","New Line","SOL 0089 into turn. New line on all sonars"]
["2018-05-13T10:14:28.760","2018-05-13T06:14:28.760","NB","Sonar","Knudsen","Gain Value",37]
["2018-05-13T10:31:51.410","2018-05-13T06:31:51.410","NB","Sonar","Knudsen","Gain Value",40]
["2018-05-13T11:21:34.740","2018-05-13T07:21:34.740","NB","Sonar","Multibeam","New Line","SOL 0091, new line on all sonars. Transitting to station. "]
["2018-05-13T11:42:21.300","2018-05-13T07:42:21.300",null,null,null,null,"AXBT Cast 12 applied to Line 0091"]
["2018-05-13T11:55:55.650","2018-05-13T07:55:55.650","MW","Sonar","All",null,"Secured for Sampling"]
["2018-05-13T14:18:12.840","2018-05-13T10:18:12.840","MW","Sonar","All",null,"Pinging and Logging during transit to next station"]
["2018-05-13T15:15:09.590","2018-05-13T11:15:09.590","MW","Sonar","All",null,"Secured for Sampling, EM302 Still Pinging"]
["2018-05-13T17:19:03.400","2018-05-13T13:19:03.400","CW","Sonar","Multibeam","Start Logging","Transiting to Station 12; MB line 0095"]
["2018-05-13T17:20:12.860","2018-05-13T13:20:12.860","CW","Sonar","EK","Start Logging"]
["2018-05-13T17:20:26.990","2018-05-13T13:20:26.990","CW","Sonar","Knudsen","Start Logging"]
["2018-05-13T18:11:44.900","2018-05-13T14:11:44.900","CW","Sonar","All","Secure","Station 12"]
["2018-05-13T20:15:58.510","2018-05-13T16:15:58.510","MW","Sonar","All",null,"Transit to Station 13"]
["2018-05-13T20:19:50.540","2018-05-13T16:19:50.540","MW","Sonar","Multibeam",null,"AXBT 013 applied to line 0096"]
["2018-05-13T20:47:14.740","2018-05-13T16:47:14.740","MW","Sonar","All",null,"Logging but not Pinging"]
["2018-05-13T21:32:43.030","2018-05-13T17:32:43.030","AB","Ship",null,null,"Floaters completed. Increasing speed and approaching trackline."]
["2018-05-13T21:36:10.390","2018-05-13T17:36:10.390","AB","Sonar",null,null,"Logging new lines all sonars."]
["2018-05-13T22:19:01.800","2018-05-13T18:19:01.800","AB","Sonar","Knudsen","Phase Mode","2500-3000"]
["2018-05-14T01:12:05.450","2018-05-13T21:12:05.450","AB","AXBT",null,null,"AXBT 014  applied to SIS line 100"]
["2018-05-14T02:20:56.220","2018-05-13T22:20:56.220","NB","Sonar","EK","Change Range","Range at 4000 m in response to sonar losing bottom"]
["2018-05-14T03:26:43.330","2018-05-13T23:26:43.330","AB","AXBT",null,null,"AXBT 15 "]
["2018-05-14T03:34:04.370","2018-05-13T23:34:04.370","AB","Sonar","Multibeam",null,"AXBT15 added to new line 0103."]
["2018-05-14T04:18:12.170","2018-05-14T00:18:12.170","AB","Sonar","Knudsen","Phase Mode","3000-3500"]
["2018-05-14T05:07:20.390","2018-05-14T01:07:20.390","AB","Sonar","Knudsen","Gain Value",39]
["2018-05-14T05:37:21.130","2018-05-14T01:37:21.130","AB","AXBT",null,null,"AXBT 16"]
["2018-05-14T05:46:29.920","2018-05-14T01:46:29.920","AB","Sonar","Multibeam",null,"AXBT 16 added to line 0105"]
["2018-05-14T07:01:18.890","2018-05-14T03:01:18.890","AB","Sonar","Multibeam","New Line",107]
["2018-05-14T07:08:50.160","2018-05-14T03:08:50.160","AB","Ship",null,null,"Reduced speed to 7 knots for on time arrival."]
["2018-05-14T08:04:59.120","2018-05-14T04:04:59.120","AB","AXBT",null,null,"AXBT 17"]
["2018-05-14T08:13:29.710","2018-05-14T04:13:29.710","AB","Sonar","Multibeam",null,"AXBT 17 added to new line 0109"]
["2018-05-14T08:29:18.380","2018-05-14T04:29:18.380","AB","Sonar","Knudsen","Gain Value",40]
["2018-05-14T08:59:41.700","2018-05-14T04:59:41.700","AB","Sonar","Multibeam",null,"Penetration filter OFF, Slope Filter ON"]
["2018-05-14T09:01:42.180","2018-05-14T05:01:42.180","AB","Sonar","Knudsen","Gain Value",36]
["2018-05-14T09:31:04.790","2018-05-14T05:31:04.790","AB","Ship",null,null,"Reduced speed to 5 knots"]
["2018-05-14T09:39:37.740","2018-05-14T05:39:37.740","NB","sonar","Multibeam","Ping Mode","Auto -> Very Deep"]
["2018-05-14T10:15:47.100","2018-05-14T06:15:47.100","NB","sonar","Knudsen","Gain Value","33 dB"]
["2018-05-14T10:31:59.740","2018-05-14T06:31:59.740","NB","sonar","Knudsen","Gain Value","37dB"]
["2018-05-14T10:44:47.530","2018-05-14T06:44:47.530","NB","AXBT",null,null,"AXBT 0018 applied to SIS line 0111"]
["2018-05-14T10:55:36.400","2018-05-14T06:55:36.400","NB","Sonar","Knudsen","Gain Value",40]
["2018-05-14T12:06:30.060","2018-05-14T08:06:30.060","MW","Sonar","All",null,"Stop Logging"]
["2018-05-14T14:27:47.610",{"$f":"IF(ISBLANK(A201),\" \",((A201)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-14T10:27:47.610"},"MW","Sonar","All",null,"Logging to Next Station"]
["2018-05-14T15:45:34.050","2018-05-14T11:45:34.050","CW","Sonar","All",null,"Secued for VIIRS Station 15"]
["2018-05-14T17:43:45.560","2018-05-14T13:43:45.560","CW","Sonar","Multibeam","Start Logging","Transit to Station 16. MB line 0115"]
["2018-05-14T17:44:59.680","2018-05-14T13:44:59.680","CW","Sonar","EK","Start Logging"]
["2018-05-14T17:45:05.160","2018-05-14T13:45:05.160","CW","Sonar","Knudsen","Start Logging"]
["2018-05-14T18:01:10.220","2018-05-14T14:01:10.220","CW","XBT",null,null,"AXBT 19; applied to MB line 0115"]
["2018-05-14T18:58:07.630","2018-05-14T14:58:07.630","CW","Sonar","All","Secure","Secued for VIIRS Station 16"]
["2018-05-14T21:00:45.290","2018-05-14T17:00:45.290","MW","Sonar","All",null,"Pinging and Logging, headed to Jacksonville"]
["2018-05-14T21:34:50.940","2018-05-14T17:34:50.940","MW",null,null,null,"XBT 020 Applied to Line 0117"]
["2018-05-14T22:44:22.120","2018-05-14T18:44:22.120","AB","AXBT",null,null,"AXBT 21"]
["2018-05-14T22:47:56.420","2018-05-14T18:47:56.420","AB","Sonar","Multibeam",null,"AXBT21 added to line 0119"]
["2018-05-14T23:25:04.230","2018-05-14T19:25:04.230","AB","Sonar",null,null,"All new lines started on all sonars"]
["2018-05-14T23:47:25.510","2018-05-14T19:47:25.510","NB","Sonar","Knudsen","Gain Value","34dB"]
["2018-05-14T23:50:28.250","2018-05-14T19:50:28.250","AB","Other",null,null,"POS Pri. DGPS for Nav Status"]
["2018-05-15T00:38:46.260","2018-05-14T20:38:46.260","NB","Other",null,null,"POS Marinestar GNSS Nav back online"]
["2018-05-15T01:23:29.480","2018-05-14T21:23:29.480","NB","AXBT",null,null,"AXBT022 applied to SIS line 0122"]
["2018-05-15T02:24:04.630","2018-05-14T22:24:04.630","NB","Sonar","Knudsen","Gain Value","36 dB"]
["2018-05-15T03:09:21.890","2018-05-14T23:09:21.890","AB","Sonar","Knudsen","Phase Mode","2500-3000, steep slope upward. Gain 39"]
["2018-05-15T03:17:47.930","2018-05-14T23:17:47.930","AB","Sonar","Knudsen","Phase Mode","2250-2750, Gain 32, Pulse 2"]
["2018-05-15T03:19:26.790","2018-05-14T23:19:26.790","AB","Sonar","Knudsen","Phase Mode","2000-2500"]
["2018-05-15T03:21:14.250","2018-05-14T23:21:14.250","AB","Sonar","Knudsen","Phase Mode","1500-2000, Gain 34"]
["2018-05-15T03:34:31.690","2018-05-14T23:34:31.690","AB","Sonar","Knudsen","Phase Mode","1250-1750"]
["2018-05-15T04:00:59.140","2018-05-15T00:00:59.140","AB","Sonar","Knudsen","Phase Mode","1000-1500"]
["2018-05-15T04:01:25.090","2018-05-15T00:01:25.090","AB","Sonar","EK","Change Range",2500]
["2018-05-15T04:29:50.590","2018-05-15T00:29:50.590","AB","Sonar","Knudsen","Phase Mode","750-1250"]
["2018-05-15T04:48:56.540","2018-05-15T00:48:56.540","AB","Sonar","Knudsen","Phase Mode","1000-1500"]
["2018-05-15T04:52:08.570","2018-05-15T00:52:08.570","AB","Sonar","Knudsen",null,"Power 1 "]
["2018-05-15T05:00:47.740","2018-05-15T01:00:47.740","AB","Sonar","Knudsen","Phase Mode","750-1250"]
["2018-05-15T05:14:43.220","2018-05-15T01:14:43.220","AB","Sonar","Knudsen","tx pulse","1, new line"]
["2018-05-15T05:21:23.660","2018-05-15T01:21:23.660","AB","Sonar","Knudsen","Phase Mode","500-1000"]
["2018-05-15T05:23:07.390","2018-05-15T01:23:07.390","Ab","AXBT",null,null,23]
["2018-05-15T05:28:51.810","2018-05-15T01:28:51.810","AB","Sonar","Multibeam",null,"AXBT23 added to new line 127"]
["2018-05-15T05:30:40.910","2018-05-15T01:30:40.910","AB","Sonar","EK",null,"Range 1500m."]
["2018-05-15T05:48:18.870","2018-05-15T01:48:18.870","AB","Sonar","Knudsen","Phase Mode","250-750"]
["2018-05-15T05:49:55.670","2018-05-15T01:49:55.670","AB","Sonar","EK","Change Range","1000m"]
["2018-05-15T05:58:47.680","2018-05-15T01:58:47.680","AB","Sonar","Knudsen",null,"Pulse 0.5 m/s, Gain 25. New line."]
["2018-05-15T06:00:58.650","2018-05-15T02:00:58.650","AB","Sonar","Multibeam",null,"Penetration filter ON, Slope OFF. New line"]
["2018-05-15T06:35:03.430","2018-05-15T02:35:03.430","AB","Sonar","EK",null,"Range 500m"]
["2018-05-15T07:03:24.400","2018-05-15T03:03:24.400","AB","Sonar","Knudsen",null,"Range 100m, 0.25m pulse, Gain 20"]
["2018-05-15T07:13:05.690","2018-05-15T03:13:05.690","AB","Sonar","Multibeam",null,"Manual shallow ping mode, slope filter on, penetration filter off. Max angles 60/60. Lost grid in SIS at 250m of water."]
["2018-05-15T07:14:01.950","2018-05-15T03:14:01.950","AB","Sonar","EK",null,"Changed ranges on all sonars to 400m"]
["2018-05-15T07:15:54.660","2018-05-15T03:15:54.660","AB","Sonar","Multibeam",null,"Max angle 75/60. Power -10"]
["2018-05-15T07:20:16.250","2018-05-15T03:20:16.250","AB","Sonar","Multibeam","Max Angle","75/75"]
["2018-05-15T07:21:21.780","2018-05-15T03:21:21.780","AB","Sonar","Knudsen","Phase Mode","150-250m Gain 16"]
["2018-05-15T08:00:44.960","2018-05-15T04:00:44.960","AB","Sonar","Knudsen","Phase Mode","100-200"]
["2018-05-15T08:43:34.120","2018-05-15T04:43:34.120","AB","AXBT",null,null,"AXBT24 added to new SIS line 0132"]
["2018-05-15T09:32:35.830","2018-05-15T05:32:35.830","AB","sonar","Knudsen","Secure","Secured."]
["2018-05-15T09:38:40.380","2018-05-15T05:38:40.380","NB","Other",null,null,"SVP feed from World Ocean Atlas. 127m water depth"]
["2018-05-15T13:54:17.340","2018-05-15T09:54:17.340","CW","Sonar","All",null,"Secured for VIIRS Station 17, Pinging but not logging."]
["2018-05-15T16:10:27.100","2018-05-15T12:10:27.100","CW","Sonar","All",null,"Transit to Station 18. Logging all Sonars. MB line 0138"]
["2018-05-15T16:12:34.580","2018-05-15T12:12:34.580","CW","Sonar","Multibeam",null,"Still running SSM SPS from WOA. "]
["2018-05-15T17:33:32.940","2018-05-15T13:33:32.940","MW","AXBT","Multibeam",null,"AXBT 025 applied to line 0139"]
["2018-05-15T17:53:06.400","2018-05-15T13:53:06.400","CW","Sonar","Multibeam",null,"Secured for Station 18"]
["2018-05-15T19:20:19.730","2018-05-15T15:20:19.730","MW","Sonar","All",null,"Logging"]
["2018-05-15T19:41:20.470","2018-05-15T15:41:20.470","MW","Sonar","Multibeam","Ping Mode","DEEP"]
["2018-05-15T19:44:30.310","2018-05-15T15:44:30.310","MW","Sonar","Multibeam","Ping Mode","Medium"]
["2018-05-15T19:51:35.900","2018-05-15T15:51:35.900","MW","Sonar","All",null,"New Line 0141"]
["2018-05-15T19:55:08.710","2018-05-15T15:55:08.710","MW","Sonar","All",null,"Survey Line 141"]
["2018-05-15T19:59:42.640","2018-05-15T15:59:42.640","MW","Sonar","Multibeam","Ping Mode","DEEP Line 142"]
["2018-05-15T20:29:31.230","2018-05-15T16:29:31.230","MW","AXBT","Multibeam",null,"Cast 026 Applied to Line 0142"]
["2018-05-15T21:32:15.850","2018-05-15T17:32:15.850","AB","Sonar","Multibeam",null,"TSP Sequence Tim eout - Lost pings"]
["2018-05-15T21:37:47.510","2018-05-15T17:37:47.510","AB","Sonar","EK",null,"Range 1500m."]
["2018-05-15T21:38:02.830","2018-05-15T17:38:02.830","AB","Sonar","Knudsen","Phase Mode","750-1250"]
["2018-05-15T21:56:40.380","2018-05-15T17:56:40.380","AB","Sonar","Knudsen","Phase Mode","500-1000. Gain 25."]
["2018-05-15T22:44:24.400",{"$f":"IF(ISBLANK(A265),\" \",((A265)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-15T18:44:24.400"},"AB","Sonar","Multibeam",null,"AXBT27 added to new line 0145"]
["2018-05-15T23:18:30.620","2018-05-15T19:18:30.620","AB","Ship",null,null,"Adjusting course and speed for helicopter evacuation operation."]
["2018-05-15T23:37:24.860","2018-05-15T19:37:24.860","AB","Ship",null,null,"Returning to course. Helicopter evacuation complete."]
["2018-05-16T02:00:44.450","2018-05-15T22:00:44.450","NB","Sonar","Knudsen","Phase Range","750-1250"]
["2018-05-16T02:03:42.710","2018-05-15T22:03:42.710","NB","Sonar","Multibeam",null,"Telnet error \"TSP Sequence timeout on board 1\" aprox. every 30 seconds"]
["2018-05-16T02:08:36.380","2018-05-15T22:08:36.380","NB","Sonar","Multibeam",null,"Telnet TSP sequence error 4 times in a row and adta drop out. Very deep and back to deep to try to reset. "]
["2018-05-16T02:09:40.500","2018-05-15T22:09:40.500","NB","Sonar","Multibeam","Ping Mode","Very Deep"]
["2018-05-16T02:10:28.190","2018-05-15T22:10:28.190","NB","Sonar","Multibeam","Ping Mode","Deep"]
["2018-05-16T02:15:15.180","2018-05-15T22:15:15.180","NB","Sonar","Multibeam",null,"Still seeing Telnet timeout every 30 seconds. Doesn't seem to be effecting data."]
["2018-05-16T02:35:27.260","2018-05-15T22:35:27.260","NB","Sonar","Multibeam","New Line","Start line 0149 after slight turn."]
["2018-05-16T04:20:27.500","2018-05-16T00:20:27.500","NB","AXBT",null,null,"028 applied to SIS line 0151"]
["2018-05-16T04:20:56.950","2018-05-16T00:20:56.950","NB","Sonar","Multibeam","New Line","SIS line 0151"]
["2018-05-16T04:28:56.870","2018-05-16T00:28:56.870","NB","Sonar","Multibeam","New Line","SOL 0152 into turn. "]
["2018-05-16T04:40:20.350","2018-05-16T00:40:20.350","NB","Sonar","Multibeam",null,"Telnet sequence timeout increased in frequency. Sparse data dropouts"]
["2018-05-16T04:51:58.090","2018-05-16T00:51:58.090","NB","Sonar","Knudsen","Phase Range","500-1000"]
["2018-05-16T05:30:01.070","2018-05-16T01:30:01.070","NB","Sonar","Multibeam","Ping Mode","Medium"]
["2018-05-16T05:30:03.500","2018-05-16T01:30:03.500","NB","Sonar","Multibeam","Ping Mode","Deep (attempt to ebb Telnet timeout error)"]
["2018-05-16T05:42:47.870","2018-05-16T01:42:47.870","NB","Sonar","Multibeam","Ping Mode","Auto -> Deep"]
["2018-05-16T05:55:56.390","2018-05-16T01:55:56.390","NB","Sonar","Knudsen","Gain Value","29dB"]
["2018-05-16T06:11:32.030","2018-05-16T02:11:32.030","NB","Sonar","Multibeam","Ping Mode","Deep"]
["2018-05-16T06:25:56.350","2018-05-16T02:25:56.350","NB","Sonar","Knudsen","Phase Range","750-1250"]
["2018-05-16T06:53:34.850","2018-05-16T02:53:34.850","AB","Sonar","Knudsen","Phase Range","500-1000"]
["2018-05-16T07:19:10.830","2018-05-16T03:19:10.830","AB","Sonar","Knudsen","Phase Range","250-750. Pulse 0.5 m/s"]
["2018-05-16T08:28:23.760","2018-05-16T04:28:23.760","NB","Sonar","Multibeam","Ping Mode","Medium"]
["2018-05-16T08:39:18.660","2018-05-16T04:39:18.660","NB","Sonar","Knudsen",null,"Range 100m, Phase 300-400, Pulse 0.25"]
["2018-05-16T08:47:36.150","2018-05-16T04:47:36.150","AB","Sonar","Knudsen","Phase Range","300-400. Gain 18"]
["2018-05-16T09:31:41.780","2018-05-16T05:31:41.780","NB","Sonar","Knudsen","Phase Range","350-450. Pulse 1. Gain 20"]
["2018-05-16T09:53:26.600","2018-05-16T05:53:26.600","NB","Sonar","Knudsen","Phase Range","400-500"]
["2018-05-16T10:05:46","2018-05-16T06:05:46","NB","Sonar","Knudsen","Tx Pulse","2 ms, Gain 26"]
["2018-05-16T10:14:58.830","2018-05-16T06:14:58.830","NB","AXBT",null,null,"29 applied ot line 0158"]
["2018-05-16T10:22:17.370","2018-05-16T06:22:17.370","NB","Sonar","Multibeam","New Line","SOL 0158 for new AXBT cast"]
["2018-05-16T10:25:44.600","2018-05-16T06:25:44.600","NB","Sonar","Knudsen","Range","200, range 500-700"]
["2018-05-16T10:32:41.450","2018-05-16T06:32:41.450","NB","Sonar","Knudsen","Phase Range","600-800"]
["2018-05-16T10:33:12.560","2018-05-16T06:33:12.560","NB","Sonar","EK","Change Range","ES 18: 1000, ES70: 1000"]
["2018-05-16T10:34:33.880","2018-05-16T06:34:33.880","NB","Sonar","Knudsen","Tx Power","TX power 2, Pulse 2, Gain 24 dB"]
["2018-05-16T10:40:05.620","2018-05-16T06:40:05.620","NB","Sonar","Multibeam","Ping Mode","Deep"]
["2018-05-16T10:53:52.470","2018-05-16T06:53:52.470","NB","Sonar","Knudsen","Gain Value","28 dB"]
["2018-05-16T14:40:01.990","2018-05-16T10:40:01.990","MW","Sonar","All",null,"Logging"]
["2018-05-16T15:24:59.200","2018-05-16T11:24:59.200","CW","Sonar","All",null,"Secure for VIIRS Station whatever"]
["2018-05-16T17:45:04.730","2018-05-16T13:45:04.730","MW","Sonar","Multibeam",null,"Secured for BIST and Troubleshooting with Kongsberg"]
["2018-05-16T21:44:01.850","2018-05-16T17:44:01.850","MW","Sonar","All",null,"Logging"]
["2018-05-16T22:02:53.740","2018-05-16T18:02:53.740","AB","Sonar",null,null,"AXBT30 added to new line 0166"]
["2018-05-16T23:57:37.070","2018-05-16T19:57:37.070","AB","Sonar","Knudsen",null,"Power 1, Pulse 2, Gain 30"]
["2018-05-17T00:03:22.600","2018-05-16T20:03:22.600","AB","Sonar","Multibeam","New Line","0167"]
["2018-05-17T00:04:21.220","2018-05-16T20:04:21.220","AB","Sonar","Knudsen","Phase Range","600-800"]
["2018-05-17T00:52:10.860","2018-05-16T20:52:10.860","AB","Sonar","Knudsen","Phase Range","700-900"]
["2018-05-17T01:05:04.040","2018-05-16T21:05:04.040","AB","Sonar","Multibeam","New Line","0169"]
["2018-05-17T01:32:42.380","2018-05-16T21:32:42.380","NB","Sonar","Knudsen","Phase Range","600-800"]
["2018-05-17T02:07:58.730","2018-05-16T22:07:58.730","NB","Sonar","Knudsen","Phase Range","700-900"]
["2018-05-17T02:52:56.880","2018-05-16T22:52:56.880","AB","Issue/Problem",null,null,"Primary DGPS on POS, altitude accuracy 0.754m"]
["2018-05-17T03:38:57.190","2018-05-16T23:38:57.190","AB","Ship",null,null,"Reduced speed to 8 knts for traffic"]
["2018-05-17T03:40:38.040","2018-05-16T23:40:38.040","NB","Sonar","Knudsen","Phase Range","600-800"]
["2018-05-17T04:22:02.160","2018-05-17T00:22:02.160","AB","AXBT",null,null,"AXBT31 added to new line 0174"]
["2018-05-17T04:43:17.690","2018-05-17T00:43:17.690","AB","Ship",null,null,"Increasing speed. Traffic situtation passed."]
["2018-05-17T04:49:18.710","2018-05-17T00:49:18.710","AB","Sonar","Knudsen","Phase Range","500-700"]
["2018-05-17T05:32:55.190","2018-05-17T01:32:55.190","NB","Sonar","EK","Change Range","18: 750, 70: 750"]
["2018-05-17T05:40:25.810","2018-05-17T01:40:25.810","NB","Sonar","Knudsen","Phase Range","400-600"]
["2018-05-17T05:41:05.310","2018-05-17T01:41:05.310","NB","Sonar","Multibeam","Ping Mode","Medium"]
["2018-05-17T06:34:06.350","2018-05-17T02:34:06.350","NB","Ship",null,null,"Moving 5-10 degrees to Port off of line to avoid traffic"]
["2018-05-17T06:34:35.080","2018-05-17T02:34:35.080","NB","Sonar","Multibeam","New Line","SOL 0177 into turn"]
["2018-05-17T06:40:58.840","2018-05-17T02:40:58.840","NB","Sonar","Knudsen","Phase Range","300-500"]
["2018-05-17T06:50:17.670","2018-05-17T02:50:17.670","NB","Sonar","Multibeam","New Line","SOL 0178, easing back onto planned line"]
["2018-05-17T07:03:33.470","2018-05-17T03:03:33.470","NB","Sonar","EK","Change Range","18: 500, 70:500"]
["2018-05-17T07:04:31.480",{"$f":"IF(ISBLANK(A328),\" \",((A328)-DATE(1970,1,1))+25569+($C$4/24))","v":"2018-05-17T03:04:31.480"},"NB","Sonar","Knudsen","Gain Value","32 dB"]
["2018-05-17T07:22:26.030","2018-05-17T03:22:26.030","NB","Sonar","Multibeam","New Line","SOL 0179 back on line"]
["2018-05-17T07:46:22.900","2018-05-17T03:46:22.900","NB","Sonar","Knudsen","Phase Range","200-400"]
["2018-05-17T07:55:10.660","2018-05-17T03:55:10.660","NB","AXBT",null,null,"cast 032 applied to new SIS line 0180. Huge change in SIS grid. Briefly applied WOA for comparison concluded Cast was better fit."]
["2018-05-17T08:18:09.950","2018-05-17T04:18:09.950","NB","Sonar","Multibeam","New Line","SOL 0181 for cast re-application"]
["2018-05-17T08:26:01.570","2018-05-17T04:26:01.570","NB","Sonar","Knudsen","Tx Pulse","TX Pulse 0.5, TX Power 1, Gain 32, Range 200-400"]
["2018-05-17T08:33:25.430","2018-05-17T04:33:25.430","NB","Sonar","Knudsen","Phase Range","100-300"]
["2018-05-17T08:34:00.110","2018-05-17T04:34:00.110","NB","Sonar","Multibeam","Ping Mode","Shallow"]
["2018-05-17T08:34:55.200","2018-05-17T04:34:55.200","NB","Sonar","EK","Change Range","18: 300, 70:300, 120:250"]
["2018-05-17T08:44:05.900","2018-05-17T04:44:05.900","NB","Sonar","Multibeam",null,"WOA Server for SV. Better agreement than cast for now. "]
["2018-05-17T08:54:33.500","2018-05-17T04:54:33.500","NB","Sonar","Multibeam","Along Direction Pitch","-1 to try and negate Eric's Horns"]
["2018-05-17T08:59:19.940","2018-05-17T04:59:19.940","NB","Sonar","Knudsen","Gain Value","27 dB"]
["2018-05-17T09:51:32.890","2018-05-17T05:51:32.890","NB","Sonar","Knudsen","Secure","Uner 150m "]
["2018-05-17T09:52:22.930","2018-05-17T05:52:22.930","NB","Sonar","EK","Change Range","18: 200, 70:175, 120:200, 200:150"]
["2018-05-17T10:21:04.520","2018-05-17T06:21:04.520","NB","Sonar","EK","Change Range","1q8:175, 70:150, 120:175, 200:150"]
["2018-05-17T10:39:23.970","2018-05-17T06:39:23.970","NB","Ship",null,null,"1-2 degree course change for traffic"]
["2018-05-17T11:09:29.500","2018-05-17T07:09:29.500","NB","Sonar","Multibeam","Ping Mode","Very Shallow"]
["2018-05-17T11:12:38.680","2018-05-17T07:12:38.680","NB","Sonar","Multibeam","New Line","SOL 0184, gradually working back to planned line"]
["2018-05-17T15:23:58.060","2018-05-17T11:23:58.060","MW","Sonar","All",null,"Logging"]
["2018-05-17T15:59:43.320","2018-05-17T11:59:43.320","CW","Sonar","Multibeam",null,"New line for course change. MB line 0188"]
["2018-05-17T15:59:45.870","2018-05-17T11:59:45.870","CW","Sonar","ek",null,"New line for course change. MB line 0188"]
["2018-05-17T17:54:12.850","2018-05-17T13:54:12.850","CW","Sonar","All",null,"Secure for last VIIRS Station"]
["2018-05-17T19:09:12.970","2018-05-17T15:09:12.970","CW","Sonar","All",null,"Logging"]
["2018-05-17T21:43:37.260","2018-05-17T17:43:37.260","AB","Sonar","Multibeam","New Line","193. Turning onto trackline"]
["2018-05-18T00:20:24.580","2018-05-17T20:20:24.580","NB","Ship",null,null,"All stop for Dolphins. Still pinging to avoid startle on restart"]
["2018-05-18T00:23:27","2018-05-17T20:23:27","NB","Ship",null,null,"Returning to transit speed"]
["2018-05-18T00:46:03.920","2018-05-17T20:46:03.920","CW","Ship",null,null,"Securing TSG."]
["2018-05-18T00:47:07.580","2018-05-17T20:47:07.580","AB","Ship",null,null,"POS in Primary DGPS"]
["2018-05-18T00:50:30.460","2018-05-17T20:50:30.460","NB","Ship",null,null,"POS in Marinestar GNSS"]
["2018-05-18T01:04:19.670","2018-05-17T21:04:19.670","NB","Ship",null,null,"POS in Primary DGPS, GAMS not ready"]
["2018-05-18T01:14:30.760","2018-05-17T21:14:30.760","NB","Sonar","Multibeam",null,"TSP Sequence Timeout error board 5. No effect on data"]
["2018-05-18T01:20:44.100","2018-05-17T21:20:44.100","NB","Ship",null,null,"POS in Marinestar GNSS, GAMS online"]
["2018-05-18T02:15:08.550","2018-05-17T22:15:08.550","NB","Ship",null,null,"POS in primary DGPS"]
["2018-05-18T04:44:15.870","2018-05-18T00:44:15.870","AB","Sonar","Multibeam","New Line","0200"]
["2018-05-18T05:20:49.970","2018-05-18T01:20:49.970","Ab","Ship",null,null,"At traffic scheme"]
["2018-05-18T05:21:11.210","2018-05-18T01:21:11.210","AB","Sonar",null,null,"EM302 and EK60 secured. "]
["2018-05-18T05:21:32.780","2018-05-18T01:21:32.780","AB","Sonar","Multibeam",null,"Closing BIST All past. PU system report exported. PU parameters exported. "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A390),\" \",((A390)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A454),\" \",((A454)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A518),\" \",((A518)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A552),\" \",((A552)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A579),\" \",((A579)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A643),\" \",((A643)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A707),\" \",((A707)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A771),\" \",((A771)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A835),\" \",((A835)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A899),\" \",((A899)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A963),\" \",((A963)-DATE(1970,1,1))+25569-($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A998),\" \",((A998)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1023),\" \",((A1023)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1087),\" \",((A1087)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1151),\" \",((A1151)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1215),\" \",((A1215)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1279),\" \",((A1279)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1343),\" \",((A1343)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1407),\" \",((A1407)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1471),\" \",((A1471)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1535),\" \",((A1535)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1599),\" \",((A1599)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1663),\" \",((A1663)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1727),\" \",((A1727)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1791),\" \",((A1791)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1855),\" \",((A1855)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1919),\" \",((A1919)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1983),\" \",((A1983)-DATE(1970,1,1))+25569+($C$4/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["AB","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DF","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["CW","Weather","Knudsen","New Line","Secure","Gain Mode"]
["DS","Watch Change","All","Max Angle",null,"Gain Value"]
["MW","XBT",null,"Spike Filter Strength",null,"Process Shift"]
["NB","AXBT",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
[null,"Issue/Problem",null,"Aeration Filter (On/Off)",null,"Range"]
[null,"Other",null,"Interference Filter (On/Off)",null,"Phase Mode"]
[null,null,null,"Start Pinging",null,"Start Pinging"]
[null,null,null,"Secure",null,"Secure"]
[null,null,null,"Start Logging",null,"Phase Range"]