{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","DropDowns"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2009,"n_cols":7,"rows_kept":2009,"cut":false,"hidden":false,"merged":[]}
["Cruise ID: EX1810","UTC to Local: ",4,"UTC 2","UTC 3","UTC 4","Cruise Details: Oct 2 - Oct 24 2018"]
[]
[null,"Ship Time","WatchStander","Item","Sonar","Variable","Note"]
[null,"Pull formula down to calc Ship Time","select from drop down","select from drop down","select from drop down","select from drop down","type in observation"]
["2018-10-02T13:39:11.550",{"$f":"IF(ISBLANK(A5),\" \",((A5)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-02T09:39:11.550"},"CW","Ship","All","Start up","BEGIN EX1810!!!"]
["2018-10-02T17:21:30.410",{"$f":"IF(ISBLANK(A6),\" \",((A6)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-02T13:21:30.410"},"MW","Sonar",null,null,"ADCP 300 logging"]
["2018-10-02T20:49:43.410","2018-10-02T16:49:43.410","SA","Sonar","Multibeam","Start Logging"]
["2018-10-02T20:58:04.310","2018-10-02T16:58:04.310","SG","Sonar","EK","Start Pinging"]
["2018-10-03T03:47:39.840","2018-10-02T23:47:39.840","KJ","Sonar","Multibeam","Max Angle","Changed from 65/65 to 75/75 for swath extinction coverage testing"]
["2018-10-03T03:57:06.750","2018-10-02T23:57:06.750","SG","XBT",null,null,"XBT001 launched"]
["2018-10-03T04:22:54.360","2018-10-03T00:22:54.360","KJ","Sonar","Multibeam",null,"XBT001 applied in line 0006"]
["2018-10-03T04:57:31.470","2018-10-03T00:57:31.470","KJ","Sonar","Multibeam","Pen. Filter Strength","Changed penetration filter from Off to Weak over soft sediments"]
["2018-10-03T05:16:58.180","2018-10-03T01:16:58.180","KJ","Sonar","Multibeam","Pen. Filter Strength","Changed back to Off"]
["2018-10-03T06:08:18.850","2018-10-03T02:08:18.850","KJ","XBT",null,null,"XBT002 launched"]
["2018-10-03T06:17:47.480","2018-10-03T02:17:47.480","KJ","Sonar","Multibeam",null,"XBT002 applied in line 0008"]
["2018-10-03T06:27:20.850","2018-10-03T02:27:20.850","JM","Sonar","Multibeam","New Line","New line for turn. Also EK60"]
["2018-10-03T06:28:54.380","2018-10-03T02:28:54.380","JM","Sonar","EK","Secure","Approachiong Pitch line"]
["2018-10-03T06:29:40.110","2018-10-03T02:29:40.110","JM","Sonar","Multibeam","Max Angle","Narrowed beam angle to 30/30"]
["2018-10-03T06:37:42.920","2018-10-03T02:37:42.920","JM","Sonar","Multibeam","New Line","Begin Pitch line #1; MB line 0010"]
["2018-10-03T07:19:56.860","2018-10-03T03:19:56.860","KJ","Sonar","Multibeam","New Line","End Pitch line #1, turn MB line 0011"]
["2018-10-03T07:35:02.820","2018-10-03T03:35:02.820","JM","Sonar","Multibeam","New Line","Begin Pitch line #2; MB line 0012"]
["2018-10-03T08:30:50.670","2018-10-03T04:30:50.670","JM","Sonar","Multibeam","New Line","End Pitch line #2; MB line 0013"]
["2018-10-03T08:34:53.080","2018-10-03T04:34:53.080","JM","Sonar","Multibeam",null,"End line. Apply pitch offset of -0.35 to SIS"]
["2018-10-03T08:38:49.360","2018-10-03T04:38:49.360","KJ","Sonar","Multibeam",null,"RX Noise testing at 3-10 kts"]
["2018-10-03T09:48:53.750","2018-10-03T05:48:53.750","KJ","Sonar","Multibeam","Max Angle","Changed from 30/30 at pitch site to 70/70 for roll calibration; approaching CTD station"]
["2018-10-03T09:55:10.320","2018-10-03T05:55:10.320","KJ","Sonar","Multibeam",null,"Some mild interference rings apparent in the water column, occasionally impacting bottom detection in the outer swath"]
["2018-10-03T10:18:21.240","2018-10-03T06:18:21.240","JM",null,null,null,"Arrive at CTD site"]
["2018-10-03T11:38:10.450","2018-10-03T07:38:10.450","JM",null,null,null,"CTD complete"]
["2018-10-03T11:39:25.370","2018-10-03T07:39:25.370","MW","XBT",null,null,"Cast 003"]
["2018-10-03T11:57:07.240","2018-10-03T07:57:07.240","JM","XBT",null,null,"CDT0001 applied to MB line 0015"]
["2018-10-03T12:03:29.790","2018-10-03T08:03:29.790","JM","Sonar","Multibeam","New Line","En route to roll cal site"]
["2018-10-03T12:12:44.720","2018-10-03T08:12:44.720","KJ","Sonar","Multibeam","New Line","Begin Roll line #1; MB line 0016"]
["2018-10-03T12:56:36.940","2018-10-03T08:56:36.940","KJ","Sonar","Multibeam","New Line","turn MB line 0019"]
["2018-10-03T13:12:35.620","2018-10-03T09:12:35.620","JM","Sonar","Multibeam","New Line","Begin Roll line #2; MB line 20"]
["2018-10-03T13:55:58.530","2018-10-03T09:55:58.530","JM","Sonar","Multibeam","New Line","End roll line #2. Begin MB line 0021"]
["2018-10-03T14:21:10.630","2018-10-03T10:21:10.630","JM","Sonar","Multibeam",null,"New roll value -0.088 entered in SIS"]
["2018-10-03T14:24:57.540","2018-10-03T10:24:57.540","JM","Sonar","Multibeam","New Line","Heading line #1; MB line 0022. Beam angle 60/10"]
["2018-10-03T14:52:01.200","2018-10-03T10:52:01.200","JM","XBT",null,null,"XBT cast # 004"]
["2018-10-03T14:58:10.420","2018-10-03T10:58:10.420","JM","XBT",null,null,"XBT cast # 004 applied to MB line 0022"]
["2018-10-03T15:09:21.680","2018-10-03T11:09:21.680","JM","Sonar","Multibeam","New Line","End Heading Line #1; turn, MB line 0023. Beam angle 70/70"]
["2018-10-03T15:42:35.200","2018-10-03T11:42:35.200","CW","Sonar","Multibeam","Max Angle","10/60, as per Kevin. Blame him."]
["2018-10-03T15:55:05.590","2018-10-03T11:55:05.590","CW","Sonar","Multibeam","New Line","Heading line #2; MB line 0024. Beam angle 60/10"]
["2018-10-03T17:02:56.090","2018-10-03T13:02:56.090","CW","Sonar","Multibeam",null,"Stop Logging and Pinging to update Patch Test results in Installation Parameters"]
["2018-10-03T17:03:38.110","2018-10-03T13:03:38.110","CW","Sonar","Multibeam",null,"Update SIS Intallation Parameter for Heading. From 0 to -0.04. Effective after MB line 0027"]
["2018-10-03T17:21:11.980","2018-10-03T13:21:11.980","KJ","Sonar","Multibeam","Max Angle","30/30 en route to pitch verification line 1"]
["2018-10-03T17:26:40.640","2018-10-03T13:26:40.640","CW","XBT",null,null,"AXBT 005"]
["2018-10-03T17:33:29.580","2018-10-03T13:33:29.580","KJ","Sonar","Multibeam","New Line","Pitch verification line 1, MB 0029"]
["2018-10-03T17:35:37.700","2018-10-03T13:35:37.700","KJ","Sonar","Multibeam",null,"XBT005 applied in line 0029"]
["2018-10-03T17:39:05.700","2018-10-03T13:39:05.700","KJ","Sonar","Multibeam",null,"PU-ZDA time difference reduced from 200-300 ms to 1 ms, remains to be seen if this improves outer swath bathy"]
["2018-10-03T18:18:35.050","2018-10-03T14:18:35.050","CW","Sonar","Multibeam",null,"End Pitch verification line 1, MB 0029"]
["2018-10-03T18:24:50.510","2018-10-03T14:24:50.510","CW","Sonar","Multibeam",null,"Turn MB line 0030"]
["2018-10-03T18:34:06.500","2018-10-03T14:34:06.500","CW","Sonar","Multibeam",null,"Begin Pitch verification line 2, MB 0031"]
["2018-10-03T19:17:57.990","2018-10-03T15:17:57.990","MW","Sonar","Multibeam",null,"End Pitch verification line , MB 0031"]
["2018-10-03T19:35:47.490","2018-10-03T15:35:47.490","MW","Sonar","Multibeam","Max Angle","Angle to 70"]
["2018-10-03T19:36:12.700","2018-10-03T15:36:12.700","MW","Sonar","Multibeam","Start Logging","Tranist Line 0032"]
["2018-10-03T19:43:01.590","2018-10-03T15:43:01.590","MW","XBT",null,null,"Cast 006"]
["2018-10-03T19:43:49.970","2018-10-03T15:43:49.970","MW","Sonar","Multibeam",null,"XBT 006 Applied to Line 0032"]
["2018-10-03T19:49:47.880","2018-10-03T15:49:47.880","MW","Sonar","Multibeam",null,"Roll Verification Line 1, MB Line 0033"]
["2018-10-03T20:32:17.810","2018-10-03T16:32:17.810","MW","Sonar","Multibeam",null,"End Roll Verification Line 1, MB Line 0033, Begin Turn Line 0034"]
["2018-10-03T20:42:17.480","2018-10-03T16:42:17.480","MW","Sonar","Multibeam",null,"Begin Roll Verification Line 2, Line 0035"]
["2018-10-03T21:25:16.090","2018-10-03T17:25:16.090","MW","Sonar","Multibeam",null,"End Roll Verification Line 2, Line 0035"]
["2018-10-03T21:27:57.780","2018-10-03T17:27:57.780","MW","Sonar","Multibeam","Max Angle","60 Port, 10 STBD"]
["2018-10-03T22:08:34.200",{"$f":"IF(ISBLANK(A63),\" \",((A63)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-03T18:08:34.200"},"CW","Sonar","Multibeam",null,"Heading Verification Line #1 (E to F); MB line 0037. Beam angle 60/10 "]
["2018-10-03T22:12:20.230","2018-10-03T18:12:20.230","SG","XBT",null,null,"Cast 007 applied to MB line 0038"]
["2018-10-03T22:56:12.980","2018-10-03T18:56:12.980","CW","Sonar","Multibeam",null,"End Heading Verification Line #1 (E to F)"]
["2018-10-03T22:56:21.830","2018-10-03T18:56:21.830","CW","Sonar","Multibeam","New Line","Begin Turn / Transit to next verification line. MB line 0039. Full speed, Open Angles, Yaw Stab off for turn, on for transit"]
["2018-10-03T23:40:48.850",{"$f":"IF(ISBLANK(A67),\" \",((A67)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-03T19:40:48.850"},"CW","Sonar","Multibeam","New Line","Heading Verification Line #2 (G to H); MB line 0040. Beam angle 10/60"]
["2018-10-04T00:24:23.980","2018-10-03T20:24:23.980","MW","Sonar","Multibeam",null,"End Heading Verification Line #2, MB Line 040"]
["2018-10-04T01:12:45.200","2018-10-03T21:12:45.200","MW","Sonar","Multibeam",null,"TRU restarted"]
["2018-10-04T01:56:15","2018-10-03T21:56:15","SG","XBT",null,null,"XBT008 launched"]
["2018-10-04T02:19:47.710",{"$f":"IF(ISBLANK(A71),\" \",((A71)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-03T22:19:47.710"},"KJ","Sonar","Multibeam","Max Angle","Changed from 65/65 to 75/75 for swath extinction coverage testing"]
["2018-10-04T02:25:48.190","2018-10-03T22:25:48.190","KJ","Sonar","Multibeam","New Line","XBT008 applied in line 0046"]
["2018-10-04T02:59:03.910","2018-10-03T22:59:03.910","KJ","Sonar","EK",null,"Started recording on transit to deep accuracy site"]
["2018-10-04T03:39:13.720","2018-10-03T23:39:13.720","KJ","Sonar","Multibeam",null,"Occasional interfernce from unknown source; bridge confirms all bridge echosounders secure"]
["2018-10-04T03:30:56","2018-10-03T23:30:56","SG","XBT",null,null,"XBT009 launched"]
["2018-10-04T03:42:53.140","2018-10-03T23:42:53.140","KJ","Sonar","Multibeam",null,"XBT009 applied in line 0047"]
["2018-10-04T05:16:32.700","2018-10-04T01:16:32.700","KJ","Sonar","Multibeam",null,"Still frequent interference in water column, occasionally impacting bottom detection - may impact upcoming RX noise vs. heading test"]
["2018-10-04T05:17:27.920","2018-10-04T01:17:27.920","KJ","Sonar","EK",null,"Secure to test interference in EM"]
["2018-10-04T05:21:20.290","2018-10-04T01:21:20.290","KJ","Sonar","EK",null,"start pinging, sychronized with EM, no obvious impact on EM water column; was also synchronized previously, but maybe needed to stop/start pinging again to re-sync?"]
["2018-10-04T06:07:27.490","2018-10-04T02:07:27.490","KJ","Sonar","Multibeam",null,"secure for octogon line pattern (RX noise vs heading test), starting on heading 100 at 8.5 kts (135 RPM), swell 3-5 ft with 1-3 wind waves, all arriving from 055"]
["2018-10-04T06:15:20.140","2018-10-04T02:15:20.140","JM","Sonar",null,null,"Changed POS MV COM 5 update rate from 2 Hz to 1 Hz, immediately improved PU-ZDA latency from several hundred ms to 1 ms"]
["2018-10-04T07:26:18.810","2018-10-04T03:26:18.810","JM",null,null,null,"Octogon test complete; EK60s still secure"]
["2018-10-04T07:30:57.760","2018-10-04T03:30:57.760","JM","XBT",null,null,"Cast #010"]
["2018-10-04T07:41:24.440","2018-10-04T03:41:24.440","JM","XBT",null,null,"Cast #010 applied to MB line 0050"]
["2018-10-04T07:46:48.420","2018-10-04T03:46:48.420","JM","Sonar","Multibeam",null,"Begin deep water roll line #1; MB line 0050"]
["2018-10-04T08:37:32.880","2018-10-04T04:37:32.880","JM","Sonar","Multibeam","Aeration Filter (On/Off)","Aeration filter On, large rolls causing dropouts"]
["2018-10-04T09:01:52.720","2018-10-04T05:01:52.720","JM","Sonar","Multibeam","Aeration Filter (On/Off)","Aeration filter off, Nearing end of line"]
["2018-10-04T09:16:43.250","2018-10-04T05:16:43.250","JM","Sonar","Multibeam","New Line","Begin deep water roll line #2; MB line 0052"]
["2018-10-04T09:26:46.230","2018-10-04T05:26:46.230","JM","Sonar",null,null,"ADCP 300 logging"]
["2018-10-04T10:02:47.560","2018-10-04T06:02:47.560","JM","Sonar","Multibeam","Secure","End logging for CTD cast and EK60 calibration"]
["2018-10-04T16:51:52","2018-10-04T12:51:52","MW","Sonar","Ek",null,"Calibrations Complete"]
["2018-10-04T18:48:48",{"$f":"IF(ISBLANK(A92),\" \",((A92)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-04T14:48:48"},"CW",null,null,null,"CTD 003; 2600m"]
["2018-10-04T20:33:48",{"$f":"IF(ISBLANK(A93),\" \",((A93)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-04T16:33:48"},"CW","Sonar","Multibeam","Start Logging","Line 0053"]
["2018-10-04T20:50:48",{"$f":"IF(ISBLANK(A94),\" \",((A94)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-04T16:50:48"},"CW",null,null,null,"CTD 003 converted to ASVP; applied to MB line 0053"]
["2018-10-04T22:47:58","2018-10-04T18:47:58","CW","Sonar","Multibeam","New Line","Start Tony's crossline. MB 0057"]
["2018-10-04T22:29:35.710","2018-10-04T18:29:35.710","CW","Sonar","Multibeam",null,"Start Tony's crossline. Still 0057"]
["2018-10-04T22:31:05.870","2018-10-04T18:31:05.870","CW","Sonar","Multibeam","New Line","Turn and transit to point I. MB line 0058"]
["2018-10-04T23:18:50.430",{"$f":"IF(ISBLANK(A98),\" \",((A98)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-04T19:18:50.430"},"CW","XBT",null,null,"AXBT 011; applied to MB line 0058"]
["2018-10-04T23:31:28.200","2018-10-04T19:31:28.200","CW","Sonar","Multibeam","New Line","At point I. Starting Deep Accuracy Crossline, Setting #1 (Southern Heading). MB line 0059. Deep Mode, FM enabled, Dual Swath Mode: Dynamic, Yaw Stabilization ON, 75/75 angles. "]
["2018-10-04T23:32:05.730","2018-10-04T19:32:05.730","KJ","Sonar","EK",null,"Secure for accuracy testing; "]
["2018-10-05T00:53:40.940","2018-10-04T20:53:40.940","KJ","Sonar","Multibeam","New Line","Deep accuracy crosslines for setting 1 are MB files 0059, 0060; new line 0061 for turn"]
["2018-10-05T01:10:40.910","2018-10-04T21:10:40.910","KJ","Sonar","Multibeam","New Line","Setting #2 (Northern heading). MB line 0062. Very Deep mode, FM enabled, Dual Swath Dynamic, Yaw stabilization ON, 75/75 swath limits"]
["2018-10-05T02:25:50.350","2018-10-04T22:25:50.350","KJ","Sonar","Multibeam","New Line","0064; end of accuracy crosslines, starting transit at 10.5 kts to personnel transfer in or around RI"]
["2018-10-05T02:52:29.940","2018-10-04T22:52:29.940","KJ","XBT",null,null,"AXBT012 launched"]
["2018-10-05T03:12:34.360","2018-10-04T23:12:34.360","KJ","Sonar","Multibeam",null,"XBT012 applied in line 0064"]
["2018-10-05T03:14:37.940","2018-10-04T23:14:37.940","KJ","Sonar","EK",null,"Start pinging for transit to RI"]
["2018-10-05T03:19:01.350","2018-10-04T23:19:01.350","KJ","Sonar","EK",null,"changed synchronization from Master to Slave with Synchronization port; interference in EM is gone"]
["2018-10-05T03:24:39.900","2018-10-04T23:24:39.900","KJ","Sonar","Multibeam","New Line","Changed mode from Very Deep to AUTO for extinction test, MB line 0065; system changed ping mode automatically to Deep, swath width went from 52/52 to 62/62"]
["2018-10-05T04:55:01.710","2018-10-05T00:55:01.710","KJ","XBT",null,null,"XBT launch failure for unknown reason; successful launch named XBT013"]
["2018-10-05T04:59:04.980","2018-10-05T00:59:04.980","KJ","Sonar","Multibeam",null,"XBT013 applied in line 0066"]
["2018-10-05T06:20:20.240","2018-10-05T02:20:20.240","JM","Sonar","Knudsen",null,"Fire it up! Test for functionality"]
["2018-10-05T06:23:13.250","2018-10-05T02:23:13.250","JM","Sonar","Knudsen",null,"Start recording, TxPower 2, TxPulse2, Gain 32"]
["2018-10-05T06:32:29.940","2018-10-05T02:32:29.940","JM","Sonar","Knudsen",null,"Auto phase not working great. No surprise there"]
["2018-10-05T07:33:04.530","2018-10-05T03:33:04.530","JM","Sonar","Knudsen",null,"Powering off. Working great. Transiting in shallow water"]
["2018-10-05T07:55:35.440","2018-10-05T03:55:35.440","JM","XBT",null,null,"XBT cast #14"]
["2018-10-05T08:04:26.380","2018-10-05T04:04:26.380","JM","XBT",null,null,"XBT cast #14 applied to MB line 0069"]
["2018-10-05T09:12:59.240","2018-10-05T05:12:59.240","KJ","Sonar","Multibeam","Secure","Secured in shallow water"]
["2018-10-05T14:55:29.260","2018-10-05T10:55:29.260","CW","Sonar","Multibeam","Secure","Stopped Pinging for Bridge Fathometer"]
["2018-10-05T16:00:00","2018-10-05T12:00:00","KJ","Sonar","Multibeam",null,"during personnel transfer in RI, the POS feed to TRU was reconfigured to run directly on dedicated serial line, replacing older arrangement which ran through buffers that induced latency in the position and attitude feeds; PU-POS latency value in SIS reduced from ~100 ms to 5 ms; previously, the ZDA feed on COM5 was changed from 2 Hz to 1 Hz, which reduced the PU-ZDA latency from ~200 ms to 0 ms in SIS, but this is now set back to 2 Hz with no issue"]
["2018-10-05T18:17:35.890","2018-10-05T14:17:35.890","MW","Sonar","Multibeam","Start Pinging","New Survey, EX1810_ECS_Transit"]
["2018-10-05T20:10:57.350","2018-10-05T16:10:57.350","CW","Sonar",null,null,"Starting SSSSM SSPSS for shallow water"]
["2018-10-06T02:56:25.790","2018-10-05T22:56:25.790","KJ","Ship",null,null,"Deviating from transit line for fishing vessels; EM still secure in shallow water, EK60s pinging/logging"]
["2018-10-06T05:28:25.570","2018-10-06T01:28:25.570","KJ","Sonar","Knudsen",null,"Start pinging and logging"]
["2018-10-06T05:31:39.070","2018-10-06T01:31:39.070","KJ","Sonar","Multibeam",null,"New line, MB 0000 start of Hudson Canyon seep survey"]
["2018-10-06T05:35:49.070",{"$f":"IF(ISBLANK(A125),\" \",((A125)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-06T01:35:49.070"},"KJ","XBT",null,null,"XBT0015 launched"]
["2018-10-06T05:39:48.280","2018-10-06T01:39:48.280","KJ","Sonar","Multibeam","New Line","XBT015 applied at end of line 0000; new line 0001 for first pass on Hudson Canyon"]
["2018-10-06T05:42:31.490","2018-10-06T01:42:31.490","Kj","Sonar","Multibeam",null,"TX power from -20 dB to Max"]
["2018-10-06T06:28:48.860","2018-10-06T02:28:48.860","KJ","XBT",null,null,"XBT016 launched"]
["2018-10-06T06:33:17.830","2018-10-06T02:33:17.830","KJ","Sonar","Multibeam",null,"XBT016 applied in line 0001"]
["2018-10-06T06:52:04.060","2018-10-06T02:52:04.060","JM","Sonar","All",null,"New line for turn, Knudsen range 200"]
["2018-10-06T07:01:21.700","2018-10-06T03:01:21.700","KJ","Sonar","Multibeam","New Line","MB line 0004"]
["2018-10-06T07:20:54.310","2018-10-06T03:20:54.310","KJ","Sonar","Multibeam",null,"Interference from possible dolphins"]
["2018-10-06T07:41:19.030","2018-10-06T03:41:19.030","KJ","Sonar","Multibeam",null,"Seep.  "]
["2018-10-06T08:01:05.500","2018-10-06T04:01:05.500","KJ","Sonar","Multibeam",null,"Seeps. End of line 0004"]
["2018-10-06T08:11:13.030","2018-10-06T04:11:13.030","KJ","Sonar","All","New Line","MB 0006 for turn"]
["2018-10-06T08:22:19.720","2018-10-06T04:22:19.720","KJ","Sonar","Multibeam","New Line","MB line 0007"]
["2018-10-06T11:29:47.250","2018-10-06T07:29:47.250","MW","Sonar","Knudsen",null,"Ping Mode: Auto"]
["2018-10-06T12:05:18.880","2018-10-06T08:05:18.880","JM","XBT",null,null,"Cast #17"]
["2018-10-06T12:15:23.770","2018-10-06T08:15:23.770","JM","XBT",null,null,"Cast #17 applied to MB line 0011"]
["2018-10-06T12:22:51.910","2018-10-06T08:22:51.910","JM","Sonar","Knudsen","Range","500; power 2; Tx pulse 0.5; new line; manual mode"]
["2018-10-06T12:50:25.700","2018-10-06T08:50:25.700","JM","Sonar","Knudsen","Tx Power",1]
["2018-10-07T12:50:25.695",{"$f":"IF(ISBLANK(A142),\" \",((A142)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-07T08:50:25.695"},"SA","XBT",null,null,"Cast #18 applied to line 0014"]
["2018-10-06T17:17:41.290","2018-10-06T13:17:41.290","MW","Sonar","Multibeam",null,"Stop logging for POSMV switch over "]
["2018-10-06T17:25:03.910","2018-10-06T13:25:03.910","MW","Sonar","Multibeam",null,"Logging after POSMV work"]
["2018-10-06T17:32:26.740","2018-10-06T13:32:26.740","MW","Sonar","Multibeam",null,"Stop Logging POSMV COM switch"]
["2018-10-06T17:43:58.760","2018-10-06T13:43:58.760","MW","Sonar","Multibeam",null,"Logging 0018 after POSMV cable switch"]
["2018-10-06T18:12:38.230","2018-10-06T14:12:38.230","MW","Sonar","Knudsen",null,"Lost communications changing POS feed"]
["2018-10-06T18:17:02.170","2018-10-06T14:17:02.170","CW","Sonar","Multibeam","Pen. Filter Strength","Off"]
["2018-10-06T18:44:33.640","2018-10-06T14:44:33.640","CW","Sonar","Multibeam","Secure","Stopped Logging for POS stuff n things"]
["2018-10-06T19:35:41.150","2018-10-06T15:35:41.150","CW","Sonar","Multibeam","Start Logging","MB line 0020"]
["2018-10-06T19:55:13.320","2018-10-06T15:55:13.320","CW","XBT",null,null,"XBT 019; applied to MB line 0020"]
["2018-10-06T20:45:02.760","2018-10-06T16:45:02.760","CW","XBT",null,null,"XBT 020; applied to SIS line 0021"]
["2018-10-06T21:13:54.100","2018-10-06T17:13:54.100","CW","XBT",null,null,"XBT 021; applied to new MB line 0022"]
["2018-10-07T01:47:16.900","2018-10-06T21:47:16.900","KJ","XBT",null,null,"XBT022 launched, higher temps possible because we've crossed the Gulf Stream, but seem much higher than expected; profile processed in SSM and applied in SIS, seafloor still frowning... launching new probe"]
["2018-10-07T01:48:56.950","2018-10-06T21:48:56.950","KJ","Sonar","Multibeam",null,"XBT022 applied in line MB 0026"]
["2018-10-07T01:50:28.840","2018-10-06T21:50:28.840","KJ","XBT",null,null,"XBT023 launched, following XBT022 temperature profile exactly, verifying that we are in a very different water mass outside the Gulf Stream"]
["2018-10-07T02:01:35.570","2018-10-06T22:01:35.570","KJ","Sonar","Multibeam",null,"XBT023 applied in line 0026"]
["2018-10-07T02:51:03.830","2018-10-06T22:51:03.830","KJ","Sonar","Multibeam",null,"Testing yaw stabilization OFF for 10 minutes to see if this is correlated with outer beam wobbles"]
["2018-10-07T03:00:47.400","2018-10-06T23:00:47.400","KJ","Sonar","Multibeam",null,"yaw stabilization back ON"]
["2018-10-07T05:51:50","2018-10-07T01:51:50","KJ","XBT",null,null,"XBT024 launched"]
["2018-10-07T06:02:55.660","2018-10-07T02:02:55.660","KJ","Sonar","Multibeam",null,"XBT024 applied in line 0030"]
["2018-10-07T06:24:21.560","2018-10-07T02:24:21.560","KJ","Sonar","Multibeam",null,"Lots of interference, possibly from dolphins"]
["2018-10-07T06:27:09.660","2018-10-07T02:27:09.660","KJ","Sonar","Knudsen","Tx Power","Changed from 3 to 2"]
["2018-10-07T10:15:30.900","2018-10-07T06:15:30.900","JM","Sonar","Knudsen","Range","200. New line"]
["2018-10-07T11:01:29.360","2018-10-07T07:01:29.360","JM","Sonar","Knudsen","Tx Power","Changed from 2 to 3"]
["2018-10-07T12:00:31.890","2018-10-07T08:00:31.890","CW","XBT",null,null,"Cast #25"]
["2018-10-07T12:20:36.820","2018-10-07T08:20:36.820","CW","XBT",null,null,"Cast #25 applied to MB line 0037"]
["2018-10-07T14:35:37","2018-10-07T10:35:37","SA","Sonar","Multibeam",null,"Logging stopped for POS configuration"]
["2018-10-07T14:47:00","2018-10-07T10:47:00","SA","Sonar","Multibeam",null,"Started logging multibeam after POS Configuration"]
["2018-10-07T14:59:00","2018-10-07T10:59:00","SA","Sonar","EK60 and Knudsen",null,"Logging stopped for POS configuration"]
["2018-10-07T15:28:49.270","2018-10-07T11:28:49.270","MW","Sonar",null,null,"Started logging EK60 and Knudsen after POS Configuration"]
["2018-10-07T17:23:26.590","2018-10-07T13:23:26.590","MW","XBT",null,null,"Cast 026"]
["2018-10-07T17:33:45.410","2018-10-07T13:33:45.410","MW","Sonar","Multibeam",null,"Cast 026 Applied to Line 0042"]
["2018-10-08T00:29:51.490","2018-10-07T20:29:51.490","KJ","XBT",null,null,"XBT 027 launched"]
["2018-10-08T00:43:22.240","2018-10-07T20:43:22.240","KJ","Sonar","Multibeam",null,"XBT 027 applied in line 0049"]
["2018-10-08T06:38:11.800","2018-10-08T02:38:11.800","KJ","XBT",null,null,"XBT028 launched and applied in MB line 0055"]
["2018-10-08T07:24:31.390","2018-10-08T03:24:31.390","JM","Sonar","Knudsen",null,"Pulse to 1. USGS end user suggested keeping pulse as low as possible. Range to 200. New line"]
["2018-10-08T12:40:00.940","2018-10-08T08:40:00.940","JM","XBT",null,null,"XBT cast #029"]
["2018-10-08T14:07:41.470","2018-10-08T10:07:41.470","JM","XBT",null,null,"XBT cast #029 applied to MB line 062"]
["2018-10-08T14:07:44.360","2018-10-08T10:07:44.360","MW","Sonar","All",null,"Stop logging for POSMV switch over "]
["2018-10-08T14:35:37.350","2018-10-08T10:35:37.350","MW","Sonar","All",null,"Logging"]
["2018-10-08T14:39:41.950","2018-10-08T10:39:41.950","MW","Sonar","Multibeam",null,"Stop logging for POSMV switch over "]
["2018-10-08T14:42:14.070","2018-10-08T10:42:14.070","MW","Sonar","Multibeam",null,"Logging"]
["2018-10-08T17:08:58.290","2018-10-08T13:08:58.290","CW","Sonar","Multibeam",null,"Stop logging for POSMV switch over "]
["2018-10-08T17:11:21.820","2018-10-08T13:11:21.820","CW","Sonar","Multibeam",null,"Logging; MB line 0068"]
["2018-10-08T17:23:47.760","2018-10-08T13:23:47.760","CW","Sonar","Multibeam",null,"Stop logging for POSMV switch over "]
["2018-10-08T17:31:48","2018-10-08T13:31:48","SA","Sonar","Multibeam",null,"Logging: MB line 0069"]
["2018-10-08T19:07:58",{"$f":"IF(ISBLANK(A188),\" \",((A188)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-08T15:07:58"},"SA","XBT",null,null,"XBT cast #30 launched"]
["2018-10-08T19:10:58","2018-10-08T15:10:58","SA","XBT",null,null,"Cast#30 applied to MB line 0070"]
["2018-10-08T19:10:34.360","2018-10-08T15:10:34.360","SA","Sonar","All",null,"new line for new heading MB line 0071"]
["2018-10-08T19:33:49.940","2018-10-08T15:33:49.940","CW","Sonar","Multibeam","Max Angle","Fiddlin with the max angles to rid out the outer beam spikes 28/28"]
["2018-10-08T19:41:09.190","2018-10-08T15:41:09.190","CW","Ship",null,null,"Begin steering pump testing. Still MB line 0071"]
["2018-10-08T19:48:52.010","2018-10-08T15:48:52.010","CW","Ship",null,null,"End steering pump tests. Still MB line 0071. They said they were successful!"]
["2018-10-09T00:43:49.690","2018-10-08T20:43:49.690","KJ","XBT",null,null,"XBT031 launched"]
["2018-10-09T00:45:15.440","2018-10-08T20:45:15.440","KJ","Ship",null,null,"coming to port slightly to get ready for turn onto line, swath width suffering greatly"]
["2018-10-09T00:51:38.510","2018-10-08T20:51:38.510","KJ","Sonar","Multibeam",null,"XBT031 applied in line 0076"]
["2018-10-09T01:07:32.450","2018-10-08T21:07:32.450","KJ","Sonar","All","New Line","On first ECS survey line, MB 0077"]
["2018-10-09T01:08:30.700","2018-10-08T21:08:30.700","KJ","Sonar","Multibeam","Max Angle","Changed swath angles from 32/32 to 52/52 in case depth mode changes from Extra Deep to Very Deep"]
["2018-10-09T05:59:09.850","2018-10-09T01:59:09.850","KJ","XBT",null,null,"XBT032 launched"]
["2018-10-09T06:05:31.280","2018-10-09T02:05:31.280","KJ","Sonar","Multibeam",null,"XBT032 applied at end of line 0081"]
["2018-10-09T07:31:14.840","2018-10-09T03:31:14.840","JM","Sonar","Knudsen","Tx Pulse","Changed to 2"]
["2018-10-09T11:46:20.490","2018-10-09T07:46:20.490","JM","XBT",null,null,"Cast #033"]
["2018-10-09T11:53:14.360","2018-10-09T07:53:14.360","JM","XBT",null,null,"Cast #033 applied to MB line 0087"]
["2018-10-09T14:09:48.030","2018-10-09T10:09:48.030","MW","Sonar","Multibeam",null,"Ping Mode: Very Deep"]
["2018-10-09T14:11:37.780","2018-10-09T10:11:37.780","MW","Sonar","Multibeam",null,"Max Angles: 45/45"]
["2018-10-09T14:46:05.350","2018-10-09T10:46:05.350","Mw","Sonar","Multibeam",null,"Angles to 40/40"]
["2018-10-09T14:46:53.070",{"$f":"IF(ISBLANK(A207),\" \",((A207)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-09T10:46:53.070"},"MW","Sonar","Multibeam",null,"Extra Deep"]
["2018-10-09T15:14:12.780","2018-10-09T11:14:12.780","CW","Sonar","All",null,"New lines for new heading to accommodate bridges incessant need for comfortable ride. MB line 0092"]
["2018-10-10T05:38:08.010","2018-10-10T01:38:08.010","KJ","XBT",null,null,"XBT034 launch attempted with canister #5; AOML software showed 'launch probe' flashing for several minuts, but no profile; retried with canister #6 and got a successful cast"]
["2018-10-10T05:51:43.010","2018-10-10T01:51:43.010","KJ","Sonar","Multibeam",null,"XBT034 applied in line 0107"]
["2018-10-10T12:29:48.030","2018-10-10T08:29:48.030","JM","XBT",null,null,"Cast #035"]
["2018-10-10T12:43:18.150","2018-10-10T08:43:18.150","JM","XBT",null,null,"Cast #035 applied to MB line 0114"]
["2018-10-10T13:51:50.190","2018-10-10T09:51:50.190","JM","Sonar","Multibeam","New Line","Turn line 0116"]
["2018-10-10T13:54:15.050","2018-10-10T09:54:15.050","JM","Sonar","All","New Line","End turn. MB line 0117"]
["2018-10-10T14:16:03.140","2018-10-10T10:16:03.140","MW","Sonar","Multibeam",null,"Ping Mode: Auto"]
["2018-10-10T16:01:37.740","2018-10-10T12:01:37.740","CW","Ship",null,null,"Swapping steering pumps. MB line 0119"]
["2018-10-10T16:04:21.540","2018-10-10T12:04:21.540","CW","Ship",null,null,"Done with swap"]
["2018-10-10T17:35:52","2018-10-10T13:35:52","MW","Ship",null,null,"Shifting to stbd a few hundred m for coverage"]
["2018-10-10T19:01:22.230","2018-10-10T15:01:22.230","CW","XBT",null,null,"AXBT 036; applied to MB line 0122"]
["2018-10-10T19:08:02.360","2018-10-10T15:08:02.360","CW","Ship",null,null,"Moving 200m to port; original line plan"]
["2018-10-10T19:21:47.750","2018-10-10T15:21:47.750","CW","Ship",null,null,"Moving another 200m to port. Now 200m port of original line plan. "]
["2018-10-11T01:00:36","2018-10-10T21:00:36","AM","XBT",null,null,"XBT037 launched"]
["2018-10-11T01:16:38.610","2018-10-10T21:16:38.610","KJ","Sonar","Multibeam",null,"XBT037 applied in line 0128"]
["2018-10-11T01:54:21.270","2018-10-10T21:54:21.270","KJ","Sonar","All","New Line","MB line 0129 for turn"]
["2018-10-11T02:17:59.890","2018-10-10T22:17:59.890","KJ","Sonar","All","New Line","MB line 0130 for new survey line"]
["2018-10-11T02:18:29.840","2018-10-10T22:18:29.840","KJ","Ship",null,null,"Coming down from 8.5 to 7 kts to try to reduce bubble sweepdown"]
["2018-10-11T02:21:36.170","2018-10-10T22:21:36.170","KJ","Ship",null,null,"Trying 6 kts… still getting a lot of bubble sweep, roughly every other ping is OK"]
["2018-10-11T02:25:20.660","2018-10-10T22:25:20.660","KJ","Sonar","Multibeam",null,"Interference filter from OFF to ON as a test"]
["2018-10-11T02:28:31.710","2018-10-10T22:28:31.710","KJ","Ship",null,null,"requested 200 m shift to port, back to original line plan to achieve more overlap"]
["2018-10-11T03:49:58.630","2018-10-10T23:49:58.630","KJ","Sonar","Multibeam",null,"Interference filter from ON to OFF as a test; no appreciable difference, still lots of bubble sweep"]
["2018-10-11T04:18:25.140","2018-10-11T00:18:25.140","KJ","Sonar","Multibeam",null,"Penetration filter from OFF to MEDIUM as a test, back to OFF"]
["2018-10-11T04:20:45.500","2018-10-11T00:20:45.500","KJ","Ship",null,null,"Slowing down from 6 to 5 kts… coverage is terrible"]
["2018-10-11T04:54:01.100","2018-10-11T00:54:01.100","KJ","Ship",null,null,"Confused seas with occasional big sets of swell; Bryan on the bridge called it 'mushy'"]
["2018-10-11T06:12:38.240","2018-10-11T02:12:38.240","KJ","Ship",null,null,"Ship slowed down to 4.5 kts at same RPM, increasing speed slightly to 5.5 kts, seeing how data looks..."]
["2018-10-11T07:46:15.150","2018-10-11T03:46:15.150","JM","XBT",null,null,"Cast #038"]
["2018-10-11T07:53:15.810","2018-10-11T03:53:15.810","JM","XBT",null,null,"Cast #038 applied to MB line 0135"]
["2018-10-11T08:34:49.950","2018-10-11T04:34:49.950","JM","Sonar","Multibeam","Aeration Filter (On/Off)","Sped ship to 6kts and turned aeration filter on"]
["2018-10-11T08:40:41.450","2018-10-11T04:40:41.450","JM","Sonar","Multibeam","Ping Mode","Changed to Very deep from Auto"]
["2018-10-11T09:15:25.460","2018-10-11T05:15:25.460","JM","Ship",null,null,"Speeding up to 7kts"]
["2018-10-11T09:39:02.950","2018-10-11T05:39:02.950","JM","Ship",null,null,"Speeding up to 8-8.5kts"]
["2018-10-11T10:55:32.090","2018-10-11T06:55:32.090","JM","Ship",null,null,"Shifting to stb 500m"]
["2018-10-11T11:09:06.300","2018-10-11T07:09:06.300","MW","Ship",null,null,"Shift to stbd 300m"]
["2018-10-11T11:17:39.220","2018-10-11T07:17:39.220","MW","ship",null,null,"shift stbd 500 m"]
["2018-10-11T11:58:09.830","2018-10-11T07:58:09.830","JM","Sonar","Multibeam","Aeration Filter (On/Off)","Off"]
["2018-10-11T12:26:34.490","2018-10-11T08:26:34.490","JM","Sonar","Multibeam","Ping Mode","Auto  "]
["2018-10-11T12:33:20.730","2018-10-11T08:33:20.730","JM","Ship",null,null,"Shifting to port 500m"]
["2018-10-11T13:01:49.060","2018-10-11T09:01:49.060","JM","Issue/Problem",null,null,"Marinestar is going in and out"]
["2018-10-11T14:03:03.850","2018-10-11T10:03:03.850","SA","XBT",null,null,"XBT Cast #039"]
["2018-10-11T14:16:38.290","2018-10-11T10:16:38.290","MW","Ship",null,null,"200m shift to port"]
["2018-10-11T14:17:21.090","2018-10-11T10:17:21.090","SA","XBT",null,null,"Cast #039 applied to MB line 0141"]
["2018-10-11T16:02:49.260","2018-10-11T12:02:49.260","CW","Ship",null,null,"Steering Pump change. MB line 0143"]
["2018-10-11T16:30:03.980","2018-10-11T12:30:03.980","CW","Sonar","All",null,"Turn line 0145. Turning style is somewhat questionable, but whatevs. "]
["2018-10-11T16:35:39.080","2018-10-11T12:35:39.080","CW","Ship",null,null,"Extended turn line distance 1km so that next survey line will have good overlap with less shifting requests. Bridge's ECTIS line will reflect. Thiers was already 600m SE of original line plan, so now it is 1600m SE. "]
["2018-10-11T16:58:49.120","2018-10-11T12:58:49.120","CW","Sonar","All",null,"Begin survey lines. MB line 0146"]
["2018-10-11T17:13:16.250","2018-10-11T13:13:16.250","CW","Ship",null,null,"Moving 200m to stbd. So now we are 1400m SE of original line plan. "]
["2018-10-11T17:29:24.150","2018-10-11T13:29:24.150","CW","Ship",null,null,"Moving 100m to stbd. So now we are 1300m SE of original line plan. "]
["2018-10-11T20:23:05.680",{"$f":"IF(ISBLANK(A257),\" \",((A257)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-11T16:23:05.680"},"CW","XBT",null,null,"AXBT 040; applied to MB line 0149"]
["2018-10-11T20:27:18.580","2018-10-11T16:27:18.580","CW","Ship",null,null,"Moving 700m to port. So now we are 2000m SE of original line plan. "]
["2018-10-11T22:53:37.220","2018-10-11T18:53:37.220","MW","Ship",null,null,"300m to STBD"]
["2018-10-12T00:00:25.910","2018-10-11T20:00:25.910","KJ","Sonar","Knudsen",null,"Changed TVG from None to 5logR (stopped / started to make a new file)"]
["2018-10-12T00:07:25.950","2018-10-11T20:07:25.950","KJ","Sonar","Knudsen",null,"Changed TVG back to None"]
["2018-10-12T00:27:47.250","2018-10-11T20:27:47.250","KJ","Ship",null,null,"Requested gentle 500 m shift to stbd for coverage"]
["2018-10-12T01:08:27.570","2018-10-11T21:08:27.570","KJ","Ship",null,null,"Another 300 m shift to stbd in anticipation of ping mode change from Very Deep to Extra Deep and accompanying reduction in swath angles to 35/35; after this shift, the line plan will be offset a total of 700 m from the original"]
["2018-10-12T01:54:46.540","2018-10-11T21:54:46.540","KJ","Ship",null,null,"Another 300 m to stbd"]
["2018-10-12T02:15:55.080","2018-10-11T22:15:55.080","KJ","XBT",null,null,"AXBT041 launched"]
["2018-10-12T02:24:51.070","2018-10-11T22:24:51.070","KJ","Sonar","Multibeam",null,"AXBT041 applied in line 0155"]
["2018-10-12T03:58:18.010","2018-10-11T23:58:18.010","KJ","Sonar","Multibeam",null,"Lots of interference, reducing RPM by 5 as a test, no improvement; spacing / frequency of interference rings is variable; turned Interference Filter ON to test; seems to be dissipating as time goes on"]
["2018-10-12T04:29:53.370","2018-10-12T00:29:53.370","KJ","Sonar","All","New Line","MB 0158 for turn"]
["2018-10-12T04:30:23.280","2018-10-12T00:30:23.280","KJ","Ship",null,null,"Shifting line plan back 400 m to NW, back to original position to try to cover gap from interference"]
["2018-10-12T04:50:36.950","2018-10-12T00:50:36.950","KJ","Sonar","All","New Line","MB 0159 heading back down the line…"]
["2018-10-12T05:15:49.880","2018-10-12T01:15:49.880","KJ","Sonar","Multibeam",null,"More interference while trying to cover gap"]
["2018-10-12T05:25:36.540",{"$f":"IF(ISBLANK(A272),\" \",((A272)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-12T01:25:36.540"},"KJ","Ship",null,null,"requested 500 m shift to starboard to reduce overlap after passing over gap"]
["2018-10-12T06:42:33.090","2018-10-12T02:42:33.090","KJ","Ship",null,null,"starting another 500 m shift to stbd to reduce overlap, for a total of 1000 m shift SE of original"]
["2018-10-12T06:49:51.600","2018-10-12T02:49:51.600","KJ","Sonar","Multibeam",null,"Turned Interference Filter OFF and Aeration Filter ON as a test… occasional swell slapping the hull, wiping out the whole swath"]
["2018-10-12T07:05:17.680","2018-10-12T03:05:17.680","KJ","Ship",null,null,"Requested another 500 m shift to stbd, total will be 1500 m from original"]
["2018-10-12T08:21:48.030","2018-10-12T04:21:48.030","JM","XBT",null,null,"Cast #042"]
["2018-10-12T08:34:17.870","2018-10-12T04:34:17.870","JM","XBT",null,null,"Cast #042 applied to MB line 0162"]
["2018-10-12T09:56:40.930","2018-10-12T05:56:40.930","JM","Ship",null,null,"Coming stb 1000m"]
["2018-10-12T11:40:38.170","2018-10-12T07:40:38.170","MW","Ship",null,null,"300m to STBD"]
["2018-10-12T13:25:52.410","2018-10-12T09:25:52.410","JM","Ship",null,null,"1000m to port"]
["2018-10-12T14:28:13.290","2018-10-12T10:28:13.290","CW","Ship",null,null,"500m to port"]
["2018-10-12T14:29:33","2018-10-12T10:29:33","SA","XBT",null,null,"Cast #043"]
["2018-10-12T14:36:06.820","2018-10-12T10:36:06.820","SA","XBT",null,null,"Cast #043 applied to MB line 0168"]
["2018-10-12T15:44:44.440","2018-10-12T11:44:44.440","MW","Ship",null,null,"New Lines, Ship is shifted 1000m to the NW, Port on this heading"]
["2018-10-12T17:00:25.970","2018-10-12T13:00:25.970","CW","Sonar","All","New Line","New lines for turn; MB line 0172"]
["2018-10-12T17:29:25.540","2018-10-12T13:29:25.540","CW","Sonar","All","New Line","New Survey Lines. MB line 0173"]
["2018-10-12T17:47:02.750","2018-10-12T13:47:02.750","CW","Ship",null,null,"Moving 200m stbd. "]
["2018-10-12T19:50:18",{"$f":"IF(ISBLANK(A288),\" \",((A288)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-12T15:50:18"},"CW","Sonar","Multibeam","Ping Mode","Manual adjust to Very Deep"]
["2018-10-12T19:54:27.420","2018-10-12T15:54:27.420","CW","Ship",null,null,"500m to port"]
["2018-10-12T20:28:25.760","2018-10-12T16:28:25.760","CW","Ship",null,null,"500m to port"]
["2018-10-12T20:58:22.090","2018-10-12T16:58:22.090","SG","XBT",null,null,"Cast 044 applied to MB line 0176"]
["2018-10-12T21:19:00.260","2018-10-12T17:19:00.260","MW","Ship",null,null,"500m shift to port, now 300m SE of original line plan"]
["2018-10-12T22:03:54.860","2018-10-12T18:03:54.860","CW","Ship",null,null,"1500m shift to port"]
["2018-10-13T00:15:49.420","2018-10-12T20:15:49.420","KJ","Ship",null,null,"Initiating very gradual shift 500 m to stbd for coverage"]
["2018-10-13T00:53:29.610","2018-10-12T20:53:29.610","KJ","Ship",null,null,"Another 500 m to stbd"]
["2018-10-13T02:42:54.370","2018-10-12T22:42:54.370","KJ","Ship",null,null,"Starting 500 m shift to stbd"]
["2018-10-13T03:26:58.720","2018-10-12T23:26:58.720","KJ","XBT",null,null,"AXBT045 launched"]
["2018-10-13T03:34:34.480","2018-10-12T23:34:34.480","KJ","Sonar","Multibeam",null,"AXBT045 applied in line 0183"]
["2018-10-13T04:09:33.520","2018-10-13T00:09:33.520","KJ","Sonar","Multibeam",null,"interference developing, causing some dropouts"]
["2018-10-13T04:35:29.610","2018-10-13T00:35:29.610","KJ","Ship",null,null,"initiating 300 m shift to stbd; seas are building slightly on the bow, more pitching, no major bubble issues yet"]
["2018-10-13T06:08:44.440","2018-10-13T02:08:44.440","KJ","Sonar","All","New Line","MB line 0186 for turn"]
["2018-10-13T06:37:07.910","2018-10-13T02:37:07.910","KJ","Sonar","All","New Line","MB line 0187"]
["2018-10-13T06:52:10.800","2018-10-13T02:52:10.800","KJ","Ship",null,null,"500 m to stbd to reduce overlap"]
["2018-10-13T09:39:59.910","2018-10-13T05:39:59.910","JM","Ship",null,null,"500m to stb"]
["2018-10-13T09:42:01.900","2018-10-13T05:42:01.900","JM","XBT",null,null,"Cast #046"]
["2018-10-13T09:48:19.290","2018-10-13T05:48:19.290","JM","XBT",null,null,"Cast #046 applied to MB line 0190"]
["2018-10-13T11:04:13.910",{"$f":"IF(ISBLANK(A307),\" \",((A307)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-13T07:04:13.910"},"MW","Ship",null,null,"1000 meter shift to STBD, 2500m SE of original line plan"]
["2018-10-13T13:29:07.710","2018-10-13T09:29:07.710","JM","Ship",null,null,"Change course bearing 65deg until we reach original line plan"]
["2018-10-13T14:53:58.540","2018-10-13T10:53:58.540","SA","Ship",null,null,"Reached original line plan"]
["2018-10-13T15:51:33","2018-10-13T11:51:33","CW","Ship",null,null,"500m to port"]
["2018-10-13T15:53:24.900","2018-10-13T11:53:24.900","CW","Ship",null,null,"Another 500m to port"]
["2018-10-13T15:53:24.900","2018-10-13T11:53:24.900","SA","XBT",null,null,"Cast #047"]
["2018-10-13T15:59:42.360","2018-10-13T11:59:42.360","SA","XBT",null,null,"Cast 047 applied to MB line 0196"]
["2018-10-13T18:39:51","2018-10-13T14:39:51","CW","Sonar","All",null,"Turn line. MB line 0200"]
["2018-10-13T18:50:04.640","2018-10-13T14:50:04.640","CW","Ship",null,null,"Shortening turn line by 500m for good overlap on next survey line. "]
["2018-10-13T19:05:24","2018-10-13T15:05:24","CW","Sonar","All",null,"New Survey Lines. MB line 0201"]
["2018-10-13T22:17:06.120","2018-10-13T18:17:06.120","AM","XBT",null,null,"XBT 48 apllied to 0204"]
["2018-10-13T22:22:31.580","2018-10-13T18:22:31.580","MW","Ship",null,null,"Port 1000m, total offset is 1000m"]
["2018-10-13T23:18:24.790","2018-10-13T19:18:24.790","MW","Ship",null,null,"Port 1000m, total offset is 2000m"]
["2018-10-14T00:23:11.480","2018-10-13T20:23:11.480","KJ","Ship",null,null,"shift 500 m to port, total offset will be 3000 m (one previous 500 m shift was not logged)"]
["2018-10-14T00:47:30.340","2018-10-13T20:47:30.340","KJ","Ship",null,null,"shift 500 m to port, total offset will be 3500 m"]
["2018-10-14T01:57:54.760","2018-10-13T21:57:54.760","KJ","Ship",null,null,"500 m shift to stbd, total 3000 m"]
["2018-10-14T02:15:33.300","2018-10-13T22:15:33.300","KJ","Ship",null,null,"500 m shift to stbd, total 2500 m"]
["2018-10-14T02:56:16.340","2018-10-13T22:56:16.340","KJ","Ship",null,null,"starting 1000 m gradual shift to stbd, total will be 1500 m"]
["2018-10-14T04:23:50","2018-10-14T00:23:50","AM","XBT",null,null,"AXBT049 launched"]
["2018-10-14T04:41:25.960","2018-10-14T00:41:25.960","AM","Sonar","Multibeam",null,"AXBT049 applied in line 0210"]
["2018-10-14T05:02:33.790","2018-10-14T01:02:33.790","KJ","Ship",null,null,"500 m to port, total 2000 m"]
["2018-10-14T06:39:29.700","2018-10-14T02:39:29.700","KJ","Sonar","All","New Line","MB line 0213 for turn"]
["2018-10-14T07:04:21.640","2018-10-14T03:04:21.640","KJ","Sonar","All","New Line","MB 0214"]
["2018-10-14T07:15:37.330","2018-10-14T03:15:37.330","KJ","Ship",null,null,"500 m shift to stbd, total 2500 m"]
["2018-10-14T08:41:55.440","2018-10-14T04:41:55.440","JM","Ship",null,null,"300m to port"]
["2018-10-14T10:18:46.680","2018-10-14T06:18:46.680","JM","Ship",null,null,"700m to stb"]
["2018-10-14T10:20:03.590","2018-10-14T06:20:03.590","JM","XBT",null,null,"Cast #050"]
["2018-10-14T10:26:32.630","2018-10-14T06:26:32.630","JM","XBT",null,null,"Cast #050 applied to MB line 0217"]
["2018-10-14T10:48:28.700","2018-10-14T06:48:28.700","JM","Issue/Problem",null,null,"Engineering had to disable TSG pump for bow thruster maintenance "]
["2018-10-14T10:53:21.720","2018-10-14T06:53:21.720","JM","Sonar","Knudsen","Phase Mode","Trying Auto mode  "]
["2018-10-14T10:58:17.600",{"$f":"IF(ISBLANK(A337),\" \",((A337)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-14T06:58:17.600"},"JM","Sonar","Knudsen","Phase Mode"," Back to manual mode"]
["2018-10-14T11:15:27","2018-10-14T07:15:27","JM","Ship",null,null,"1000m to stb"]
["2018-10-14T13:00:16.500","2018-10-14T09:00:16.500","JM","Ship",null,null,"1000m to port"]
["2018-10-14T13:53:48.280","2018-10-14T09:53:48.280","JM","Ship",null,null,"200m to port"]
["2018-10-14T14:04:34.420","2018-10-14T10:04:34.420","JM","Ship",null,null,"1400m to port"]
["2018-10-14T15:09:01.120","2018-10-14T11:09:01.120","MW","Ship",null,null,"1200m to port at 063"]
["2018-10-14T16:30:29","2018-10-14T12:30:29","CW","Ship",null,null,"1500m to port at 059"]
["2018-10-14T16:57:17.890","2018-10-14T12:57:17.890","CW","Ship",null,null,"500m to port"]
["2018-10-14T17:31:27.120","2018-10-14T13:31:27.120","CW","Sonar","Multibeam","Ping Mode","Manual Extra Deep"]
["2018-10-14T17:41:39.540","2018-10-14T13:41:39.540","CW","Ship",null,null,"200m to port "]
["2018-10-14T18:17:32.970","2018-10-14T14:17:32.970","CW","Ship",null,null,"Not moving - 2200m to port from Bridge ECTIS line"]
["2018-10-14T18:38:33","2018-10-14T14:38:33","SA","XBT",null,null,"Cast #051"]
["2018-10-14T18:42:45.220","2018-10-14T14:42:45.220","SA","XBT",null,null,"Cast 051 applied to MB line 0225"]
["2018-10-14T19:04:25","2018-10-14T15:04:25","CW","Sonar","All","New Line","Turn lines. MB line 0226"]
["2018-10-14T19:24:41.630","2018-10-14T15:24:41.630","CW","Sonar","All","New Line","New survey lines. MB line 0227"]
["2018-10-14T19:24:43.530","2018-10-14T15:24:43.530","CW","Ship",null,null,"500m to stbd (north)"]
["2018-10-14T21:28:37.580","2018-10-14T17:28:37.580","MW","Ship",null,null,"initiated a 1200 m shift to port at heading 234"]
["2018-10-14T21:48:47.470","2018-10-14T17:48:47.470","CW","Sonar","Multibeam","Ping Mode","Manual Very Deep"]
["2018-10-14T22:25:22.640","2018-10-14T18:25:22.640","CW","Ship",null,null,"500m to port"]
["2018-10-14T23:37:46.500","2018-10-14T19:37:46.500","KJ","Ship",null,null,"1000 m to port, aiming for a COG of 245m, heading 250"]
["2018-10-15T00:08:13.840","2018-10-14T20:08:13.840","KJ","Ship",null,null,"1000 m to port, heading 245"]
["2018-10-15T01:17:47.610","2018-10-14T21:17:47.610","SG","XBT",null,null,"Cast 052"]
["2018-10-15T01:31:38.860","2018-10-14T21:31:38.860","AM","XBT",null,null,"Cast 052 applied to MB line 0233"]
["2018-10-15T02:27:13.840","2018-10-14T22:27:13.840","KJ","Ship",null,null,"initiating 1000 m shift to stbd with 3 deg COG change to track coverage"]
["2018-10-15T03:06:12.680","2018-10-14T23:06:12.680","KJ","Sonar","Knudsen",null,"Started recording; appears to have stopped recording 38 minutes ago based on file modification times"]
["2018-10-15T03:21:12.300","2018-10-14T23:21:12.300","KJ","Ship",null,null,"500 m to stbd at 4 deg heading change"]
["2018-10-15T03:46:45.960","2018-10-14T23:46:45.960","KJ","Ship",null,null,"Another 500 m to stbd"]
["2018-10-15T05:08:35.550","2018-10-15T01:08:35.550","KJ","Sonar","Multibeam",null,"Qimera crashed while Akim was appending lines to a Dynamic Surface, and project will not open; making a backup to the Public/Cruises/EX1810 drive before continuing to attempt opening project"]
["2018-10-15T05:41:10.450","2018-10-15T01:41:10.450","KJ","Sonar","Multibeam",null,"Qimera was crashing while loading a large grid during open-up ('loading layers'); removed the grid folder from the project's GridData directory and deleted the CRASHED file from the project's main directory; Qimera project opened fine after this; grid was rebuilt without issue; celebratory tea was sipped with pinkies up"]
["2018-10-15T07:00:45.030","2018-10-15T03:00:45.030","JM","Sonar","All","New Line","Begin turn MB line 0239"]
["2018-10-15T07:07:13.620","2018-10-15T03:07:13.620","JM","XBT",null,null,"Cast #053"]
["2018-10-15T07:10:39.080","2018-10-15T03:10:39.080","JM","XBT",null,null,"Noticed the GPS input in the XBT recorder software is not updating. This means the location of the casts in the XBT and ASVP files are not accurate. It appears the sound speed manager takes position from SIS so the info pulled from the catalog is good. Position of casts #50-53 are the same. Restarting software to see if position updates return."]
["2018-10-15T07:17:37.540","2018-10-15T03:17:37.540","JM","XBT",null,null,"Cast #053 applied to MB line 0239"]
["2018-10-15T07:47:57.400","2018-10-15T03:47:57.400","JM","Sonar","All","New Line","End turn. MB line 0240"]
["2018-10-15T11:18:38.180","2018-10-15T07:18:38.180","MW","Ship",null,null,"Speed Increased 8.5-9"]
["2018-10-15T14:25:37.230","2018-10-15T10:25:37.230","SA","XBT",null,null,"Cast #054"]
["2018-10-15T14:31:37.310","2018-10-15T10:31:37.310","SA","XBT",null,null,"Cast 054 applied to MB line 0246"]
["2018-10-15T14:50:40.160","2018-10-15T10:50:40.160","MW","Sonar","All",null,"Turn line 0248"]
["2018-10-15T14:56:48.720","2018-10-15T10:56:48.720","MW","Sonar","All",null,"New Line 0249 "]
["2018-10-15T14:57:03.950","2018-10-15T10:57:03.950","MW","Ship",null,null,"Slowing down for traffic"]
["2018-10-15T16:00:09.790","2018-10-15T12:00:09.790","MW","Sonar","All",null,"Turn Line 0251"]
["2018-10-15T16:05:14.770","2018-10-15T12:05:14.770","CW","Sonar","All",null,"New Survey Lines. MB line 0252"]
["2018-10-15T17:41:06.980","2018-10-15T13:41:06.980","CW","Ship",null,null,"3000m to port at 060 deg"]
["2018-10-15T18:43:36.560","2018-10-15T14:43:36.560","MW","Ship",null,null,"500m to port at 060"]
["2018-10-15T19:38:40.370","2018-10-15T15:38:40.370","CW","Ship",null,null,"Bridge needs to move to stbd a few degrees to avoid some kind of debris in the water. Hopefully the overlap will not be lost…"]
["2018-10-15T19:44:32.380","2018-10-15T15:44:32.380","CW","Ship",null,null,"Bridge now needs to slow or even possibly stop. Debris might be something more signifigant. "]
["2018-10-15T19:48:46.080","2018-10-15T15:48:46.080","CW","Ship",null,null,"Back to normal. "]
["2018-10-15T20:41:38.320","2018-10-15T16:41:38.320","CW","XBT",null,null,"AXBT 055; applied to MB line 0257"]
["2018-10-15T20:50:07","2018-10-15T16:50:07","CW","Ship",null,null,"Extending line 10km past waypoint, as per Herr White."]
["2018-10-15T22:46:50.690","2018-10-15T18:46:50.690","CW","Sonar","All",null,"Turn lines at beginning of MB line 0260"]
["2018-10-15T23:05:36.330","2018-10-15T19:05:36.330","CW","Sonar","All",null,"Turn lines. MB line 0261"]
["2018-10-15T23:10:30.200","2018-10-15T19:10:30.200","CW","Sonar","All",null,"New survey lines. MB line 0262"]
["2018-10-16T00:19:00.590","2018-10-15T20:19:00.590","CW","POS",null,null,"Pri. DGPS / GAMS Not Ready"]
["2018-10-16T00:25:10.640","2018-10-15T20:25:10.640","KJ","POS",null,null,"Wiggled the Primary GNSS cable, tightened connector in back of POS to test - there are Primary GNSS dropouts in the POS log that appear to be the initial event each time there is a reduction in data quality (Position red light, or GAMS not in use, etc.)... This is similar to (but much less severe than) the Primary GNSS dropouts observed during EX1806, which was due to a faulty / flimsy soft cable connector between the rigid antenna cable and the back of the POS; connector was removed after EX1806 and it is believed the antenna cable was reterminated"]
["2018-10-16T01:26:57.280","2018-10-15T21:26:57.280","KJ","Ship",null,null,"500 m to port, total 4000 m shift from original"]
["2018-10-16T02:36:37.570","2018-10-15T22:36:37.570","KJ","XBT",null,null,"XBT056 launched"]
["2018-10-16T02:47:21.980","2018-10-15T22:47:21.980","KJ","XBT",null,null,"XBT files 052-055 were on 2018-10-15 UTC but were named 20181014; renamed these files with the correct date code in the XBT and ASVP folders on E: and M: drive; re-copied these files to the svpabscoeff folder on the SIS machine, but left the originals because it's not certain how SIS references these (also so the exact file applied during acquisition is still archived in the sisdata/common/svpabscoeff folder"]
["2018-10-16T02:52:50.220","2018-10-15T22:52:50.220","KJ","Sonar","Multibeam",null,"Cast 056 applied in line 0265"]
["2018-10-16T02:57:35.940","2018-10-15T22:57:35.940","KJ","Ship",null,null,"Initiating 3000 m shift to port at COG of 239"]
["2018-10-16T03:54:36.570","2018-10-15T23:54:36.570","KJ","Ship",null,null,"still merging onto the most recently shifted line, approaching 500 m from the shifted line plan, decided to add another 500 m shift"]
["2018-10-16T03:59:51.850","2018-10-15T23:59:51.850","KJ","Ship",null,null,"heading change 2 deg to stbd, resulting in some extra overlap, due to vessel traffic"]
["2018-10-16T04:11:26.490","2018-10-16T00:11:26.490","KJ","Ship",null,null,"EM302 changed from Extra Deep to Very Deep, swath starting to increase a little beyond 35/35 heading up the slope; adding another 500 m shift to port that will bring us onto the original unshifted line plan"]
["2018-10-16T05:50:00.440","2018-10-16T01:50:00.440","KJ","Sonar","All","New Line","MB 0269 for turn"]
["2018-10-16T05:50:21.420","2018-10-16T01:50:21.420","KJ","Ship",null,null,"heading to start of next survey line, cutting corner short over existing coverage and increasing speed from 140 RPM to 165 RPM until next line"]
["2018-10-16T06:19:45.310",{"$f":"IF(ISBLANK(A401),\" \",((A401)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-16T02:19:45.310"},"KJ","Sonar","All","New Line","MB 0270 for new survey line"]
["2018-10-16T06:22:54.070","2018-10-16T02:22:54.070","KJ","Ship",null,null,"500 m to stbd"]
["2018-10-16T07:44:26.630","2018-10-16T03:44:26.630","KJ","Ship",null,null,"3000 m shift to port, turning slowly to COG of 060 for coverage"]
["2018-10-16T08:20:27.500","2018-10-16T04:20:27.500","CB","XBT",null,null,"Cast #057"]
["2018-10-16T08:29:06.690","2018-10-16T04:29:06.690","CB","XBT",null,null,"Cast #057 applied to MB line 0272"]
["2018-10-16T08:51:25.540","2018-10-16T04:51:25.540","JM","Ship",null,null,"Shifted original trackline 4300m to port, approaching it at COG of 61deg"]
["2018-10-16T10:36:15.900","2018-10-16T06:36:15.900","JM","Ship",null,null,"450m to port"]
["2018-10-16T11:38:37.640","2018-10-16T07:38:37.640","JM","Sonar","All","New Line","Begin turn, MB line 0276"]
["2018-10-16T12:04:04.750","2018-10-16T08:04:04.750","JM","Sonar","All","New Line","End turn, MB line 0277"]
["2018-10-16T13:56:52.230","2018-10-16T09:56:52.230","JM","Ship",null,null,"Change COG to 240deg. until intersection of line plan. Shifting original line plan 500m to port."]
["2018-10-16T14:48:29.180","2018-10-16T10:48:29.180","CB","XBT",null,null,"Cast #058"]
["2018-10-16T14:55:51.580","2018-10-16T10:55:51.580","CB","XBT",null,null,"Cast 058 applied to MB line 0279"]
["2018-10-16T16:34:18.660","2018-10-16T12:34:18.660","MW","Ship",null,null,"500m to stb at 255"]
["2018-10-16T17:10:08.090","2018-10-16T13:10:08.090","MW","Ship",null,null,"500m to stb at 255"]
["2018-10-16T20:38:43.020","2018-10-16T16:38:43.020","SG","XBT",null,null,"Cast #059"]
["2018-10-16T20:49:17.890","2018-10-16T16:49:17.890","SG","XBT",null,null,"Cast 059 applied to MB line 0285"]
["2018-10-16T21:23:51.020","2018-10-16T17:23:51.020","MW","Ship",null,null,"Shift 500m to STBD at 255"]
["2018-10-16T21:59:53.780","2018-10-16T17:59:53.780","CW","Ship",null,null,"Changed course to 257 for some siiiiiick overlap."]
["2018-10-17T00:44:39.940","2018-10-16T20:44:39.940","KJ","Sonar","All","New Line","Merged onto new westbound exploration line, heading toward Cape Canaveral to watch the launch!"]
["2018-10-17T02:46:53.300","2018-10-16T22:46:53.300","SG","XBT",null,null,"Cast 060"]
["2018-10-17T02:53:22.300","2018-10-16T22:53:22.300","SG","XBT",null,null,"Cast 060 applied to MB line 0292"]
["2018-10-17T04:05:30.740","2018-10-17T00:05:30.740","KJ",null,null,null,"stepping outside to watch Atlas V launch from Cape Canaveral…"]
["2018-10-17T06:27:36.450","2018-10-17T02:27:36.450","KJ","Sonar","Multibeam",null,"Lost bottom for several pings for unknown reason; possibly related to temporary change in 'soft startup time' field in Runtime Parameters from 0 to 5 minutes to make a screenshot for the SIS SOP; TX Power remained at 0.00 (max) in the realtime display, which suggests no reduction in TX power for mammal protection / soft startup, but the timing is about right"]
["2018-10-17T07:16:28.270","2018-10-17T03:16:28.270","KJ","Sonar","Multibeam",null,"Max depth changed from 5500 to 6000 m"]
["2018-10-17T09:07:42.850","2018-10-17T05:07:42.850","JM","XBT",null,null,"Cast #061"]
["2018-10-17T09:16:57.900","2018-10-17T05:16:57.900","JM","XBT",null,null,"Cast #061 applied to MB line 0298"]
["2018-10-17T09:54:32.620","2018-10-17T05:54:32.620","JM","Sonar","All","New Line","Begin turn MB line 0300"]
["2018-10-17T10:16:18.250","2018-10-17T06:16:18.250","JM","Sonar","All","New Line","End turn MB line 0301"]
["2018-10-17T15:08:30.410","2018-10-17T11:08:30.410","CB","XBT",null,null,"Cast #062"]
["2018-10-17T15:30:55.260","2018-10-17T11:30:55.260","CB","XBT",null,null,"Cast 062 applied to MB line 0306"]
["2018-10-17T17:26:29.970","2018-10-17T13:26:29.970","SA","Ship",null,null,"2000m shift stbd"]
["2018-10-17T19:00:23.400","2018-10-17T15:00:23.400","CW","Sonar","Multibeam",null,"Repeated interference on all sonars. Possibly a  Russian sub with silent propulsion. MB line 0309"]
["2018-10-17T19:04:09.210","2018-10-17T15:04:09.210","CW","Sonar","Multibeam","Ping Mode","Manual Very Deep"]
["2018-10-17T19:39:26.450","2018-10-17T15:39:26.450","CW","Sonar","All",null,"New lines for new heading back on to survey area. MB line 0311"]
["2018-10-17T21:02:37.320","2018-10-17T17:02:37.320","SG","xbt",null,null,"cast 063"]
["2018-10-17T21:09:41.930","2018-10-17T17:09:41.930","SG","XBT",null,null,"Cast 063 applied to MB line 0312"]
["2018-10-17T21:32:43","2018-10-17T17:32:43","CW","Sonar","Multibeam",null,"2700m to stbd at course of 079"]
["2018-10-17T22:44:12.600","2018-10-17T18:44:12.600","MW","Sonar","Multibeam",null,"SIS  CRASH"]
["2018-10-17T23:10:54.380","2018-10-17T19:10:54.380","MW","Sonar","Multibeam",null,"SIS is Back"]
["2018-10-17T23:11:10.470","2018-10-17T19:11:10.470","MW","Sonar","Multibeam",null,"Turned around to re-run lost coverage, logging line 0314; NOTE, this is the same file number that was recording when SIS crashed; the two 0314 files can be distinguished by the different times in the file names"]
["2018-10-18T03:32:51.850","2018-10-17T23:32:51.850","KJ","Sonar","Multibeam",null,"water column screen went completely red and purple for three pings… then returned to normal"]
["2018-10-18T03:35:13.500","2018-10-17T23:35:13.500","KJ","Ship",null,null,"initiating 1000 m shift to stbd with 3 deg COG change to track coverage"]
["2018-10-18T03:47:37.080","2018-10-17T23:47:37.080","KJ","XBT",null,null,"XBT064 launched"]
["2018-10-18T03:51:22.420","2018-10-17T23:51:22.420","KJ","Sonar","Multibeam",null,"XBT064 applied in line 0318"]
["2018-10-18T05:06:50.910","2018-10-18T01:06:50.910","KJ","Ship",null,null,"Initiating 6000 m shift to port at COG of 060 for coverage… total shift of 5000 m to NW of original line plan"]
["2018-10-18T07:27:31.350","2018-10-18T03:27:31.350","KJ","Sonar","Knudsen",null,"Beautiful subbottom data!"]
["2018-10-18T09:57:56.790","2018-10-18T05:57:56.790","JM","XBT",null,null,"Cast #065"]
["2018-10-18T10:04:47.500","2018-10-18T06:04:47.500","JM","XBT",null,null,"Cast #065 applied to MB line 0324"]
["2018-10-18T10:06:54.330","2018-10-18T06:06:54.330","JM","Sonar","Multibeam","Ping Mode","Auto"]
["2018-10-18T11:53:26.180","2018-10-18T07:53:26.180","JM","Ship",null,null,"Shift line stb (north) 250m after turn"]
["2018-10-18T12:21:16.400","2018-10-18T08:21:16.400","JM","Sonar","All","New Line","Begin turn. MB line 0328"]
["2018-10-18T12:48:25.340","2018-10-18T08:48:25.340","JM","Sonar","All","New Line","End turn. MB line 0329"]
["2018-10-18T12:54:25.040","2018-10-18T08:54:25.040","JM","Ship",null,null,"Shift line stb 250m"]
["2018-10-18T16:23:26.570","2018-10-18T12:23:26.570","SA","XBT",null,null,"Cast #066"]
["2018-10-18T16:32:14.010","2018-10-18T12:32:14.010","SA","XBT",null,null,"Cast 066 applied to MB line 0332"]
["2018-10-18T17:36:11.410","2018-10-18T13:36:11.410","CW","Ship",null,null,"4000 to port at COG 245"]
["2018-10-18T23:13:19.480","2018-10-18T19:13:19.480","SG","XBT",null,null,"Cast 067"]
["2018-10-18T23:20:00.040","2018-10-18T19:20:00.040","SG","XBT",null,null,"Cast 067 applied to MB line 0339"]
["2018-10-19T01:51:20.860","2018-10-18T21:51:20.860","KJ","Ship",null,null,"Starting 3000 m shift to stbd at COG of 260 for coverage; net 2500 m to stbd of original line"]
["2018-10-19T04:09:01.110","2018-10-19T00:09:01.110","KJ","Sonar","All","New Line","Turn MB 0345"]
["2018-10-19T04:40:52.120","2018-10-19T00:40:52.120","KJ","Sonar","All","New Line","Final survey line for this mapping area; MB 0346; offset 2500 m to NW from original line plan"]
["2018-10-19T04:57:56.840","2018-10-19T00:57:56.840","KJ","Ship",null,null,"500 m to stbd, 2000 m net off original line"]
["2018-10-19T05:05:13.920","2018-10-19T01:05:13.920","KJ","Sonar","Multibeam",null,"water column screen went completely red and purple for three pings… then returned to normal"]
["2018-10-19T05:28:48.430","2018-10-19T01:28:48.430","KJ","Ship",null,null,"2500 m shift to stbd at COG 080 for coverage; net will be 500 m to SE of original line"]
["2018-10-19T06:13:06.010",{"$f":"IF(ISBLANK(A465),\" \",((A465)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-19T02:13:06.010"},"KJ","Ship",null,null,"Swell coming more from the fwd direction, starting to get occasional bubble sweep down"]
["2018-10-19T08:03:54.930","2018-10-19T04:03:54.930","KJ","XBT",null,null,"XBT068 launched; looks suspect; launching another; looks normal, keeping number 068"]
["2018-10-19T08:17:05.380","2018-10-19T04:17:05.380","KJ","Sonar","Multibeam",null,"XBT 068 applied in line 0349"]
["2018-10-19T09:44:31.880","2018-10-19T05:44:31.880","JM","Sonar","Multibeam","Aeration Filter (On/Off)","Aeration filter On  "]
["2018-10-19T10:50:06.260","2018-10-19T06:50:06.260","JM","Sonar","Multibeam","Ping Mode","Very Deep"]
["2018-10-19T10:53:47.130","2018-10-19T06:53:47.130","JM","Ship",null,null,"Shift to port 800m"]
["2018-10-19T11:14:10.530","2018-10-19T07:14:10.530","MW","Sonar","Multibeam",null,"Angles 37/37"]
["2018-10-19T11:17:14.100","2018-10-19T07:17:14.100","MW","Sonar","Multibeam",null,"Angles 35/35"]
["2018-10-19T13:20:17.900","2018-10-19T09:20:17.900","JM","Sonar","Multibeam",null,"Angles 38/38"]
["2018-10-19T13:45:36.710","2018-10-19T09:45:36.710","JM","Ship",null,null,"Course change to 055deg"]
["2018-10-19T14:00:35.420","2018-10-19T10:00:35.420","JM","Ship",null,null,"Course change to 057deg"]
["2018-10-19T14:19:19.060","2018-10-19T10:19:19.060","SA","XBT",null,null,"Cast #069"]
["2018-10-19T14:26:45.670","2018-10-19T10:26:45.670","SA","XBT",null,null,"Cast 069 applied to MB line 0355"]
["2018-10-19T15:13:59.900","2018-10-19T11:13:59.900","MW","Sonar",null,null,"Angles 35/35"]
["2018-10-19T16:01:16.140","2018-10-19T12:01:16.140","CW","Sonar","Multibeam","Ping Mode","Manual Extra Deep"]
["2018-10-19T16:01:54.990","2018-10-19T12:01:54.990","CW","Ship",null,null,"Settling into COG 072"]
["2018-10-19T17:20:12.880","2018-10-19T13:20:12.880","CW","POS",null,null,"Pri. DGPS / Gams Online"]
["2018-10-19T20:28:44.190","2018-10-19T16:28:44.190","SA","XBT",null,null,"Cast #070"]
["2018-10-19T20:33:45.610","2018-10-19T16:33:45.610","SA","XBT",null,null,"Cast 070 applied to MB line 0361"]
["2018-10-19T22:22:04.410","2018-10-19T18:22:04.410","CW","Sonar","All",null,"Turn lines. MB line 0364"]
["2018-10-19T22:47:21.840","2018-10-19T18:47:21.840","CW","Sonar","All",null,"New Survey Lines. MB line 0365"]
["2018-10-19T22:45:28",{"$f":"IF(ISBLANK(A486),\" \",((A486)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-19T18:45:28"},"CW","Sonar","Multibeam",null,"Nadir blowouts! Lame-O. Beginning of MB line 0365"]
["2018-10-19T22:47:28.480","2018-10-19T18:47:28.480","CW","Ship",null,null,"500m to port"]
["2018-10-20T01:35:08.480","2018-10-19T21:35:08.480","KJ","Ship",null,null,"initiating 300 m shift to stbd for coverage"]
["2018-10-20T02:38:46.630","2018-10-19T22:38:46.630","SG","XBT",null,null,"XBT071 launched"]
["2018-10-20T02:41:58.230","2018-10-19T22:41:58.230","SG","XBT",null,null,"CAST 071 APPLIED TO MB LINE 0368"]
["2018-10-20T02:53:39.370","2018-10-19T22:53:39.370","KJ","Ship",null,null,"7000 m to port at COG of 240"]
["2018-10-20T05:30:23.050","2018-10-20T01:30:23.050","KJ","Ship",null,null,"back on original line"]
["2018-10-20T06:58:34.160","2018-10-20T02:58:34.160","KJ","Ship",null,null,"2000 m to port at COG of 245"]
["2018-10-20T08:16:08.090","2018-10-20T04:16:08.090","JM","XBT",null,null,"Cast #072"]
["2018-10-20T08:18:43.150","2018-10-20T04:18:43.150","JM","XBT",null,null,"First cast was bad. Trying again"]
["2018-10-20T08:29:38.220","2018-10-20T04:29:38.220","JM","XBT",null,null,"Cast #072, redo"]
["2018-10-20T08:38:02.470","2018-10-20T04:38:02.470","JM","XBT",null,null,"Cast #072 applied to MB line 0374"]
["2018-10-20T08:45:38.630","2018-10-20T04:45:38.630","JM","Sonar","Multibeam","Ping Mode","Very Deep"]
["2018-10-20T09:18:28.840","2018-10-20T05:18:28.840","JM","Sonar","All","New Line","Begin turn. MB line 0376"]
["2018-10-20T09:45:49.050","2018-10-20T05:45:49.050","JM","Sonar","All","New Line","End turn. MB line 0377"]
["2018-10-20T10:40:18","2018-10-20T06:40:18","JM","Ship",null,null,"1200m to port at bearing 066"]
["2018-10-20T13:03:03.510","2018-10-20T09:03:03.510","JM","Ship",null,null,"Decrease speed to 7-7.5kts to see if improves bottom tracking"]
["2018-10-20T13:59:48.210","2018-10-20T09:59:48.210","JM","Ship",null,null,"Change course to 059"]
["2018-10-20T14:29:55.140","2018-10-20T10:29:55.140","SA","XBT",null,null,"Cast #073"]
["2018-10-20T14:36:22.310","2018-10-20T10:36:22.310","SA","XBT",null,null,"Cast 073 applied to MB line 0381"]
["2018-10-20T17:59:07.200","2018-10-20T13:59:07.200","MW","Sonar",null,null,"End ECS Surveym Line 0385"]
["2018-10-20T21:01:57.870","2018-10-20T17:01:57.870","AM","XBT",null,null,"cast #074 applied to MB line 0389"]
["2018-10-20T21:39:25.840","2018-10-20T17:39:25.840","CW","Ship",null,null,"Diverting for contact"]
["2018-10-21T01:26:31.850","2018-10-20T21:26:31.850","KJ","Sonar","Multibeam","Ping Mode","Changed from Very Deep to Auto"]
["2018-10-21T03:08:41.520","2018-10-20T23:08:41.520","AM","XBT",null,null,"Cast 075 applied to MB line 0396"]
["2018-10-21T09:49:15.210","2018-10-21T05:49:15.210","JM","XBT",null,null,"Cast # 076"]
["2018-10-21T09:57:36.630","2018-10-21T05:57:36.630","JM","XBT",null,null,"Cast # 076 applied to MB line 0402"]
["2018-10-21T11:35:44.360","2018-10-21T07:35:44.360","JM","Sonar",null,null,"Briefly paused the Knudsen and EK60 to see if the EM30 stb artifact would improve. It did not."]
["2018-10-21T14:04:17.450","2018-10-21T10:04:17.450","JM","Sonar","Multibeam","Aeration Filter (On/Off)","ON. Looking like its improving the outer beams"]
["2018-10-21T15:35:32.150","2018-10-21T11:35:32.150","CW","POS",null,null,"Pri. DGPS, GAMS Not Ready status; intermitent"]
["2018-10-21T18:49:09.080","2018-10-21T14:49:09.080","SA","XBT",null,null,"Cast #077"]
["2018-10-21T18:56:24.910","2018-10-21T14:56:24.910","SA","XBT",null,null,"Cast #077 applied to MB line 0411"]
["2018-10-22T01:30:33","2018-10-21T21:30:33","SG","XBT",null,null,"Cast 078"]
["2018-10-22T01:41:00.740","2018-10-21T21:41:00.740","SG","XBT",null,null,"CAST 078 APPLIED TO MB LINE 0418"]
["2018-10-22T08:43:31.270","2018-10-22T04:43:31.270","JM","XBT",null,null,"Cast #079"]
["2018-10-22T08:50:55.370","2018-10-22T04:50:55.370","JM","XBT",null,null,"Cast #079 applied to MB line 0425"]
["2018-10-22T13:19:42.230","2018-10-22T09:19:42.230","JM","Sonar","All","New Line","Begin turn MB line 0431"]
["2018-10-22T13:20:15.790","2018-10-22T09:20:15.790","JM","Sonar","Knudsen","Range",1000]
["2018-10-22T14:44:30.210","2018-10-22T10:44:30.210","CB","XBT",null,null,"Cast #080"]
["2018-10-22T14:53:25.330","2018-10-22T10:53:25.330","CB","Sonar",null,null,"stop and started subbottom/ multibeam line 4332-433"]
["2018-10-22T15:02:52.630","2018-10-22T11:02:52.630","CB","XBT",null,null,"cast #080 applied to line 0433"]
["2018-10-22T20:56:29.420","2018-10-22T16:56:29.420","CW","Sonar","All","New Line","New lines for new heading. MB line 0439"]
["2018-10-22T22:08:50.080","2018-10-22T18:08:50.080","CW","XBT",null,null,"AXBT 081; applied to MB line 0440"]
["2018-10-22T23:10:34","2018-10-22T19:10:34","CW","Sonar","Multibeam",null," Water Column goes red, Seabed Image has blippy lines, but Geographic looks okay. I thinhk this is the same thing Kevin described this earlier. I've never seen it before. Time for some Mary J. Blige."]
["2018-10-23T06:52:35.400",{"$f":"IF(ISBLANK(A530),\" \",((A530)-DATE(1970,1,1))+25569-($C$1/24))","v":"2018-10-23T02:52:35.400"},"JM","XBT",null,null,"Cast #082"]
["2018-10-23T06:59:44.150","2018-10-23T02:59:44.150","JM","XBT",null,null,"Cast #082 applied to MB line 0449"]
["2018-10-23T09:47:24.660","2018-10-23T05:47:24.660","JM","Sonar","All","New Line","Turn to approach the trench. MB line 0452. "]
["2018-10-23T10:04:19.320","2018-10-23T06:04:19.320","JM","Sonar","Knudsen","Tx Power","Set to 4. Wake up!"]
["2018-10-23T11:08:44.460","2018-10-23T07:08:44.460","JM","Sonar","Multibeam","Max Angle","set to 20"]
["2018-10-23T11:43:55.200","2018-10-23T07:43:55.200","JM","Sonar","Multibeam","Max Angle","set to 15"]
["2018-10-23T12:14:06.840","2018-10-23T08:14:06.840","JM","Sonar","Multibeam","Max Angle","set to 20/15"]
["2018-10-23T12:23:28.370","2018-10-23T08:23:28.370","JM","Sonar","Multibeam","Max Angle","set to 15"]
["2018-10-23T12:55:31.390","2018-10-23T08:55:31.390","JM","XBT",null,null,"Cast #083"]
["2018-10-23T13:02:27.670","2018-10-23T09:02:27.670","JM","Sonar","Multibeam","Max Angle","set to 10"]
["2018-10-23T13:07:08.270","2018-10-23T09:07:08.270","JM","XBT",null,null,"Cast #083 applied to MB line 0455"]
["2018-10-23T14:03:21.970","2018-10-23T10:03:21.970","JM","Sonar","Multibeam","Max Angle","set to 12"]
["2018-10-23T14:16:21.160","2018-10-23T10:16:21.160","JM","Sonar","Multibeam","Max Angle","set to 20"]
["2018-10-23T14:54:19.860","2018-10-23T10:54:19.860","CB",null,null,null,"0458 stern thruster testing"]
["2018-10-23T15:10:50.680","2018-10-23T11:10:50.680","CB","Sonar","Multibeam",null,"0459 stern thruster test over back on course"]
["2018-10-23T20:01:56","2018-10-23T16:01:56","MW","Sonar","Multibeam","Secure","Major EM302 failure at start of MB file 0464 - spent the next several hours swapping boards and troubleshooting with support from KM Lynnwood.  Net result: swapped out 12 V power supply; TX board in slot 17 (18th board) was showing Low Voltage repeatedly, and followed the board to different slots during swaps; put the board from slot 0 into slot 17 (removed the board from slot 17 altogether) and put a brand new spare TX board in slot 0; this fixed the TX Channels BIST failures.  System was not pinging and it was discovered that EXTERNAL TRIGGER had been turned ON at some point in the troubleshooting.  This was turned OFF and the system started pinging normally."]
["2018-10-23T23:41:49.240","2018-10-23T19:41:49.240","KJ","Sonar","Multibeam",null,"pinging and logging en route to acc crossline"]
["2018-10-23T23:43:00.120","2018-10-23T19:43:00.120","KJ","XBT",null,null,"XBT 084 launched"]
["2018-10-23T23:53:09.680","2018-10-23T19:53:09.680","KJ","Sonar","EK","Secure","EK and Knudsen secure for EM302 MEDIUM accuracy crossline"]
["2018-10-24T00:12:35.620","2018-10-23T20:12:35.620","KJ","Sonar","Multibeam",null,"XBT084 applied earlier in line 0465"]
["2018-10-24T00:13:08.110","2018-10-23T20:13:08.110","KJ","Sonar","Multibeam","New Line","MB line 0466 MEDIUM accuracy crossline 1"]
["2018-10-24T00:25:05.820","2018-10-23T20:25:05.820","KJ","Sonar","Multibeam","Pen. Filter Strength","Off to Weak to fix nadir tracking on slope with soft sediments"]
["2018-10-24T00:41:01.020","2018-10-23T20:41:01.020","KJ","Sonar","Multibeam","New Line","0467 for turn"]
["2018-10-24T00:55:39.320","2018-10-23T20:55:39.320","KJ","Sonar","Multibeam","New Line","0468 MEDIUM accuracy crossline 2"]
["2018-10-24T01:26:10.030","2018-10-23T21:26:10.030","KJ","Sonar","Multibeam","New Line","0469 turn to start of reference surface"]
["2018-10-24T01:45:56.710","2018-10-23T21:45:56.710","KJ","Sonar","Multibeam","Max Angle","from 75/75 during crossline to 65/65 for reference surface with tight spacing"]
["2018-10-24T01:53:14.430","2018-10-23T21:53:14.430","KJ","Sonar","Multibeam","New Line","470 first line of reference surface"]
["2018-10-24T02:03:39.750","2018-10-23T22:03:39.750","KJ","Ship",null,null,"Increasing speed from 7.5-8 to 8.5"]
["2018-10-24T02:19:15.760","2018-10-23T22:19:15.760","KJ","Sonar","Multibeam","New Line","471 turn"]
["2018-10-24T02:30:26.040","2018-10-23T22:30:26.040","KJ","Sonar","Multibeam","New Line","472 survey line, increasing speed to 9 kts"]
["2018-10-24T02:52:42.710","2018-10-23T22:52:42.710","KJ","Sonar","Multibeam","New Line","473 turn"]
["2018-10-24T02:57:40.750","2018-10-23T22:57:40.750","KJ","Sonar","Multibeam","New Line","474 survey line"]
["2018-10-24T03:22:48.590","2018-10-23T23:22:48.590","KJ","Sonar","Multibeam","New Line","475 turn"]
["2018-10-24T03:31:55.560","2018-10-23T23:31:55.560","KJ","Sonar","Multibeam","New Line","476 survey line"]
["2018-10-24T03:55:09.580","2018-10-23T23:55:09.580","KJ","XBT",null,null,"XBT085 launched"]
["2018-10-24T03:58:11.910","2018-10-23T23:58:11.910","KJ","Sonar","Multibeam","New Line","0477 turn"]
["2018-10-24T03:58:34.870","2018-10-23T23:58:34.870","KJ","Sonar","Multibeam",null,"XBT085 applied in line 0477"]
["2018-10-24T04:03:40.460","2018-10-24T00:03:40.460","KJ","Sonar","Multibeam","New Line","0478 survey line"]
["2018-10-24T04:28:08.180","2018-10-24T00:28:08.180","KJ","Sonar","Multibeam","New Line","0479 turn"]
["2018-10-24T04:36:55.290","2018-10-24T00:36:55.290","KJ","Sonar","Multibeam","New Line","0480 survey line"]
["2018-10-24T05:01:16.050","2018-10-24T01:01:16.050","KJ","Sonar","Multibeam","New Line","0481 turn"]
["2018-10-24T05:09:21.400","2018-10-24T01:09:21.400","KJ","Sonar","Multibeam","New Line","0482 survey line"]
["2018-10-24T05:34:39.630","2018-10-24T01:34:39.630","KJ","Sonar","Multibeam","New Line","0483 turn"]
["2018-10-24T05:44:19.160","2018-10-24T01:44:19.160","KJ","Sonar","Multibeam","New Line","0484 survey line"]
["2018-10-24T06:09:44.320","2018-10-24T02:09:44.320","KJ","Sonar","Multibeam","New Line","End medium accuracy reference surface.  New line 0485 start of transit to San Juan (short line to start of RX Noise BIST vs speed testing…)"]
["2018-10-24T06:10:38.560","2018-10-24T02:10:38.560","KJ","Ship",null,null,"Slowing down to 0 kts for speed noise test"]
["2018-10-24T06:14:46.700","2018-10-24T02:14:46.700","KJ","Sonar","Multibeam",null,"Secure for RX Noise BIST testing"]
["2018-10-24T07:49:17.800","2018-10-24T03:49:17.800","KJ","Sonar","Multibeam",null,"Finished with RX Noise BIST testing (0-10 kts in 1-kt increments), now pinging again en route to 'sea buoy'"]
["2018-10-24T07:51:05.490","2018-10-24T03:51:05.490","KJ","Sonar","All","New Line","MB line 0486, all sonars now logging en route to 'sea buoy'"]
["2018-10-24T08:24:05.970","2018-10-24T04:24:05.970","KJ","Ship",null,null,"Maneuvering around traffic, variable speeds"]
["2018-10-24T09:07:40.070","2018-10-24T05:07:40.070","KJ","Sonar","All","Secure","Arriving at setup point for entry to San Juan; final MB line is 0487"]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A595),\" \",((A595)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A603),\" \",((A603)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A659),\" \",((A659)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A723),\" \",((A723)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A787),\" \",((A787)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A851),\" \",((A851)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A915),\" \",((A915)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A979),\" \",((A979)-DATE(1970,1,1))+25569-($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1014),\" \",((A1014)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1039),\" \",((A1039)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1103),\" \",((A1103)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1167),\" \",((A1167)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1231),\" \",((A1231)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1295),\" \",((A1295)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1359),\" \",((A1359)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1423),\" \",((A1423)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1487),\" \",((A1487)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1551),\" \",((A1551)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1615),\" \",((A1615)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1679),\" \",((A1679)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1743),\" \",((A1743)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1807),\" \",((A1807)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1871),\" \",((A1871)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1935),\" \",((A1935)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null,{"$f":"IF(ISBLANK(A1999),\" \",((A1999)-DATE(1970,1,1))+25569+($C$1/24))","v":" "}]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]

{"sheet":"DropDowns","index":1,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Watchstanders","Note","Sonar","Multibeam","EK60","Knudsen","All"]
["MW","Sonar","Multibeam","Ping Mode","Change Range","Tx Power","Start up"]
["DS","Ship","EK","Along Direction Pitch","Start Pinging","Tx Pulse","Secure"]
["KJ","Weather","Knudsen","New Line","Secure","Gain Mode","New Line"]
["JM","Watch Change","All","Max Angle",null,"Gain Value"]
["CW","XBT",null,"Spike Filter Strength",null,"Process Shift"]
["SG","Issue/Problem",null,"Slope Filter (On/Off)",null,"Tx Blanking"]
["CB","Other",null,"Aeration Filter (On/Off)",null,"Range"]
["SA",null,null,"Interference Filter (On/Off)",null,"Phase Mode"]
["AM",null,null,"Pen. Filter Strength",null,"Start Pinging"]
[null,null,null,"Start Pinging",null,"Secure"]
[null,null,null,"Secure",null,"Phase Range"]
[null,null,null,"Start Logging"]